
HM2-TRAFFICMGMT-MIB DEFINITIONS ::= BEGIN

--
-- *************************************************************
-- Hirschmann Traffic Management MIB
-- *************************************************************
--
IMPORTS
    MODULE-IDENTITY,
    OBJECT-TYPE,
    Unsigned32					FROM SNMPv2-SMI -- RFC 2578
    ifIndex             		FROM IF-MIB
    hm2ConfigurationMibs,
    HmEnabledStatus             FROM HM2-TC-MIB;

hm2TrafficMgmtMib MODULE-IDENTITY
    LAST-UPDATED "201103160000Z" -- March 16, 2011
    ORGANIZATION "Hirschmann Automation and Control GmbH"
    CONTACT-INFO
        "Postal:     Stuttgarter Str. 45-51
                     72654 Neckartenzlingen
                     Germany
         Phone:      +49 7127 140
         E-mail:     hac.support@belden.com"
    DESCRIPTION
        "Hirschmann Traffic Management MIB.
         Copyright (C) 2011. All Rights Reserved."
    REVISION     "201103160000Z" -- March 16, 2011
    DESCRIPTION
         "Initial version."
    ::= { hm2ConfigurationMibs 31 }

--
-- *************************************************************
-- hm2TrafficMgmtMib
-- *************************************************************
--
hm2TrafficMgmtMibNotifications		OBJECT IDENTIFIER ::= { hm2TrafficMgmtMib 0 }
hm2TrafficMgmtMibObjects			OBJECT IDENTIFIER ::= { hm2TrafficMgmtMib 1 }
-- hm2TrafficMgmtMibConformance			OBJECT IDENTIFIER ::= { hm2TrafficMgmtMib 2 }
hm2TrafficMgmtMibExtensionGroup		OBJECT IDENTIFIER ::= { hm2TrafficMgmtMib 3 }

--
-- *************************************************************
-- hm2TrafficTable
-- *************************************************************
--

hm2TrafficMgmtIfTable OBJECT-TYPE
	SYNTAX SEQUENCE OF Hm2TrafficMgmtIfEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION "A list of management objects for traffic control per interface."
	::= { hm2TrafficMgmtMibObjects 1 }

hm2TrafficMgmtIfEntry OBJECT-TYPE
	SYNTAX Hm2TrafficMgmtIfEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION "Traffic Mgmt table entry."
	INDEX { ifIndex }
	::= { hm2TrafficMgmtIfTable 1 }

Hm2TrafficMgmtIfEntry ::= SEQUENCE {
						 hm2TrafficMgmtIfFlowControl 						HmEnabledStatus,
						 hm2TrafficMgmtIfEgressShapingRate					Unsigned32,
						 hm2TrafficMgmtIfEgressShapingRateUnit				INTEGER,
 					     hm2TrafficMgmtIfIngressStormCtlThresholdUnit 		INTEGER,
						 hm2TrafficMgmtIfIngressStormCtlBcastMode			HmEnabledStatus,
						 hm2TrafficMgmtIfIngressStormCtlBcastThreshold		Unsigned32,
						 hm2TrafficMgmtIfIngressStormCtlMcastMode			HmEnabledStatus,
						 hm2TrafficMgmtIfIngressStormCtlMcastThreshold		Unsigned32,
						 hm2TrafficMgmtIfIngressStormCtlUcastMode			HmEnabledStatus,
						 hm2TrafficMgmtIfIngressStormCtlUcastThreshold		Unsigned32 
						}

hm2TrafficMgmtIfFlowControl OBJECT-TYPE
	SYNTAX 			HmEnabledStatus
	MAX-ACCESS 		read-write
	STATUS 		 	current
	DESCRIPTION		"Enables or disables flow control per port"
	DEFVAL  		{ enable }
	::= { hm2TrafficMgmtIfEntry 1 }

hm2TrafficMgmtIfEgressShapingRate OBJECT-TYPE
	SYNTAX      	Unsigned32 
    MAX-ACCESS  	read-write
    STATUS     		current
    DESCRIPTION     "Maximum bandwidth allowed for this interface as a 
                     whole, typically used to shape the outbound 
                     transmission rate. The value is either specified in terms 
                     of percentage of overall link speed for the port in 
                     1% increments or absolute in kbps. 
                     A value of 0 means there is no maximum bandwidth limit 
                     in effect. The default value is 0.
                     Valid value ranges depend on the value returned by 
                     object hm2TrafficMgmtIfEgressShapingRateUnit. If that 
                     object returns percent(1), hm2TrafficMgmtIfEgressShapingRate
                     accepts values 0..100.  If that object returns kbps(2),
                     hm2TrafficMgmtIfEgressShapingRate accepts values 
                     0,64..4294967295."
	DEFVAL 			{ 0 }	
	::= { hm2TrafficMgmtIfEntry 2 }
	
hm2TrafficMgmtIfEgressShapingRateUnit OBJECT-TYPE
    SYNTAX      	INTEGER {
                   		percent(1),
                   		kbps(2)
                	}
	MAX-ACCESS  	read-only
    STATUS      	current
    DESCRIPTION
                    "The unit of the interface shaping value.
                     Can be either percentage of port speed 
                     or kilobits per second (kbps)."
	DEFVAL 			{ percent }
    ::= { hm2TrafficMgmtIfEntry 3 }


hm2TrafficMgmtIfIngressStormCtlThresholdUnit OBJECT-TYPE
         SYNTAX      INTEGER {
                     percent(1),
                     pps(2)
                  }
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "Configures the units of the threshold value(s) to percentage of
                     port speed or absolute packets per second."
         DEFVAL { percent }
         ::= { hm2TrafficMgmtIfEntry 4}

     
hm2TrafficMgmtIfIngressStormCtlBcastMode OBJECT-TYPE
	SYNTAX      	HmEnabledStatus
    MAX-ACCESS  	read-write
    STATUS      	current
    DESCRIPTION
                     "If enabled, broadcast storm recovery will function on this port.
                     When you specify Enable for Broadcast Storm Recovery and the broadcast
                     traffic on this Ethernet port exceeds the configured threshold, the
                     switch blocks (discards) the broadcast traffic."
    DEFVAL 		{ disable }
    ::= { hm2TrafficMgmtIfEntry 5 }      
    

hm2TrafficMgmtIfIngressStormCtlBcastThreshold OBJECT-TYPE
	SYNTAX      	Unsigned32 (0..14880000)
   	MAX-ACCESS 		read-write
   	STATUS      	current
   	DESCRIPTION
                    "Configures the broadcast storm recovery threshold for this port
                     as a percentage of port speed in 1% increments or as an absolute pps rate.
                     This threshold is also valid for multicasts or unknown unicasts,
                     when the device does not support a separate limiter per storm type.
                     (A separate limiter per storm-type is supported when 
                      hm2TrafficMgmtIngressStormBucketType has the value 'multi-bucket')"
	DEFVAL 			{ 0 }
   ::= { hm2TrafficMgmtIfEntry 6 }

                    
hm2TrafficMgmtIfIngressStormCtlMcastMode OBJECT-TYPE
	SYNTAX      	HmEnabledStatus
    MAX-ACCESS  	read-write
    STATUS      	current
    DESCRIPTION
                     "If enabled, multicast storm recovery will function on this port.
                     When you specify Enable for multicast Storm Recovery and the multicast
                     traffic on this Ethernet port exceeds the configured threshold, the
                     switch blocks (discards) the multicast traffic."
    DEFVAL 		{ disable }
    ::= { hm2TrafficMgmtIfEntry 7 }      
    

hm2TrafficMgmtIfIngressStormCtlMcastThreshold OBJECT-TYPE
	SYNTAX      	Unsigned32 (0..14880000)
   	MAX-ACCESS 		read-write
   	STATUS      	current
   	DESCRIPTION
                    "Configures the multicast storm recovery threshold for this port
                     as a percentage of port speed in 1% increments or as an absolute pps rate."
	DEFVAL 			{ 0 }
   ::= { hm2TrafficMgmtIfEntry 8 }

                  
hm2TrafficMgmtIfIngressStormCtlUcastMode OBJECT-TYPE
	SYNTAX      	HmEnabledStatus
    MAX-ACCESS  	read-write
    STATUS      	current
    DESCRIPTION
                     "If enabled, unknown unicast storm recovery will function on this port.
                     When you specify Enable for unicast Storm Recovery and the unknown 
                     unicast traffic on this Ethernet port exceeds the configured threshold, the
                     switch blocks (discards) the unknown unicast traffic."
    DEFVAL 		{ disable }
    ::= { hm2TrafficMgmtIfEntry 9 }      
    

hm2TrafficMgmtIfIngressStormCtlUcastThreshold OBJECT-TYPE
	SYNTAX      	Unsigned32 (0..14880000)
   	MAX-ACCESS 		read-write
   	STATUS      	current
   	DESCRIPTION
                    "Configures the unicast storm recovery threshold for this port
                     as a percentage of port speed in 1% increments or as an absolute pps rate."
	DEFVAL 			{ 0 }
   ::= { hm2TrafficMgmtIfEntry 10 }

        
--
-- *************************************************************
-- hm2TrafficMgmt Objects
-- *************************************************************
--

hm2TrafficMgmtFlowControl OBJECT-TYPE
	  SYNTAX HmEnabledStatus
	  MAX-ACCESS read-write
	  STATUS	 current
      DESCRIPTION
	        	 "Enables or disables flow control for the
	             switch unit."
	  DEFVAL  { disable }
	  ::= { hm2TrafficMgmtMibObjects 2 }

hm2TrafficMgmtIngressStormBucketType OBJECT-TYPE
	  SYNTAX  INTEGER {
                  single-bucket(1),
                  multi-bucket(2)
              }
	  MAX-ACCESS read-only
	  STATUS	 current
	  DESCRIPTION
			"Enables or disables ingress storm admin state."
	  ::= { hm2TrafficMgmtMibObjects 3 }

--
--***************************************************************************
-- hm2TrafficMgmtMibExtensionGroup
--***************************************************************************

hm2TrafficMgmtNoFlowControl OBJECT-IDENTITY
	  STATUS        current
	  DESCRIPTION  "Do not change the flowcontrol settings for the Fast/Gigabit Ethernet SFP ports."
	  ::= { hm2TrafficMgmtMibExtensionGroup 1 }

END
