
HM2-TIMESYNC-MIB DEFINITIONS ::= BEGIN

--
-- *************************************************************
-- Hirschmann Time Sync MIB
-- *************************************************************
--

IMPORTS
    MODULE-IDENTITY, 
    OBJECT-TYPE,
    NOTIFICATION-TYPE,
	OBJECT-IDENTITY,
    Integer32					FROM SNMPv2-SMI -- RFC 2578
    TEXTUAL-CONVENTION,
    DisplayString,
    TruthValue, RowStatus       FROM SNMPv2-TC
    InetAddressType, 
    InetAddress,
	InetPortNumber              FROM INET-ADDRESS-MIB -- RFC4001  
    HmEnabledStatus,
    hm2ConfigurationMibs,
    HmTimeSeconds1970	        FROM HM2-TC-MIB
    InterfaceIndexOrZero,
    ifIndex     				FROM IF-MIB;

hm2TimeSyncMib MODULE-IDENTITY
	LAST-UPDATED "201809070000Z" -- Sep 07, 2018
    ORGANIZATION "Hirschmann Automation and Control GmbH"
    CONTACT-INFO
        "Postal:     Stuttgarter Str. 45-51
                     72654 Neckartenzlingen
                     Germany
         Phone:      +49 7127 140
         E-mail:     hac.support@belden.com"
    DESCRIPTION
        "Hirschmann Time Sync MIB.
         Copyright (C) 2011. All Rights Reserved."
    REVISION     "201809070000Z" -- Sep 07, 2018
    DESCRIPTION
         "Initial version."
    ::= { hm2ConfigurationMibs 50 }

--
-- *************************************************************
-- Textual Conventions                                          
-- *************************************************************
--
HmSntpClientServerStatus ::= TEXTUAL-CONVENTION
    STATUS current
    DESCRIPTION
        "The status of the last received response from a
         configured server.

          other
            - None of the following enumeration values.

          success
            - The SNTP operation was successful and the system time
              was updated.

          requestTimedOut
            - An SNTP poll request timed out without receiving a
              response from the SNTP server.

          badDateEncoded
            - The time provided by the SNTP server was not valid.

          versionNotSupported
            - The SNTP version supported by the server is not compatible
              with the version supported by the client. This is indicated
              by the server returning a version later than the version
              configured for that server or a version of '0'.

          serverUnsychronized
            - The SNTP server is not synchronized with its peers.  This
              is indicated via the 'leap indicator' field on the SNTP
              message.

          serverKissOfDeath
            - The SNTP server indicated that no further polls are to be
              sent to this server. This is indicated by a stratum field
              field equal to 0 in a message received from a server."

    REFERENCE
        "RFC 4330 - Simple Network Time Protocol (SNTP) Version 4
                    for IPv4, IPv6 and OSI; Section 4."
    SYNTAX INTEGER {
      other(1),
      success(2),
      requestTimedOut(3),
      badDateEncoded(4),
      versionNotSupported(5),
      serverUnsychronized(6),
      serverKissOfDeath(7)
    }
    
Hm2Ptp2LogSyncIntervalTc ::= TEXTUAL-CONVENTION
		STATUS current
		DESCRIPTION
			"Logarithm to the base of 2 of the mean synchronization interval."
		SYNTAX 		INTEGER {
							msec-125 (-3),
							msec-250 (-2),
							msec-500 (-1),
							sec-1 (0),
							sec-2 (1)
							}
Hm2Ptp2LogPdelayReqIntervalTc ::= TEXTUAL-CONVENTION
		STATUS current
		DESCRIPTION
			"Logarithm to the base of 2 of the minimum PDelay Request interval (used for p2p-delay)."
		SYNTAX 		INTEGER {
							sec-1 (0),
							sec-2 (1),
							sec-4 (2),
							sec-8 (3),
							sec-16 (4),
							sec-32 (5)
							}
PtpTimeInterval ::= TEXTUAL-CONVENTION
    STATUS       current
    DESCRIPTION
			"The scaledNanoseconds member is the time interval expressed in units of nanoseconds and multiplied by
			 2^+16. Positive or negative time intervals outside the maximum range of this data type shall be encoded as the
			 largest positive and negative values of the data type respectively.
			 For example: 2.5 ns is expressed as: (hex) 0x0000 0000 0002 8000"
	REFERENCE
			"IEEE 1588-2008 Standard for a Precision Clock
			 Synchronization Protocol for Networked
			 Measurement and Control Systems"			 
    SYNTAX   OCTET STRING (SIZE (8))

PtpTimeStamp ::= TEXTUAL-CONVENTION
   STATUS current
   DESCRIPTION
      "first 48 bit: seconds since 1.1.1970
      last 32 bit: nanoseconds"
   REFERENCE 
      "IEEE P1588 Standard "
   SYNTAX OCTET STRING (SIZE (10))
   
PtpPortIdentity ::= TEXTUAL-CONVENTION
    STATUS       current
    DESCRIPTION
			"The PtpPortIdentity type identifies a PTP port.
			 The first 8 octets within this value specifies the ClockIdentity.
			 The last 2 octets within this value specifies the port number.
			 For example: '00 80 63 FF FF 00 00 00 00 01'. ClockIdentity is
			 '008063FFFF000000' and port number is '0001'"
	REFERENCE
			"IEEE 1588-2008 Standard for a Precision Clock
			 Synchronization Protocol for Networked
			 Measurement and Control Systems"
    SYNTAX   OCTET STRING (SIZE (10))

PtpClockIdentity ::= TEXTUAL-CONVENTION
    STATUS       current
    DESCRIPTION
			"The PtpClockIdentity type identifies a PTP clock.
			 The PtpClockIdentity shall be in the IEEE EUI-64
			 format.
			 For example: '008063FFFF000000'"
	REFERENCE
			"IEEE 1588-2008 Standard for a Precision Clock
			 Synchronization Protocol for Networked
			 Measurement and Control Systems"
    SYNTAX   OCTET STRING (SIZE (8))

PtpClockQuality ::= TEXTUAL-CONVENTION
    STATUS       current
    DESCRIPTION
			"The PtpClockQuality represents the quality of a clock.
			 The first octet represents the clock class. The second
			 octet represents the clockAccuracy and the last two octets
			 represent the offsetScaledLogVariance
			 For example: "
	REFERENCE
			"IEEE 1588-2008  Standard for a Precision Clock
			 Synchronization Protocol for Networked
			 Measurement and Control Systems"
    SYNTAX   OCTET STRING (SIZE (4))

--
-- *************************************************************
-- hm2TimeSyncMib
-- *************************************************************
--
hm2TimeSyncMibNotifications			OBJECT IDENTIFIER ::= { hm2TimeSyncMib 0 }
hm2TimeSyncMibObjects				OBJECT IDENTIFIER ::= { hm2TimeSyncMib 1 }
-- hm2TimeSyncMibConformance			OBJECT IDENTIFIER ::= { hm2TimeSyncMib 2 }
hm2TimeSyncMibSNMPExtensionGroup 	OBJECT IDENTIFIER ::= { hm2TimeSyncMib 3 }

--
-- *************************************************************
-- hm2TimeSyncMib groups
-- *************************************************************
--
hm2SystemTimeGroup OBJECT IDENTIFIER ::= { hm2TimeSyncMibObjects 1 }
hm2SntpGroup       OBJECT IDENTIFIER ::= { hm2TimeSyncMibObjects 2 }
hm2NtpGroup        OBJECT IDENTIFIER ::= { hm2TimeSyncMibObjects 3 }
hm2PtpGroup        OBJECT IDENTIFIER ::= { hm2TimeSyncMibObjects 4 }
hm2IrigGroup       OBJECT IDENTIFIER ::= { hm2TimeSyncMibObjects 5 }
hm2Dot1asGroup     OBJECT IDENTIFIER ::= { hm2TimeSyncMibObjects 6 }

--
-- *************************************************************
-- hm2SystemTimeGroup
-- *************************************************************
--
hm2SystemUtcTime OBJECT-TYPE
			SYNTAX			 HmTimeSeconds1970		
			MAX-ACCESS		 read-write
			STATUS			 current
			DESCRIPTION
				"Time measured in seconds since 00:00:00 UTC, January 1, 1970.
				 The clock of the device may be set using this variable."
			::= { hm2SystemTimeGroup 1 }

hm2SystemTimeSource OBJECT-TYPE
			SYNTAX			 INTEGER {
							  local (1),
							  sntp  (2),
							  ntp   (3),
							  ptp   (4),
							  gps   (5)
							 }		
			MAX-ACCESS		 read-only
			STATUS			 current
			DESCRIPTION
				"Shows the source of the system time."
			::= { hm2SystemTimeGroup 2 }
			
hm2SystemLocalTime OBJECT-TYPE
			SYNTAX			 HmTimeSeconds1970		
			MAX-ACCESS		 read-write
			STATUS			 current
			DESCRIPTION
				"The current local time. This includes the timezone offset and if supported summertime offset.
				 Measured in seconds since 00:00:00, January 1, 1970."
			::= { hm2SystemTimeGroup 3 }			
			
hm2SystemLocalOffset OBJECT-TYPE
			SYNTAX Integer32 (-780..840)
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
			"The difference between the local timezone and UTC in minutes."
			DEFVAL { 60 }			
			::= { hm2SystemTimeGroup 4 }
			
--
-- *************************************************************
-- hm2Sntp groups
-- *************************************************************
--
hm2SntpServerGroup  		OBJECT IDENTIFIER ::= { hm2SntpGroup 1 }
hm2SntpServerBroadcastGroup  	OBJECT IDENTIFIER ::= { hm2SntpGroup 2 }
hm2SntpClientGroup  		OBJECT IDENTIFIER ::= { hm2SntpGroup 3 }

--
-- *************************************************************
-- hm2SNTPServer group
-- *************************************************************
--
hm2SntpServerAdminState OBJECT-TYPE
   SYNTAX 		HmEnabledStatus
   MAX-ACCESS 	read-write
   STATUS     	current
   DESCRIPTION
       			"Enables/disables SNTP server admin mode."
   DEFVAL { disable }       
   ::= { hm2SntpServerGroup 1 }

hm2SntpServerPort  OBJECT-TYPE
   SYNTAX 		InetPortNumber (1..65535)
   MAX-ACCESS 	read-write
   STATUS 		current
   DESCRIPTION
       			"The local port number used to listen for client requests."
   DEFVAL { 123 }       
   ::= { hm2SntpServerGroup 2 }

hm2SntpServerOnlyIfSync OBJECT-TYPE
   SYNTAX 		HmEnabledStatus
   MAX-ACCESS 	read-write
   STATUS     	current
   DESCRIPTION
       			"The SNTP server is enabled only if synchronized
       			 to another external time reference. (e.g. NTP or PTP)."
   REFERENCE
           		"RFC4330 - 6.  SNTP Server Operations"
   DEFVAL { disable }       
   ::= { hm2SntpServerGroup 3 }

hm2SntpServerStatus OBJECT-TYPE
   SYNTAX INTEGER {
      				disabled (1),
      			    notSynchronized(2),
                    syncToLocal(3),
                    syncToRefclock(4),
                    syncToRemoteServer(5)
				   }
   MAX-ACCESS 	read-only
   STATUS 		current
   DESCRIPTION
       			"Operational status of the SNTP server."
   ::= { hm2SntpServerGroup 4 }

hm2SntpServerInterface OBJECT-TYPE
   SYNTAX      InterfaceIndexOrZero
   MAX-ACCESS 	read-write
   STATUS 		current
   DESCRIPTION
       			"Interface used by the SNTP server."
   DEFVAL { 0 }
   ::= { hm2SntpServerGroup 5 }
   
--
-- *************************************************************
-- hm2SNTPServerBroadcast group
-- *************************************************************
--
hm2SntpServerBroadcastAdminState OBJECT-TYPE
   SYNTAX 		HmEnabledStatus
   MAX-ACCESS 	read-write
   STATUS     	current
   DESCRIPTION
		"Enables/disables SNTP server broadcast admin mode."
   DEFVAL { disable }       
   ::= { hm2SntpServerBroadcastGroup 1 }

hm2SntpServerBroadcastAddrType OBJECT-TYPE
   SYNTAX     InetAddressType
   MAX-ACCESS read-write
   STATUS     current
   DESCRIPTION
       "Address type."
   DEFVAL { ipv4 }         
   ::= { hm2SntpServerBroadcastGroup 2 }

hm2SntpServerBroadcastAddr  OBJECT-TYPE
   SYNTAX     InetAddress
   MAX-ACCESS read-write
   STATUS     current
   DESCRIPTION
       "Destination address for SNTP broadcast or
        multicast."
   DEFVAL {  '00000000'h } 
   ::= { hm2SntpServerBroadcastGroup 3 }

hm2SntpServerBroadcastPort  OBJECT-TYPE
   SYNTAX 		InetPortNumber (1..65535)
   MAX-ACCESS 	read-write
   STATUS 		current
   DESCRIPTION
		"The port number to send the broadcast packets
		 to the clients."
   DEFVAL { 123 }       
   ::= { hm2SntpServerBroadcastGroup 4 }

hm2SntpServerBroadcastInterval OBJECT-TYPE
   SYNTAX     Integer32 (64..1024)
   MAX-ACCESS read-write
   STATUS     current
   DESCRIPTION
		"Interval of SNTP broadcast messages send in seconds."
   REFERENCE
		"RFC4330 - 6.  SNTP Server Operations"
   DEFVAL  { 128 }        
   ::= { hm2SntpServerBroadcastGroup 5 }

hm2SntpServerBroadcastVlanTable OBJECT-TYPE
   SYNTAX SEQUENCE OF Hm2SntpServerBroadcastVlanEntry
   MAX-ACCESS 		not-accessible
   STATUS 			current
   DESCRIPTION
		"This table contains all VLANs used for SNTP server 
		broadcast or multicast messages."
   ::= { hm2SntpServerBroadcastGroup 10 }

hm2SntpServerBroadcastVlanEntry OBJECT-TYPE
   SYNTAX 		Hm2SntpServerBroadcastVlanEntry
   MAX-ACCESS 	not-accessible
   STATUS 		current
   DESCRIPTION 
		"The SNTP broadcast server VLAN objects."
   INDEX { hm2SntpServerBroadcastVlan }
   ::= { hm2SntpServerBroadcastVlanTable 1 }

Hm2SntpServerBroadcastVlanEntry ::= SEQUENCE {
   hm2SntpServerBroadcastVlan 						Integer32,
   hm2SntpServerBroadcastVlanRowStatus		RowStatus
   }

-- *************************************************************
-- hm2SntpServerBroadcastVlanEntry
-- *************************************************************
hm2SntpServerBroadcastVlan OBJECT-TYPE
   SYNTAX 			Integer32 (1..4042)
   MAX-ACCESS 		read-only
   STATUS 			current
   DESCRIPTION
		"VLAN used for SNTP server broadcast or multicast messages."
   ::= { hm2SntpServerBroadcastVlanEntry 1 }
   
hm2SntpServerBroadcastVlanRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
		"Indicates the status of an entry in this table,
		 and is used to create/delete entries. Objects
		 within this table can by changed while the status
		 is 'active'."
    ::= { hm2SntpServerBroadcastVlanEntry 2 }

--   
-- *************************************************************
-- hm2SntpClient group
-- *************************************************************
--
hm2SntpClientAdminState OBJECT-TYPE
   SYNTAX 		HmEnabledStatus
   MAX-ACCESS 	read-write
   STATUS     	current
   DESCRIPTION
		"Enables/disables the SNTP client admin mode."
   DEFVAL { disable }       
   ::= { hm2SntpClientGroup 1 }

hm2SntpClientOperatingMode OBJECT-TYPE
   SYNTAX 		INTEGER {
      					 unicast (1),
     					 broadcast (2)
   						}
   MAX-ACCESS 	read-write
   STATUS 		current
   DESCRIPTION
		"Enables/disables SNTP client operating mode. 
		 In 'unicast' mode, the client sends a request
		 to a designated unicast server and expects a
		 reply from that server.
		 In 'broadcast' client mode, it sends no request and waits for
		 a broadcast from one or more broadcast servers."
   REFERENCE
        "RFC4330 - 5.  SNTP Client Operations"
   DEFVAL { unicast }
   ::= { hm2SntpClientGroup 2 }

hm2SntpClientDisableAfterSync OBJECT-TYPE
   SYNTAX 		HmEnabledStatus
   MAX-ACCESS 	read-write
   STATUS     	current
   DESCRIPTION
		"When set to 'enable' the SNTP client is
		 disabled after the device is synchronized the first
		 time successfully to a SNTP server."
   DEFVAL { disable }       
   ::= { hm2SntpClientGroup 3 }

hm2SntpClientRequestInterval    OBJECT-TYPE
   SYNTAX     	Integer32 (5..3600)
   MAX-ACCESS 	read-write
   STATUS     	current
   DESCRIPTION
		"SNTP client request interval in seconds."
   DEFVAL  { 30 }         
   ::= { hm2SntpClientGroup 4 }

hm2SntpClientStatus OBJECT-TYPE
   SYNTAX INTEGER {
      				disabled (1),
      			    notSynchronized(2),
                    synchronizedToRemoteServer(5)
   				  }
   MAX-ACCESS 	read-only
   STATUS 		current
   DESCRIPTION
		"Overall operational status of the SNTP client."
   ::= { hm2SntpClientGroup 5 }

hm2SntpClientBroadcastRecvTimeout    OBJECT-TYPE
   SYNTAX     	Integer32 (128..2048)
   MAX-ACCESS 	read-write
   STATUS     	current
   DESCRIPTION
		"Time in seconds after the client in broadcast client mode 
                 will change the status from 'synchronizedToRemoteServer' 
                 to 'notSynchronized' if no broadcast packets are received."
   DEFVAL  { 320 }         
   ::= { hm2SntpClientGroup 6 }
   
hm2SntpClientInterface OBJECT-TYPE
   SYNTAX      InterfaceIndexOrZero
   MAX-ACCESS 	read-write
   STATUS 		current
   DESCRIPTION
       			"Interface used by the SNTP client."
   DEFVAL { 0 }
   ::= { hm2SntpClientGroup 7 }
   
hm2SntpClientServerAddrTable OBJECT-TYPE
   SYNTAX SEQUENCE OF Hm2SntpClientServerAddrEntry
   MAX-ACCESS 		not-accessible
   STATUS 			current
   DESCRIPTION
		"This table contains objects to configure
		 SNTP client connections."
   ::= { hm2SntpClientGroup 10 }

hm2SntpClientServerAddrEntry OBJECT-TYPE
   SYNTAX 		Hm2SntpClientServerAddrEntry
   MAX-ACCESS 	not-accessible
   STATUS 		current
   DESCRIPTION 
		"The SNTP client connection objects."
   INDEX { hm2SntpClientServerIndex }
   ::= { hm2SntpClientServerAddrTable 1 }

Hm2SntpClientServerAddrEntry ::= SEQUENCE {
   hm2SntpClientServerIndex 		Integer32,
   hm2SntpClientServerAddrType 	InetAddressType,
   hm2SntpClientServerAddr 			InetAddress,
   hm2SntpClientServerPort	 		InetPortNumber,
   hm2SntpClientServerDescr	 		DisplayString,
   hm2SntpClientServerStatus 		INTEGER,
   hm2SntpClientServerRowStatus		RowStatus
   }

-- *************************************************************
-- hm2SntpClientServer entry
-- *************************************************************
hm2SntpClientServerIndex OBJECT-TYPE
   SYNTAX 			Integer32 (1..4)
   MAX-ACCESS 		not-accessible
   STATUS 			current
   DESCRIPTION
		"Index for server table."
   ::= { hm2SntpClientServerAddrEntry 1 }

hm2SntpClientServerAddrType OBJECT-TYPE
   SYNTAX 			InetAddressType
   MAX-ACCESS 		read-create
   STATUS 			current
   DESCRIPTION
		"Address type."
   DEFVAL { ipv4 }         
   ::= { hm2SntpClientServerAddrEntry 2 }

hm2SntpClientServerAddr  OBJECT-TYPE
   SYNTAX 		InetAddress
   MAX-ACCESS 	read-create
   STATUS 		current
   DESCRIPTION
		"The address of the external time server."
   DEFVAL { '00000000'H } -- 0.0.0.0       			
   ::= { hm2SntpClientServerAddrEntry 3 }

hm2SntpClientServerPort  OBJECT-TYPE
   SYNTAX 		InetPortNumber (1..65535)
   MAX-ACCESS 	read-create
   STATUS 		current
   DESCRIPTION
		"The port number of the external time server."
   DEFVAL { 123 }       
   ::= { hm2SntpClientServerAddrEntry 4 }

hm2SntpClientServerDescr  OBJECT-TYPE
   SYNTAX 		DisplayString
   MAX-ACCESS 	read-create
   STATUS 		current
   DESCRIPTION
   	   "The description of the server configured."
   ::= { hm2SntpClientServerAddrEntry 5 }
   
hm2SntpClientServerStatus OBJECT-TYPE
   SYNTAX 		HmSntpClientServerStatus
   MAX-ACCESS 	read-only
   STATUS 		current
   DESCRIPTION
		"Status of the SNTP client - server connection."
   ::= { hm2SntpClientServerAddrEntry 6 }
   
hm2SntpClientServerRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
		"Indicates the status of an entry in this table,
		 and is used to create/delete entries. Objects
		 within this table can by changed while the status
		 is 'active'."
    ::= { hm2SntpClientServerAddrEntry 7 }
--
-- *************************************************************
-- hm2NtpGroup 
-- *************************************************************
--
hm2NtpGeneralGroup OBJECT IDENTIFIER ::= { hm2NtpGroup 1 }

hm2NtpOperatingState OBJECT-TYPE
    SYNTAX      INTEGER { disabled(1),
                          notSynchronized(2),
                          syncToLocal(3),
                          syncToRefclock(4),
                          syncToRemoteServer(5)
                        }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION 
        "Operational status of the NTP server/client."
    ::= { hm2NtpGeneralGroup 1 }

hm2NtpServerGroup OBJECT IDENTIFIER ::= { hm2NtpGroup 2 }
hm2NtpServerConfigGroup OBJECT IDENTIFIER ::= { hm2NtpServerGroup 1 }

hm2NtpServerAdminState OBJECT-TYPE
    SYNTAX      HmEnabledStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION 
        "Enables/disables the NTP server."
    DEFVAL      { disable }
    ::= { hm2NtpServerConfigGroup 1 }

hm2NtpServerOperatingMode OBJECT-TYPE
    SYNTAX      INTEGER { symmetric(1), client-server(2) }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION 
        "NTP server operating mode."
    DEFVAL      { client-server }
    ::= { hm2NtpServerConfigGroup 2 }

hm2NtpServerLocalClockStratum OBJECT-TYPE
    SYNTAX      Integer32 (1..16)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION 
        "The stratum to be used for the case that
         the server is only synchronized to the local clock"
    DEFVAL      { 12 }
    ::= { hm2NtpServerConfigGroup 3 }

hm2NtpClientGroup OBJECT IDENTIFIER ::= { hm2NtpGroup 3 }
hm2NtpClientConfigGroup OBJECT IDENTIFIER ::= { hm2NtpClientGroup 1 }

hm2NtpClientAdminState OBJECT-TYPE
    SYNTAX      HmEnabledStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION 
        "Enables/disables the NTP client."
    DEFVAL      { disable }
    ::= { hm2NtpClientConfigGroup 1 }

hm2NtpClientOperatingMode OBJECT-TYPE
    SYNTAX      INTEGER { unicast(1), broadcast(2) }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION 
        "NTP client operating mode."
    DEFVAL      { unicast }
    ::= { hm2NtpClientConfigGroup 2 }

hm2NtpClientServerAddrTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF Hm2NtpClientServerAddrEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION 
        "This table contains variables for each interface of
         the switch."
    ::= { hm2NtpClientGroup 4 }

hm2NtpClientServerAddrEntry OBJECT-TYPE
    SYNTAX      Hm2NtpClientServerAddrEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION 
        "This entry contains variables for each interface of
         the switch."
    INDEX       { hm2NtpClientServerIndex }
    ::= { hm2NtpClientServerAddrTable 1 }

Hm2NtpClientServerAddrEntry ::= SEQUENCE {
    hm2NtpClientServerIndex         Integer32,
    hm2NtpClientServerAddressType   InetAddressType,
    hm2NtpClientServerAddress       InetAddress,
    hm2NtpClientServerPort          InetPortNumber,
    hm2NtpClientServerInitialBurst  HmEnabledStatus,
    hm2NtpClientServerBurst         HmEnabledStatus,
    hm2NtpClientServerPrefer        TruthValue,
    hm2NtpClientServerStatus        INTEGER,
    hm2NtpClientServerRowStatus     RowStatus
}

hm2NtpClientServerIndex OBJECT-TYPE
    SYNTAX      Integer32 (1..4)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION 
        "Index for Server table."
    ::= { hm2NtpClientServerAddrEntry 1 }

hm2NtpClientServerAddressType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION 
        "Address type for external time server.
         Currently, only IPv4, IPv6 and DNS are supported."
    DEFVAL      { ipv4 }
    ::= { hm2NtpClientServerAddrEntry 2 }

hm2NtpClientServerAddress OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION 
        "The address of the external time server."
    DEFVAL      { '00000000'H }
    ::= { hm2NtpClientServerAddrEntry 3 }

hm2NtpClientServerPort OBJECT-TYPE
    SYNTAX      InetPortNumber
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION 
        "The port number of the external time server. Zero is not allowed
         as port number."
    DEFVAL      { 123 }
    ::= { hm2NtpClientServerAddrEntry 4 }

hm2NtpClientServerInitialBurst OBJECT-TYPE
    SYNTAX      HmEnabledStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION 
        "The initial burst is intended to speed up the initial synchronization.
         Use with caution as it can cause a overload situation on the server."
    REFERENCE   
        "RFC5905 - 52.  Poll Process Operations"
    DEFVAL      { disable }
    ::= { hm2NtpClientServerAddrEntry 5 }

hm2NtpClientServerBurst OBJECT-TYPE
    SYNTAX      HmEnabledStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION 
        "The burst mode can be used to increase the precision
         on links with high jitter e.g. GSM/UMTS links"
    REFERENCE   
        "RFC5905 - 52.  Poll Process Operations"
    DEFVAL      { disable }
    ::= { hm2NtpClientServerAddrEntry 6 }

hm2NtpClientServerPrefer OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The prefer flag can be used to mark the peer as preferred.
         Among a set of correctly operating peers, this one will be chosen
         as synchronization source."
    REFERENCE   
        "RFC5905 - 96.  System Process"
    DEFVAL      { false }
    ::= { hm2NtpClientServerAddrEntry 7 }

hm2NtpClientServerStatus OBJECT-TYPE
    SYNTAX      INTEGER { disabled(1),
                          protocolError(2),
                          notSynchronized(3),
                          notResponding(4),
                          synchronizing(5),
                          synchronized(6),
                          genericError(7)
                        }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION 
        "Status of the NTP client server connection."
    ::= { hm2NtpClientServerAddrEntry 10 }

hm2NtpClientServerRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION 
        "Indicates the status of an entry in this table,
         and is used to create/delete entries. Objects
         within this table can be changed while the status
         is 'active'."
    ::= { hm2NtpClientServerAddrEntry 11 }

hm2NtpClientListenAddrTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF Hm2NtpClientListenAddrEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION 
        "Client table."
    ::= { hm2NtpClientGroup 5 }

hm2NtpClientListenAddrEntry OBJECT-TYPE
    SYNTAX      Hm2NtpClientListenAddrEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION 
        "Client entry."
    INDEX       { hm2NtpClientListenAddrIndex }
    ::= { hm2NtpClientListenAddrTable 1 }

Hm2NtpClientListenAddrEntry ::= SEQUENCE {
    hm2NtpClientListenAddrIndex         Integer32,
    hm2NtpClientListenAddrAddressType   InetAddressType,
    hm2NtpClientListenAddrAddress       InetAddress,
    hm2NtpClientListenAddrPort          InetPortNumber,
    hm2NtpClientListenAddrStatus        INTEGER,
    hm2NtpClientListenAddrRowStatus     RowStatus
}

hm2NtpClientListenAddrIndex OBJECT-TYPE
    SYNTAX      Integer32 (1..4)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION 
        "Index for server table."
    ::= { hm2NtpClientListenAddrEntry 1 }

hm2NtpClientListenAddrAddressType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION 
        "Address type for external time server.
         Currently, only IPv4, IPv6 and DNS are supported."
    DEFVAL      { ipv4 }
    ::= { hm2NtpClientListenAddrEntry 2 }

hm2NtpClientListenAddrAddress OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION 
        "The address of the external time server."
    DEFVAL      { '00000000'H }
    ::= { hm2NtpClientListenAddrEntry 3 }

hm2NtpClientListenAddrPort OBJECT-TYPE
    SYNTAX      InetPortNumber
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION 
        "The port number of the external time server. Zero is not allowed
         as port number."
    DEFVAL      { 123 }
    ::= { hm2NtpClientListenAddrEntry 4 }

hm2NtpClientListenAddrStatus OBJECT-TYPE
    SYNTAX      INTEGER { disabled(1),
                          protocolError(2), 
                          notSynchronized(3),
                          notResponding(4), 
                          synchronizing(5),
                          synchronized(6),
                          genericError(7)
                        }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION 
        "Status of the NTP client server connection."
    ::= { hm2NtpClientListenAddrEntry 10 }

hm2NtpClientListenAddrRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION 
        "Indicates the status of an entry in this table,
         and is used to create/delete entries. Objects
         within this table can by changed while the status
         is 'active'."
    ::= { hm2NtpClientListenAddrEntry 11 }

--
-- *************************************************************
-- hm2PtpGroup 
-- *************************************************************
--
hm2PtpGlobal	OBJECT IDENTIFIER ::= { hm2PtpGroup 1 }

hm2PtpEnable OBJECT-TYPE
		SYNTAX HmEnabledStatus
		MAX-ACCESS 	read-write
		STATUS 		current
		DESCRIPTION
			"Enable or disable the Precision Time Protocol (PTP)
			on this node."		
		DEFVAL  { disable }
		::= { hm2PtpGlobal 1 }


hm2PtpClockMode OBJECT-TYPE
		SYNTAX		INTEGER {
					v2-boundary-clock (2),
					v2-transparent-clock (3)
					}
		MAX-ACCESS	read-write
		STATUS		current
		DESCRIPTION
			"This members value shall indicate which clock mode is used."			 
		DEFVAL  { v2-transparent-clock }
		::= { hm2PtpGlobal 2 }

hm2PtpProfile OBJECT-TYPE
		SYNTAX		INTEGER {
					user-defined (1),
					default-e2e (2),
					default-p2p (3)
					}
		MAX-ACCESS	read-write
		STATUS		current
		DESCRIPTION
			"Configures PTP parameters to a specific profile. Setting the object
			 to user-defined (1) has no effect."
		DEFVAL  { default-e2e }
		::= { hm2PtpGlobal 3 }

hm2PtpIsSynchronized OBJECT-TYPE
		SYNTAX		INTEGER {
					true (1),
					false (2)
					}
		MAX-ACCESS	read-only
		STATUS		current
		DESCRIPTION
			"If the clock is synchronized to the current Master this object is set to true. 
			Otherwise it is set to false. The clock sets this object to true, if the offset (ns)
			to the current Master is less than hm2PtpSyncLowerBound. The clock sets this object to false, 
			if the offset (ns) to the current Master is bigger than hm2PtpSyncUpperBound."
		::= { hm2PtpGlobal 4 }


hm2PtpSyncLowerBound OBJECT-TYPE
		SYNTAX		Integer32(1..999999999)
		MAX-ACCESS	read-write
		STATUS		current
		DESCRIPTION
			"This object defines when the hm2PtpIsSynchronized object is set to true. 
			If the absolute value of the offset is smaller than hm2PtpSyncLowerBound, 
			the hm2PtpIsSynchronized is set true.
			The value is interpreted as nanoseconds."
		DEFVAL  { 30 }			
		::= { hm2PtpGlobal 5 }


hm2PtpSyncUpperBound OBJECT-TYPE
		SYNTAX		Integer32(31..1000000000)
		MAX-ACCESS	read-write
		STATUS		current
		DESCRIPTION
			"This object defines when the hm2PtpIsSynchronized object is set to false. 
			If the absolute value of the offset is bigger than hm2PtpSyncUpperBound, the hm2PtpIsSynchronized is set false.
			The value is interpreted as nanoseconds."
		DEFVAL  { 5000 }			
		::= { hm2PtpGlobal 6 }

hm2PtpAbsMaxOffset OBJECT-TYPE
		SYNTAX		Integer32 
		MAX-ACCESS	read-only
		STATUS		current
		DESCRIPTION
			"This members value shall indicate the absolute value for the maximum offset between its parent and this node. 
			The value is set to zero if the offset is the first time smaller than hm2PtpSyncLowerBound.
			Offsets bigger than +/-1 second are indicated by the maximum value."
		::= { hm2PtpGlobal 7 }

hm2PtpTimeSeconds OBJECT-TYPE
		SYNTAX		PtpTimeStamp 
		MAX-ACCESS	read-only
		STATUS		current
		DESCRIPTION
			"Current PTP time in PTP timescale"
		::= { hm2PtpGlobal 8 }
		
hm2PtpManagement	OBJECT-TYPE
		SYNTAX 		TruthValue
		MAX-ACCESS 	read-write
		STATUS 		current
		DESCRIPTION
			"If set to true PTP management via PTP management messages is enabled."
		DEFVAL  { false }
		::= { hm2PtpGlobal 9 }

--
-- ptp2-group (IEEE 1588-2008)  --
--

hm2Ptp2Objects			OBJECT IDENTIFIER ::= { hm2PtpGroup 2 }
hm2Ptp2Configuration	OBJECT IDENTIFIER ::= { hm2Ptp2Objects 1 }

hm2Ptp2TwoStepClock OBJECT-TYPE
		SYNTAX		TruthValue
		MAX-ACCESS	read-only
		STATUS		current
		DESCRIPTION
			"A value of true indicates that this node is a two-step device."
		::= { hm2Ptp2Configuration 1 }

hm2Ptp2ClockIdentity OBJECT-TYPE
		SYNTAX		PtpClockIdentity	
		MAX-ACCESS	read-only
		STATUS		current
		DESCRIPTION
			"This value is the clock identity of the local clock."
		::= { hm2Ptp2Configuration 2 }

hm2Ptp2ClockQuality OBJECT-TYPE
		SYNTAX		PtpClockQuality
		MAX-ACCESS	read-only
		STATUS		current
		DESCRIPTION
			"Clock quality of the local clock."
		::= { hm2Ptp2Configuration 3 }

hm2Ptp2ClockClass OBJECT-TYPE
		SYNTAX		Integer32 (0..255)
		MAX-ACCESS	read-only
		STATUS		current
		DESCRIPTION
			"First octet of hm2Ptp2ClockQuality. This represents the clock class of the local clock."
		::= { hm2Ptp2Configuration 4 }
		
hm2Ptp2ClockAccuracy OBJECT-TYPE
		SYNTAX		INTEGER {
							within25ns(32), -- 20H
						    within100ns(33), -- 21H
						    within250ns(34), -- 22H
						    within1000ns(35), -- 23H
						    within2500ns(36), -- 24H
						    within10us(37), -- 25H
						    within25us(38), -- 26H
						    within100us(39), -- 27H
						    within250us(40), -- 28H
						    within1000us(41), -- 29H
						    within2500us(42), -- 2AH
						    within10ms(43), -- 2BH
						    within25ms(44), -- 2CH
						    within100ms(45), -- 2DH
						    within250ms(46), -- 2EH
						    within1s(47), -- 2FH
						    within10s(48), -- 30H
						    beyond10s(49), -- 31H
						    unknown(254) -- FEH
							}
		MAX-ACCESS	read-only
		STATUS		current
		DESCRIPTION
			"Second octet of hm2Ptp2ClockQuality. This represents the clock accuracy of the local clock."
		::= { hm2Ptp2Configuration 5 }
		
hm2Ptp2ClockVariance OBJECT-TYPE
		SYNTAX		Integer32
		MAX-ACCESS	read-only
		STATUS		current
		DESCRIPTION
			"Last two octets of hm2Ptp2ClockQuality. This represents the clock variance of the local clock."
		::= { hm2Ptp2Configuration 6 }

hm2Ptp2Priority1 OBJECT-TYPE
		SYNTAX		Integer32(0..255)
		MAX-ACCESS	read-write
		STATUS		current
		DESCRIPTION
			"Priority 1 value of the local clock"
		DEFVAL  { 128 } 			
		::= { hm2Ptp2Configuration 7 }

hm2Ptp2Priority2 OBJECT-TYPE
		SYNTAX		Integer32(0..255)
		MAX-ACCESS	read-write
		STATUS		current
		DESCRIPTION
			"Priority 2 value of the local clock"
		DEFVAL  { 128 } 			
		::= { hm2Ptp2Configuration 8 }

hm2Ptp2DomainNumber OBJECT-TYPE
		SYNTAX		Integer32(0..255) 
		MAX-ACCESS	read-write
		STATUS		current
		DESCRIPTION
			"PTP domain number of the local clock."
		DEFVAL  { 0 } 			
		::= { hm2Ptp2Configuration 9 }

hm2Ptp2StepsRemoved OBJECT-TYPE
		SYNTAX		Integer32
		MAX-ACCESS	read-only
		STATUS		current
		DESCRIPTION
			"The value of hm2Ptp2StepsRemoved is the number of communication paths traversed between the local
			 clock and the grandmaster clock."
		::= { hm2Ptp2Configuration 10 }

hm2Ptp2OffsetFromMaster OBJECT-TYPE
		SYNTAX		PtpTimeInterval
		MAX-ACCESS	read-only
		STATUS		current
		DESCRIPTION
			"Current value of the time difference between master and slave measured by this clock."
		::= { hm2Ptp2Configuration 11 }

hm2Ptp2MeanPathDelay OBJECT-TYPE
		SYNTAX		PtpTimeInterval 
		MAX-ACCESS	read-only
		STATUS		current
		DESCRIPTION
			"Current value of the mean propagation time (e2e-delay) between Master and Slave. 
			 This is only valid if hm2Ptp2DelayMechanism is set to e2e on the current slave port."
		::= { hm2Ptp2Configuration 12 }

hm2Ptp2ParentPortIdentity OBJECT-TYPE
		SYNTAX		PtpPortIdentity
		MAX-ACCESS	read-only
		STATUS		current
		DESCRIPTION
			"The port identity value of the port on the master that issues the synchronization
			 messages used to synchronize this clock."
		::= { hm2Ptp2Configuration 13 }

hm2Ptp2ParentStats OBJECT-TYPE
		SYNTAX		TruthValue
		MAX-ACCESS	read-only
		STATUS		current
		DESCRIPTION
			"A value of True indicates that the objects hm2Ptp2ObservedParentOffsetScaledLogVariance 
			 and hm2Ptp2ObservedParentClockPhaseChangeRate are valid."
		::= { hm2Ptp2Configuration 14 }

hm2Ptp2ObservedParentOffsetScaledLogVariance OBJECT-TYPE
		SYNTAX		Integer32
		MAX-ACCESS	read-only
		STATUS		current
		DESCRIPTION
			"Estimate of the parent clocks PTP variance observed by this clock."
		::= { hm2Ptp2Configuration 15 }

hm2Ptp2ObservedParentClockPhaseChangeRate OBJECT-TYPE
		SYNTAX		Integer32
		MAX-ACCESS	read-only
		STATUS		current
		DESCRIPTION
			"Estimate of the phase change rate (drift) observed by this clock."
		::= { hm2Ptp2Configuration 16 }

hm2Ptp2GrandmasterIdentity OBJECT-TYPE
		SYNTAX		PtpClockIdentity
		MAX-ACCESS	read-only
		STATUS		current
		DESCRIPTION
			"ClockIdentity of the Grandmaster clock synchronizing this clock."
		::= { hm2Ptp2Configuration 17 }

hm2Ptp2GrandmasterClockQuality OBJECT-TYPE
		SYNTAX		PtpClockQuality
		MAX-ACCESS	read-only
		STATUS		current
		DESCRIPTION
			"ClockQuality of the Grandmaster clock synchronizing this clock."
		::= { hm2Ptp2Configuration 18 }

hm2Ptp2GrandmasterClockClass OBJECT-TYPE
		SYNTAX		Integer32 (0..255)
		MAX-ACCESS	read-only
		STATUS		current
		DESCRIPTION
			"First octet of hm2Ptp2GrandmasterClockQuality. This represents the grand masters clock class."
		::= { hm2Ptp2Configuration 19 }
		
hm2Ptp2GrandmasterClockAccuracy OBJECT-TYPE
		SYNTAX		INTEGER {
							within25ns(32), -- 20H
						    within100ns(33), -- 21H
						    within250ns(34), -- 22H
						    within1000ns(35), -- 23H
						    within2500ns(36), -- 24H
						    within10us(37), -- 25H
						    within25us(38), -- 26H
						    within100us(39), -- 27H
						    within250us(40), -- 28H
						    within1000us(41), -- 29H
						    within2500us(42), -- 2AH
						    within10ms(43), -- 2BH
						    within25ms(44), -- 2CH
						    within100ms(45), -- 2DH
						    within250ms(46), -- 2EH
						    within1s(47), -- 2FH
						    within10s(48), -- 30H
						    beyond10s(49), -- 31H
						    unknown(254) -- FEH
							}
		MAX-ACCESS		read-only
		STATUS		current
		DESCRIPTION
			"Second octet of hm2Ptp2GrandmasterClockAccuracy. This represents the grand masters clock accuracy."
		::= { hm2Ptp2Configuration 20 }
		
hm2Ptp2GrandmasterClockVariance OBJECT-TYPE
		SYNTAX		Integer32
		MAX-ACCESS	read-only
		STATUS		current
		DESCRIPTION
			"Last two octets of hm2Ptp2GrandmasterClockQuality. This represents the grand masters clock variance."
		::= { hm2Ptp2Configuration 21 }

hm2Ptp2GrandmasterPriority1 OBJECT-TYPE
		SYNTAX		Integer32
		MAX-ACCESS	read-only
		STATUS		current
		DESCRIPTION
			"Priority 1 value of the grand master clock."
		::= { hm2Ptp2Configuration 22 }

hm2Ptp2GrandmasterPriority2 OBJECT-TYPE
		SYNTAX		Integer32
		MAX-ACCESS	read-only
		STATUS		current
		DESCRIPTION
			"Priority 2 value of the grand master clock."
		::= { hm2Ptp2Configuration 23 }

hm2Ptp2CurrentUtcOffset OBJECT-TYPE
		SYNTAX		Integer32 (-32768..32767)
		MAX-ACCESS	read-write
		STATUS		current
		DESCRIPTION
			"Current difference between the PTP timescale (TAI) and UTC in seconds."
		DEFVAL  { 37 }
		::= { hm2Ptp2Configuration 24 }

hm2Ptp2CurrentUtcOffsetValid OBJECT-TYPE
		SYNTAX		TruthValue
		MAX-ACCESS	read-write
		STATUS		current
		DESCRIPTION
			"A value of True indicates that the hm2Ptp2CurrentUtcOffset is known to be correct."
		DEFVAL  { false }			
		::= { hm2Ptp2Configuration 25 }

hm2Ptp2Leap59 OBJECT-TYPE
		SYNTAX		TruthValue
		MAX-ACCESS	read-only
		STATUS		current
		DESCRIPTION
			"A value of true indicates that the last minute of the current UTC day contains 59 seconds."
		::= { hm2Ptp2Configuration 26 }

hm2Ptp2Leap61 OBJECT-TYPE
		SYNTAX		TruthValue
		MAX-ACCESS	read-only
		STATUS		current
		DESCRIPTION
			"A value of true indicates that the last minute of the current UTC day contains 61 seconds."
		::= { hm2Ptp2Configuration 27 }

hm2Ptp2TimeTraceable OBJECT-TYPE
		SYNTAX		TruthValue
		MAX-ACCESS	read-only
		STATUS		current
		DESCRIPTION
			"A value of True indicates that the current time is traceable to a primary reference."
		::= { hm2Ptp2Configuration 28 }

hm2Ptp2FrequencyTraceable OBJECT-TYPE
		SYNTAX		TruthValue
		MAX-ACCESS	read-only
		STATUS		current
		DESCRIPTION
			"A value of True indicates that the frequency determining 
			 the timescale is traceable to a primary reference."
		::= { hm2Ptp2Configuration 29 }

hm2Ptp2PtpTimescale OBJECT-TYPE
		SYNTAX		TruthValue
		MAX-ACCESS	read-only
		STATUS		current
		DESCRIPTION
			"A value of True indicates that the clocks timescale is PTP."
		::= { hm2Ptp2Configuration 30 }

hm2Ptp2TimeSource OBJECT-TYPE
		SYNTAX		INTEGER {
							atomicClock(16), -- 10H
							gps(32), -- 20H
							terrestrialRadio(48), -- 30H
							ptp(64), -- 40H
							ntp(80), --50H
							handSet(96), --60H
							other(144), --90H
							internalOscillator(160) --A0H
							}
		MAX-ACCESS	read-write
		STATUS		current
		DESCRIPTION
			"The source of time used by the Grandmaster clock."
		DEFVAL  { internalOscillator }
		::= { hm2Ptp2Configuration 31 }
		
		
hm2Ptp2PortTable OBJECT-TYPE
		SYNTAX			SEQUENCE OF Hm2Ptp2PortEntry
		MAX-ACCESS		not-accessible
		STATUS			current
		DESCRIPTION
			"This table contains variables for each PTP2 port of
			the switch."
		::= { hm2Ptp2Objects 2 }

hm2Ptp2PortEntry OBJECT-TYPE
		SYNTAX 		 Hm2Ptp2PortEntry
		MAX-ACCESS 	 not-accessible
		STATUS 		 current
		DESCRIPTION     "Entry for one port."
		INDEX		{ ifIndex }
		::= { hm2Ptp2PortTable 1 }

Hm2Ptp2PortEntry ::= SEQUENCE {
		hm2Ptp2PortEnable HmEnabledStatus,
		hm2Ptp2PortState INTEGER,
		hm2Ptp2LogDelayReqInterval	Integer32,
		hm2Ptp2PeerMeanPathDelay PtpTimeInterval,
		hm2Ptp2LogAnnounceInterval INTEGER,
		hm2Ptp2AnnounceReceiptTimeout Integer32,
		hm2Ptp2LogSyncInterval INTEGER,
		hm2Ptp2DelayMechanism INTEGER,
		hm2Ptp2LogPdelayReqInterval Hm2Ptp2LogPdelayReqIntervalTc,
		hm2Ptp2VersionNumber INTEGER,
		hm2Ptp2NetworkProtocol INTEGER,
		hm2Ptp2V1Compatibility INTEGER,
		hm2Ptp2DelayAsymmetry Integer32,
		hm2Ptp2PortCapability BITS,
		hm2Ptp2VlanID Integer32,
		hm2Ptp2VlanPriority Integer32
		}

hm2Ptp2PortEnable	OBJECT-TYPE
		SYNTAX 		HmEnabledStatus
		MAX-ACCESS 	read-write
		STATUS 		current
		DESCRIPTION
			"Enable or disable the sending and receiving / processing of PTP synchronization messages."
		DEFVAL  { enable }			
		::= { hm2Ptp2PortEntry 1 }
		
hm2Ptp2PortState OBJECT-TYPE
		SYNTAX		INTEGER {
					initializing (1),
					faulty (2),
					disabled (3),
					listening (4),
					pre-master (5),
					master (6),
					passive (7),
					uncalibrated (8),
					slave (9)
					}
		MAX-ACCESS 		 read-only
		STATUS 		 current
		DESCRIPTION
			"State of the PTP2 port instance."
		::= { hm2Ptp2PortEntry 2 }

hm2Ptp2LogDelayReqInterval		OBJECT-TYPE
		SYNTAX 		Integer32
		MAX-ACCESS 	read-only
		STATUS 		current
		DESCRIPTION
			"Logarithm to the base of 2 of the minimum DelayRequest interval used to measure the e2e-delay."
		::= { hm2Ptp2PortEntry 3 }

hm2Ptp2PeerMeanPathDelay		OBJECT-TYPE
		SYNTAX 		PtpTimeInterval
		MAX-ACCESS 	read-only
		STATUS 		current
		DESCRIPTION
			"If hm2Ptp2DelayMechanism is set to p2p this value is an estimate of the current one-way propagation delay (p2p-delay)."
		::= { hm2Ptp2PortEntry 4 }

hm2Ptp2LogAnnounceInterval	OBJECT-TYPE
		SYNTAX 		INTEGER {
					sec-1 (0),
					sec-2 (1),
					sec-4 (2),
					sec-8 (3),
					sec-16 (4)
					}
		MAX-ACCESS 	read-write
		STATUS 		current
		DESCRIPTION
			"Logarithm to the base of 2 of the mean announce interval."
		DEFVAL  { sec-2 }			
		::= { hm2Ptp2PortEntry 5 }

hm2Ptp2AnnounceReceiptTimeout	OBJECT-TYPE
		SYNTAX 		Integer32 (2..10)
		MAX-ACCESS 		read-write
		STATUS 		current
		DESCRIPTION
			"Announce receipt timeout in multiples of hm2Ptp2LogAnnounceInterval."
		DEFVAL  { 3 }			
		::= { hm2Ptp2PortEntry 6 }

hm2Ptp2LogSyncInterval	OBJECT-TYPE
		SYNTAX 		Hm2Ptp2LogSyncIntervalTc
		MAX-ACCESS 		read-write
		STATUS 		current
		DESCRIPTION
			"Logarithm to the base of 2 of the mean synchronization interval."
		DEFVAL  { sec-1 }
		::= { hm2Ptp2PortEntry 7 }

hm2Ptp2DelayMechanism	OBJECT-TYPE
		SYNTAX 	INTEGER {
							e2e(1),
							p2p(2),
							disabled(254) -- FEH
						}
		MAX-ACCESS 	read-write
		STATUS 		current
		DESCRIPTION
			"This value indicates the propagation delay measuring option used by this port."
		DEFVAL  { e2e }			
		::= { hm2Ptp2PortEntry 8 }

hm2Ptp2LogPdelayReqInterval	OBJECT-TYPE
		SYNTAX 		Hm2Ptp2LogPdelayReqIntervalTc
		MAX-ACCESS 		read-write
		STATUS 		current
		DESCRIPTION
			"Logarithm to the base of 2 of the minimum PDelay Request interval (used for p2p-delay)."
		DEFVAL  { sec-1 }			
		::= { hm2Ptp2PortEntry 9 }

hm2Ptp2VersionNumber	OBJECT-TYPE
		SYNTAX 		INTEGER {
								ptpVersion1 (1),
								ptpVersion2 (2)
							}
		MAX-ACCESS 		read-write
		STATUS 			current
		DESCRIPTION
			"PTP version in use on this port (always ptpVersion2)."
		DEFVAL  { ptpVersion2 }			
		::= { hm2Ptp2PortEntry 10 }

hm2Ptp2NetworkProtocol	OBJECT-TYPE
		SYNTAX 		INTEGER {
						    	udpIpv4    (1),
						    	ieee8023   (3)
							}
		MAX-ACCESS 		read-write
		STATUS 			current
		DESCRIPTION
			"Current configured network transport protocol of this port."
		DEFVAL  { ieee8023 }		
		::= { hm2Ptp2PortEntry 11 }

hm2Ptp2V1Compatibility 	OBJECT-TYPE
		SYNTAX 		INTEGER {
								on   (1),
								off  (2),
								auto (3)
							}
		MAX-ACCESS 		read-write
		STATUS 		current
		DESCRIPTION
			"If set to on all PTPv2 messages will be padded to the length of a PTPv1 frame. This is required by some hardware."
		DEFVAL  { auto }			
		::= { hm2Ptp2PortEntry 12 }

hm2Ptp2DelayAsymmetry  	OBJECT-TYPE
		SYNTAX 		Integer32(-2000000000..2000000000)
		MAX-ACCESS 	read-write
		STATUS 		current
		DESCRIPTION
			"Asymmetry of the link connected to this port in nanoseconds. 
			The hm2Ptp2DelayAsymmetry is positive when the master-to-slave 
			propagation time is longer than the slave-to-master propagation time."
		DEFVAL  { 0 }
		::= { hm2Ptp2PortEntry 13 }
		
hm2Ptp2PortCapability  	OBJECT-TYPE 
	   SYNTAX      BITS {
	                  reserved(0),
	                  one-step(1),
	                  e2e-delay(2),
	                  p2p-delay(3),
	                  ptp2Ieee8023(4),
	                  ptp2UdpIpv4(5),
	                  ptp2UdpIpv6(6),
	                  asymmCorrection(7),
	                  halfDuplex(8),
	                  ptp2UdpE2EGlobal(9)
	               }
	   MAX-ACCESS  read-only
	   STATUS      current 
	   DESCRIPTION 
	      "This object shows the capability of the ptp port."
	   ::= { hm2Ptp2PortEntry 14 }
	   
hm2Ptp2VlanID	OBJECT-TYPE
		SYNTAX 		Integer32(-1..4042)
		MAX-ACCESS 	read-write
		STATUS 		current
		DESCRIPTION
			"VLAN in which PTP packets are send. With a value of -1 all packets are send untagged"
		DEFVAL  { -1 }
		::= { hm2Ptp2PortEntry 15 }

hm2Ptp2VlanPriority	OBJECT-TYPE
		SYNTAX 		Integer32(0..7)
		MAX-ACCESS 	read-write
		STATUS 		current
		DESCRIPTION
			"VLAN priority of tagged ptp packets"
		DEFVAL  { 6 }
		::= { hm2Ptp2PortEntry 16 }
		
--
-- hm2Ptp2TCConfiguration / Transparent Clock configuration (IEEE1588-2008) --
--

hm2Ptp2TCObjects		OBJECT IDENTIFIER ::= { hm2PtpGroup 3 }
hm2Ptp2TCConfiguration	OBJECT IDENTIFIER ::= { hm2Ptp2TCObjects 1 }

hm2Ptp2TCClockIdentity	OBJECT-TYPE
		SYNTAX 		PtpClockIdentity
		MAX-ACCESS 	read-only
		STATUS 		current
		DESCRIPTION
			"This value is the clock identity of the transparent clock."
		::= { hm2Ptp2TCConfiguration 1 }

hm2Ptp2TCDelayMechanism	OBJECT-TYPE
		SYNTAX 		INTEGER{
							e2e(1),
							p2p(2),
							e2e-optimized(3),
							disabled(254) -- FEH
							}
		MAX-ACCESS 		read-write
		STATUS 		current
		DESCRIPTION
			"Configures the transparent clock to be either a e2e- or p2p-transparent clock.
			If supported a value of e2e-optimized sets the clock to e2e mode where delay requests 
			are only forwarded on the port where the current Master (hm2Ptp2TCCurrentMaster) is connected."
		DEFVAL  { e2e }
		::= { hm2Ptp2TCConfiguration 2 }

hm2Ptp2TCPrimaryDomain	OBJECT-TYPE
		SYNTAX 		Integer32(0..255)
		MAX-ACCESS 	read-write
		STATUS 		current
		DESCRIPTION
			"PTP domain number of the primary syntonization domain."
		DEFVAL  { 0 }
		::= { hm2Ptp2TCConfiguration 3 }

hm2Ptp2TCSyntonized	OBJECT-TYPE
		SYNTAX 		TruthValue
		MAX-ACCESS 	read-write
		STATUS 		current
		DESCRIPTION
			"A value of true indicates that the syntonization of the transparent clock is enabled."
		DEFVAL  { true }
		::= { hm2Ptp2TCConfiguration 4 }

hm2Ptp2TCNetworkProtocol	OBJECT-TYPE
		SYNTAX 		INTEGER {
						    udpIpv4    (1),
						    ieee8023   (3)
							}
		MAX-ACCESS 		read-write
		STATUS 		current
		DESCRIPTION
			"Current configured network transport protocol of the transparent clock."
		DEFVAL  { ieee8023 }
		::= { hm2Ptp2TCConfiguration 5 }

hm2Ptp2TCCurrentMaster OBJECT-TYPE
		SYNTAX 		PtpPortIdentity
		MAX-ACCESS 	read-only
		STATUS 		current
		DESCRIPTION
			"The port identity value of the port on the master that issues the synchronization
			 messages used to syntonize/synchronize this clock."
		::= { hm2Ptp2TCConfiguration 6 }

hm2Ptp2TCMultiDomainMode	OBJECT-TYPE
		SYNTAX 		TruthValue
		MAX-ACCESS 	read-write
		STATUS 		current
		DESCRIPTION
			"If set to false, PTP messages from domains other than hm2Ptp2TCPrimaryDomain are ignored."
		DEFVAL  { false }
		::= { hm2Ptp2TCConfiguration 7 }
		
hm2Ptp2TCSyncLocalClock	OBJECT-TYPE
		SYNTAX 		TruthValue
		MAX-ACCESS 	read-write
		STATUS 		current
		DESCRIPTION
			"Enable synchronisation of the local clock (TC hybrid mode). This requires syntonization to be enabled.
			 All transparent clock operations are still done based on the syntonized clock."
		DEFVAL  { false }
		::= { hm2Ptp2TCConfiguration 8 }
		
hm2Ptp2TCOffsetFromMaster OBJECT-TYPE
		SYNTAX		PtpTimeInterval
		MAX-ACCESS	read-only
		STATUS		current
		DESCRIPTION
			"Current value of the time difference between Master and this clock measured by this clock. 
			 This object is only valid if hm2Ptp2TCSyncLocalClock is set to true."
		::= { hm2Ptp2TCConfiguration 9 }

hm2Ptp2TCMeanPathDelay OBJECT-TYPE
		SYNTAX		PtpTimeInterval 
		MAX-ACCESS	read-only
		STATUS		current
		DESCRIPTION
			"Current value of the mean propagation time (e2e-delay) between Master and Slave. 
			 This object is only valid for e2e-transparent-clock and hm2Ptp2TCSyncLocalClock is set to true."
		::= { hm2Ptp2TCConfiguration 10 }	
		
hm2Ptp2TCVlanID	OBJECT-TYPE
		SYNTAX 		Integer32(-1..4095)
		MAX-ACCESS 	read-write
		STATUS 		current
		DESCRIPTION
			"VLAN in which PTP packets are send. With a value of -1 all packets are send untagged."
		DEFVAL  { -1 }
		::= { hm2Ptp2TCConfiguration 11 }

hm2Ptp2TCVlanPriority	OBJECT-TYPE
		SYNTAX 		Integer32(0..7)
		MAX-ACCESS 	read-write
		STATUS 		current
		DESCRIPTION
			"VLAN priority of tagged PTP packets."
		DEFVAL  { 6 }
		::= { hm2Ptp2TCConfiguration 12 }
				
hm2Ptp2TCCapability  OBJECT-TYPE 
	   SYNTAX      BITS {
	                  reserved(0),
	                  one-step(1),
	                  e2e-delay(2),
	                  p2p-delay(3),
	                  ptp2Ieee8023(4),
	                  ptp2UdpIpv4(5),
	                  ptp2UdpIpv6(6),
	                  asymmCorrection(7),
	                  halfDuplex(8)     
	               }
	   MAX-ACCESS  read-only
	   STATUS      current 
	   DESCRIPTION 
	      "This object shows the capability of the TC."
	   ::= { hm2Ptp2TCConfiguration 13 }

hm2Ptp2TCPortTable OBJECT-TYPE
		SYNTAX			SEQUENCE OF Hm2Ptp2TCPortEntry
		MAX-ACCESS		not-accessible
		STATUS			current
		DESCRIPTION
			"This table contains variables for each PTP2 TC port of
			the switch."
		::= { hm2Ptp2TCObjects 2 }

hm2Ptp2TCPortEntry OBJECT-TYPE
		SYNTAX 		 Hm2Ptp2TCPortEntry
		MAX-ACCESS 	 not-accessible
		STATUS 		 current
		DESCRIPTION     "Entry for one port."
		INDEX		{ ifIndex }
		::= { hm2Ptp2TCPortTable 1 }

Hm2Ptp2TCPortEntry ::= SEQUENCE {
		hm2Ptp2TCPortEnable HmEnabledStatus,
		hm2Ptp2TCLogPdelayReqInterval Hm2Ptp2LogPdelayReqIntervalTc,
		hm2Ptp2TCFaulty TruthValue,
		hm2Ptp2TCPeerMeanPathDelay PtpTimeInterval,
		hm2Ptp2TCDelayAsymmetry Integer32
		}

hm2Ptp2TCPortEnable		OBJECT-TYPE
		SYNTAX 		HmEnabledStatus
		MAX-ACCESS 	read-write
		STATUS 		current
		DESCRIPTION
			"Enable or disable the sending and receiving / processing of PTP synchronization messages."
		DEFVAL  { enable }			
		::= { hm2Ptp2TCPortEntry 1 }

hm2Ptp2TCLogPdelayReqInterval	OBJECT-TYPE
		SYNTAX 		Hm2Ptp2LogPdelayReqIntervalTc
		MAX-ACCESS 	read-write
		STATUS 		current
		DESCRIPTION
			"Logarithm to the base of 2 of the minimum PDelay Request interval (used for p2p-delay)."
		DEFVAL  { sec-1 }
		::= { hm2Ptp2TCPortEntry 2 }

hm2Ptp2TCFaulty	OBJECT-TYPE
		SYNTAX 		TruthValue
		MAX-ACCESS 	read-only
		STATUS 		current
		DESCRIPTION
			"True if port is in Faulty state."
		::= { hm2Ptp2TCPortEntry 3 }

hm2Ptp2TCPeerMeanPathDelay	OBJECT-TYPE
		SYNTAX 		PtpTimeInterval 
		MAX-ACCESS 	read-only
		STATUS 		current
		DESCRIPTION
			"This value is an estimate of the current one way propagation delay of a p2p-transparent-clock."
		::= { hm2Ptp2TCPortEntry 4 }

hm2Ptp2TCDelayAsymmetry  	OBJECT-TYPE
		SYNTAX 		Integer32(-2000000000..2000000000)
		MAX-ACCESS 	read-write
		STATUS 		current
		DESCRIPTION
			"Asymmetry of the link connected to this port in nanoseconds. 
			The hm2Ptp2TCDelayAsymmetry is positive when the master-to-slave 
			propagation time is longer than the slave-to-master propagation time."
		DEFVAL  { 0 }			
		::= { hm2Ptp2TCPortEntry 5 }

-- *************************************************************
-- hm2IrigGroup
-- *************************************************************
hm2IrigAdminStatus OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
	  "Enables/disables the IRIG-B output."
   DEFVAL { disable }
   ::= { hm2IrigGroup 1 }

hm2IrigMode OBJECT-TYPE
   SYNTAX INTEGER {
	  irig-b000 (0),
	  irig-b001 (1),
	  irig-b002 (2),
	  irig-b003 (3),
	  irig-b004 (4),
	  irig-b005 (5),
	  irig-b006 (6),
	  irig-b007 (7)
   }
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
	  "Set the IRIG Mode, allowed values:
	  (See https://wsmrc2vger.wsmr.army.mil/rcc/manuals/200-04/TT-45.pdf)
	  irig-b000 (0) - Mode IRIG B000, BCDtoy, CF, SBS
	  irig-b001 (1) - Mode IRIG B001, BCDtoy, CF
	  irig-b002 (2) - Mode IRIG B002, BCDtoy
	  irig-b003 (3) - Mode IRIG B003, BCDtoy, SBS
	  irig-b004 (4) - Mode IRIG B004, BCDtoy, BCDyear, CF, SBS
	  irig-b005 (5) - Mode IRIG B005, BCDtoy, BCDyear, CF
	  irig-b006 (6) - Mode IRIG B006, BCDtoy, BCDyear
	  irig-b007 (7) - Mode IRIG B007, BCDtoy, BCDyear, SBS
	  with 
		BCDtoy: binary coded decimal time of year
		BCDyear: binary coded decimal year
		CF: control functions
		SBS: straight binary seconds of day
	  only modes b002,B003,B006 and b007 are supported."
   DEFVAL { irig-b003 }
   ::= { hm2IrigGroup 2 }

hm2IrigPpsAdminStatus OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
	  "Enables/disables the pps output."
   DEFVAL { disable }
   ::= { hm2IrigGroup 3 }

hm2IrigTimeMode OBJECT-TYPE
   SYNTAX INTEGER {
	utc (1),
	local(2)
   }
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
	  "Define the IRIG-B time base (UTC or local)."
   DEFVAL { utc }
   ::= { hm2IrigGroup 4 }

hm2IrigOperStatus OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS read-only
   STATUS current
   DESCRIPTION
	  "Current operational status of the IRIG-B output. "
   ::= { hm2IrigGroup 5 }

hm2IrigTimeQuality OBJECT-TYPE
   SYNTAX INTEGER {
	  locked(0),
	  within1ns(1),
	  within10ns(2),
	  within100ns(3),
	  within1us(4),
	  within10us(5),
	  within100us(6),
	  within1ms(7),
	  within10ms(8),
	  within100ms(9),
	  within1s(10),
	  within10s(11),
	  within100s(12),
	  within1000s(13),
	  within10000s(14),
	  failure(15)
   }   
   MAX-ACCESS read-only
   STATUS current
   DESCRIPTION
	  "Current IRIG-B time quality according to IEEE 1344."
   ::= { hm2IrigGroup 6 }


--
-- *************************************************************
-- hm2Dot1asGroup
-- *************************************************************
--
hm2Dot1asGlobal	OBJECT IDENTIFIER ::= { hm2Dot1asGroup 1 }

hm2Dot1asEnable OBJECT-TYPE
		SYNTAX HmEnabledStatus
		MAX-ACCESS 	read-write
		STATUS 		current
		DESCRIPTION
			"Enable or disable the 802.1AS Protocol
			on this node."
		DEFVAL  { disable }
		::= { hm2Dot1asGlobal 1 }

hm2Dot1asIsSynchronized OBJECT-TYPE
		SYNTAX		INTEGER {
					true (1),
					false (2)
					}
		MAX-ACCESS	read-only
		STATUS		current
		DESCRIPTION
			"If the clock is synchronized to the current Master this object is set to true.
			Otherwise it is set to false. The clock sets this object to true, if the offset (ns)
			to the current Master is less than hm2dot1asSyncLowerBound. The clock sets this object to false,
			if the offset (ns) to the current Master is bigger than hm2dot1asSyncUpperBound."
		::= { hm2Dot1asGlobal 2 }

hm2Dot1asSyncLowerBound OBJECT-TYPE
		SYNTAX		Integer32(1..999999999)
		MAX-ACCESS	read-write
		STATUS		current
		DESCRIPTION
			"This object defines when the hm2dot1asIsSynchronized object is set to true.
			If the absolute value of the offset is smaller than hm2dot1asSyncLowerBound,
			the hm2dot1asIsSynchronized is set true.
			The value is interpreted as nanoseconds."
		DEFVAL  { 30 }
		::= { hm2Dot1asGlobal 3 }

hm2Dot1asSyncUpperBound OBJECT-TYPE
		SYNTAX		Integer32(31..1000000000)
		MAX-ACCESS	read-write
		STATUS		current
		DESCRIPTION
			"This object defines when the hm2dot1asIsSynchronized object is set to false.
			If the absolute value of the offset is bigger than hm2dot1asSyncUpperBound, the hm2dot1asIsSynchronized is set false.
			The value is interpreted as nanoseconds."
		DEFVAL  { 5000 }
		::= { hm2Dot1asGlobal 4 }

hm2Dot1asAbsMaxOffset OBJECT-TYPE
		SYNTAX		Integer32
		MAX-ACCESS	read-only
		STATUS		current
		DESCRIPTION
			"This members value shall indicate the absolute value for the maximum offset between its parent and this node. 
			The value is set to zero if the offset is the first time smaller than hm2dot1asSyncLowerBound.
			Offsets bigger than +/-1 second are indicated by the maximum value."
		::= { hm2Dot1asGlobal 5 }

-- ***********************************************************
-- hm2TimeSyncSNMPExtensionGroup
-- ***********************************************************
hm2TimeSyncSystemTimeSESGroup 	OBJECT IDENTIFIER ::= { hm2TimeSyncMibSNMPExtensionGroup 1 }
hm2TimeSyncSntpSESGroup 		OBJECT IDENTIFIER ::= { hm2TimeSyncMibSNMPExtensionGroup 2 }
hm2TimeSyncNtpSESGroup	 		OBJECT IDENTIFIER ::= { hm2TimeSyncMibSNMPExtensionGroup 3 }
hm2TimeSyncPtpSESGroup	 		OBJECT IDENTIFIER ::= { hm2TimeSyncMibSNMPExtensionGroup 4 }
hm2TimeSyncIrigSESGroup	 		OBJECT IDENTIFIER ::= { hm2TimeSyncMibSNMPExtensionGroup 5 }
hm2TimeSyncDot1asSESGroup	 	OBJECT IDENTIFIER ::= { hm2TimeSyncMibSNMPExtensionGroup 6 }

-- ***********************************************************
-- hm2TimeSyncSntpSESGroup
-- ***********************************************************
hm2TimeSyncSntpSESIpv4PortNumberPairInUse OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION 
           		"Indicates that the given IPv4 address / port number combination is already in use."
           ::= { hm2TimeSyncSntpSESGroup 1 }

hm2TimeSyncSntpSESDnsPortNumberPairInUse OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION 
           		"Indicates that the given DNS name / port number combination is already in use."
           ::= { hm2TimeSyncSntpSESGroup 2 }

hm2TimeSyncSntpSESIpv6PortNumberPairInUse OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION
           		"Indicates that the given IPv6 address / port number combination is already in use."
           ::= { hm2TimeSyncSntpSESGroup 3 }

-- ***********************************************************
-- hm2TimeSyncPtpSESGroup
-- ***********************************************************
hm2TimeSyncPtpSESPortIsNotCapable OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION
                "Indicates that the given port number is not PTP capable."
           ::= { hm2TimeSyncPtpSESGroup 1 }
    
-- *************************************************************
-- Notifications
-- *************************************************************
   
-- *************************************************************
-- Ptp2 notifications
-- *************************************************************
hm2Ptp2SynchronizationChange  NOTIFICATION-TYPE
	OBJECTS		{ hm2PtpIsSynchronized }
	STATUS		current
	DESCRIPTION 
	"This notification is sent if the PTP synchronization status is changed."
	::= { hm2TimeSyncMibNotifications 1 }

-- *************************************************************
-- SNTP notifications
-- *************************************************************
hm2SntpClientSynchronizationChangeTrap  NOTIFICATION-TYPE
	OBJECTS		{ hm2SntpClientStatus }
	STATUS		current
	DESCRIPTION 
	"This notification is sent if the SNTP synchronization status (hm2SntpClientStatus) is changed."
	::= { hm2TimeSyncMibNotifications 10 }

-- *************************************************************
-- Dot1as notifications
-- *************************************************************
hm2Dot1asSynchronizationChange  NOTIFICATION-TYPE
	OBJECTS		{ hm2Dot1asIsSynchronized }
	STATUS		current
	DESCRIPTION 
	"This notification is sent if the dot1as synchronization status is changed."
	::= { hm2TimeSyncMibNotifications 20 }

END

