--******************************************************************************
-- HM-NAT-MIB: Managed objects for 
--
-- May 2011
-- 
-- Copyright (c) Hirschmann Automation & Control GmbH 2011
--******************************************************************************

HM2-NAT-MIB DEFINITIONS ::= BEGIN
IMPORTS 
	OBJECT-TYPE, MODULE-IDENTITY, NOTIFICATION-TYPE,
	Integer32, Unsigned32, Counter64
		FROM SNMPv2-SMI
	RowStatus, DisplayString, TruthValue
		FROM SNMPv2-TC	
	MODULE-COMPLIANCE, OBJECT-GROUP, NOTIFICATION-GROUP
                FROM SNMPv2-CONF
        InterfaceIndex, InterfaceIndexOrZero
        	FROM IF-MIB
        hm2ConfigurationMibs, HmActionValue, HmTimeSeconds1970		   
        	FROM HM2-TC-MIB        
        StorageType  FROM SNMPv2-TC
	;

hm2NatMib MODULE-IDENTITY
	LAST-UPDATED "201111300000Z" -- Nov 30, 2011
	ORGANIZATION "Hirschmann Automation and Control GmbH"
	CONTACT-INFO
        "Postal:     Stuttgarter Str. 45-51
                     72654 Neckartenzlingen
                     Germany
         Phone:      +49 - 7127 -14 -0
         E-mail:     hac.support@belden.com"
        DESCRIPTION
         "This MIB defines the SNMP interface for Hirschmann DNAT/SNAT/
	  Double NAT/1:1 NAT implementations

          Copyright (C) "
        REVISION     "201111300000Z" -- Nov 30, 2011
        DESCRIPTION
         	 "- Added missing protocol information
         	  - Changed stats to 64bit values
         	 "  
        REVISION     "201110240000Z" -- Oct 24, 2011
        DESCRIPTION
         	 "Removed all address types to be in sync with the FW MIB.
         	  The address type is now determined by the parser
         	  automatically.
         	 "  
        REVISION     "201109130000Z" -- Sep 13, 2011
        DESCRIPTION
         	 "- Added commit and pending actions variables
         	  - Added interface mapping tables
         	  - Use HmActionValue instead of TruthValue
         	 "         
        REVISION     "201107010000Z" -- July 1, 2011
        DESCRIPTION
         	 "- Modifications to address representation
         	 "
        REVISION     "201105310000Z" -- May 31, 2011
        DESCRIPTION
          "Initial version."
	::= { hm2ConfigurationMibs 80 }


hm2NatNotifications OBJECT IDENTIFIER ::= { hm2NatMib 0 }

hm2NatObjects OBJECT IDENTIFIER ::= { hm2NatMib 1 }

hm2NatConformance OBJECT IDENTIFIER ::= { hm2NatMib 2}

hm2NatGeneralSettings OBJECT IDENTIFIER ::= { hm2NatObjects 1 }

hm2NatSNMPExtensionGroup OBJECT IDENTIFIER ::= { hm2NatMib 5 }
--******************************************************************************
--                         General Settings Objects
--******************************************************************************


hm2DnatMaxRules OBJECT-TYPE
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Maximum number of allowed rules for DNAT."
        ::= { hm2NatGeneralSettings 2 }

hm2OneToOneNatMaxRules OBJECT-TYPE
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Maximum number of allowed rules for 1:1 NAT."
        ::= { hm2NatGeneralSettings 3 }
	
hm2MasqMaxRules OBJECT-TYPE
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Maximum number of allowed rules for Masquerading."
        ::= { hm2NatGeneralSettings 4 }

hm2DoubleNatMaxRules OBJECT-TYPE
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Maximum number of allowed rules for Double NAT."
        ::= { hm2NatGeneralSettings 5 }

hm2NatResetStatistics OBJECT-TYPE
	SYNTAX HmActionValue
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"Setting this value to action(2) will reset the statistics of 
		 the whole NAT module. It will be set to noop(1) automatically
		 after reset."
		 ::= { hm2NatGeneralSettings 6 }

--******************************************************************************
--                          DNAT Rules Definition
--******************************************************************************

hm2DnatRuleAppliedTrap NOTIFICATION-TYPE
	OBJECTS { hm2DnatRuleIndex }
	STATUS current
	DESCRIPTION
		"A rule of DNAT was applied. The rule is 
		 identified by the given rule index of the rule table."
		 ::= { hm2NatNotifications 1 }

hm2DnatRuleAppliedAndLoggedTrap NOTIFICATION-TYPE
	OBJECTS { hm2DnatRuleIndex }
	STATUS current
	DESCRIPTION
		"A rule of DNAT was applied and logged according to
		 the current logging mechanism. The rule is identified by the 
		 given rule index of the rule table."
		 ::= { hm2NatNotifications 2 }

hm2Dnat OBJECT IDENTIFIER ::= { hm2NatObjects 2 }
	
hm2DnatRules OBJECT IDENTIFIER ::= { hm2Dnat 1 }

hm2DnatRulesObjects OBJECT IDENTIFIER ::= { hm2DnatRules 1 }	

hm2DnatRuleCount OBJECT-TYPE
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Number of current DNAT rules"
	::= { hm2DnatRulesObjects 1 }

hm2DnatIfMappingRuleCount OBJECT-TYPE
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Number of current DNAT IF mapping entries."
	::={ hm2DnatRulesObjects 2 }

hm2DnatRulePendingActions OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"This value describes, whether the DNAT rule table was modified
		 but not yet written to the firewall implementation (set to 
		 true). After writing all modifications to the firewall, the 
		 value switches automatically back to false."
	DEFVAL { false }	 
		 ::={ hm2DnatRulesObjects 3 }

hm2DnatCommitPendingActions OBJECT-TYPE
	SYNTAX HmActionValue
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"Setting this value to action(2) writes not yet committed changes
		 to the firewall (DNAT and Interface Mapping Table). After 
		 writing all modifications, the value switches automatically 
		 back to noop(1)."
	DEFVAL { noop }	 
		 ::={ hm2DnatRulesObjects 4 }

hm2DnatRulesTables OBJECT IDENTIFIER ::= { hm2DnatRules 2 }

hm2DnatRuleTable OBJECT-TYPE 
	SYNTAX SEQUENCE OF Hm2DnatRuleEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"The list of DNAT rules for this firewall."
		::= { hm2DnatRulesTables 1 }	
	
	 hm2DnatRuleEntry OBJECT-TYPE
		SYNTAX Hm2DnatRuleEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"DNAT rule entry."
		INDEX { hm2DnatRuleIndex }
		::= { hm2DnatRuleTable 1 }
		
Hm2DnatRuleEntry ::=
	SEQUENCE {
		hm2DnatRuleIndex Integer32,
		hm2DnatSourceAddress DisplayString,
		hm2DnatSourcePort DisplayString,
		hm2DnatTargetAddress DisplayString,
		hm2DnatTargetPort DisplayString,		
		hm2DnatNewTargetAddress DisplayString,
		hm2DnatNewTargetPort DisplayString,
		hm2DnatProto INTEGER,
		hm2DnatRuleParams DisplayString,
		hm2DnatLog TruthValue,
		hm2DnatTrap TruthValue,
		hm2DnatRowStatus RowStatus,
        hm2DnatDescription DisplayString
	}
		
hm2DnatRuleIndex OBJECT-TYPE
	SYNTAX Integer32 ( 1..255 )
	MAX-ACCESS accessible-for-notify
	STATUS current
	DESCRIPTION
		"Rule index of this DNAT rule."
	::= { hm2DnatRuleEntry 1 }

hm2DnatSourceAddress OBJECT-TYPE
	SYNTAX DisplayString ( SIZE(1..20) )
	MAX-ACCESS read-create
	STATUS current
	DESCRIPTION
		"Source address of packets to be NATed. Can be:
            - Single address (a.b.c.d), 
            - address range in CIDR notation (a.b.c.d/n) 
            - the name of a Netobject ($NetobjectName)
            - 'any' for no filtering at all
            - a prepending '!' selects the complement set"
	DEFVAL  { "any" }     
	::= { hm2DnatRuleEntry 3 }

hm2DnatSourcePort OBJECT-TYPE
	SYNTAX DisplayString ( SIZE(1..50) )
	MAX-ACCESS read-create
	STATUS current
	DESCRIPTION
		"The source port of the packet to reroute. Allowed formats are:
		- keyword 'any' for no filtering or a protocol without ports
		- single port ('10')
		- port range with first and last port separated by hyphen 
		  ('10-15')
		- comma separated list of ports ('1235,25,123')
		- combination of the points above ('10,25-30,125,1993')

        The number of named ports (1 for each individual port, 2 for port
        ranges) must not exceed 15."
	DEFVAL { "any" }
	::= { hm2DnatRuleEntry 4 }

hm2DnatTargetAddress OBJECT-TYPE
	SYNTAX DisplayString ( SIZE(1..20) )
	MAX-ACCESS read-create
	STATUS current
	DESCRIPTION
		"Destination address of packets to be NATed. Can be:
            - Single address (a.b.c.d), 
            - address range in CIDR notation (a.b.c.d/n) 
            - the name of a Netobject ($NetobjectName)
            - 'any' for no filtering at all
            - a prepending '!' selects the complement set"
	::= { hm2DnatRuleEntry 5 }

hm2DnatTargetPort OBJECT-TYPE
	SYNTAX DisplayString ( SIZE(1..50) )
	MAX-ACCESS read-create
	STATUS current
	DESCRIPTION
		"The target port of the packet to reroute. Allowed formats are:
		- keyword 'any'
		- single port ('10')
		- port range with first and last port separated by hyphen 
		  ('10-15')
		- comma separated list of ports ('1235,25,123')
		- combination of the points above ('10,25-30,125,1993')

        The number of named ports (1 for each individual port, 2 for port
        ranges) must not exceed 15."
	DEFVAL { "any" }
	::= { hm2DnatRuleEntry 6 }

hm2DnatNewTargetAddress OBJECT-TYPE
	SYNTAX DisplayString ( SIZE(1..20) )
	MAX-ACCESS read-create
	STATUS current
	DESCRIPTION
		"The IP address of the machine to reroute packets to. Must be a single 
        IP address (a.b.c.d)."
	::= { hm2DnatRuleEntry 7 }

hm2DnatNewTargetPort OBJECT-TYPE
	SYNTAX DisplayString ( SIZE(1..50) )
	MAX-ACCESS read-create
	STATUS current
	DESCRIPTION
		"The port to reroute packets to. Must be a single port or 'any'."
	::= { hm2DnatRuleEntry 8 }

hm2DnatProto OBJECT-TYPE
	SYNTAX		 INTEGER { 
		                   icmp(1), 
		                   igmp(2),
		                   ipip(3),
		                   tcp(4),
		                   udp(5),
		                   esp(6),
		                   ah(7),
		                   icmpv6(8),
		                   any(9)		                 
			}
	MAX-ACCESS 	 read-create
	STATUS 		 current
	DESCRIPTION
		 "The IP protocol (RFC 791) for protocol-independent
                  filtering. The following values are currently
                  supported:
                  o  icmp(1): Internet Control Message Protocol (RFC 792)
                  o  igmp(2): Internet Group Management Protocol
                  o  ipip(3): IP in IP tunneling (RFC 1853)
                  o  tcp(4): Transmission Control Protocol (RFC 793)
                  o  udp(5): User Datagram Protocol (RFC 768)
                  o  esp(6): IPsec Encapsulated Security Payload (RFC 2406)
                  o  ah(7): IPsec Authentication Header (RFC 2402)
                  o  icmpv6(8): Internet Control Message Protocol for IPv6
                  o  any(9): apply to all protocols"
	 DEFVAL  { any }
	 ::= { hm2DnatRuleEntry 9 }

hm2DnatRuleParams OBJECT-TYPE
 	 SYNTAX DisplayString ( SIZE(0..50) )
 	 MAX-ACCESS read-create
 	 STATUS current
 	 DESCRIPTION
 	 	 "Additional parameters to this rule as string. 
		  Currently only the value 'none' is valid.
		  Reserved for future use."
 	 ::= { hm2DnatRuleEntry 10 }	 

hm2DnatLog OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-create
	STATUS current
	DESCRIPTION
		"Set to true if application of this rule shall be logged."
	DEFVAL { false }
	::={ hm2DnatRuleEntry 11 }


hm2DnatTrap OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-create
	STATUS current
	DESCRIPTION
		"Set to true if application of this rule shall send a trap."
	DEFVAL { false }
	::={ hm2DnatRuleEntry 12 }
		

hm2DnatRowStatus OBJECT-TYPE
	SYNTAX RowStatus
	MAX-ACCESS read-create
	STATUS current
	DESCRIPTION
		"This is a standard row status value:
            - active(1): The rule is active. Note that until committed, the rule
              will not be applied.
            - notInService(2): The rule is inactive because of user action.
            - notReady(3):The rule is inactive because it has an incomplete
              configuration.
            - createAndGo(4): Create the rule with default parameters
              activated.
            - createAndWait(5): Create the rule inactive.
            - destroy(6): Delete the rule. You cannot delete a rule with
              interface mappings to it."
		::= { hm2DnatRuleEntry 13 }

hm2DnatDescription OBJECT-TYPE
	SYNTAX DisplayString ( SIZE(0..32) )
	MAX-ACCESS read-create
	STATUS current
	DESCRIPTION "User defined textual description related to this rule."
	DEFVAL  { "" }     
	::= { hm2DnatRuleEntry 14 }
	
hm2DnatRuleIfMappingTable OBJECT-TYPE
	SYNTAX SEQUENCE OF Hm2DnatRuleIfMappingEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Table for mapping DNAT rules to interfaces."
		::={ hm2DnatRulesTables 2 }
	
hm2DnatRuleIfMappingEntry OBJECT-TYPE
	SYNTAX Hm2DnatRuleIfMappingEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Entry in rule interface mapping table."
	INDEX { hm2DnatIfmInterface, hm2DnatIfmDirection, hm2DnatIfmRuleIndex } 
		::={ hm2DnatRuleIfMappingTable 1 }

Hm2DnatRuleIfMappingEntry ::= SEQUENCE {	
	hm2DnatIfmRuleIndex Integer32,
	hm2DnatIfmDirection INTEGER,
	hm2DnatIfmPriority Unsigned32,
	hm2DnatIfmInterface InterfaceIndex,
	hm2DnatIfmRowStatus RowStatus
}

hm2DnatIfmRuleIndex OBJECT-TYPE
	SYNTAX Integer32 (1..2048)
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"The index of the DNAT rule this mapping entry is assigned to."
		::={ hm2DnatRuleIfMappingEntry 1 }

	
hm2DnatIfmDirection OBJECT-TYPE
	SYNTAX INTEGER {
			ingress(1),
			egress(2),
			both(3)
	}
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
        "For DNAT, this can only be set to ingress, which is the interface on
        which a packet that is to be forwarded will arrive."
		::={ hm2DnatRuleIfMappingEntry 2 }
	
hm2DnatIfmPriority OBJECT-TYPE
	SYNTAX Unsigned32 (1..6500)
	MAX-ACCESS read-create
	STATUS current
	DESCRIPTION
        "The priority is the sorting key for rules in the chain to this
        interface. They don't need to be unique per interface, but in
        that case, no clear order can be assumed.
        Priorities are processed in ascending order (0 highest
        priority)."
		::={ hm2DnatRuleIfMappingEntry 3 }
	
hm2DnatIfmInterface OBJECT-TYPE
	SYNTAX InterfaceIndex
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"The interface this mapping entry is assigned to. This has to be either
        an hm2AgentSwitchIpInterfaceIfIndex or an hm2AgentSwitchIpVlanIfIndex.
        Note that for physical interfaces this only works if the corresponding
        hm2AgentSwitchIpInterfaceRoutingMode is set to enable."
		::={ hm2DnatRuleIfMappingEntry 4 }
	
hm2DnatIfmRowStatus OBJECT-TYPE
	SYNTAX RowStatus
	MAX-ACCESS read-create
	STATUS current
	DESCRIPTION
		"The RowStatus value for this entry with the usual meanings:
        
            - active(1): The interface mapping is in place
            - notInService(2): The interface mapping is not in place because the
              user said so
            - notReady(3): The interface mapping is not in place because the
              agent said so
            - createAndGo(4): Create this mapping with the default priority and
              activate it.
            - createAndWait(5): Create this mapping deactivated.
            - destroy(6): Destroy this interface mapping."
		::={ hm2DnatRuleIfMappingEntry 5 }

	
	

hm2DnatStats OBJECT IDENTIFIER ::= { hm2Dnat 2 }

hm2DnatGlobalStats OBJECT IDENTIFIER ::= { hm2DnatStats 1 }

hm2DnatStatsTotalPck OBJECT-TYPE
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Total number of packets processed by the DNAT firewall."
		::= { hm2DnatGlobalStats 1 }
	
hm2DnatStatsTotalPckSize OBJECT-TYPE
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Total number of bytes processed by the DNAT firewall."
		::= { hm2DnatGlobalStats 2 }
	
hm2DnatStatsTotalPckDenDrop OBJECT-TYPE
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Total number of packets dropped or denied by the DNAT firewall."
		::={ hm2DnatGlobalStats 3 }



hm2DnatStatsTotalPckAccepted OBJECT-TYPE
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Total number of packets accepted by the DNAT firewall."
		::={ hm2DnatGlobalStats 4 }
	
hm2DnatRuleStats OBJECT IDENTIFIER ::= { hm2DnatStats 2 }
	
hm2DnatStatsRuleTable OBJECT-TYPE
	SYNTAX SEQUENCE OF Hm2DnatStatsRuleTableEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Table of per-rule statistics of the DNAT firewall."
		::= { hm2DnatRuleStats 1 }
	
hm2DnatStatsRuleTableEntry OBJECT-TYPE
	SYNTAX Hm2DnatStatsRuleTableEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Statistics table entry for DNAT."
	INDEX { hm2DnatRuleIndex }
	::={ hm2DnatStatsRuleTable 1 }
	
Hm2DnatStatsRuleTableEntry ::= SEQUENCE {
	hm2DnatStatsPckCount Counter64,	
	hm2DnatStatsPckSize Counter64,	
	hm2DnatStatsLastApplied HmTimeSeconds1970
}

hm2DnatStatsPckCount OBJECT-TYPE
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Number of packets DNATed."
		::={ hm2DnatStatsRuleTableEntry 1 }

hm2DnatStatsPckSize OBJECT-TYPE
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Number of bytes DNATed."
		::={ hm2DnatStatsRuleTableEntry 2 }
	
hm2DnatStatsLastApplied OBJECT-TYPE
	SYNTAX HmTimeSeconds1970
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Time of last application of the rule in seconds since 1.1.1970."
		::={ hm2DnatStatsRuleTableEntry 3 }
	
--******************************************************************************
--			1:1 NAT
--******************************************************************************

hm21to1RuleAppliedTrap NOTIFICATION-TYPE
	OBJECTS { hm21to1RuleIndex }
	STATUS current
	DESCRIPTION
		"A rule of 1:1 NAT was applied. The rule is 
		 identified by the given rule index of the rule table."
		 ::= { hm2NatNotifications 5 }

hm21to1RuleAppliedAndLoggedTrap NOTIFICATION-TYPE
	OBJECTS { hm21to1RuleIndex }
	STATUS current
	DESCRIPTION
		"A rule of 1:1 NAT was applied and logged according
		 the current logging mechanism. The rule is identified by the 
		 given rule index of the rule table."
		 ::= { hm2NatNotifications 6 }

hm21to1 OBJECT IDENTIFIER ::= { hm2NatObjects 4 }

hm21to1RuleObjects OBJECT IDENTIFIER ::= { hm21to1 1 }

hm21to1RuleCount OBJECT-TYPE
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Number of current 1:1 NAT rules."
	::= { hm21to1RuleObjects 1 }

hm21to1IfMappingRuleCount OBJECT-TYPE
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Number of current 1:1 NAT IF mapping entries."
	::={ hm21to1RuleObjects 2 }

hm21to1RulePendingActions OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"This value describes, whether the 1:1 NAT rule table was 
		 modified but not yet written to the firewall implementation 
		 (set to true). After writing all modifications to the firewall,
		 the value switches automatically back to false."
	DEFVAL { false }	 
		 ::={ hm21to1RuleObjects 3 }

hm21to1CommitPendingActions OBJECT-TYPE
	SYNTAX HmActionValue
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"Setting this value to action(2) writes not yet committed changes
		 to the firewall (1:1 NAT and Interface Mapping Table). After 
		 writing all modifications, the value switches automatically 
		 back to noop(1)."
	DEFVAL { noop }	 
		 ::={ hm21to1RuleObjects 4 }

hm21to1Alg OBJECT-TYPE
    SYNTAX BITS {
           ftp(0),
           icmp(1)
           }
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
        "Global bitmask for application level gateway of all the 1:1 NAT rules."
    DEFVAL    { {icmp, ftp} }
    ::= { hm21to1RuleObjects 5 }

hm21to1PublicIntf OBJECT-TYPE
    SYNTAX InterfaceIndexOrZero
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "The index of the public interface defined on the uplink port."
    DEFVAL { 0 }
    ::= { hm21to1RuleObjects 6 }

hm21to1RuleTables OBJECT IDENTIFIER ::= { hm21to1 2 }

hm21to1RuleTable OBJECT-TYPE 
	SYNTAX SEQUENCE OF Hm21to1RuleEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"The list of 1:1 NAT rules for this firewall."
		::= { hm21to1RuleTables 1 }
	
 hm21to1RuleEntry OBJECT-TYPE	
	SYNTAX Hm21to1RuleEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"1:1 NAT rule entry."
	INDEX { hm21to1RuleIndex }
	::= { hm21to1RuleTable 1 }
	
Hm21to1RuleEntry ::=
	SEQUENCE {
		hm21to1RuleIndex Integer32,		
		hm21to1TargetAddress DisplayString,
		hm21to1NewTargetAddress DisplayString,		
		hm21to1RuleParams DisplayString,
		hm21to1Log TruthValue,
		hm21to1Trap TruthValue,
		hm21to1RowStatus RowStatus,
        hm21to1Description DisplayString,
        hm21to1IngressIntf InterfaceIndexOrZero,
        hm21to1EgressIntf InterfaceIndexOrZero,
        hm21to1Priority Unsigned32,
        hm21to1StorageType StorageType
	}

hm21to1RuleIndex OBJECT-TYPE
	SYNTAX Integer32 ( 1..255 )
	MAX-ACCESS accessible-for-notify
	STATUS current
	DESCRIPTION
		"Rule index of this 1:1 NAT rule."
	::= { hm21to1RuleEntry 1 }

hm21to1TargetAddress OBJECT-TYPE
	SYNTAX DisplayString ( SIZE(1..20) )
	MAX-ACCESS read-create
	STATUS current
	DESCRIPTION
		"Destination address of packets to be NATed. Can be:
            - Single address (a.b.c.d), 
            - address range in CIDR notation (a.b.c.d/n) 
            - the name of a Netobject ($NetobjectName)
            - 'any' for no filtering at all"
	::= { hm21to1RuleEntry 2 }

hm21to1NewTargetAddress OBJECT-TYPE
	SYNTAX DisplayString ( SIZE(1..20) )
	MAX-ACCESS read-create
	STATUS current
	DESCRIPTION
		"New Destination address of packets to be NATed. Can be:
            - Single address (a.b.c.d), 
            - address range in CIDR notation (a.b.c.d/n) 
            - the name of a Netobject ($NetobjectName)
            - 'any' for no filtering at all"
		::= { hm21to1RuleEntry 3 }
	
hm21to1RuleParams OBJECT-TYPE
	SYNTAX DisplayString ( SIZE(0..50) )
 	MAX-ACCESS read-create
 	STATUS current
 	DESCRIPTION
	 	 "Additional parameters to this rule as string. 
		  Currently only the value 'none' is valid.
		  Reserved for future use."
 		 ::= { hm21to1RuleEntry 4 }	 

hm21to1Log OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-create
	STATUS current
	DESCRIPTION
		"Set to true if application of this rule shall be logged."
	DEFVAL { false }
	::={ hm21to1RuleEntry 5 }


hm21to1Trap OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-create
	STATUS current
	DESCRIPTION
		"Set to true if application of this rule shall send a trap."
	DEFVAL { false }
	::={ hm21to1RuleEntry 6 }

hm21to1RowStatus OBJECT-TYPE
	SYNTAX RowStatus
	MAX-ACCESS read-create
	STATUS current
	DESCRIPTION
		"This is a standard row status value:
            - active(1): The rule is active. Note that until committed, the rule
              will not be applied.
            - notInService(2): The rule is inactive because of user action.
            - notReady(3):The rule is inactive because it has an incomplete
              configuration.
            - createAndGo(4): Create the rule with default parameters
              activated.
            - createAndWait(5): Create the rule inactive.
            - destroy(6): Delete the rule. You cannot delete a rule with
              interface mappings to it."
		::= { hm21to1RuleEntry 7 }
	
hm21to1Description OBJECT-TYPE
	SYNTAX DisplayString ( SIZE(0..32) )
	MAX-ACCESS read-create
	STATUS current
	DESCRIPTION "User defined textual description related to this rule."
	DEFVAL  { "" }     
	::= { hm21to1RuleEntry 8 }

hm21to1IngressIntf OBJECT-TYPE
    SYNTAX InterfaceIndexOrZero
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "The index of the interface on which packets going to the target address
        will arrive. This has to be either an hm2AgentSwitchIpInterfaceIfIndex
        or an hm2AgentSwitchIpVlanIfIndex.  Note that for physical interfaces
        this only works if the corresponding
        hm2AgentSwitchIpInterfaceRoutingMode is set to enable."
    DEFVAL { 0 }
    ::= { hm21to1RuleEntry 9 }

hm21to1EgressIntf OBJECT-TYPE
    SYNTAX InterfaceIndexOrZero
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "The index of the interface from which the new target address can be
        reached. This has to be either an hm2AgentSwitchIpInterfaceIfIndex
        or an hm2AgentSwitchIpVlanIfIndex.  Note that for physical interfaces
        this only works if the corresponding
        hm2AgentSwitchIpInterfaceRoutingMode is set to enable."

    DEFVAL { 0 }
    ::= { hm21to1RuleEntry 10 }

hm21to1Priority OBJECT-TYPE
    SYNTAX Unsigned32 (0..6500)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "The priority is the sorting key for rules in the chain to this
        interface. They don't need to be unique per interface, but in that case,
        no clear order can be assumed.
        Priorities are processed in ascending order (0 highest priority)."
    DEFVAL { 0 }
    ::= { hm21to1RuleEntry 11 }

hm21to1StorageType OBJECT-TYPE
    SYNTAX StorageType
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "The storage type for this row.  Rows having the value 
        'volatile' are not saved."
    DEFVAL { nonVolatile }
    ::= { hm21to1RuleEntry 12 }

hm21to1Stats OBJECT IDENTIFIER ::={ hm21to1 3 }

hm21to1GeneralStats OBJECT IDENTIFIER ::= { hm21to1Stats 1 }

hm21to1StatsTotalPck OBJECT-TYPE
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Total number of packets processed by 1:1 NAT."
		::= { hm21to1GeneralStats 1 }

hm21to1StatsTotalPckSize OBJECT-TYPE
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Total number of bytes processed by the 1:1 NAT."
		::= { hm21to1GeneralStats 2 }

hm21to1StatsTotalPckDenDrop OBJECT-TYPE
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Total number of packets dropped or denied by 1:1 NAT."
		::={ hm21to1GeneralStats 3 }

hm21to1StatsTotalPckAccepted OBJECT-TYPE
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Total number of packets accepted by 1:1 NAT."
		::={ hm21to1GeneralStats 4 }
	
hm21to1StatsTables OBJECT IDENTIFIER ::= { hm21to1Stats 2 }
	
hm21to1StatsRuleTable OBJECT-TYPE
	SYNTAX SEQUENCE OF Hm2OtoStatsRuleTableEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Table of per-rule statistics of 1:1 NAT."
		::= { hm21to1StatsTables 1 }
	
Hm2OtoStatsRuleTableEntry ::= SEQUENCE {
	hm21to1StatsPckCount Counter64,
	hm21to1StatsPckSize Counter64,
	hm21to1StatsLastApplied HmTimeSeconds1970
}

hm21to1StatsRuleTableEntry OBJECT-TYPE
	SYNTAX Hm2OtoStatsRuleTableEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Statistics table entry for 1:1 NAT."
	INDEX { hm21to1RuleIndex }
	::={ hm21to1StatsRuleTable 1 }
	
hm21to1StatsPckCount OBJECT-TYPE
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Number of packets matched by this rule."
		::={ hm21to1StatsRuleTableEntry 1 }
	
hm21to1StatsPckSize OBJECT-TYPE
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Number of bytes processed by this rule."
		::={ hm21to1StatsRuleTableEntry 2 }
	
hm21to1StatsLastApplied OBJECT-TYPE
	SYNTAX HmTimeSeconds1970
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Time of last application of the rule in seconds since 1.1.1970."
		::={ hm21to1StatsRuleTableEntry 3 }
	
--******************************************************************************
--				Masquerading
--******************************************************************************

hm2MasqRuleAppliedTrap NOTIFICATION-TYPE
	OBJECTS { hm2MasqRuleIndex }
	STATUS current
	DESCRIPTION
		"A rule of masquerading was applied. The rule is 
		 identified by the given rule index of the rule table."
		 ::= { hm2NatNotifications 7 }

hm2MasqRuleAppliedAndLoggedTrap NOTIFICATION-TYPE
	OBJECTS { hm2MasqRuleIndex }
	STATUS current
	DESCRIPTION
		"A rule of masquerading was applied and logged according
		 the current logging mechanism. The rule is identified by the 
		 given rule index of the rule table."
		 ::= { hm2NatNotifications 8 }

hm2Masquerading OBJECT IDENTIFIER ::= { hm2NatObjects 5 }

hm2MasqRuleObjects OBJECT IDENTIFIER ::= { hm2Masquerading 1 }

hm2MasqRuleCount OBJECT-TYPE
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Number of current masquerading rules."
	::= { hm2MasqRuleObjects 1 }

hm2MasqIfMappingRuleCount OBJECT-TYPE
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Number of current masquerading IF mapping entries."
	::={ hm2MasqRuleObjects 2 }

hm2MasqRulePendingActions OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"This value describes, whether the masquerading rule table was 
		 modified but not yet written to the firewall implementation 
		 (set to true). After writing all modifications to the firewall,
		 the value switches automatically back to false."
	DEFVAL { false }	 
		 ::={ hm2MasqRuleObjects 3 }

hm2MasqCommitPendingActions OBJECT-TYPE
	SYNTAX HmActionValue
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"Setting this value to action(2) writes not yet committed changes
		 to the firewall (DNAT and Interface Mapping Table). After 
		 writing all modifications, the value switches automatically 
		 back to noop(1)."
	DEFVAL { noop }	 
		 ::={ hm2MasqRuleObjects 4 }

hm2MasqRuleTables OBJECT IDENTIFIER ::= { hm2Masquerading 2 } 

hm2MasqRuleTable OBJECT-TYPE 
	SYNTAX SEQUENCE OF Hm2MasqRuleEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"The list of masquerading rules for this firewall."
		::= { hm2MasqRuleTables 1 }

hm2MasqRuleEntry OBJECT-TYPE	
	SYNTAX Hm2MasqRuleEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Masquerading rule entry."
	INDEX { hm2MasqRuleIndex }
	::= { hm2MasqRuleTable 1 }

Hm2MasqRuleEntry ::=
	SEQUENCE {
		hm2MasqRuleIndex Integer32,		
		hm2MasqSourceAddress DisplayString,
		hm2MasqSourcePort DisplayString,
		hm2MasqProto INTEGER,
		hm2MasqRuleParams DisplayString,
		hm2MasqLog TruthValue,
		hm2MasqTrap TruthValue,
		hm2MasqRowStatus RowStatus,
		hm2MasqDescription DisplayString,
		hm2MasqIpsecExempt TruthValue
	}

hm2MasqRuleIndex OBJECT-TYPE
	SYNTAX Integer32 ( 1..128 )
	MAX-ACCESS accessible-for-notify
	STATUS current
	DESCRIPTION
		"Rule index of this masquerading rule."
	::= { hm2MasqRuleEntry 1 }

hm2MasqSourceAddress OBJECT-TYPE
	SYNTAX DisplayString ( SIZE(1..20) )
	MAX-ACCESS read-create
	STATUS current
	DESCRIPTION
		"The source address of the packets to reroute. Allowed formats are:
		- keyword 'any'
		- IP address  ('10.0.0.1')
        - IP address range ('10.0.0.0/8')
        - a prepending '!' selects the complement set
        "
	::= { hm2MasqRuleEntry 2 }

hm2MasqSourcePort OBJECT-TYPE
	SYNTAX DisplayString ( SIZE(1..50) )
	MAX-ACCESS read-create
	STATUS current
	DESCRIPTION
		"The source port of the packet to reroute. Allowed formats are:
		- keyword 'any'
		- single  ('10')
		-  range with first and last separated by hyphen 
		  ('10-15')
		- comma separated list of s ('1235,25,123')
		- combination of the points above ('10,25-30,125,1993')

        The number of named ports (1 for each individual port, 2 for port
        ranges) must not exceed 15."
	DEFVAL { "any" }
	::= { hm2MasqRuleEntry 3 }

hm2MasqProto OBJECT-TYPE
	SYNTAX		 INTEGER { 
		                   tcp(4),
		                   udp(5),
		                   any(9)		                 
			}
	MAX-ACCESS 	 read-create
	STATUS 		 current
	DESCRIPTION
		 "The IP protocol (RFC 791) for protocol-independent
                  filtering. The following values are currently
                  supported:
                  o  tcp(4): transmission control protocol (RFC 793)
                  o  udp(5): user datagram protocol (RFC 768)
                  o  any(9): apply to all protocols"
	 DEFVAL  { any }
	 ::= { hm2MasqRuleEntry 4 }


hm2MasqRuleParams OBJECT-TYPE
 	 SYNTAX DisplayString ( SIZE(0..50) )
 	 MAX-ACCESS read-create
 	 STATUS current
 	 DESCRIPTION
 	 	 "Additional parameters to this rule as string. 
		  Currently only the value 'none' is valid.
		  Reserved for future use."
 	 ::= { hm2MasqRuleEntry 5 }	 

hm2MasqLog OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-create
	STATUS current
	DESCRIPTION
		"Set to true if application of this rule shall be logged."
	DEFVAL { false }
	::={ hm2MasqRuleEntry 6 }


hm2MasqTrap OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-create
	STATUS current
	DESCRIPTION
		"Set to true if application of this rule shall send a trap."
	DEFVAL { false }
	::={ hm2MasqRuleEntry 7 }

hm2MasqRowStatus OBJECT-TYPE
	SYNTAX RowStatus
	MAX-ACCESS read-create
	STATUS current
	DESCRIPTION
		"This is a standard row status value:
            - active(1): The rule is active. Note that until committed, the rule
              will not be applied.
            - notInService(2): The rule is inactive because of user action.
            - notReady(3):The rule is inactive because it has an incomplete
              configuration.
            - createAndGo(4): Create the rule with default parameters
              activated.
            - createAndWait(5): Create the rule inactive.
            - destroy(6): Delete the rule. You cannot delete a rule with
              interface mappings to it."
	::= { hm2MasqRuleEntry 8 }

hm2MasqDescription OBJECT-TYPE
	SYNTAX DisplayString ( SIZE(0..32) )
	MAX-ACCESS read-create
	STATUS current
	DESCRIPTION "User defined textual description related to this rule."
	DEFVAL  { "" }     
	::= { hm2MasqRuleEntry 9 }

hm2MasqIpsecExempt OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-create
	STATUS current
	DESCRIPTION
		"Set to true if application of this rule should ignore IPsec traffic."
	DEFVAL { false }
	::= { hm2MasqRuleEntry 10 }

hm2MasqRuleIfMappingTable OBJECT-TYPE
	SYNTAX SEQUENCE OF Hm2MasqRuleIfMappingEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Table for mapping masquerading rules to interfaces."
		::={ hm2MasqRuleTables 2 }


hm2MasqRuleIfMappingEntry OBJECT-TYPE
	SYNTAX Hm2MasqRuleIfMappingEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Entry in rule interface mapping table."
	INDEX { hm2MasqIfmInterface, hm2MasqIfmDirection, hm2MasqIfmRuleIndex } 
		::={ hm2MasqRuleIfMappingTable 1 }

Hm2MasqRuleIfMappingEntry ::= SEQUENCE {	
	hm2MasqIfmRuleIndex Integer32,
	hm2MasqIfmDirection INTEGER,
	hm2MasqIfmPriority Unsigned32,
	hm2MasqIfmInterface InterfaceIndex,
	hm2MasqIfmRowStatus RowStatus
}
hm2MasqIfmRuleIndex OBJECT-TYPE
	SYNTAX Integer32 (1..2048)
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"The index of the 1:1 NAT rule this mapping entry is assigned 
		 to."
		::={ hm2MasqRuleIfMappingEntry 1 }

	
hm2MasqIfmDirection OBJECT-TYPE
	SYNTAX INTEGER {
			ingress(1),
			egress(2),
			both(3)
	}
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
        "For masquerading, this can only be set to egress which is the interface
        packets will be masqueraded to."
		::={ hm2MasqRuleIfMappingEntry 2 }
	
hm2MasqIfmPriority OBJECT-TYPE
	SYNTAX Unsigned32 (1..6500)
	MAX-ACCESS read-create
	STATUS current
	DESCRIPTION
        "The priority is the sorting key for rules in the chain to this
        interface. They don't need to be unique per interface, but in that case,
        no clear order can be assumed.
        Priorities are processed in ascending order (0 highest priority)."
		::={ hm2MasqRuleIfMappingEntry 3 }
	
hm2MasqIfmInterface OBJECT-TYPE
	SYNTAX InterfaceIndex
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"The interface this mapping entry is assigned to. This has to be either
        an hm2AgentSwitchIpInterfaceIfIndex or an hm2AgentSwitchIpVlanIfIndex.
        Note that for physical interfaces this only works if the corresponding
        hm2AgentSwitchIpInterfaceRoutingMode is set to enable."
		::={ hm2MasqRuleIfMappingEntry 4 }
	
hm2MasqIfmRowStatus OBJECT-TYPE
	SYNTAX RowStatus
	MAX-ACCESS read-create
	STATUS current
	DESCRIPTION
		"The RowStatus value for this entry with the usual meanings:
        
            - active(1): The interface mapping is in place
            - notInService(2): The interface mapping is not in place because the
              user said so
            - notReady(3): The interface mapping is not in place because the
              agent said so
            - createAndGo(4): Create this mapping with the default priority and
              activate it.
            - createAndWait(5): Create this mapping deactivated.
            - destroy(6): Destroy this interface mapping."
		::={ hm2MasqRuleIfMappingEntry 5 }	


hm2MasqStats OBJECT IDENTIFIER ::={ hm2Masquerading 3 }

hm2MasqGeneralStats OBJECT IDENTIFIER ::= { hm2MasqStats 1 }

hm2MasqStatsTotalPck OBJECT-TYPE
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Total number of packets processed by Masquerading"
		::= { hm2MasqGeneralStats 1 }

	
hm2MasqStatsTotalPckSize OBJECT-TYPE
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Total number of bytes processed by Masquerading"
		::= { hm2MasqGeneralStats 2 }

hm2MasqStatsTotalPckDenDrop OBJECT-TYPE
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Total number of packets dropped or denied by Masquerading"
		::={ hm2MasqGeneralStats 3 }

hm2MasqStatsTotalPckAccepted OBJECT-TYPE
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Total number of packets accepted by masquerading."
		::={ hm2MasqGeneralStats 4 }
	
hm2MasqStatsRuleTables OBJECT IDENTIFIER ::= { hm2MasqStats 2 }
	
hm2MasqStatsRuleTable OBJECT-TYPE
	SYNTAX SEQUENCE OF Hm2MasqStatsRuleTableEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Table of per-rule statistics of masquerading."
		::= { hm2MasqStatsRuleTables 1 }

hm2MasqStatsRuleTableEntry OBJECT-TYPE
	SYNTAX Hm2MasqStatsRuleTableEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Statistics table entry for masquerading."
	INDEX { hm2MasqRuleIndex }
	::={ hm2MasqStatsRuleTable 1 }
	
Hm2MasqStatsRuleTableEntry ::= SEQUENCE {
	hm2MasqStatsPckCount Counter64,
	hm2MasqStatsPckSize Counter64,
	hm2MasqStatsLastApplied HmTimeSeconds1970
}
hm2MasqStatsPckCount OBJECT-TYPE
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Number of packets matched by this rule."
		::={ hm2MasqStatsRuleTableEntry 1 }
	
hm2MasqStatsPckSize OBJECT-TYPE
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Number of bytes processed by this rule."
		::={ hm2MasqStatsRuleTableEntry 2 }
	
hm2MasqStatsLastApplied OBJECT-TYPE
	SYNTAX HmTimeSeconds1970
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Time of last application of the rule in seconds since 1.1.1970"
		::={ hm2MasqStatsRuleTableEntry 3 }
	

--******************************************************************************
--                         Double NAT
--******************************************************************************

hm2DonatRuleAppliedTrap NOTIFICATION-TYPE
	OBJECTS { hm2DonatRuleIndex }
	STATUS current
	DESCRIPTION
		"A rule of double NAT was applied. The rule is 
		 identified by the given rule index of the rule table."
		 ::= { hm2NatNotifications 9 }

hm2DonatRuleAppliedAndLoggedTrap NOTIFICATION-TYPE
	OBJECTS { hm2DonatRuleIndex }
	STATUS current
	DESCRIPTION
		"A rule of double NAT was applied and logged according
		 the current logging mechanism. The rule is identified by the 
		 given rule index of the rule table."
		 ::= { hm2NatNotifications 10 }

hm2DoubleNat OBJECT IDENTIFIER ::= { hm2NatObjects 6 }

hm2DoubleNatRuleObjects OBJECT IDENTIFIER ::= { hm2DoubleNat 1 }


hm2DoubleNatRuleCount OBJECT-TYPE
	SYNTAX Integer32
	MAX-ACCESS read-only	
	STATUS current
	DESCRIPTION
		"Current number of rules for double NAT."
		::= { hm2DoubleNatRuleObjects 1 }

hm2DoubleNatIfMappingRuleCount OBJECT-TYPE
	SYNTAX Integer32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Number of current double NAT IF mapping entries."
	::={ hm2DoubleNatRuleObjects 2 }	
	
hm2DoubleNatRulePendingActions OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"This value describes, whether the double NAT rule table was 
		 modified but not yet written to the firewall implementation 
		 (set to true). After writing all modifications to the firewall,
		 the value switches automatically back to false."
	DEFVAL { false }	 
		 ::={ hm2DoubleNatRuleObjects 3 }

hm2DoubleNatCommitPendingActions OBJECT-TYPE
	SYNTAX HmActionValue
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"Setting this value to action(2) writes not yet committed changes
		 to the firewall (double NAT and interface mapping table). After 
		 writing all modifications, the value switches automatically 
		 back to noop(1)."
	DEFVAL { noop }	 
		 ::={ hm2DoubleNatRuleObjects 4 }
	
hm2DoubleNatRuleTables OBJECT IDENTIFIER ::= { hm2DoubleNat 2 }

hm2DoubleNatRuleTable OBJECT-TYPE
	SYNTAX SEQUENCE OF Hm2DoubleNatRuleEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Table of double NAT rules."
		::= { hm2DoubleNatRuleTables 1 }
	
 hm2DoubleNatRuleEntry OBJECT-TYPE
	SYNTAX Hm2DoubleNatRuleEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Entry within double NAT rule table."
	INDEX { hm2DonatRuleIndex }	
		::= { hm2DoubleNatRuleTable 1 }
		
Hm2DoubleNatRuleEntry ::= SEQUENCE {
	hm2DonatRuleIndex Integer32,
	hm2DonatLocalInternalIp DisplayString,
	hm2DonatLocalExternalIp DisplayString,
	hm2DonatRemoteInternalIp DisplayString,
	hm2DonatRemoteExternalIp DisplayString,
	hm2DonatRuleParams DisplayString,
	hm2DonatLog TruthValue,
	hm2DonatTrap TruthValue,
	hm2DonatRowStatus RowStatus,
    hm2DonatDescription DisplayString
}

hm2DonatRuleIndex OBJECT-TYPE
	SYNTAX Integer32 (1..255)
	MAX-ACCESS accessible-for-notify
	STATUS current
	DESCRIPTION
		"Index of the rule within table."
		::= { hm2DoubleNatRuleEntry 1 }
	
hm2DonatLocalInternalIp OBJECT-TYPE
	SYNTAX DisplayString ( SIZE(1..20) )
	MAX-ACCESS read-create
	STATUS current
	DESCRIPTION
        "The real IP address of the first net/machine you want to double NAT.
        Allowed formats are:
		- keyword 'any'
		- IP address  ('10.0.0.1')
        - IP address range ('10.0.0.0/8')"
		::= { hm2DoubleNatRuleEntry 2 }
	
hm2DonatLocalExternalIp OBJECT-TYPE
	SYNTAX DisplayString ( SIZE(1..20) )
	MAX-ACCESS read-create
	STATUS current
	DESCRIPTION
        "The IP address where you want the first net/machine to be reachable
        from the second net/machine.
        Allowed formats are:
		- keyword 'any'
		- IP address  ('10.0.0.1')
        - IP address range ('10.0.0.0/8')"
		::= { hm2DoubleNatRuleEntry 3 }
	
hm2DonatRemoteInternalIp OBJECT-TYPE
	SYNTAX DisplayString ( SIZE(1..20) )
	MAX-ACCESS read-create
	STATUS current
	DESCRIPTION
        "The real IP address of the second net/machine you want to double NAT.
        Allowed formats are:
		- keyword 'any'
		- IP address  ('10.0.0.1')
        - IP address range ('10.0.0.0/8')"
		::= { hm2DoubleNatRuleEntry 4 }

hm2DonatRemoteExternalIp OBJECT-TYPE
	SYNTAX DisplayString ( SIZE(1..20) )
	MAX-ACCESS read-create
	STATUS current
	DESCRIPTION
        "The IP address where you want the second net/machine to be reachable
        from the first net/machine.
        Allowed formats are:
		- keyword 'any'
		- IP address  ('10.0.0.1')
        - IP address range ('10.0.0.0/8')"
		::= { hm2DoubleNatRuleEntry 5 }

hm2DonatRuleParams OBJECT-TYPE
 	 SYNTAX DisplayString ( SIZE(0..50) )
 	 MAX-ACCESS read-create
 	 STATUS current
 	 DESCRIPTION
 	 	 "Additional parameters to this rule as string. 
		  Currently only the value 'none' is valid.
		  Reserved for future use."
 	 ::= { hm2DoubleNatRuleEntry 6 }	 
	
hm2DonatLog OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-create
	STATUS current
	DESCRIPTION
		"Set to true if application of this rule shall be logged."
	DEFVAL { false }
	::={ hm2DoubleNatRuleEntry 7 }


hm2DonatTrap OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-create
	STATUS current
	DESCRIPTION
		"Set to true if application of this rule shall send a trap."
	DEFVAL { false }
	::={ hm2DoubleNatRuleEntry 8 }

hm2DonatRowStatus OBJECT-TYPE
	SYNTAX RowStatus
	MAX-ACCESS read-create
	STATUS current
	DESCRIPTION
		"This is a standard row status value:
            - active(1): The rule is active. Note that until committed, the rule
              will not be applied.
            - notInService(2): The rule is inactive because of user action.
            - notReady(3):The rule is inactive because it has an incomplete
              configuration.
            - createAndGo(4): Create the rule with default parameters
              activated.
            - createAndWait(5): Create the rule inactive.
            - destroy(6): Delete the rule. You cannot delete a rule with
              interface mappings to it."
		::= { hm2DoubleNatRuleEntry 9 }

hm2DonatDescription OBJECT-TYPE
	SYNTAX DisplayString ( SIZE(0..32) )
	MAX-ACCESS read-create
	STATUS current
	DESCRIPTION "User defined textual description related to this rule."
	DEFVAL  { "" }
	::= { hm2DoubleNatRuleEntry 10 }

hm2DonatRuleIfMappingTable OBJECT-TYPE
	SYNTAX SEQUENCE OF Hm2DonatRuleIfMappingEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Table for mapping double NAT rules to interfaces."
		::={ hm2DoubleNatRuleTables 2 }
	
hm2DonatRuleIfMappingEntry OBJECT-TYPE
	SYNTAX Hm2DonatRuleIfMappingEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Entry in rule interface mapping table."
	INDEX { hm2DonatIfmInterface, hm2DonatIfmDirection, hm2DonatIfmRuleIndex } 
		::={ hm2DonatRuleIfMappingTable 1 }

Hm2DonatRuleIfMappingEntry ::= SEQUENCE {	
	hm2DonatIfmRuleIndex Integer32,
	hm2DonatIfmDirection INTEGER,
	hm2DonatIfmPriority Unsigned32,
	hm2DonatIfmInterface InterfaceIndex,
	hm2DonatIfmRowStatus RowStatus
}

hm2DonatIfmRuleIndex OBJECT-TYPE
	SYNTAX Integer32 (1..2048)
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"The index of the double NAT rule this mapping entry is assigned 
		 to."
		::={ hm2DonatRuleIfMappingEntry 1 }

	
hm2DonatIfmDirection OBJECT-TYPE
	SYNTAX INTEGER {
			ingress(1),
			egress(2),
			both(3)
	}
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
        "Meanings:
            - ingress(1): The first net/machine can be reached through this
              interface
            - egress(2): The second net/machine can be reached through this
              interface
            - both(3): Both machines/nets can be reached through this interface"
		::={ hm2DonatRuleIfMappingEntry 2 }
	
hm2DonatIfmPriority OBJECT-TYPE
	SYNTAX Unsigned32 (1..6500)
	MAX-ACCESS read-create
	STATUS current
	DESCRIPTION
        "The priority is the sorting key for rules in the chain to this
        interface. They don't need to be unique per interface, but in that case,
        no clear order can be assumed.
        Priorities are processed in ascending order (0 highest priority)."
		::={ hm2DonatRuleIfMappingEntry 3 }
	
hm2DonatIfmInterface OBJECT-TYPE
	SYNTAX InterfaceIndex
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"The interface this mapping entry is assigned to. This has to be either
        an hm2AgentSwitchIpInterfaceIfIndex or an hm2AgentSwitchIpVlanIfIndex.
        Note that for physical interfaces this only works if the corresponding
        hm2AgentSwitchIpInterfaceRoutingMode is set to enable."
		::={ hm2DonatRuleIfMappingEntry 4 }
	
hm2DonatIfmRowStatus OBJECT-TYPE
	SYNTAX RowStatus
	MAX-ACCESS read-create
	STATUS current
	DESCRIPTION
		"The RowStatus value for this entry with the usual meanings:
        
            - active(1): The interface mapping is in place
            - notInService(2): The interface mapping is not in place because the
              user said so
            - notReady(3): The interface mapping is not in place because the
              agent said so
            - createAndGo(4): Create this mapping with the default priority and
              activate it.
            - createAndWait(5): Create this mapping deactivated.
            - destroy(6): Destroy this interface mapping."
		::={ hm2DonatRuleIfMappingEntry 5 }	

	
hm2DonatStats OBJECT IDENTIFIER ::={ hm2DoubleNat 3 }

hm2DonatGeneralStats OBJECT IDENTIFIER ::= { hm2DonatStats 1 }

hm2DonatStatsTotalPck OBJECT-TYPE
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Total number of packets processed by double NAT."
		::= { hm2DonatGeneralStats 1 }
	
hm2DonatStatsTotalPckSize OBJECT-TYPE
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Total number of bytes processed by double NAT."
		::= { hm2DonatGeneralStats 2 }

hm2DonatStatsTotalPckDenDrop OBJECT-TYPE
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Total number of packets dropped or denied by double NAT."
		::={ hm2DonatGeneralStats 3 }
	
hm2DonatStatsTotalPckAcc OBJECT-TYPE
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Total number of packets accepted by double NAT."
		::={ hm2DonatGeneralStats 4 }
	
hm2DonatStatsRuleTables OBJECT IDENTIFIER ::= { hm2DonatStats 2 }
	
hm2DonatStatsRuleTable OBJECT-TYPE
	SYNTAX SEQUENCE OF Hm2DonatStatsRuleTableEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Table of per-rule statistics of double NAT."
		::= { hm2DonatStatsRuleTables 1 }
	
hm2DonatStatsRuleTableEntry OBJECT-TYPE
	SYNTAX Hm2DonatStatsRuleTableEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
		"Statistics table entry for double NAT."
	INDEX { hm2DonatRuleIndex }
	::={ hm2DonatStatsRuleTable 1 }
	
Hm2DonatStatsRuleTableEntry ::= SEQUENCE {
	hm2DonatStatsPckCount Counter64,
	hm2DonatStatsPckSize Counter64,
	hm2DonatStatsLastApplied HmTimeSeconds1970
}

hm2DonatStatsPckCount OBJECT-TYPE
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Number of packets matched by this rule."
		::={ hm2DonatStatsRuleTableEntry 1 }

hm2DonatStatsPckSize OBJECT-TYPE
	SYNTAX Counter64
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Number of bytes processed by this rule."
		::={ hm2DonatStatsRuleTableEntry 2 }

hm2DonatStatsLastApplied OBJECT-TYPE
	SYNTAX HmTimeSeconds1970
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
		"Time of last application of the rule in seconds since 1.1.1970."
		::={ hm2DonatStatsRuleTableEntry 3 }

--******************************************************************************
--			Compliance statements
--******************************************************************************

hm2NatCompliances OBJECT IDENTIFIER ::= { hm2NatConformance 1 }
hm2NatGroups OBJECT IDENTIFIER ::= { hm2NatConformance 2 }

hm2NatCompliance MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
        "The compliance statement for an SNMP entity which
         implements the Hirschmann NAT MIB."
    MODULE     -- this module
    MANDATORY-GROUPS { hm2NatGeneralGroup, hm2NatNotificationsGroup }
    ::= { hm2NatCompliances 1 }

hm2NatGeneralGroup OBJECT-GROUP
    OBJECTS {
    	hm2DnatMaxRules,
    	hm2OneToOneNatMaxRules,
    	hm2DoubleNatMaxRules,
    	hm2MasqMaxRules,
    	hm2NatResetStatistics,

    	hm2DnatIfMappingRuleCount,
	hm2DnatRulePendingActions,
    	hm2DnatCommitPendingActions,
	hm2DnatRuleCount,
	hm2DnatRuleIndex,
	hm2DnatSourceAddress,
	hm2DnatSourcePort,
	hm2DnatTargetAddress,
	hm2DnatTargetPort,	
	hm2DnatNewTargetAddress,
	hm2DnatNewTargetPort,
	hm2DnatProto,
	hm2DnatRuleParams,
	hm2DnatLog,
	hm2DnatTrap,
        hm2DnatDescription,
	hm2DnatRowStatus,
	hm2DnatIfmPriority,
	hm2DnatIfmRowStatus,	
        hm2DnatStatsPckCount,
        hm2DnatStatsPckSize,
	hm2DnatStatsLastApplied,
	hm2DnatStatsTotalPck,
	hm2DnatStatsTotalPckSize,
	hm2DnatStatsTotalPckDenDrop,
	hm2DnatStatsTotalPckAccepted,
	
	hm21to1IfMappingRuleCount,
	hm21to1RulePendingActions,
    	hm21to1CommitPendingActions,
	hm21to1RuleCount,
	hm21to1RuleIndex,	
	hm21to1TargetAddress,	
	hm21to1NewTargetAddress,
	hm21to1RuleParams,
	hm21to1Log,
	hm21to1Trap,
        hm21to1Description,
        hm21to1IngressIntf,
        hm21to1EgressIntf,
        hm21to1Priority,

	hm21to1RowStatus,
        hm21to1StatsPckCount,
        hm21to1StatsPckSize,
	hm21to1StatsLastApplied,
	hm21to1StatsTotalPck,
	hm21to1StatsTotalPckSize,
	hm21to1StatsTotalPckDenDrop,
	hm21to1StatsTotalPckAccepted,
	
	hm2MasqIfMappingRuleCount,
	hm2MasqRulePendingActions,
    	hm2MasqCommitPendingActions,
	hm2MasqRuleCount,
	hm2MasqRuleIndex,	
	hm2MasqSourceAddress,
	hm2MasqSourcePort,
	hm2MasqProto,
	hm2MasqRuleParams,
	hm2MasqLog,
	hm2MasqTrap,
        hm2MasqDescription,
	hm2MasqRowStatus,
	hm2MasqIfmPriority,
	hm2MasqIfmRowStatus,	
        hm2MasqStatsPckCount,
        hm2MasqStatsPckSize,
	hm2MasqStatsLastApplied,
	hm2MasqStatsTotalPck,
	hm2MasqStatsTotalPckSize,
	hm2MasqStatsTotalPckDenDrop,
	hm2MasqStatsTotalPckAccepted,
	
	hm2DoubleNatIfMappingRuleCount,
	hm2DoubleNatRulePendingActions,
    	hm2DoubleNatCommitPendingActions,
	hm2DoubleNatRuleCount,
	hm2DonatRuleIndex,	
	hm2DonatLocalInternalIp,	
	hm2DonatLocalExternalIp,
	hm2DonatRemoteInternalIp,	
	hm2DonatRemoteExternalIp,
	hm2DonatRuleParams,
	hm2DonatLog,
	hm2DonatTrap,
        hm2DonatDescription,
	hm2DonatIfmPriority,
	hm2DonatIfmRowStatus,	
	hm2DonatRowStatus,
	hm2DonatStatsPckCount,
	hm2DonatStatsPckSize,
	hm2DonatStatsLastApplied,
	hm2DonatStatsTotalPck,
	hm2DonatStatsTotalPckSize,
	hm2DonatStatsTotalPckDenDrop,
	hm2DonatStatsTotalPckAcc
	
    }
    STATUS      current
    DESCRIPTION
        "A collection of all Hirschmann objects provided by the Firewall
        module."
    ::= { hm2NatGroups 1 }

hm2NatNotificationsGroup  NOTIFICATION-GROUP
	NOTIFICATIONS {
		
		hm2DnatRuleAppliedTrap,
		hm2DnatRuleAppliedAndLoggedTrap,
		
		hm21to1RuleAppliedTrap,
		hm21to1RuleAppliedAndLoggedTrap,
		
		hm2MasqRuleAppliedTrap,
		hm2MasqRuleAppliedAndLoggedTrap,
		
		hm2DonatRuleAppliedTrap,
		hm2DonatRuleAppliedAndLoggedTrap
	}
	STATUS current
	DESCRIPTION
		"A collection of all Hirschmann notifications provided by the
		NAT module."
		::= { hm2NatGroups 2 }

--******************************************************************************
--                      hm2NatSNMPExtensionGroup
--******************************************************************************

hm2NatSNMPExtensionEgressInterfaceInvalid OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "Indicates that the 1 to 1 NAT rule entry contains an invalid value
                        for egress interface that cannot be processed."
           ::= { hm2NatSNMPExtensionGroup 1 }

hm2NatSNMPExtensionIngressInterfaceInvalid OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "Indicates that the 1 to 1 NAT rule entry contains an invalid value
                        for ingress interface that cannot be processed."
           ::= { hm2NatSNMPExtensionGroup 2 }

hm2NatSNMPExtensionIPsecExemptInvalid OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "Indicates that the masquerading NAT rule entry contains an invalid value
                        for ipsec exempt that cannot be processed."
           ::= { hm2NatSNMPExtensionGroup 3 }

hm2NatSNMPExtensionLocalExternalIPInvalid OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "Indicates that the double NAT rule entry contains an invalid value
                        for local external IP address that cannot be processed."
           ::= { hm2NatSNMPExtensionGroup 4 }

hm2NatSNMPExtensionLocalInternalIPInvalid OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "Indicates that the double NAT rule entry contains an invalid value
                        for local internal IP  address that cannot be processed."
           ::= { hm2NatSNMPExtensionGroup 5 }

hm2NatSNMPExtensionNewDestAddrInvalid OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "Indicates that the 1 to 1/destination NAT rule entry contains an invalid value
                        for new destination address that cannot be processed."
           ::= { hm2NatSNMPExtensionGroup 6 }

hm2NatSNMPExtensionNewDestPortInvalid OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "Indicates that the destination NAT rule entry contains an invalid value
                        for new destination port that cannot be processed."
           ::= { hm2NatSNMPExtensionGroup 7 }

hm2NatSNMPExtensionRemoteExternalIPInvalid OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "Indicates that the double NAT rule entry contains an invalid value
                        for remote external IP address that cannot be processed."
           ::= { hm2NatSNMPExtensionGroup 8 }

hm2NatSNMPExtensionRemoteInternalIPInvalid OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "Indicates that the double NAT rule entry contains an invalid value
                        for remote internal IP address that cannot be processed."
           ::= { hm2NatSNMPExtensionGroup 9 }

hm2NatSNMPExtensionBadDestAddr OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "Indicates that the 1 to 1 NAT rule entry contains an invalid
                        destination IP address range and cannot be processed."
           ::= { hm2NatSNMPExtensionGroup 10 }

hm2NatSNMPExtensionBadNewDestAddr OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "Indicates that the 1 to 1 NAT rule entry contains an invalid
                        new destination IP address range and cannot be processed."
           ::= { hm2NatSNMPExtensionGroup 11 }

hm2NatSNMPExtensionDestAndNewDestAddrSubnetError OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "Indicates that the 1 to 1 NAT rule entry contains destination IP address
                        and new destination IP address which are not on the same subnet and cannot
                        be processed."
           ::= { hm2NatSNMPExtensionGroup 12 }

hm2NatSNMPExtensionBadRuleParameter OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "Indicates that the 1 to 1 NAT rule entry contains invalid rule parameters
                        that cannot be processed."
           ::= { hm2NatSNMPExtensionGroup 13 }

hm2NatSNMPExtensionIngressAndEgressIntfEqualError OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "Indicates that the 1 to 1 NAT rule entry contains the same values for ingress
                        and egress interfaces and cannot be processed."
           ::= { hm2NatSNMPExtensionGroup 14 }
END


