
HM2-NETCONFIG-MIB DEFINITIONS ::= BEGIN

--
-- *************************************************************
-- Hirschmann Network Configuration MIB
-- *************************************************************
--

IMPORTS
	NOTIFICATION-TYPE,
    MODULE-IDENTITY, 
    OBJECT-TYPE,
    Unsigned32,
    Integer32					FROM SNMPv2-SMI  
    TEXTUAL-CONVENTION,
    DisplayString,
    RowStatus,
    MacAddress                	FROM SNMPv2-TC
	TimeFilter					FROM RMON2-MIB
    InetAddressType,
    InetAddress, 
    InetAddressPrefixLength
    			                FROM INET-ADDRESS-MIB
    ifIndex,
   	InterfaceIndex              FROM IF-MIB
	IpAddressOriginTC           FROM IP-MIB
    hm2ConfigurationMibs,
    HmEnabledStatus             FROM HM2-TC-MIB;


hm2NetConfigMib MODULE-IDENTITY
	LAST-UPDATED "201103160000Z" -- March 16, 2011
    ORGANIZATION "Hirschmann Automation and Control GmbH"
    CONTACT-INFO
        "Postal:     Stuttgarter Str. 45-51
                     72654 Neckartenzlingen
                     Germany
         Phone:      +49 7127 140
         E-mail:     hac.support@belden.com"
    DESCRIPTION
        "Hirschmann Network Configuration MIB.
         Copyright (C) 2012. All Rights Reserved."
    REVISION     "201103160000Z" -- March 16, 2011
    DESCRIPTION
         "Initial version."
    ::= { hm2ConfigurationMibs 20 }

--
-- *************************************************************
-- hm2NetConfigMib
-- *************************************************************
--
hm2NetConfigMibNotifications	OBJECT IDENTIFIER ::= { hm2NetConfigMib 0 }
hm2NetConfigMibObjects			OBJECT IDENTIFIER ::= { hm2NetConfigMib 1 }
-- hm2NetConfigMibConformance			OBJECT IDENTIFIER ::= { hm2NetConfigMib 2 }

--
-- *************************************************************
-- hm2NetConfigMib groups
-- *************************************************************
--
hm2NetStaticGroup		OBJECT IDENTIFIER ::= { hm2NetConfigMibObjects 1 }
hm2NetACDGroup			OBJECT IDENTIFIER ::= { hm2NetConfigMibObjects 2 }
hm2NetMacGroup			OBJECT IDENTIFIER ::= { hm2NetConfigMibObjects 3 }
hm2NetHiDiscoveryGroup	OBJECT IDENTIFIER ::= { hm2NetConfigMibObjects 4 }
hm2NetMacACDGroup		OBJECT IDENTIFIER ::= { hm2NetConfigMibObjects 5 }
hm2NetOobMgmtGroup		OBJECT IDENTIFIER ::= { hm2NetConfigMibObjects 6 }
hm2NetOobUsbMgmtGroup	OBJECT IDENTIFIER ::= { hm2NetConfigMibObjects 7 }


--
-- *************************************************************
-- hm2NetStaticGroup
-- *************************************************************
--

hm2NetConfigProtocol	OBJECT-TYPE
			SYNTAX		INTEGER {
								none(1),
								bootp(2),
								dhcp(3)
						}
			MAX-ACCESS	read-write
			STATUS		current
			DESCRIPTION
					"The switch's network configuration protocol.
					 The default value is dependent of the device type."
			DEFVAL { dhcp }
			::= { hm2NetStaticGroup 1 }


hm2NetLocalIPAddrType	OBJECT-TYPE
			SYNTAX		InetAddressType
			MAX-ACCESS	read-write
			STATUS		current
			DESCRIPTION
					"Local IP address type."
			DEFVAL { ipv4 }
			::= { hm2NetStaticGroup 2 }


hm2NetLocalIPAddr		OBJECT-TYPE
			SYNTAX		InetAddress
			MAX-ACCESS	read-write
			STATUS		current
			DESCRIPTION
					"IP address of the management agent board.
					Changing this value will take effect after activating
					with hm2NetAction."
			DEFVAL { '00000000'H }
			::= { hm2NetStaticGroup 3 }

hm2NetPrefixLength		OBJECT-TYPE
			SYNTAX		InetAddressPrefixLength
			MAX-ACCESS	read-write
			STATUS		current
			DESCRIPTION
					"The length of the IP netmask."
            DEFVAL { 0 }
			::= { hm2NetStaticGroup 4 }

hm2NetGatewayIPAddrType	OBJECT-TYPE
			SYNTAX		InetAddressType
			MAX-ACCESS	read-write
			STATUS		current
			DESCRIPTION
					"Default gateway IP address type."
			DEFVAL { ipv4 }
			::= { hm2NetStaticGroup 5 }


hm2NetGatewayIPAddr		OBJECT-TYPE
			SYNTAX		InetAddress
			MAX-ACCESS	read-write
			STATUS		current
			DESCRIPTION
					"IP address of the default gateway.
					 Changing this value will take effect after activating
					 with hm2NetAction."
			DEFVAL { '00000000'H }
			::= { hm2NetStaticGroup 6 }

hm2NetVlanID			OBJECT-TYPE
			SYNTAX		Integer32 (1..4042)
			MAX-ACCESS	read-write
			STATUS		current
			DESCRIPTION
					"VLAN-ID of the IP protocol stack. The VLAN-ID value means
					 that only traffic of the appropriate VLAN is accepted and
					 outgoing traffic uses this VLAN-ID."
			DEFVAL { 1 }
			::= { hm2NetStaticGroup 7 }

hm2NetVlanPriority		OBJECT-TYPE
			SYNTAX		Integer32 (0..7)
			MAX-ACCESS	read-write
			STATUS		current
			DESCRIPTION
					"VLAN Priority which is used in management replies."
			DEFVAL { 0 }
			::= { hm2NetStaticGroup 8 }

hm2NetIpDscpPriority	OBJECT-TYPE
			SYNTAX		Integer32 (0..63)
			MAX-ACCESS	read-write
			STATUS		current
			DESCRIPTION
					"IP DSCP value which is used in management replies."
			DEFVAL { 0 }			
			::= { hm2NetStaticGroup 9 }

hm2NetMgmtPort OBJECT-TYPE
			SYNTAX      Integer32
			MAX-ACCESS  read-write
			STATUS      current
			DESCRIPTION
					"The port number of the Ethernet port, which gets the access to
					 the switch management.
					 If the value is set to 0, the access to the switch management is 
					 permitted from all ports of the switch.
					 This object is only applicable for embedded switches which are 
					 integrated into customer devices."
		    DEFVAL { 0 }
			::= { hm2NetStaticGroup 10 }

hm2NetDHCPClientId OBJECT-TYPE 
		    SYNTAX       DisplayString (SIZE (0..255))
    		MAX-ACCESS   read-only
    		STATUS       current 
    		DESCRIPTION 
      			"The identifier string that is currently used by the client in the 
      			 request packets to the server for obtaining lease information." 
			::= { hm2NetStaticGroup 11 }

hm2NetDHCPClientConfigLoad OBJECT-TYPE
			SYNTAX  HmEnabledStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
					"Enables/disables the DHCP options 4/42 (time servers) and 66/67 
					(Load config over TFTP on boot) on DHCP/BOOTP client."
			DEFVAL { enable }
			::= { hm2NetStaticGroup 20 }

hm2NetDHCPClientLeaseTime OBJECT-TYPE
			SYNTAX  Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
					"Displays the remaining lease of the management IP time in seconds."
			::= { hm2NetStaticGroup 21 }

hm2NetIPv6AdminStatus OBJECT-TYPE
			SYNTAX HmEnabledStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Enable/Disable IPv6 feature. A (1) enables, a (2) disables."
			DEFVAL { enable }
			::= { hm2NetStaticGroup 30 }

hm2NetIPv6ConfigProtocol	OBJECT-TYPE
			SYNTAX		INTEGER {
								none(1),
								auto(2),
								dhcpv6(3),
								all(4)
						}
			MAX-ACCESS	read-write
			STATUS		current
			DESCRIPTION
					"The switch's network IPv6 configuration protocol."
			DEFVAL { auto }
			::= { hm2NetStaticGroup 31 }

hm2NetIPv6GatewayAddrType	OBJECT-TYPE
			SYNTAX		InetAddressType
			MAX-ACCESS	read-write
			STATUS		current
			DESCRIPTION
					"Default gateway IPv6 address type."
			DEFVAL { ipv6 }
			::= { hm2NetStaticGroup 32 }


hm2NetIPv6GatewayAddr	OBJECT-TYPE
			SYNTAX		InetAddress
			MAX-ACCESS	read-write
			STATUS		current
			DESCRIPTION
					"IPv6 address of the default gateway."
			DEFVAL { '00000000000000000000000000000000'H }
			::= { hm2NetStaticGroup 33 }

hm2NetIPv6DupAddrDetectTrans		OBJECT-TYPE
			SYNTAX		Integer32 (0..5)
			MAX-ACCESS	read-write
			STATUS		current
			DESCRIPTION
					"Number of Neighbor Solicitations for DAD mechanism."
			DEFVAL { 1 }
			::= { hm2NetStaticGroup 34 }

hm2NetIPv6DHCPClientId   OBJECT-TYPE
		    SYNTAX       DisplayString (SIZE (0..255))
    		MAX-ACCESS   read-only
    		STATUS       current
    		DESCRIPTION
					"The identifier string that is currently used by the client in the
      				IPv6 implementation to request packets to the server to obtain
					lease information."
			::= { hm2NetStaticGroup 35 }

hm2NetIPv6LocalAddrTable OBJECT-TYPE
			SYNTAX  SEQUENCE OF Hm2NetIPv6LocalAddrEntry
			MAX-ACCESS  not-accessible
			STATUS      current
			DESCRIPTION
					"The list of IPv6 addresses and their prefixes
					for the network port."
			::=  { hm2NetStaticGroup 36 }

hm2NetIPv6LocalAddrEntry OBJECT-TYPE
			SYNTAX  Hm2NetIPv6LocalAddrEntry
			MAX-ACCESS  not-accessible
			STATUS      current
			DESCRIPTION
				"An interface entry containing objects of
				a particular IPv6 address prefix"
			INDEX   {
					hm2NetIPv6LocalAddrPrefixType,
					hm2NetIPv6LocalAddrPrefix,
					hm2NetIPv6LocalAddrPrefixLength
					}
			::= { hm2NetIPv6LocalAddrTable 1 }
			Hm2NetIPv6LocalAddrEntry ::= SEQUENCE {
				hm2NetIPv6LocalAddrPrefixType      InetAddressType,
				hm2NetIPv6LocalAddrPrefix          InetAddress,
				hm2NetIPv6LocalAddrPrefixLength    INTEGER,
				hm2NetIPv6LocalAddrType            InetAddressType,
				hm2NetIPv6LocalAddr                InetAddress,
				hm2NetIPv6LocalAddrEuiFlag         INTEGER,
				hm2NetIPv6LocalAddrOrigin          IpAddressOriginTC,
				hm2NetIPv6LocalAddrStatus          RowStatus
			}

			hm2NetIPv6LocalAddrPrefixType OBJECT-TYPE
				SYNTAX      InetAddressType
				MAX-ACCESS  not-accessible
				STATUS      current
				DESCRIPTION
					"The management IPv6 prefix type"
			    ::=  { hm2NetIPv6LocalAddrEntry 1 }

			hm2NetIPv6LocalAddrPrefix OBJECT-TYPE
				SYNTAX      InetAddress
				MAX-ACCESS  not-accessible
				STATUS      current
				DESCRIPTION
					"IPv6 prefix of the management agent board."
				::=  { hm2NetIPv6LocalAddrEntry 2 }

			hm2NetIPv6LocalAddrPrefixLength OBJECT-TYPE
				SYNTAX      INTEGER (0..128)
				MAX-ACCESS  not-accessible
				STATUS      current
				DESCRIPTION
					"The management IPv6 address prefix length."
				::=  { hm2NetIPv6LocalAddrEntry 3 }
				
			hm2NetIPv6LocalAddrType OBJECT-TYPE
				SYNTAX      InetAddressType
				MAX-ACCESS  read-write
				STATUS      current
				DESCRIPTION
					"The management IPv6 address type"
				DEFVAL      { ipv6 }
			    ::=  { hm2NetIPv6LocalAddrEntry 4 }

			hm2NetIPv6LocalAddr OBJECT-TYPE
				SYNTAX      InetAddress
				MAX-ACCESS  read-write
				STATUS      current
				DESCRIPTION
					"IPv6 address of the management agent board."
				DEFVAL { '00000000000000000000000000000000'H }
				::=  { hm2NetIPv6LocalAddrEntry 5 }

			hm2NetIPv6LocalAddrEuiFlag OBJECT-TYPE
				SYNTAX      HmEnabledStatus
				MAX-ACCESS  read-write
				STATUS      current
				DESCRIPTION
					"The management IPv6 EUI flag."
				DEFVAL { disable }
				::=  { hm2NetIPv6LocalAddrEntry 6 }

			hm2NetIPv6LocalAddrOrigin OBJECT-TYPE
				SYNTAX      IpAddressOriginTC
				MAX-ACCESS  read-write
				STATUS      current
				DESCRIPTION
					"Origin of IPv6 address."
				DEFVAL { manual }
				::=  { hm2NetIPv6LocalAddrEntry 7 }

			hm2NetIPv6LocalAddrStatus OBJECT-TYPE
				SYNTAX      RowStatus
				MAX-ACCESS  read-create
				STATUS      current
				DESCRIPTION
					""
			    ::= { hm2NetIPv6LocalAddrEntry 8 }

hm2NetAction			OBJECT-TYPE
			SYNTAX		INTEGER {
								other (1),
								activate (2)
						}
			MAX-ACCESS	read-write
			STATUS		current
			DESCRIPTION
					"This object, when read, always returns a value of other(1).
					Setting the object to activate(2) causes a reconfiguration
					of the IP protocol stack with the current values of 
					hm2NetLocalIPAddr, hm2NetGatewayIPAddr and hm2NetMask."
			DEFVAL { other }
			::= { hm2NetStaticGroup 50 }



--
-- *************************************************************
-- hm2NetACDGroup
-- *************************************************************
--
hm2NetACDStatus OBJECT-TYPE
			SYNTAX  HmEnabledStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
         	"Sets the status of the ip address conflict detection mechanism on this device.
         	 With activating the ACD status an internal check of duplicated IP-addresses is
         	 enabled."
			DEFVAL     { enable }				
			::= { hm2NetACDGroup 1 }
			
hm2NetACDDetectionMode OBJECT-TYPE
			SYNTAX INTEGER {
				activeAndPassive(1),
				activeDetectionOnly(2),
				passiveDetectionOnly(3)
			}
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
         	"Sets the mode of the ip address conflict detection mechanism on this device.
         	activeAndPassive (1): Both active and passive detection are active.
         	activeDetectionOnly (2): During configuration of a local ip address 
         	the device actively probes the network for this ip address.
         	passiveDetectionOnly (3): The device listens passively on the network 
         	if another device with an already locally configured ip address appears. 
         	In this case the own ip address is actively defended by transmitting gratituous ARP's."
			DEFVAL { activeAndPassive }
			::= { hm2NetACDGroup 2 }

hm2NetACDOngoingProbeStatus OBJECT-TYPE
			SYNTAX HmEnabledStatus
			MAX-ACCESS read-write
  			STATUS current
  			DESCRIPTION
         	"If enabled, the device sends periodic ARP or NDP probes every 90-120 seconds."
  		    DEFVAL	{ enable }			
  			::= { hm2NetACDGroup 3 }

hm2NetACDDelay OBJECT-TYPE
  			SYNTAX Integer32 (20..500)
  			MAX-ACCESS read-write
  			STATUS current
  			DESCRIPTION
         	"Time gap between ARP or NDP probes being sent." 
  		    DEFVAL	{ 200 }						
  			::= { hm2NetACDGroup 5 }

hm2NetACDReleaseDelay OBJECT-TYPE
  			SYNTAX Integer32 (3..3600)
  			MAX-ACCESS read-write
  			STATUS current
  			DESCRIPTION
         	"Delay in seconds to the next ARP or NDP probe cycle after an ip address conflict was detected."
  		    DEFVAL	{ 15 }			
  			::= { hm2NetACDGroup 7 }

hm2NetACDMaxProtection OBJECT-TYPE
  			SYNTAX Integer32 (0..100)
  			MAX-ACCESS read-write
  			STATUS current
  			DESCRIPTION
  			"The number of ARP announcement packets (gratuitous ARP packets) in passive(ongoing) mode to be received
  			 within hm2NetACDProtectInterval until the agent detects this as a conflict."
  		    DEFVAL { 1 }			
  			::= { hm2NetACDGroup 9 }

hm2NetACDProtectInterval OBJECT-TYPE
  			SYNTAX Integer32 (20..10000)
  			MAX-ACCESS read-write
  			STATUS current
  			DESCRIPTION
  			"Delay in milliseconds between two protections. See also hm2NetACDMaxProtection."
  		    DEFVAL	{ 10000 }			
  			::= { hm2NetACDGroup 11 }
  			
hm2NetACDFaultState OBJECT-TYPE
			SYNTAX INTEGER {
				true(1),
				false(2)
			}
  			MAX-ACCESS read-only
  			STATUS current
  			DESCRIPTION
  			"true(1) if an active address conflict is detected.
  			false(2) if no present address conflict."
  			::= { hm2NetACDGroup 13 }
  			
hm2NetACDTrapEnable		OBJECT-TYPE
			SYNTAX      HmEnabledStatus
			MAX-ACCESS  read-write
			STATUS      current
			DESCRIPTION
				"If enabled this trap reports an address conflict."
 			DEFVAL { enable }      
			::= { hm2NetACDGroup 15 }

-- ACD address conflict table 	
hm2NetACDAddrTable OBJECT-TYPE
		    SYNTAX      SEQUENCE OF Hm2NetACDAddrEntry
		    MAX-ACCESS  not-accessible
		    STATUS      current
		    DESCRIPTION
		            "This table contains address conflict detection information
		             on the local system known to this agent."
		    ::= { hm2NetACDGroup 20 }

hm2NetACDAddrEntry OBJECT-TYPE
		    SYNTAX      Hm2NetACDAddrEntry
		    MAX-ACCESS	not-accessible
		    STATUS      current
		    DESCRIPTION
		            "IP Address conflict detection information about a particular 
		            address on the local system known to this agent.
		            There may be multiple addresses configured on the system.
		            Entries may be created and deleted in this table by the
		            agent."
		    INDEX   { hm2NetACDTimeMark }
		    ::= { hm2NetACDAddrTable 1 }

Hm2NetACDAddrEntry ::= SEQUENCE {
			hm2NetACDTimeMark	TimeFilter,
			hm2NetACDAddrType	InetAddressType,
			hm2NetACDIPAddr		InetAddress,
			hm2NetACDMAC		MacAddress,
			hm2NetACDifIndex	InterfaceIndex
}

hm2NetACDTimeMark  OBJECT-TYPE
			SYNTAX      TimeFilter
			MAX-ACCESS	read-only
		    STATUS      current
		    DESCRIPTION
		            "A TimeFilter for this entry.  See the TimeFilter textual
		            convention in IETF RFC 2021 and 
		            http://www.ietf.org/IESG/Implementations/RFC2021-Implementation.txt
		            to see how TimeFilter works."
		    REFERENCE 
		            "IETF RFC 2021 section 6"
		    ::= { hm2NetACDAddrEntry 1 }
    
hm2NetACDAddrType  OBJECT-TYPE
		    SYNTAX      InetAddressType
		    MAX-ACCESS 	read-only
		    STATUS      current
		    DESCRIPTION
            	"Local IP Address Type"
		    ::= { hm2NetACDAddrEntry 3 }

hm2NetACDIPAddr  OBJECT-TYPE
		    SYNTAX      InetAddress
		    MAX-ACCESS 	read-only
		    STATUS      current
		    DESCRIPTION
		            "IP address used to identify the management address
					component associated with the local system."
		    ::= { hm2NetACDAddrEntry 5 }

hm2NetACDMAC  OBJECT-TYPE
		    SYNTAX      MacAddress
		    MAX-ACCESS 	read-only
		    STATUS      current
		    DESCRIPTION
            	"The physical address of the device that was detected 
            	causing the ip address conflict."

		    ::= { hm2NetACDAddrEntry 7 }

hm2NetACDifIndex  OBJECT-TYPE
		    SYNTAX      InterfaceIndex
		    MAX-ACCESS 	read-only
		    STATUS      current
		    DESCRIPTION
            	"The interface index on the local system 
            	where the ip address conflict was detected."

		    ::= { hm2NetACDAddrEntry 9 }		    

--
-- *************************************************************
-- hm2NetMacGroup
-- *************************************************************
--

hm2NetLocalBurnedInMacAddr	OBJECT-TYPE
			SYNTAX		MacAddress
			MAX-ACCESS	read-only
			STATUS		current
			DESCRIPTION
					"Physical base address (MAC address) of the agent.
					 This is the burned in MAC address from the production"
			::= { hm2NetMacGroup 1 }

hm2NetLocalAdminMacAddress	OBJECT-TYPE
			SYNTAX		MacAddress
			MAX-ACCESS	read-write
			STATUS		current
			DESCRIPTION
					"The switch's network locally administered MAC address.
					 This is the locally MAC address from the administrator. If
					 the hm2NetLocalAdminMacAddress is nonzero, the device starts 
					 with this MAC address at the next boot.
					 If the variable is changed, they must be stored by the 
					 configuration manager. 
					 A MAC address with a set multicast bit will not be accepted"
			DEFVAL { '000000000000'h }
			::= { hm2NetMacGroup 2 }

hm2NetMacAddressType	OBJECT-TYPE
			SYNTAX		INTEGER {
								burned-in(1),
								local(2)
						}
			MAX-ACCESS	read-only
			STATUS		current
			DESCRIPTION
					"Shows the currently used MAC address at boot time.
					The device starts with the burned in MAC address when 
					hm2NetLocalAdminMacAddress is zero, otherwise with the 
					Local-Admin-MAC-Address." 
			::= { hm2NetMacGroup 3 }


--
-- *************************************************************
-- hm2NetHiDiscoveryGroup
-- *************************************************************
--

hm2NetHiDiscoveryOperation 	OBJECT-TYPE
			SYNTAX			HmEnabledStatus
			MAX-ACCESS		read-write
			STATUS			current
			DESCRIPTION
				"Enables/disables the HiDiscovery protocol
				on this device.
				This protocol allows a remote host to detect
				devices without an IP configuration.
				It also allows the host to set IP parameters,
				like the ip address, the netmask and 
				the gateway address."
			DEFVAL  		{ enable }
			::= { hm2NetHiDiscoveryGroup 1 }

hm2NetHiDiscoveryMode 		OBJECT-TYPE
			SYNTAX			INTEGER {
								readWrite(1),
								readOnly(2)
							}
			MAX-ACCESS		read-write
			STATUS			current
			DESCRIPTION
				"In the read only mode only detecting and 
				reading the IP parameters is permitted.
				The read write mode gives full access to
				the device."
			DEFVAL  		{ readWrite }
			::= { hm2NetHiDiscoveryGroup 2 }

hm2NetHiDiscoveryBlinking	OBJECT-TYPE
			SYNTAX			HmEnabledStatus
			MAX-ACCESS		read-write
			STATUS			current
			DESCRIPTION
				"Enables/disables the HiDiscovery blinking sequence
				on this device. This object will not be saved."
			DEFVAL  		{ disable }
			::= { hm2NetHiDiscoveryGroup 3 }

hm2NetHiDiscoveryProtocol	OBJECT-TYPE
			SYNTAX			BITS { none(0), v1(1), v2(2) }
			MAX-ACCESS		read-only
			STATUS			current
			DESCRIPTION
				"Shows the HiDiscovery protocols supported by the device."
			::= { hm2NetHiDiscoveryGroup 4 }
			
hm2NetHiDiscoveryRelay	    OBJECT-TYPE
			SYNTAX			HmEnabledStatus
			MAX-ACCESS		read-write
			STATUS			current
			DESCRIPTION
				"Relay/bridge HiDiscovery frames."
			DEFVAL  		{ enable }
			::= { hm2NetHiDiscoveryGroup 5 }

--
-- *************************************************************
-- hm2NetMacACDGroup
-- *************************************************************
--
hm2NetMacACDStatus OBJECT-TYPE
			SYNTAX  HmEnabledStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
         	"Sets the status of the MAC address conflict detection mechanism on this device."
			DEFVAL { disable }				
			::= { hm2NetMacACDGroup 1 }

hm2NetMacACDConflictAddress	OBJECT-TYPE
			SYNTAX		MacAddress
			MAX-ACCESS	read-only
			STATUS		current
			DESCRIPTION
					"MAC address in case of a conflict."					 
			::= { hm2NetMacACDGroup 2 }

-- 
-- ***********************************************************
-- hm2NetConfigMibNotifications
-- ***********************************************************
hm2NetACDNotification NOTIFICATION-TYPE
		OBJECTS	{ hm2NetACDTimeMark, hm2NetACDAddrType, hm2NetACDIPAddr, hm2NetACDMAC, hm2NetACDifIndex }
		STATUS  current
		DESCRIPTION	
		"This trap reports an address conflict."
		::= { hm2NetConfigMibNotifications 1 }

hm2NetMacACDNotification NOTIFICATION-TYPE
		OBJECTS	{ ifIndex, hm2NetMacACDConflictAddress }
		STATUS  current
		DESCRIPTION	
		"This trap reports a MAC address conflict with it's own MAC address."
		::= { hm2NetConfigMibNotifications 2 }

--
-- *************************************************************
-- hm2NetOobMgmtGroup
-- *************************************************************
--
hm2NetOobMgmtAdminState		OBJECT-TYPE
			SYNTAX  		HmEnabledStatus
			MAX-ACCESS 		read-write
			STATUS 			current
			DESCRIPTION
         			"The status of the Out-of-band management on this device."
			DEFVAL { enable }				
			::= { hm2NetOobMgmtGroup 1 }

hm2NetOobMgmtProtocol	OBJECT-TYPE
			SYNTAX		INTEGER {
								none(1),
								bootp(2),
								dhcp(3)
						}
			MAX-ACCESS	read-write
			STATUS		current
			DESCRIPTION
					"The switch's out-of-band network configuration protocol.
					 The default value is dependent of the device type."
			DEFVAL { none }
			::= { hm2NetOobMgmtGroup 2 }

hm2NetOobMgmtIPAddrType	OBJECT-TYPE
			SYNTAX		InetAddressType
			MAX-ACCESS	read-write
			STATUS		current
			DESCRIPTION
					"Out-of-band IP address type."
			DEFVAL { ipv4 }
			::= { hm2NetOobMgmtGroup 3 }

hm2NetOobMgmtIPAddr		OBJECT-TYPE
			SYNTAX		InetAddress
			MAX-ACCESS	read-write
			STATUS		current
			DESCRIPTION
					"Out-of-band IP address of the management agent board.
					Changing this value will take effect after activating
					with hm2NetOobMgmtAction."
			DEFVAL { '00000000'H }
			::= { hm2NetOobMgmtGroup 4 }

hm2NetOobMgmtPrefixLength		OBJECT-TYPE
			SYNTAX		InetAddressPrefixLength
			MAX-ACCESS	read-write
			STATUS		current
			DESCRIPTION
					"The length of the IP netmask."
			DEFVAL { 0 }
			::= { hm2NetOobMgmtGroup 5 }

hm2NetOobMgmtGatewayIPAddrType	OBJECT-TYPE
			SYNTAX		InetAddressType
			MAX-ACCESS	read-write
			STATUS		current
			DESCRIPTION
					"Out-of-band default gateway IP address type."
			DEFVAL { ipv4 }
			::= { hm2NetOobMgmtGroup 6 }

hm2NetOobMgmtGatewayIPAddr		OBJECT-TYPE
			SYNTAX		InetAddress
			MAX-ACCESS	read-write
			STATUS		current
			DESCRIPTION
					"Out-of-band IP address of the default gateway.
					 Changing this value will take effect after activating
					 with hm2NetOobMgmtAction."
			DEFVAL { '00000000'H }
			::= { hm2NetOobMgmtGroup 7 }

hm2NetOobMgmtMacAddress		OBJECT-TYPE
			SYNTAX		MacAddress
			MAX-ACCESS	read-only
			STATUS		current
			DESCRIPTION
					"Out-of-band MAC address of the interface."
			::= { hm2NetOobMgmtGroup 8 }

hm2NetOobMgmtOperState		OBJECT-TYPE
			SYNTAX		INTEGER {
								up (1),
								down (2)
						}
			MAX-ACCESS	read-only
			STATUS		current
			DESCRIPTION
					"Out-of-band interface current operational state."
			::= { hm2NetOobMgmtGroup 9 }
			
hm2NetOobMgmtDHCPClientLeaseTime OBJECT-TYPE
			SYNTAX  Unsigned32
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION
					"Displays the remaining lease of the management(OOB) IP time in seconds."
			::= { hm2NetOobMgmtGroup 10 }

hm2NetOobMgmtAction		OBJECT-TYPE
			SYNTAX		INTEGER {
								other (1),
								activate (2)
						}
			MAX-ACCESS	read-write
			STATUS		current
			DESCRIPTION
					"This object, when read, always returns a value of other(1).
					Setting the object to activate(2) causes a reconfiguration
					of the out-of-band IP protocol stack with the current values of 
					hm2NetOobMgmtLocalIPAddr, hm2NetOobMgmtPrefixLength and hm2NetOobMgmtGatewayIPAddr."
			DEFVAL { other }
			::= { hm2NetOobMgmtGroup 50 }


--
-- *************************************************************
-- hm2NetOobUsbMgmtGroup
-- *************************************************************
--
hm2NetOobUsbMgmtAdminState		OBJECT-TYPE
			SYNTAX  		HmEnabledStatus
			MAX-ACCESS 		read-write
			STATUS 			current
			DESCRIPTION
         			"The status of the USB Out-of-band management on this device."
			DEFVAL { enable }				
			::= { hm2NetOobUsbMgmtGroup 1 }

hm2NetOobUsbMgmtIPAddrType	OBJECT-TYPE
			SYNTAX		InetAddressType
			MAX-ACCESS	read-write
			STATUS		current
			DESCRIPTION
					"USB Out-of-band Device IP address type."
			DEFVAL { ipv4 }
			::= { hm2NetOobUsbMgmtGroup 3 }

hm2NetOobUsbMgmtIPAddr		OBJECT-TYPE
			SYNTAX		InetAddress
			MAX-ACCESS	read-write
			STATUS		current
			DESCRIPTION
					"USB Out-of-band device IP address.
					Changing this value will take effect after activating
					with hm2NetOobUsbMgmtAction."
			DEFVAL { '00000000'H }
			::= { hm2NetOobUsbMgmtGroup 4 }

hm2NetOobUsbMgmtPrefixLength		OBJECT-TYPE
			SYNTAX		InetAddressPrefixLength
			MAX-ACCESS	read-write
			STATUS		current
			DESCRIPTION
					"The length of the IP netmask."
			DEFVAL { 0 }
			::= { hm2NetOobUsbMgmtGroup 5 }

hm2NetOobUsbMgmtHostMacAddress		OBJECT-TYPE
			SYNTAX		MacAddress
			MAX-ACCESS	read-only
			STATUS		current
			DESCRIPTION
					"USB Out-of-band MAC address of the host interface."
			::= { hm2NetOobUsbMgmtGroup 7 }

hm2NetOobUsbMgmtDeviceMacAddress		OBJECT-TYPE
			SYNTAX		MacAddress
			MAX-ACCESS	read-only
			STATUS		current
			DESCRIPTION
					"USB Out-of-band MAC address of the device interface."
			::= { hm2NetOobUsbMgmtGroup 8 }

hm2NetOobUsbMgmtAction		OBJECT-TYPE
			SYNTAX		INTEGER {
								other (1),
								activate (2)
						}
			MAX-ACCESS	read-write
			STATUS		current
			DESCRIPTION
					"This object, when read, always returns a value of other(1).
					Setting the object to activate(2) causes a reconfiguration
					of the USB out-of-band IP protocol stack with the current values of 
					hm2NetOobUsbMgmtLocalIPAddr and hm2NetOobUsbMgmtPrefixLength."
			DEFVAL { other }
			::= { hm2NetOobUsbMgmtGroup 50 }

END

