
HM2-DIAGNOSTIC-MIB DEFINITIONS ::= BEGIN

--
-- ***********************************************************
-- Hirschmann Diagnostic MIB
-- ***********************************************************
--

IMPORTS
    MODULE-IDENTITY,
    OBJECT-TYPE,
    NOTIFICATION-TYPE,
    OBJECT-IDENTITY,
	Integer32, Unsigned32       FROM SNMPv2-SMI -- RFC 2578
    TEXTUAL-CONVENTION, 
    TruthValue			        FROM SNMPv2-TC
    ifIndex					    FROM IF-MIB
    hm2ConfigurationMibs,
    HmEnabledStatus,
    HmTimeSeconds1970			FROM HM2-TC-MIB
    hm2PSID                     FROM HM2-PWRMGMT-MIB
    hm2IfacePhysIndex			FROM HM2-DEVMGMT-MIB;

hm2DiagnosticMib MODULE-IDENTITY
	LAST-UPDATED "201208280000Z" -- Aug 28, 2012
    ORGANIZATION "Hirschmann Automation and Control GmbH"
    CONTACT-INFO
        "Postal:     Stuttgarter Str. 45-51
                     72654 Neckartenzlingen
                     Germany
         Phone:      +49 7127 140
         E-mail:     hac.support@belden.com"
    DESCRIPTION
        "Hirschmann Diagnostic MIB.
         Copyright (C) 2012. All Rights Reserved."
	REVISION     "201208280000Z" -- Aug 28, 2012
    DESCRIPTION
         	 " Type of LEDs available updated.
         	 "         
    REVISION     "201103160000Z" -- March 16, 2011
    DESCRIPTION
         "Initial version."
    ::= { hm2ConfigurationMibs 22 }


--
-- *************************************************************
-- Textual Conventions
-- *************************************************************
--
Hm2LedType 	::= TEXTUAL-CONVENTION
    STATUS       current
    DESCRIPTION  "Types of LEDs available"
    SYNTAX       INTEGER { 
					        power(1),
        					status(2),
        					rm(3),
        					envm(4),
        					i1(5),
        					i2(6)
        				 }

Hm2LedStatus ::= TEXTUAL-CONVENTION
    STATUS       current
    DESCRIPTION  "Status of LEDs available"
    SYNTAX       INTEGER { 
				off(1),
				greenSolid(2),		-- Solid green
				greenBlink1(3),		-- Blinking green 1 time per period
				greenBlink3(4),		-- Blinking green 3 time per period
				greenBlink4(5),		-- Blinking green 4 time per period
				greenBlink5(6),		-- Blinking green 5 time per period
				greenBlink5i(7),	-- Blinking green 5 time per period inverse
				yellowSolid(8),		-- Solid yellow
				yellowBlink1(9),	-- Blinking yellow 1 time per period
				yellowBlink3(10),	-- Blinking yellow 3 time per period
				yellowBlink4(11),	-- Blinking yellow 4 time per period
				yellowBlink5(12),	-- Blinking yellow 5 time per period
				redSolid(13),		-- Solid red
				redBlink1(14),		-- Blinking red 1 time per period
				redBlink3(15),		-- Blinking red 3 time per period
				redBlink4(16),		-- Blinking red 4 time per period
				redBlink5(17)		-- Blinking red 5 time per period
			    }

-- 
-- ***********************************************************
-- hm2DiagnosticMib
-- ***********************************************************
--
hm2DiagnosticMibNotifications		OBJECT IDENTIFIER ::= { hm2DiagnosticMib 0 }
hm2DiagnosticMibObjects				OBJECT IDENTIFIER ::= { hm2DiagnosticMib 1 }
-- hm2DiagnosticMibConformance			OBJECT IDENTIFIER ::= { hm2DiagnosticMib 2 }
hm2DiagnosticSNMPExtensionGroup     OBJECT IDENTIFIER ::= { hm2DiagnosticMib 3 }
        
--
-- ***********************************************************
-- hm2Diagnostic groups
-- ***********************************************************
--

hm2DiagSelftestGroup 				OBJECT IDENTIFIER ::= { hm2DiagnosticMibObjects 1 }
hm2DiagBootGroup				    OBJECT IDENTIFIER ::= { hm2DiagnosticMibObjects 2 }
hm2DiagDeviceMonitorGroup 	        OBJECT IDENTIFIER ::= { hm2DiagnosticMibObjects 3 }
hm2DiagLedGroup						OBJECT IDENTIFIER ::= { hm2DiagnosticMibObjects 4 }
hm2DiagIfaceUtilizationGroup        OBJECT IDENTIFIER ::= { hm2DiagnosticMibObjects 5 }
hm2DiagCableTesterGroup             OBJECT IDENTIFIER ::= { hm2DiagnosticMibObjects 6 }
hm2PortMonitorGroup		    		OBJECT IDENTIFIER ::= { hm2DiagnosticMibObjects 7 }
hm2DiagResourcesGroup				OBJECT IDENTIFIER ::= { hm2DiagnosticMibObjects 8 }
--
-- ***********************************************************
-- hm2DiagSelftestGroup
-- ***********************************************************
--
hm2DiagSelftestRAM   OBJECT-TYPE
			 SYNTAX			 HmEnabledStatus
			 MAX-ACCESS      read-write
			 STATUS			 current
			 DESCRIPTION
				 "Controls RAM self-test on cold start of the device.
				 When disabled the device booting time is reduced."
			 DEFVAL			 { enable }
			 ::= { hm2DiagSelftestGroup 1 }
			 
hm2DiagSelftestBootTime   OBJECT-TYPE
            SYNTAX      Integer32
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
              "Internal boot time in Milliseconds until activating ports."
            ::= { hm2DiagSelftestGroup 2 }
 

hm2DiagSelftestActionTable OBJECT-TYPE
			SYNTAX		SEQUENCE OF Hm2DiagSelftestActionEntry
			MAX-ACCESS	not-accessible
			STATUS		current
			DESCRIPTION "Diag self test action group."
			::= { hm2DiagSelftestGroup 10 }

hm2DiagSelftestActionEntry OBJECT-TYPE
			SYNTAX		Hm2DiagSelftestActionEntry
			MAX-ACCESS	not-accessible
			STATUS		current
			DESCRIPTION 
					"Diag self test action entry."
			INDEX { hm2DiagSelftestActionCause }
			::= { hm2DiagSelftestActionTable 1 }

Hm2DiagSelftestActionEntry::= SEQUENCE {
			hm2DiagSelftestActionCause			INTEGER,
			hm2DiagSelftestAction				INTEGER
}

hm2DiagSelftestActionCause OBJECT-TYPE
			SYNTAX		INTEGER{
							task(1),
							resource(2),
							software(3),
							hardware(4) 
						}
			
			MAX-ACCESS	read-only
			STATUS	current
			DESCRIPTION
					"The area of the cause for the action the self-test
					wants to take."
			::= { hm2DiagSelftestActionEntry 1 }

hm2DiagSelftestAction OBJECT-TYPE
			SYNTAX		INTEGER{
							logOnly(1),
							sendTrap(2),
							reboot(3)
						}
			MAX-ACCESS	read-write
			STATUS		current
			DESCRIPTION
					"The action that the self-test component should take.
					The cause is always logged to the system log,
					additionally a trap can be sent to the management 
					station or a reboot can be performed."
			DEFVAL { reboot }
			::= { hm2DiagSelftestActionEntry 2 }

--
-- ***********************************************************
-- hm2DiagBootGroup
-- ***********************************************************
--

hm2BootSystemMonitor	OBJECT-TYPE
        	SYNTAX  	HmEnabledStatus
         	MAX-ACCESS	read-write
         	STATUS		current
         	DESCRIPTION	"Enable or disable the System Monitor access during 
						the boot phase. Please note: If the System Monitor 
						is disabled, it is possible to lose access to the 
						device permanently in case of loosing administrator
						password or misconfiguration."
        	DEFVAL		{ enable }
         	         	::= { hm2DiagBootGroup 1 }

hm2BootDefaultConfigOnError	OBJECT-TYPE
        	SYNTAX  	HmEnabledStatus
         	MAX-ACCESS	read-write
         	STATUS		current
         	DESCRIPTION	"Enable or disable loading of the default configuration
         				in case there is any error loading the configuration during
         				the boot phase. If disabled the system will be halted."
        	DEFVAL		{ enable }
         	         	::= { hm2DiagBootGroup 2 }

hm2BootConfigPushButton OBJECT-TYPE
			SYNTAX 		HmEnabledStatus
			MAX-ACCESS 	read-write
			STATUS 		current
			DESCRIPTION "Enable or disable the push button functionality on the device."
			DEFVAL 		{ enable }
						::= { hm2DiagBootGroup 3 }

--
-- ***********************************************************
-- hm2SignalContactGroup
-- ***********************************************************
--
hm2SignalContactGroup OBJECT IDENTIFIER ::= { hm2DiagDeviceMonitorGroup 1 }

-- *************************************************************
-- Signal Contact Common Table
-- *************************************************************
hm2SigConCommonTable OBJECT-TYPE
   SYNTAX SEQUENCE OF Hm2SigConCommonEntry
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION
      "This table contains all variables to configure the behavior
      of the signalling contacts."
   ::= { hm2SignalContactGroup 1 }

hm2SigConCommonEntry OBJECT-TYPE
   SYNTAX Hm2SigConCommonEntry
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION 
      "The entry of the hm2SigConConfigTable."
   INDEX { hm2SigConID }
   ::= { hm2SigConCommonTable 1 }

Hm2SigConCommonEntry ::= SEQUENCE {
   hm2SigConID Integer32,
   hm2SigConTrapEnable HmEnabledStatus,
   hm2SigConTrapCause INTEGER,
   hm2SigConTrapCauseIndex Integer32,
   hm2SigConMode INTEGER,
   hm2SigConOperState INTEGER,
   hm2SigConOperTimeStamp HmTimeSeconds1970,
   hm2SigConManualActivate INTEGER,
   hm2SigConSenseLinkFailure HmEnabledStatus,
   hm2SigConSenseTemperature HmEnabledStatus,
   hm2SigConSenseFan HmEnabledStatus,
   hm2SigConSenseModuleRemoval HmEnabledStatus,
   hm2SigConSenseExtNvmRemoval HmEnabledStatus,
   hm2SigConSenseExtNvmNotInSync HmEnabledStatus,
   hm2SigConSenseRingRedundancy HmEnabledStatus,
   hm2SigConSenseEthernetLoops HmEnabledStatus,
   hm2SigConSenseHumidity HmEnabledStatus,
   hm2SigConSenseStpPortBlock HmEnabledStatus
   }

hm2SigConID OBJECT-TYPE
   SYNTAX Integer32 (1..2)
   MAX-ACCESS read-only
   STATUS current
   DESCRIPTION
      "This index is used to identify the associated signalling contact."
   ::= { hm2SigConCommonEntry 1 }

hm2SigConTrapEnable OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Determines whether a trap shall be sent or not, when
      the signal contact operating state changes."
   DEFVAL  { disable }                
   ::= { hm2SigConCommonEntry 2 }

hm2SigConTrapCause OBJECT-TYPE
   SYNTAX INTEGER {
      none(1),
      power-supply(2),
      link-failure(3),
      temperature(4),
      fan-failure(5),
      module-removal(6),
      ext-nvm-removal(7),
      ext-nvm-not-in-sync(8),
      ring-redundancy(9),
      password-change(10),
      password-min-length(11),
      password-policy-not-configured(12),
      password-policy-inactive(13),
      telnet-enabled(14),
      http-enabled(15),
      snmp-unsecure(16),
      sysmon-enabled(17),
      ext-nvm-update-enabled(18),
      no-link(19),
      hidisc-enabled(20),
      ext-nvm-config-load-unsecure(21),
      https-certificate-warning(23),
      modbus-tcp-enabled(24),
      ethernet-ip-enabled(25),
      profinet-io-enabled(26),
      ethernet-loops(27),
      humidity(28),
      pml-disabled(29),
      stp-port-blocked(30)
      }
   MAX-ACCESS read-only
   STATUS current
   DESCRIPTION
      "This object identifies the cause for a trap. 
      The index of the entity which produces the trap
      is specified by hm2SigConTrapCauseIndex."
   ::= { hm2SigConCommonEntry 3 }

hm2SigConTrapCauseIndex OBJECT-TYPE
   SYNTAX Integer32
   MAX-ACCESS read-only
   STATUS current
   DESCRIPTION
      "This attribute specifies the entity which produces the trap.
      power-supply: 		index of power-supply table
      link-failure: 		index of interface table
      temperature:  		0
      ext-nvm-removal:		(1) sd, (2) usb, (3) serial (not supported yet)
      ext-nvm-not-in-sync: 	(1) sd, (2) usb, (3) serial (not supported yet)
      ring-redundancy:		(1) MRP, (2) PRP, (3) HSR, (4) DLR  
      ext-nvm-update-enabled:	(1) sd, (2) usb, (3) serial (not supported yet)
      no-link:			index of interface table
      ethernet-loops:       index of interface table
      humidity:         0
      stp-port-blocked:          index of interface table    
      0: other errors"
   ::= { hm2SigConCommonEntry 4 }

hm2SigConMode   OBJECT-TYPE
   SYNTAX INTEGER { 
      manual(1), 
      monitor(2), 
      deviceState(3),
      deviceSecurity(4),
      deviceStateAndSecurity(5)
   }
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "This attribute specifies the behavior of the relay contact.
      The factory settings for signal contact 1 is monitoring the
      correct operation of entries specified to be survived.
      When the device has also a second signal contact, the factory 
      setting for it is the manual mode."
   ::= { hm2SigConCommonEntry 5 }

hm2SigConOperState OBJECT-TYPE
   SYNTAX INTEGER { 
      open(1), 
      close(2) }
   MAX-ACCESS read-only
   STATUS current
   DESCRIPTION
      "This attribute shows the current operating state of the
      signal contact."
   ::= { hm2SigConCommonEntry 6 }

hm2SigConOperTimeStamp OBJECT-TYPE
   SYNTAX HmTimeSeconds1970
   MAX-ACCESS read-only
   STATUS current
   DESCRIPTION
   		"This attribute shows local system time (hm2SystemLocalTime) of the last hm2SigConOperState change."
      ::= { hm2SigConCommonEntry 7 }
      
hm2SigConManualActivate OBJECT-TYPE
   SYNTAX INTEGER { 
      open(1),
      close(2) } 
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "When operating in manual mode, the signal contact state can
      be set by this attribute."
   ::= { hm2SigConCommonEntry 8 }

hm2SigConSenseLinkFailure OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Sets the monitoring of the network connection(s)."
   DEFVAL { disable }                
   ::= { hm2SigConCommonEntry 9 }

hm2SigConSenseTemperature OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Sets the monitoring of the device temperature."
   DEFVAL  { enable }                
   ::= { hm2SigConCommonEntry 10 }

hm2SigConSenseFan OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Sets the monitoring of the device fan modules." 
   DEFVAL  { enable }                
   ::= { hm2SigConCommonEntry 11 }

hm2SigConSenseModuleRemoval OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Sets the monitoring of module removal (platform dependant)."
   DEFVAL  { disable }                
   ::= { hm2SigConCommonEntry 12 }

hm2SigConSenseExtNvmRemoval OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Sets the monitoring of the external non-volatile memory removal."
   DEFVAL { disable }                
   ::= { hm2SigConCommonEntry 13 }

hm2SigConSenseExtNvmNotInSync OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS     read-write
   STATUS      current
   DESCRIPTION
      "Sets the monitoring whether the external non-volatile memory is in
      sync with the configuration in NVRAM."
   DEFVAL  { disable }
   ::= { hm2SigConCommonEntry 14 }

hm2SigConSenseRingRedundancy OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Sets the monitoring of the ring redundancy."
   DEFVAL  { disable }                
   ::= { hm2SigConCommonEntry 15 }

hm2SigConSenseEthernetLoops OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Sets the monitoring for Ethernet loops."
   DEFVAL  { disable }                
   ::= { hm2SigConCommonEntry 16 }
   
hm2SigConSenseHumidity OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Sets the monitoring of the device humidity."
   DEFVAL  { enable }
   ::= { hm2SigConCommonEntry 17 }

hm2SigConSenseStpPortBlock OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Sets the monitoring for STP loops."
   DEFVAL  { enable }
   ::= { hm2SigConCommonEntry 18 }

-- *************************************************************
-- Signal Contact Power Supply Table
-- *************************************************************
hm2SigConPSTable OBJECT-TYPE
   SYNTAX SEQUENCE OF Hm2SigConPSEntry
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION
      "This table contains the configuration of all power supply states."
   ::= { hm2SignalContactGroup 2 }
   
hm2SigConPSEntry OBJECT-TYPE
   SYNTAX Hm2SigConPSEntry
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION 
      "The entry of the hm2SigConPSTable."
   INDEX { hm2SigConID, hm2PSID }
   ::= { hm2SigConPSTable 1 }

Hm2SigConPSEntry ::= SEQUENCE {
   hm2SigConSensePSState HmEnabledStatus
   }

hm2SigConSensePSState OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Sets the monitoring of the power supply state."
   DEFVAL { enable }                
   ::= { hm2SigConPSEntry 1 }

-- *************************************************************
-- Signal Contact Interface Table
-- *************************************************************
hm2SigConInterfaceTable OBJECT-TYPE
   SYNTAX SEQUENCE OF Hm2SigConInterfaceEntry
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION
      "This table contains all variables to mask an alarm for the
      signalling relay, produced by a link. The index for a link
      corresponds with ifIndex. The table is also used
      for the device monitoring configuration."
   ::= { hm2SignalContactGroup 3 }

hm2SigConInterfaceEntry OBJECT-TYPE
   SYNTAX Hm2SigConInterfaceEntry
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION
      "The entry of the hm2SigConLinkTable."
   INDEX { hm2SigConID, ifIndex }
   ::= { hm2SigConInterfaceTable 1 }

Hm2SigConInterfaceEntry ::= SEQUENCE {
   hm2SigConSenseIfLinkAlarm HmEnabledStatus
   }

hm2SigConSenseIfLinkAlarm OBJECT-TYPE
   SYNTAX HmEnabledStatus 
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Indicates whether an alarm for the signalling relay of the
      associated link will be produced or not, so you can mask the
      value of ifMauMediaAvailable."
   DEFVAL { disable }                
   ::= { hm2SigConInterfaceEntry 1 }

-- *************************************************************
-- Signal Contact Module Table
-- *************************************************************
hm2SigConModuleTable OBJECT-TYPE
   SYNTAX SEQUENCE OF Hm2SigConModuleEntry
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION
      "This table contains all variables to mask a module for the
      signaling relay. The index for a module corresponds with the 
      slot number."
   ::= { hm2SignalContactGroup 4 }

hm2SigConModuleEntry OBJECT-TYPE
   SYNTAX Hm2SigConModuleEntry
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION
      "The entry of the hm2SigConModuleTable."
   INDEX { hm2SigConID, hm2SigConModID }
   ::= { hm2SigConModuleTable 1 }

Hm2SigConModuleEntry ::= SEQUENCE {
   hm2SigConModID Integer32,
   hm2SigConSenseModule HmEnabledStatus
   }

hm2SigConModID OBJECT-TYPE
   SYNTAX Integer32 (1..7)
   MAX-ACCESS read-only
   STATUS current
   DESCRIPTION
      "This index is used to identify the associated module."
   ::= { hm2SigConModuleEntry 1 }
   
hm2SigConSenseModule OBJECT-TYPE
   SYNTAX HmEnabledStatus 
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Indicates whether an alarm for the signalling relay of the
      associated module will be produced or not."
   DEFVAL { disable }                
   ::= { hm2SigConModuleEntry 2 }
   
-- *************************************************************
-- Signal Contact Fan Module Table
-- *************************************************************
hm2SigConFanModuleTable OBJECT-TYPE
   SYNTAX SEQUENCE OF Hm2SigConFanModuleEntry
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION
      "This table contains all variables to mask a fan module for the
      signaling relay. The index for a module corresponds with the 
      module number."
   ::= { hm2SignalContactGroup 5 }

hm2SigConFanModuleEntry OBJECT-TYPE
   SYNTAX Hm2SigConFanModuleEntry
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION
      "The entry of the hm2SigConFanModuleTable."
   INDEX { hm2SigConID, hm2SigConFanModID }
   ::= { hm2SigConFanModuleTable 1 }

Hm2SigConFanModuleEntry ::= SEQUENCE {
   hm2SigConFanModID Integer32,
   hm2SigConSenseFanModule HmEnabledStatus
   }

hm2SigConFanModID OBJECT-TYPE
   SYNTAX Integer32 (1..7)
   MAX-ACCESS read-only
   STATUS current
   DESCRIPTION
      "This index is used to identify the associated fan module."
   ::= { hm2SigConFanModuleEntry 1 }
   
hm2SigConSenseFanModule OBJECT-TYPE
   SYNTAX HmEnabledStatus 
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Indicates whether an alarm for the signalling relay of the
      associated fan module will be produced or not."
   DEFVAL { enable }                
   ::= { hm2SigConFanModuleEntry 2 }

-- *************************************************************
-- Signal Contact Status Table
-- *************************************************************
hm2SigConStatusTable OBJECT-TYPE
   SYNTAX SEQUENCE OF Hm2SigConStatusEntry
   MAX-ACCESS 	not-accessible
   STATUS 		current
   DESCRIPTION
      "This table shows the current monitored entities
       for which there is a trap cause (hm2SigConTrapCause) active."
   ::= { hm2SignalContactGroup 10 }

hm2SigConStatusEntry OBJECT-TYPE
   SYNTAX Hm2SigConStatusEntry
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION 
      "The entry of the hm2SigConStatusTable."
   INDEX { hm2SigConID, hm2SigConStatusIndex }
   ::= { hm2SigConStatusTable 1 }

Hm2SigConStatusEntry ::= SEQUENCE {
   hm2SigConStatusIndex             Integer32,
   hm2SigConStatusTimeStamp         HmTimeSeconds1970,
   hm2SigConStatusTrapCause 		INTEGER,
   hm2SigConStatusTrapCauseIndex 	Integer32
   }

hm2SigConStatusIndex OBJECT-TYPE
   SYNTAX 		Integer32
   MAX-ACCESS 	not-accessible
   STATUS 		current
   DESCRIPTION
      "This index is used to identify the occured event."
   ::= { hm2SigConStatusEntry 1 }

hm2SigConStatusTimeStamp OBJECT-TYPE
   SYNTAX 		HmTimeSeconds1970
   MAX-ACCESS 	read-only
   STATUS 		current
   DESCRIPTION
      "This attribute shows the local system time (hm2SystemLocalTime) of occuration the event."
   ::= { hm2SigConStatusEntry 2 }

hm2SigConStatusTrapCause OBJECT-TYPE
   SYNTAX INTEGER {
      none(1),
      power-supply(2),
      link-failure(3),
      temperature(4),
      fan-failure(5),
      module-removal(6),
      ext-nvm-removal(7),
      ext-nvm-not-in-sync(8),
      ring-redundancy(9),
      password-change(10),
      password-min-length(11),
      password-policy-not-configured(12),
      password-policy-inactive(13),
      telnet-enabled(14),
      http-enabled(15),
      snmp-unsecure(16),
      sysmon-enabled(17),
      ext-nvm-update-enabled(18),
      no-link(19),
      hidisc-enabled(20),
      ext-nvm-config-load-unsecure(21),
      iec61850-mms-enabled(22),
      https-certificate-warning(23),
      modbus-tcp-enabled(24),
      ethernet-ip-enabled(25),
      profinet-io-enabled(26),
      ethernet-loops(27),
      humidity(28),
      stp-port-blocked(30)
      }
   MAX-ACCESS 	read-only
   STATUS 		current
   DESCRIPTION
      "This object identifies the cause for a trap. 
      The index of the entity which produces the trap
      is specified by hm2SigConTrapCauseIndex."
   ::= { hm2SigConStatusEntry 3 }

hm2SigConStatusTrapCauseIndex OBJECT-TYPE
   SYNTAX 		Integer32
   MAX-ACCESS 	read-only
   STATUS 		current
   DESCRIPTION
      "This attribute specifies the entity which produces the trap.
      power-supply: 			index of power-supply table
      link-failure: 			index of interface table
      temperature:  			0
      ext-nvm-removal:			(1) sd, (2) usb, (3) serial (not supported yet)
      ext-nvm-not-in-sync: 		(1) sd, (2) usb, (3) serial (not supported yet)
      ring-redundancy:			(1) MRP, (2) PRP, (3) HSR, (4) DLR 
      ext-nvm-update-enabled:	(1) sd, (2) usb, (3) serial (not supported yet)
      no-link:					index of interface table
      ethernet-loops:           index of interface table
      humidity:                 0
      stp-port-blocked:              index of interface table
      0: 						other errors"
   ::= { hm2SigConStatusEntry 4 }
   
-- ### part 2
--
-- ***********************************************************
-- hm2DeviceMonitorGroup
-- ***********************************************************
--
hm2DeviceMonitorGroup OBJECT IDENTIFIER ::= { hm2DiagDeviceMonitorGroup 2 }

-- *************************************************************
-- hm2DeviceMonitorConfigGroup
-- *************************************************************
hm2DevMonCommonTable OBJECT-TYPE
   SYNTAX SEQUENCE OF Hm2DevMonCommonEntry
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION
      "This table contains all variables to configure the behavior
      of the signalling contacts."
   ::= { hm2DeviceMonitorGroup 1 }

hm2DevMonCommonEntry OBJECT-TYPE
   SYNTAX Hm2DevMonCommonEntry
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION 
      "The entry of the hm2DevMonConfigTable."
   INDEX { hm2DevMonID }
   ::= { hm2DevMonCommonTable 1 }

Hm2DevMonCommonEntry ::= SEQUENCE {
   hm2DevMonID Integer32,
   hm2DevMonTrapEnable HmEnabledStatus,
   hm2DevMonTrapCause INTEGER,
   hm2DevMonTrapCauseIndex Integer32,
   hm2DevMonOperState INTEGER,
   hm2DevMonOperTimeStamp HmTimeSeconds1970,
   hm2DevMonSenseLinkFailure HmEnabledStatus,
   hm2DevMonSenseTemperature HmEnabledStatus,
   hm2DevMonSenseFan HmEnabledStatus,
   hm2DevMonSenseModuleRemoval HmEnabledStatus,
   hm2DevMonSenseExtNvmRemoval HmEnabledStatus,
   hm2DevMonSenseExtNvmNotInSync HmEnabledStatus,
   hm2DevMonSenseRingRedundancy HmEnabledStatus,
   hm2DevMonSenseHumidity HmEnabledStatus,
   hm2DevMonSenseStpPortBlock HmEnabledStatus
   }

hm2DevMonID OBJECT-TYPE
   SYNTAX Integer32 (1..1)
   MAX-ACCESS read-only
   STATUS current
   DESCRIPTION
      "This index is used to identify the associated device monitoring group.
      Currently only one group is supported"
   ::= { hm2DevMonCommonEntry 1 }

hm2DevMonTrapEnable OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Determines whether a trap shall be sent or not when
      the signal contact operating state changes."
   DEFVAL  { enable }                
   ::= { hm2DevMonCommonEntry 2 }

hm2DevMonTrapCause OBJECT-TYPE
   SYNTAX INTEGER {
      none(1),
      power-supply(2),
      link-failure(3),
      temperature(4),
      fan-failure(5),
      module-removal(6),
      ext-nvm-removal(7),
      ext-nvm-not-in-sync(8),
      ring-redundancy(9),
      humidity(28),
      stp-port-blocked(30)
      }
   MAX-ACCESS read-only
   STATUS current
   DESCRIPTION
      "This object identifies the cause for a trap. 
      The index of the entity which produces the trap
      is specified by hm2DevMonTrapCauseIndex."
   ::= { hm2DevMonCommonEntry 3 }

hm2DevMonTrapCauseIndex OBJECT-TYPE
   SYNTAX Integer32
   MAX-ACCESS read-only
   STATUS current
   DESCRIPTION
      "This attribute specifies the entity which produces the trap.
      power-supply: 		index of power supply table
      link-failure: 		index of interface table
      temperature:  		0
      ext-nvm-removal:		(1) sd, (2) usb, (3) Serial (not supported yet)
      ext-nvm-not-in-sync: 	(1) sd, (2) usb, (3) Serial (not supported yet)
      ring-redundancy:		(1) MRP, (2) PRP, (3), HSR, (4) DLR 
      humidity:         0
      stp-port-blocked:          index of interface table    
      0: other errors"
   ::= { hm2DevMonCommonEntry 4 }

hm2DevMonOperState OBJECT-TYPE
   SYNTAX INTEGER { 
      noerror(1), 
      error(2) }
   MAX-ACCESS read-only
   STATUS current
   DESCRIPTION
      "This attribute shows the current operating state of the
      signal contact."
   ::= { hm2DevMonCommonEntry 5 }

hm2DevMonOperTimeStamp OBJECT-TYPE
   SYNTAX HmTimeSeconds1970
   MAX-ACCESS read-only
   STATUS current
   DESCRIPTION
   		"This attribute shows the local system time (hm2SystemLocalTime) of the last hm2DevMonOperState change."
   ::= { hm2DevMonCommonEntry 6 }
      
hm2DevMonSenseLinkFailure OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Sets the monitoring of the network connection(s)."
   DEFVAL { disable }                
   ::= { hm2DevMonCommonEntry 7 }
   
hm2DevMonSenseTemperature OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Sets the monitoring of the device temperature."
   DEFVAL  { enable }                
   ::= { hm2DevMonCommonEntry 8 }

hm2DevMonSenseFan OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Sets the monitoring of the device fan modules."
   DEFVAL  { enable }                
   ::= { hm2DevMonCommonEntry 9 }

hm2DevMonSenseModuleRemoval OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Sets the monitoring of module removal (platform dependent)."
   DEFVAL  { disable }                
   ::= { hm2DevMonCommonEntry 10 }

hm2DevMonSenseExtNvmRemoval OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Sets the monitoring of the external non-volatile memory removal."
   DEFVAL { disable }                
   ::= { hm2DevMonCommonEntry 11 }

hm2DevMonSenseExtNvmNotInSync OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS     read-write
   STATUS      current
   DESCRIPTION
      "Sets the monitoring whether the external non-volatile memory is in
      sync with the configuration in NVRAM."
   DEFVAL  { disable }
   ::= { hm2DevMonCommonEntry 12 }

hm2DevMonSenseRingRedundancy OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Sets the monitoring of the ring redundancy."
   DEFVAL  { disable }                
   ::= { hm2DevMonCommonEntry 13 }

hm2DevMonSenseHumidity OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Sets the monitoring of the device humidity."
   DEFVAL  { enable }
   ::= { hm2DevMonCommonEntry 14 }

hm2DevMonSenseStpPortBlock OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Sets the monitoring whether a port was blocked by STP."
   DEFVAL  { enable }
   ::= { hm2DevMonCommonEntry 15 }

-- *************************************************************
-- Device Monitor Power Supply Table
-- *************************************************************
hm2DevMonPSTable OBJECT-TYPE
   SYNTAX SEQUENCE OF Hm2DevMonPSEntry
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION
      "This table contains the configuration of all power supply states."
   ::= { hm2DeviceMonitorGroup 2 }
   
hm2DevMonPSEntry OBJECT-TYPE
   SYNTAX Hm2DevMonPSEntry
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION 
      "The entry of the hm2DevMonPSTable."
   INDEX { hm2DevMonID, hm2PSID }
   ::= { hm2DevMonPSTable 1 }

Hm2DevMonPSEntry ::= SEQUENCE {
   hm2DevMonSensePSState HmEnabledStatus
   }

hm2DevMonSensePSState OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Sets the monitoring of the power supply state."
   DEFVAL { enable }                
   ::= { hm2DevMonPSEntry 1 }

-- *************************************************************
-- Device Monitor Interface Table
-- *************************************************************
hm2DevMonInterfaceTable OBJECT-TYPE
   SYNTAX SEQUENCE OF Hm2DevMonInterfaceEntry
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION
      "This table contains all variables to mask an alarm for the
      signalling relay, produced by a link. The index for a link
      corresponds with ifIndex. The table is also used
      for the device monitoring configuration."
   ::= { hm2DeviceMonitorGroup 3 }

hm2DevMonInterfaceEntry OBJECT-TYPE
   SYNTAX Hm2DevMonInterfaceEntry
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION
      "The entry of the hm2DevMonLinkTable."
   INDEX { hm2DevMonID, ifIndex }
   ::= { hm2DevMonInterfaceTable 1 }

Hm2DevMonInterfaceEntry ::= SEQUENCE {
   hm2DevMonSenseIfLinkAlarm HmEnabledStatus
   }

hm2DevMonSenseIfLinkAlarm OBJECT-TYPE
   SYNTAX HmEnabledStatus 
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Indicates whether an alarm for the signalling relay of the
      associated link will be produced or not, so you can mask the
      value of ifMauMediaAvailable."
   DEFVAL { disable }                
   ::= { hm2DevMonInterfaceEntry 1 }

-- *************************************************************
-- Device Monitor Module Table
-- *************************************************************
hm2DevMonModuleTable OBJECT-TYPE
   SYNTAX SEQUENCE OF Hm2DevMonModuleEntry
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION
      "This table contains all variables to mask a module for the
      device status. The index for a module corresponds with the
      slot number."
   ::= { hm2DeviceMonitorGroup 4 }

hm2DevMonModuleEntry OBJECT-TYPE
   SYNTAX Hm2DevMonModuleEntry
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION
      "The entry of the hm2DevMonModuleTable."
   INDEX { hm2DevMonID, hm2DevMonModID }
   ::= { hm2DevMonModuleTable 1 }

Hm2DevMonModuleEntry ::= SEQUENCE {
   hm2DevMonModID Integer32,
   hm2DevMonSenseModule HmEnabledStatus   
   }

hm2DevMonModID OBJECT-TYPE
   SYNTAX Integer32 (1..7)
   MAX-ACCESS read-only
   STATUS current
   DESCRIPTION
      "This index is used to identify the associated module."
   ::= { hm2DevMonModuleEntry 1 }
   
hm2DevMonSenseModule OBJECT-TYPE
   SYNTAX HmEnabledStatus 
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Indicates whether an alarm for the device status of the
      associated module will be produced or not."
   DEFVAL { disable }                
   ::= { hm2DevMonModuleEntry 2 }
   
-- *************************************************************
-- Device Monitor Fan Module Table
-- *************************************************************
hm2DevMonFanModuleTable OBJECT-TYPE
   SYNTAX SEQUENCE OF Hm2DevMonFanModuleEntry
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION
      "This table contains all variables to mask a fan module for the
      device status. The index for a module corresponds with the
      module number."
   ::= { hm2DeviceMonitorGroup 5 }

hm2DevMonFanModuleEntry OBJECT-TYPE
   SYNTAX Hm2DevMonFanModuleEntry
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION
      "The entry of the hm2DevMonFanModuleTable."
   INDEX { hm2DevMonID, hm2DevMonFanModID }
   ::= { hm2DevMonFanModuleTable 1 }

Hm2DevMonFanModuleEntry ::= SEQUENCE {
   hm2DevMonFanModID Integer32,
   hm2DevMonSenseFanModule HmEnabledStatus   
   }

hm2DevMonFanModID OBJECT-TYPE
   SYNTAX Integer32 (1..7)
   MAX-ACCESS read-only
   STATUS current
   DESCRIPTION
      "This index is used to identify the associated fan module."
   ::= { hm2DevMonFanModuleEntry 1 }
   
hm2DevMonSenseFanModule OBJECT-TYPE
   SYNTAX HmEnabledStatus 
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Indicates whether an alarm for the device status of the
      associated fan module will be produced or not."
   DEFVAL { enable }                
   ::= { hm2DevMonFanModuleEntry 2 }

-- *************************************************************
-- Device Monitor Status Table
-- *************************************************************
hm2DevMonStatusTable OBJECT-TYPE
   SYNTAX SEQUENCE OF Hm2DevMonStatusEntry
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION
      "This table shows the current monitored entities in the hm2DeviceMonitorGroup
       for which there is a trap cause (hm2DevMonStatusTrapCause) active."
   ::= { hm2DeviceMonitorGroup 10 }

hm2DevMonStatusEntry OBJECT-TYPE
   SYNTAX Hm2DevMonStatusEntry
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION 
      "The entry of the hm2DevMonStatusTable."
   INDEX { hm2DevMonID, hm2DevMonStatusIndex }
   ::= { hm2DevMonStatusTable 1 }

Hm2DevMonStatusEntry ::= SEQUENCE {
   hm2DevMonStatusIndex             Integer32,
   hm2DevMonStatusTimeStamp         HmTimeSeconds1970,
   hm2DevMonStatusTrapCause 		INTEGER,
   hm2DevMonStatusTrapCauseIndex 	Integer32
   }

hm2DevMonStatusIndex OBJECT-TYPE
   SYNTAX 		Integer32
   MAX-ACCESS 	not-accessible
   STATUS 		current
   DESCRIPTION
      "This index is used to identify the occured event."
   ::= { hm2DevMonStatusEntry 1 }

hm2DevMonStatusTimeStamp OBJECT-TYPE
   SYNTAX 		HmTimeSeconds1970
   MAX-ACCESS 	read-only
   STATUS 		current
   DESCRIPTION
      "This attribute shows the local system time (hm2SystemLocalTime) of occuration the event."
   ::= { hm2DevMonStatusEntry 2 }

hm2DevMonStatusTrapCause OBJECT-TYPE
   SYNTAX 		INTEGER {
      none(1),
      power-supply(2),
      link-failure(3),
      temperature(4),
      fan-failure(5),
      module-removal(6),
      ext-nvm-removal(7),
      ext-nvm-not-in-sync(8),
      ring-redundancy(9),
      humidity(28),
      stp-port-blocked(30)
      }
   MAX-ACCESS 	read-only
   STATUS 		current
   DESCRIPTION
      "This object identifies the cause for a trap. 
      The index of the entity which produces the trap
      is specified by hm2DevMonTrapCauseIndex."
   ::= { hm2DevMonStatusEntry 3 }

hm2DevMonStatusTrapCauseIndex OBJECT-TYPE
   SYNTAX 		Integer32
   MAX-ACCESS 	read-only
   STATUS 		current
   DESCRIPTION
      "This attribute specifies the entity which produces the trap.
      power-supply: 		index of power supply table
      link-failure: 		index of interface table
      temperature:  		0
      ext-nvm-removal:		(1) sd, (2) usb, (3) Serial (not supported yet)
      ext-nvm-not-in-sync: 	(1) sd, (2) usb, (3) Serial (not supported yet)
      ring-redundancy:		(1) MRP, (2) PRP, (3) HSR, (4) DLR 
      humidity:         0
      stp-port-blocked: 		    index of interface table
      0: other errors"
   ::= { hm2DevMonStatusEntry 4 }
         
-- ### part 3
--
-- ***********************************************************
-- hm2DeviceSecurityGroup
-- ***********************************************************
--
hm2DeviceSecurityGroup OBJECT IDENTIFIER ::= { hm2DiagDeviceMonitorGroup 3 }

-- *************************************************************
-- Device Security Config Group
-- *************************************************************
hm2DevSecConfigGroup OBJECT IDENTIFIER ::= { hm2DeviceSecurityGroup 1 }
hm2DevSecTrapEnable OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Determines whether a trap shall be sent or not, when
      the device security operating state changes."
   DEFVAL  { disable }                
   ::= { hm2DevSecConfigGroup 1 }

hm2DevSecTrapCause OBJECT-TYPE
   SYNTAX INTEGER {
      none(1),
      password-change(10),
      password-min-length(11),
      password-policy-not-configured(12),
      password-policy-inactive(13),
      telnet-enabled(14),
      http-enabled(15),
      snmp-unsecure(16),
      sysmon-enabled(17),
      ext-nvm-update-enabled(18),
      no-link(19),
      hidisc-enabled(20),
      ext-nvm-config-load-unsecure(21),
      iec61850-mms-enabled(22),
      https-certificate-warning(23),
      modbus-tcp-enabled(24),
      ethernet-ip-enabled(25),
      profinet-io-enabled(26),
      pml-disabled(29)
      }
   MAX-ACCESS read-only
   STATUS current
   DESCRIPTION
      "This object identifies the cause for a trap. 
       The index of the entity which produces the trap
       is specified by hm2DevMonTrapCauseIndex."
   ::= { hm2DevSecConfigGroup 2 }

hm2DevSecTrapCauseIndex OBJECT-TYPE
   SYNTAX Integer32
   MAX-ACCESS read-only
   STATUS current
   DESCRIPTION
      "This attribute specifies the entity which produces the trap.
       ext-nvm-update-enabled:	(1) sd, (2) usb, (3) serial (not supported yet)
       no-link:	index of interface table
       0: other errors."
   ::= { hm2DevSecConfigGroup 3 }

hm2DevSecOperState OBJECT-TYPE
   SYNTAX INTEGER { 
      noerror(1), 
      error(2) }
   MAX-ACCESS read-only
   STATUS current
   DESCRIPTION
      "This attribute shows the current operating state of the signal contact."
   ::= { hm2DevSecConfigGroup 4 }

hm2DevSecOperTimeStamp OBJECT-TYPE
   SYNTAX HmTimeSeconds1970
   MAX-ACCESS read-only
   STATUS current
   DESCRIPTION
   		"This attribute shows the local system time (hm2SystemLocalTime) of the last hm2DevSecOperState change."
   ::= { hm2DevSecConfigGroup 5 }

hm2DevSecSensePasswordChange OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Enable or disable to check if default passwords for 'user' and 'admin' are not changed."
   DEFVAL { enable }
   ::= { hm2DevSecConfigGroup 6 }
   
hm2DevSecSensePasswordMinLength OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Enable or disable to check if configured minimum password length is < 8 characters."
   DEFVAL { enable }
   ::= { hm2DevSecConfigGroup 7 }
   
hm2DevSecSensePasswordStrengthNotConfigured OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Enable or disable minimum password strength to check if
       (1 uppercase, 1 lowercase, 1 number, 1 non-alphanumeric) is not configured."
   DEFVAL { enable }   
   ::= { hm2DevSecConfigGroup 8 }

hm2DevSecSenseBypassPasswordStrength OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Enable or disable to check if at least one user is configured to bypass strength check."
   DEFVAL { disable }
   ::= { hm2DevSecConfigGroup 9 }

hm2DevSecSenseTelnetEnabled OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Enable or disable to check if telnet is enabled on the switch."
   DEFVAL { enable }
   ::= { hm2DevSecConfigGroup 10 }

hm2DevSecSenseHttpEnabled OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Enable or disable to check if HTTP is enabled on the switch."
   DEFVAL { enable }   
   ::= { hm2DevSecConfigGroup 11 }

hm2DevSecSenseSnmpUnsecure OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Enable or disable to check if SNMP v1/v2 is enabled or v3 encryption is disabled."
   DEFVAL { enable }
   ::= { hm2DevSecConfigGroup 12 }

hm2DevSecSenseSysmonEnabled OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Enable or disable to check if sysmon1 access is not disabled."
   DEFVAL { disable }
   ::= { hm2DevSecConfigGroup 13 }
   
hm2DevSecSenseExtNvmUpdateEnabled OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Enable or disable to check if external non-volatile memory update is not disabled."
   DEFVAL { disable }
   ::= { hm2DevSecConfigGroup 14 }

hm2DevSecSenseNoLinkEnabled OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Enable or disable to check if at least one port has no link but admin state is up."
   DEFVAL { disable }
   ::= { hm2DevSecConfigGroup 15 }   

hm2DevSecSenseHiDiscoveryEnabled OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Enable or disable to check if HiDiscovery is enabled and the mode is 'read-write'."
   DEFVAL { enable }
   ::= { hm2DevSecConfigGroup 16 }   

hm2DevSecSenseExtNvmConfigLoadUnsecure OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Enable or disable to check if the configuration load from external NVM is unsecure.
       (The configuration priority of the external NVM is set 
       to 'first', 'second' or 'third' and the configuration encryption
       is not active.)"
   DEFVAL { enable }
   ::= { hm2DevSecConfigGroup 17 }
   
hm2DevSecSenseIec61850MmsEnabled OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Enable or disable to check if IEC 61850 MMS is enabled on the switch."
   DEFVAL { enable }
   ::= { hm2DevSecConfigGroup 18 }

hm2DevSecSenseHttpsCertificateWarning OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
       "Enable or disable to check for the presence of the auto generated self-signed HTTPS certificate."
   DEFVAL { enable }
   ::= { hm2DevSecConfigGroup 19 }

hm2DevSecSenseModbusTcpEnabled OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Enable or disable to check if Modbus/TCP server is enabled on the switch."
   DEFVAL { enable }
   ::= { hm2DevSecConfigGroup 20 } 
  
hm2DevSecSenseEtherNetIpEnabled OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Enable or disable to check if EtherNet/IP protocol is enabled on the switch."
   DEFVAL { enable }
   ::= { hm2DevSecConfigGroup 21 } 
   
hm2DevSecSenseProfinetIOEnabled OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Enable or disable to check if ProfinetIO protocol is enabled on the switch."
   DEFVAL { enable }
   ::= { hm2DevSecConfigGroup 22 }
   
hm2DevSecSensePMLDisabled OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Enable or disable to check if Port MAC Locking is disabled on the switch."
   DEFVAL { enable }   
   ::= { hm2DevSecConfigGroup 23 }

-- *************************************************************
-- Device Security Interface Table
-- *************************************************************
hm2DevSecInterfaceTable OBJECT-TYPE
   SYNTAX SEQUENCE OF Hm2DevSecInterfaceEntry
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION
      "This table contains all variables to mask an alarm for the
      signalling relay, produced by a link. The index for a link
      corresponds with ifIndex. The table is also used
      for the device monitoring configuration."
   ::= { hm2DeviceSecurityGroup 2 }

hm2DevSecInterfaceEntry OBJECT-TYPE
   SYNTAX Hm2DevSecInterfaceEntry
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION
      "The entry of the hm2DevSecLinkTable."
   INDEX { ifIndex }
   ::= { hm2DevSecInterfaceTable 1 }

Hm2DevSecInterfaceEntry ::= SEQUENCE {
   hm2DevSecSenseIfNoLink HmEnabledStatus
   }

hm2DevSecSenseIfNoLink OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Port has no link but admin state is up"
   DEFVAL { disable }
   ::= { hm2DevSecInterfaceEntry 1 }

-- *************************************************************
-- Device Security Status Group
-- *************************************************************
hm2DevSecStatusTable OBJECT-TYPE
   SYNTAX SEQUENCE OF Hm2DevSecStatusEntry
   MAX-ACCESS 		not-accessible
   STATUS 			current
   DESCRIPTION
      "This table shows the current monitored entities in the hm2DevSecConfigGroup
       for which there is a trap cause (hm2DevSecStatusTrapCause) active."
   ::= { hm2DeviceSecurityGroup 10 }

hm2DevSecStatusEntry OBJECT-TYPE
   SYNTAX 		Hm2DevSecStatusEntry
   MAX-ACCESS 	not-accessible
   STATUS 		current
   DESCRIPTION 
      "The entry of the hm2DevSecStatusTable."
   INDEX { hm2DevSecStatusIndex }
   ::= { hm2DevSecStatusTable 1 }

Hm2DevSecStatusEntry ::= SEQUENCE {
   hm2DevSecStatusIndex             Integer32,
   hm2DevSecStatusTimeStamp         HmTimeSeconds1970,
   hm2DevSecStatusTrapCause 		INTEGER,
   hm2DevSecStatusTrapCauseIndex	Integer32
   }

hm2DevSecStatusIndex OBJECT-TYPE
   SYNTAX 		Integer32
   MAX-ACCESS 	not-accessible
   STATUS 		current
   DESCRIPTION
      "This index is used to identify the occured event."
   ::= { hm2DevSecStatusEntry 1 }

hm2DevSecStatusTimeStamp OBJECT-TYPE
   SYNTAX 		HmTimeSeconds1970
   MAX-ACCESS 	read-only
   STATUS 		current
   DESCRIPTION
      "This attribute shows the local system time (hm2SystemLocalTime) of occuration the event."
   ::= { hm2DevSecStatusEntry 2 }
   
hm2DevSecStatusTrapCause OBJECT-TYPE
   SYNTAX   	INTEGER {
      none(1),
      password-change(10),
      password-min-length(11),
      password-policy-not-configured(12),
      password-policy-inactive(13),
      telnet-enabled(14),
      http-enabled(15),
      snmp-unsecure(16),
      sysmon-enabled(17),
      ext-nvm-update-enabled(18),
      no-link(19),
      hidisc-enabled(20),
      ext-nvm-config-load-unsecure(21),
      iec61850-mms-enabled(22),
      https-certificate-warning(23),
      modbus-tcp-enabled(24),
      ethernet-ip-enabled(25),
      profinet-io-enabled(26),
      pml-disabled(29)
      }
   MAX-ACCESS 	read-only
   STATUS 		current
   DESCRIPTION
      "This object identifies the cause for a trap. 
       The index of the entity which produces the trap
       is specified by hm2DevSecTrapCauseIndex."
   ::= { hm2DevSecStatusEntry 3 }

hm2DevSecStatusTrapCauseIndex OBJECT-TYPE
   SYNTAX Integer32
   MAX-ACCESS read-only
   STATUS current
   DESCRIPTION
      "This attribute specifies the entity which produces the trap.
       ext-nvm-update-enabled:	(1) sd, (2) usb, (3) serial (not supported yet)
       no-link:					index of interface table
       0: 						other errors."
   ::= { hm2DevSecStatusEntry 4 }

--
-- *************************************************************
-- Led Group
-- *************************************************************
--

--
-- *************************************************************
-- hm2LedGlobalTable
-- *************************************************************
--
hm2LedGlobalTable OBJECT-TYPE
   SYNTAX SEQUENCE OF Hm2LedGlobalEntry
   MAX-ACCESS 		not-accessible
   STATUS 			current
   DESCRIPTION
      "."
   ::= { hm2DiagLedGroup 1 }

hm2LedGlobalEntry OBJECT-TYPE
   SYNTAX 		Hm2LedGlobalEntry
   MAX-ACCESS	not-accessible
   STATUS 		current
   DESCRIPTION
      "."
   INDEX { hm2LedGlobalLedType }
   ::= { hm2LedGlobalTable 1 }

Hm2LedGlobalEntry ::= SEQUENCE {
	   	hm2LedGlobalLedType		Hm2LedType,
	   	hm2LedGlobalStatus		Hm2LedStatus
   }

hm2LedGlobalLedType 	OBJECT-TYPE
   SYNTAX 			Hm2LedType
   MAX-ACCESS 		not-accessible
   STATUS 			current
   DESCRIPTION
      "."
   ::= { hm2LedGlobalEntry 1 }

hm2LedGlobalStatus 	OBJECT-TYPE
   SYNTAX 			Hm2LedStatus
   MAX-ACCESS 		read-only
   STATUS 			current
   DESCRIPTION
      "."
   ::= { hm2LedGlobalEntry 2 }

--
-- *************************************************************
-- hm2LedPortTable
-- *************************************************************
--
hm2LedPortTable OBJECT-TYPE
   SYNTAX SEQUENCE OF Hm2LedPortEntry
   MAX-ACCESS 		not-accessible
   STATUS 			current
   DESCRIPTION
      "."
   ::= { hm2DiagLedGroup 2 }

hm2LedPortEntry OBJECT-TYPE
   SYNTAX 		Hm2LedPortEntry
   MAX-ACCESS	not-accessible
   STATUS 		current
   DESCRIPTION
      "."
   INDEX { hm2IfacePhysIndex }
   ::= { hm2LedPortTable 1 }

Hm2LedPortEntry ::= SEQUENCE {
	   	hm2LedPortStatus		Hm2LedStatus,
	   	hm2LedPortPoeStatus		Hm2LedStatus,
	   	hm2LedPortSignaling     HmEnabledStatus
   }

hm2LedPortStatus 	OBJECT-TYPE
   SYNTAX 			Hm2LedStatus
   MAX-ACCESS 		read-only
   STATUS 			current
   DESCRIPTION
      "."
   ::= { hm2LedPortEntry 1 }

hm2LedPortPoeStatus OBJECT-TYPE
   SYNTAX 			Hm2LedStatus
   MAX-ACCESS 		read-only
   STATUS 			current
   DESCRIPTION
      "."
   ::= { hm2LedPortEntry 2 }
   
hm2LedPortSignaling OBJECT-TYPE
   SYNTAX 			HmEnabledStatus
   MAX-ACCESS 		read-write
   STATUS 			current
   DESCRIPTION
      "Enable for LED port signaling."
   DEFVAL  { disable } 
   ::= { hm2LedPortEntry 3 }
   
--
-- *************************************************************
-- hm2LedControlGroup
-- *************************************************************
--
hm2LedControlGroup						OBJECT IDENTIFIER ::= { hm2DiagLedGroup 3 }

hm2LedPortMode 	OBJECT-TYPE
   SYNTAX 					INTEGER {
         			  			portpanel (0),
                     			servicepanel (1)
                  			  }
   MAX-ACCESS 		read-write
   STATUS 			current
   DESCRIPTION
      "Switch LED signalling between the port LEDs on front side (port panel) and 
	   the port LEDs on the back side (service panel) of the device."
   DEFVAL  { servicepanel } 
   ::= { hm2LedControlGroup 1 }
 
-- *************************************************************
-- hm2DiagIfaceUtilizationTable
-- *************************************************************

hm2DiagIfaceUtilizationTable   OBJECT-TYPE
   SYNTAX SEQUENCE OF Hm2DiagIfaceUtilizationEntry
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION
       "This table contains variables for each interface of
       the switch."
   ::= { hm2DiagIfaceUtilizationGroup 1 }

hm2DiagIfaceUtilizationEntry     OBJECT-TYPE
   SYNTAX Hm2DiagIfaceUtilizationEntry
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION "The entry of the hm2DiagIfaceUtilizationTable."
   INDEX { ifIndex }
   ::= { hm2DiagIfaceUtilizationTable 1 }

Hm2DiagIfaceUtilizationEntry ::= SEQUENCE {
   hm2DiagIfaceUtilization Integer32,
   hm2DiagIfaceUtilizationControlInterval Integer32,
   hm2DiagIfaceUtilizationAlarmLowerThreshold Integer32,
   hm2DiagIfaceUtilizationAlarmUpperThreshold Integer32,
   hm2DiagIfaceUtilizationAlarmCondition TruthValue
   }

hm2DiagIfaceUtilization OBJECT-TYPE
   SYNTAX Integer32 (0..10000)
   MAX-ACCESS read-only
   STATUS current
   DESCRIPTION
       "The best estimate of the mean physical layer
       network utilization on this interface during the 
       last sampling interval, in hundredth of one percent.
       The first historyControlInterval (rfc1757) of this
       interface is used as sampling interval."
   DEFVAL { 0 }
   ::= { hm2DiagIfaceUtilizationEntry 1 }

hm2DiagIfaceUtilizationControlInterval    OBJECT-TYPE
   SYNTAX Integer32 (1..3600)
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "The interval in seconds over which the data is
      sampled for hm2DiagIfaceUtilization.
      This interval can be any number of seconds
      between 1 and 3600 (1 hour).
      The first historyControlInterval (rfc1757) of this
      interface is used as sampling interval."
   DEFVAL { 30 }
   ::= { hm2DiagIfaceUtilizationEntry 2 }

hm2DiagIfaceUtilizationAlarmLowerThreshold OBJECT-TYPE
   SYNTAX Integer32 (0..10000)
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
        "Surveys the interface utilization hm2DiagIfaceUtilization and
         generates an alarm for this interfaces, if  
         the utilization value is below the given limit.
         A value of 0 disables the alarm generation."
   DEFVAL { 0 }
   ::= { hm2DiagIfaceUtilizationEntry 3 }

hm2DiagIfaceUtilizationAlarmUpperThreshold OBJECT-TYPE
   SYNTAX Integer32 (0..10000)
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
        "Surveys the interface utilization hm2DiagIfaceUtilization and
         generates an alarm for this interfaces, if the given
         limit is exceeded. 
         A value of 0 disables the alarm generation."
   DEFVAL { 0 }
   ::= { hm2DiagIfaceUtilizationEntry 4 }


hm2DiagIfaceUtilizationAlarmCondition OBJECT-TYPE
   SYNTAX TruthValue
   MAX-ACCESS read-only
   STATUS current
   DESCRIPTION
        "The alarm condition is given (true), if the given
         hm2DiagIfaceUtilizationAlarmUpperThreshold limit is exceeded 
         by the interface utilization or if the utilization value falls below 
         hm2DiagIfaceUtilizationAlarmLowerThreshold limit. 
         The alarm condition will be removed, when the interface utilization 
         value falls in between hm2DiagIfaceUtilizationAlarmLowerThreshold 
         hm2DiagIfaceUtilizationAlarmUpperThreshold."
   
   ::= { hm2DiagIfaceUtilizationEntry 5 }

-- *************************************************************
-- hm2DiagEgressIfaceUtilizationTable
-- *************************************************************

hm2DiagEgressIfaceUtilizationTable   OBJECT-TYPE
   SYNTAX SEQUENCE OF Hm2DiagEgressIfaceUtilizationEntry
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION
       "This table contains egress variables for each interface of
       the switch."
   ::= { hm2DiagIfaceUtilizationGroup 2 }

hm2DiagEgressIfaceUtilizationEntry     OBJECT-TYPE
   SYNTAX Hm2DiagEgressIfaceUtilizationEntry
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION "The entry of the hm2DiagEgressIfaceUtilizationTable."
   INDEX { ifIndex }
   ::= { hm2DiagEgressIfaceUtilizationTable 1 }

Hm2DiagEgressIfaceUtilizationEntry ::= SEQUENCE {
   hm2DiagEgressIfaceUtilization Integer32,
   hm2DiagEgressIfaceUtilizationControlInterval Integer32,
   hm2DiagEgressIfaceUtilizationAlarmLowerThreshold Integer32,
   hm2DiagEgressIfaceUtilizationAlarmUpperThreshold Integer32,
   hm2DiagEgressIfaceUtilizationAlarmCondition TruthValue
   }

hm2DiagEgressIfaceUtilization OBJECT-TYPE
   SYNTAX Integer32 (0..10000)
   MAX-ACCESS read-only
   STATUS current
   DESCRIPTION
       "The best estimate of the mean physical layer
       network egress utilization on this interface during the
       last sampling interval, in hundredth of one percent.
       The first historyControlInterval (rfc1757) of this
       interface is used as sampling interval."
   DEFVAL { 0 }
   ::= { hm2DiagEgressIfaceUtilizationEntry 1 }

hm2DiagEgressIfaceUtilizationControlInterval    OBJECT-TYPE
   SYNTAX Integer32 (1..3600)
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "The interval in seconds over which the egress data is
      sampled for hm2DiagEgressIfaceUtilization.
      This interval can be any number of seconds
      between 1 and 3600 (1 hour).
      The first historyControlInterval (rfc1757) of this
      interface is used as sampling interval."
   DEFVAL { 30 }
   ::= { hm2DiagEgressIfaceUtilizationEntry 2 }

hm2DiagEgressIfaceUtilizationAlarmLowerThreshold OBJECT-TYPE
   SYNTAX Integer32 (0..10000)
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
        "Surveys the egress interface utilization hm2DiagEgressIfaceUtilization and
         generates an alarm for this interface, if
         the utilization value is below the given limit.
         A value of 0 disables the alarm generation."
   DEFVAL { 0 }
   ::= { hm2DiagEgressIfaceUtilizationEntry 3 }

hm2DiagEgressIfaceUtilizationAlarmUpperThreshold OBJECT-TYPE
   SYNTAX Integer32 (0..10000)
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
        "Surveys the egress interface utilization hm2DiagEgressIfaceUtilization and
         generates an alarm for this interface, if the given
         limit is exceeded.
         A value of 0 disables the alarm generation."
   DEFVAL { 0 }
   ::= { hm2DiagEgressIfaceUtilizationEntry 4 }


hm2DiagEgressIfaceUtilizationAlarmCondition OBJECT-TYPE
   SYNTAX TruthValue
   MAX-ACCESS read-only
   STATUS current
   DESCRIPTION
        "The alarm condition is given (true), if the given
         hm2DiagEgressIfaceUtilizationAlarmUpperThreshold limit is exceeded 
         by the egress interface utilization or if the utilization value falls below 
         hm2DiagEgressIfaceUtilizationAlarmLowerThreshold limit. 
         The alarm condition will be removed, when the egress interface utilization 
         value falls in between hm2DiagEgressIfaceUtilizationAlarmLowerThreshold 
         hm2DiagEgressIfaceUtilizationAlarmUpperThreshold."

   ::= { hm2DiagEgressIfaceUtilizationEntry 5 }


--
-- *************************************************************
-- Cable Tester Group
-- *************************************************************
--

hm2DiagCableTesterStatus OBJECT-TYPE
   SYNTAX     INTEGER {
         active(1),
         success(2),
         failure(3),
         uninitialized(4)
         }
   MAX-ACCESS read-write
   STATUS     current
   DESCRIPTION
         "Status of the Virtual Cable Tester
          active(1)        - Cable testing is in progress.  
                             Set to this value to start the test.
          success(2)       - A successful test was performed.  
                             Cannot be set.
          failure(3)       - A failure was encountered during the test.
                             Cannot be set.
          uninitialized(4) - No test has been performed yet. 
                             Cannot be set."
   DEFVAL { uninitialized }
   ::= { hm2DiagCableTesterGroup 1 }

hm2DiagCableTesterIfIndex OBJECT-TYPE
   SYNTAX      Unsigned32
   MAX-ACCESS  read-write
   STATUS      current
   DESCRIPTION
         "Determines on which port to perform the cable test.  
          Limited to copper based ports."
   DEFVAL { 0 }
   ::= { hm2DiagCableTesterGroup 2 }

hm2DiagCableTesterCableTable   OBJECT-TYPE
   SYNTAX SEQUENCE OF Hm2DiagCableTesterCableEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
         "This table contains variables for each pair of
          the cable."
   ::= { hm2DiagCableTesterGroup 10 }

hm2DiagCableTesterCableEntry     OBJECT-TYPE
   SYNTAX      Hm2DiagCableTesterCableEntry
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION "The entry of the hm2DiagCableTesterCableTable."
   INDEX { hm2DiagCableTesterCablePair }
   ::= { hm2DiagCableTesterCableTable 1 }

Hm2DiagCableTesterCableEntry ::= SEQUENCE {
   hm2DiagCableTesterCablePair Integer32,
   hm2DiagCableTesterCableStatus INTEGER,
   hm2DiagCableTesterCableMinimumLength Unsigned32,
   hm2DiagCableTesterCableMaximumLength Unsigned32,
   hm2DiagCableTesterCableFailureLocation Unsigned32
   }

hm2DiagCableTesterCablePair OBJECT-TYPE
   SYNTAX      Integer32 (1..4)
   MAX-ACCESS  not-accessible
   STATUS      current
   DESCRIPTION
         "Index of the hm2DiagCableTesterCableTable.
          If a PHY does not support the measurement per pair, 
          the first index is used to show the values."
   ::= { hm2DiagCableTesterCableEntry 1 }
      
hm2DiagCableTesterCableStatus OBJECT-TYPE
   SYNTAX      INTEGER {
         normal(1),
         open(2),
         short(3),
         unknown(4)
         }
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
         "Indicates the results of the Cable Test.
          normal(1)        - The cable is working correctly.
          open(2)          - The cable is disconnected or there is a faulty
                             connector.
          short(3)         - There is an electrical short in the cable.
          unknown(4)       - No test has been performed yet, or a test is
                             currently in progress."
   DEFVAL { unknown }
   ::= { hm2DiagCableTesterCableEntry 2 }

hm2DiagCableTesterCableMinimumLength OBJECT-TYPE
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
         "The estimated length of the cable in meters.  This value
          indicates the shortest length estimated.  This object will
          return 0 if hm2DiagCableTesterStatus is not success(2) or the cable
          length is unknown."
   DEFVAL { 0 }
   ::= { hm2DiagCableTesterCableEntry 3 }

hm2DiagCableTesterCableMaximumLength OBJECT-TYPE
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
         "The estimated length of the cable in meters.  This value
          indicates the longest length estimated.  This object will
          return 0 if hm2DiagCableTesterStatus is not success(2) or the cable
          length is unknown."
   DEFVAL { 0 }
   ::= { hm2DiagCableTesterCableEntry 4 }

hm2DiagCableTesterCableFailureLocation OBJECT-TYPE
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
         "The estimated distance in meters from the end of the cable to
          the failure location.  This object will return 0 if
          hm2DiagCableTesterStatus is not success(2)."
   DEFVAL { 0 }
   ::= { hm2DiagCableTesterCableEntry 5 }
         
   
--
-- *************************************************************
-- hm2PortMonitorGroup
-- *************************************************************
--

--hm2PortMonitorGroup		OBJECT IDENTIFIER ::= { hm2ConfigurationMibs 0 }

hm2PortMonitorAdminMode	OBJECT-TYPE
			SYNTAX			TruthValue
			MAX-ACCESS		read-write
			STATUS			current
			DESCRIPTION
			"Global switch to enable / disable the port state actions,
			which are performed if a condition becomes true"
			DEFVAL			{ false }
			::= { hm2PortMonitorGroup 1 }

hm2PortMonitorIntfTable	OBJECT-TYPE
			SYNTAX			SEQUENCE OF Hm2PortMonitorIntfEntry
			MAX-ACCESS		not-accessible
			STATUS			current
			DESCRIPTION
			"Port state mode interface table."
			::= { hm2PortMonitorGroup 2 }

hm2PortMonitorIntfEntry	OBJECT-TYPE
			SYNTAX			Hm2PortMonitorIntfEntry
			MAX-ACCESS		not-accessible
			STATUS			current
			DESCRIPTION
			"Port state mode interface entry."
			INDEX			{ ifIndex }
			::= { hm2PortMonitorIntfTable 1 }

Hm2PortMonitorIntfEntry ::=
			SEQUENCE		{				
					hm2PortMonitorIntfReset	TruthValue,
					hm2PortMonitorIntfAction	INTEGER
					}



hm2PortMonitorIntfReset	OBJECT-TYPE
			SYNTAX			TruthValue
			MAX-ACCESS		read-write
			STATUS			current
			DESCRIPTION
			"Port monitor interface reset."
			DEFVAL			{ false }
			::= { hm2PortMonitorIntfEntry 2 }

hm2PortMonitorIntfAction	OBJECT-TYPE
			SYNTAX			INTEGER {
							port-disable(1),
							trap-only (2),
							auto-disable(3)
							}
			MAX-ACCESS		read-write
			STATUS			current
			DESCRIPTION
			"Interface link disable state."
			DEFVAL			{ auto-disable }
			::= { hm2PortMonitorIntfEntry 3 }



hm2PortMonitorConditionGroup	OBJECT IDENTIFIER ::= { hm2PortMonitorGroup 3 }

hm2KbpsUnitTrafficTypeInvalid OBJECT-IDENTITY
			STATUS        current
			DESCRIPTION   "Interface {0}: 'Kbps' unit can only be used for traffic type 'all'."
			 ::= { hm2PortMonitorGroup 4}

hm2PortMonitorConditionIntfTable	OBJECT-TYPE
			SYNTAX			SEQUENCE OF Hm2PortMonitorConditionIntfEntry
			MAX-ACCESS		not-accessible
			STATUS			current
			DESCRIPTION
			"Port state condition interface table."
			::= { hm2PortMonitorConditionGroup 1 }

hm2PortMonitorConditionIntfEntry	OBJECT-TYPE
			SYNTAX			Hm2PortMonitorConditionIntfEntry
			MAX-ACCESS		not-accessible
			STATUS			current
			DESCRIPTION
			"Port state action interface entry."
			INDEX			{ ifIndex }
			::= { hm2PortMonitorConditionIntfTable 1 }
			
Hm2PortMonitorConditionIntfEntry ::=
			SEQUENCE		{
				hm2PortMonitorConditionField BITS,
				hm2PortMonitorConditionLinkFlapMode TruthValue,
				hm2PortMonitorConditionCrcFragmentsMode TruthValue,
				hm2PortMonitorConditionDuplexMismatchDetectionMode TruthValue,
				hm2PortMonitorConditionOverloadDetectionMode TruthValue,				
				hm2PortMonitorConditionSpeedDuplexMode		 TruthValue
					}

hm2PortMonitorConditionField				OBJECT-TYPE
		   	SYNTAX      		BITS {
		   					none(0),
		   					link-flap(1),
		   					crcFragments(2),
		   					duplexMismatch(3),
		   					overload-detection(4),
    	               		speed-duplex (5)}
			MAX-ACCESS		read-only
			STATUS			current
			DESCRIPTION
			"Condition type field."
			::= { hm2PortMonitorConditionIntfEntry 1 }

hm2PortMonitorConditionLinkFlapMode			OBJECT-TYPE
			SYNTAX			TruthValue
			MAX-ACCESS		read-write
			STATUS			current
			DESCRIPTION
			"Interface link flap mode."
			DEFVAL			{ false }
			::= { hm2PortMonitorConditionIntfEntry 2 }

hm2PortMonitorConditionCrcFragmentsMode		OBJECT-TYPE
			SYNTAX			TruthValue
			MAX-ACCESS		read-write
			STATUS			current
			DESCRIPTION
			"Interface CrcFragments mode."
			DEFVAL			{ false }
			::= { hm2PortMonitorConditionIntfEntry 3 }
			
hm2PortMonitorConditionDuplexMismatchDetectionMode OBJECT-TYPE
			SYNTAX TruthValue
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
			"Interface duplex mismatch detection mode."
			DEFVAL { false }
			::= { hm2PortMonitorConditionIntfEntry 4 }

hm2PortMonitorConditionOverloadDetectionMode		OBJECT-TYPE
		SYNTAX			TruthValue
		MAX-ACCESS		read-write
		STATUS			current
		DESCRIPTION
			"Interface Overload Detection mode."
		DEFVAL			{ false }
	::= { hm2PortMonitorConditionIntfEntry 5 }
			
hm2PortMonitorConditionSpeedDuplexMode		OBJECT-TYPE
		SYNTAX			TruthValue
		MAX-ACCESS		read-write
		STATUS			current
		DESCRIPTION
			"Interface Speed and Duplex monitor mode."
		DEFVAL			{ false }
	::= { hm2PortMonitorConditionIntfEntry 6 }
	
hm2PortMonitorConditionLinkFlapGroup	OBJECT IDENTIFIER ::= { hm2PortMonitorConditionGroup 2 }

hm2PortMonitorConditionLinkFlapIntfTable	OBJECT-TYPE
			SYNTAX			SEQUENCE OF Hm2PortMonitorConditionLinkFlapIntfEntry
			MAX-ACCESS		not-accessible
			STATUS			current
			DESCRIPTION
			"Port condition link flap interface table."
			::= { hm2PortMonitorConditionLinkFlapGroup 1 }

hm2PortMonitorConditionLinkFlapIntfEntry	OBJECT-TYPE
			SYNTAX			Hm2PortMonitorConditionLinkFlapIntfEntry
			MAX-ACCESS		not-accessible
			STATUS			current
			DESCRIPTION
			"Port condition link flap interface entry."
			INDEX			{ ifIndex }
			::= { hm2PortMonitorConditionLinkFlapIntfTable 1 }

Hm2PortMonitorConditionLinkFlapIntfEntry ::=
			SEQUENCE		{					
					hm2PortMonitorConditionLinkFlapInterval Integer32,
					hm2PortMonitorConditionLinkFlapCount Integer32,
					hm2PortMonitorConditionLinkFlapCountInterval Integer32,
					hm2PortMonitorConditionLinkFlapCountTotal Integer32
					}

hm2PortMonitorConditionLinkFlapInterval		OBJECT-TYPE
			SYNTAX			Integer32(1..180)
			MAX-ACCESS		read-write
			STATUS			current
			DESCRIPTION
			"Measure interval in seconds (1-180s) for link flap detection."
			DEFVAL			{ 10 }
			::= { hm2PortMonitorConditionLinkFlapIntfEntry 1 }

hm2PortMonitorConditionLinkFlapCount	OBJECT-TYPE
			SYNTAX			Integer32(1..100)
			MAX-ACCESS		read-write
			STATUS			current
			DESCRIPTION
			"Link flap counter (1-100)."
			DEFVAL			{ 5 }
			::= { hm2PortMonitorConditionLinkFlapIntfEntry 2 }
			
hm2PortMonitorConditionLinkFlapCountInterval	OBJECT-TYPE
			SYNTAX			Integer32
			MAX-ACCESS		read-only
			STATUS			current
			DESCRIPTION
			"Link flap count that occured in last interval."
			::= { hm2PortMonitorConditionLinkFlapIntfEntry 3 }

hm2PortMonitorConditionLinkFlapCountTotal	OBJECT-TYPE
			SYNTAX			Integer32
			MAX-ACCESS		read-only
			STATUS			current
			DESCRIPTION
			"Total link flap count."
			::= { hm2PortMonitorConditionLinkFlapIntfEntry 4 }

	
hm2PortMonitorConditionCrcFragmentsGroup	OBJECT IDENTIFIER ::= { hm2PortMonitorConditionGroup 3 }

hm2PortMonitorConditionCrcFragmentsIntfTable	OBJECT-TYPE
			SYNTAX			SEQUENCE OF Hm2PortMonitorConditionCrcFragmentsIntfEntry
			MAX-ACCESS		not-accessible
			STATUS			current
			DESCRIPTION
			"Port condition CrcFragments interface table."
			::= { hm2PortMonitorConditionCrcFragmentsGroup 1 }

hm2PortMonitorConditionCrcFragmentsIntfEntry	OBJECT-TYPE
			SYNTAX			Hm2PortMonitorConditionCrcFragmentsIntfEntry
			MAX-ACCESS		not-accessible
			STATUS			current
			DESCRIPTION
			"Port condition CrcFragments interface entry."
			INDEX			{ ifIndex }
			::= { hm2PortMonitorConditionCrcFragmentsIntfTable 1 }

Hm2PortMonitorConditionCrcFragmentsIntfEntry ::=
			SEQUENCE		{
					hm2PortMonitorConditionCrcFragmentsInterval Integer32,
					hm2PortMonitorConditionCrcFragmentsCount Integer32,
					hm2PortMonitorConditionCrcFragmentsCountInterval Integer32,
					hm2PortMonitorConditionCrcFragmentsCountTotal Integer32
					}
hm2PortMonitorConditionCrcFragmentsInterval		OBJECT-TYPE
			SYNTAX			Integer32(5..180)
			MAX-ACCESS		read-write
			STATUS			current
			DESCRIPTION
			"Measure interval in seconds (5-180s) for CrcFragments detection."
			DEFVAL			{ 10 }
			::= { hm2PortMonitorConditionCrcFragmentsIntfEntry 1 }

hm2PortMonitorConditionCrcFragmentsCount		OBJECT-TYPE
			SYNTAX			Integer32(1..1000000)
			MAX-ACCESS		read-write
			STATUS			current
			DESCRIPTION
			"CrcFragments counter (1-1000000)."
			DEFVAL			{ 1000 }
			::= { hm2PortMonitorConditionCrcFragmentsIntfEntry 2 }

hm2PortMonitorConditionCrcFragmentsCountInterval	OBJECT-TYPE
			SYNTAX			Integer32
			MAX-ACCESS		read-only
			STATUS			current
			DESCRIPTION
			"CrcFragments count that occured in last interval."
			::= { hm2PortMonitorConditionCrcFragmentsIntfEntry 3 }

hm2PortMonitorConditionCrcFragmentsCountTotal	OBJECT-TYPE
			SYNTAX			Integer32
			MAX-ACCESS		read-only
			STATUS			current
			DESCRIPTION
			"Total CrcFragments count."
			::= { hm2PortMonitorConditionCrcFragmentsIntfEntry 4 }


			
hm2PortMonitorConditionOverloadDetectionGroup	OBJECT IDENTIFIER ::= { hm2PortMonitorConditionGroup 4 }


hm2PortMonitorConditionOvldDetIntfTable	OBJECT-TYPE
		SYNTAX	SEQUENCE OF Hm2PortMonitorConditionOvldDetIntfEntry
		MAX-ACCESS		not-accessible
		STATUS			current
		DESCRIPTION
			"Port condition overload detection interface table."
	::= { hm2PortMonitorConditionOverloadDetectionGroup 1 }

hm2PortMonitorConditionOvldDetIntfEntry	OBJECT-TYPE
		SYNTAX			Hm2PortMonitorConditionOvldDetIntfEntry
		MAX-ACCESS		not-accessible
		STATUS			current
		DESCRIPTION
				"Port condition overload detection interface entry."
		INDEX			{ ifIndex }
	::= { hm2PortMonitorConditionOvldDetIntfTable 1 }
	
	
	Hm2PortMonitorConditionOvldDetIntfEntry ::= SEQUENCE		
	{
	hm2PortMonitorConditionOvldDetTrfcType 			INTEGER,
	hm2PortMonitorConditionOvldDetTholdType 			INTEGER,
	hm2PortMonitorConditionOvldDetLwrTholdVal 	Integer32,
	hm2PortMonitorConditionOvldDetUprTholdVal 	Integer32,
	hm2PortMonitorConditionOvldDetIntvl 				Integer32,
	hm2PortMonitorConditionOvldDetPkgCntAll 			Integer32,
	hm2PortMonitorConditionOvldDetPkgCntBC 	Integer32,
	hm2PortMonitorConditionOvldDetPkgCntMC 	Integer32,
	hm2PortMonitorConditionOvldDetPkgCntKbit 			Integer32
	}


hm2PortMonitorConditionOvldDetTrfcType 	OBJECT-TYPE
		SYNTAX 		INTEGER{
							all (1),
					 		bc (2),
					 		bc-mc (3)
							}
		MAX-ACCESS		read-write
		STATUS			current
		DESCRIPTION
			"Overload detection condition traffic type."
		DEFVAL			{ bc }
	::= { hm2PortMonitorConditionOvldDetIntfEntry 1 }

hm2PortMonitorConditionOvldDetTholdType 	OBJECT-TYPE
			SYNTAX 		INTEGER{
						pps(1),
						kbps(2)
						}
		MAX-ACCESS		read-write
		STATUS			current
		DESCRIPTION
			"Overload detection conditon threshold type."
		DEFVAL			{ pps }
	::= { hm2PortMonitorConditionOvldDetIntfEntry 2 }

hm2PortMonitorConditionOvldDetLwrTholdVal 	OBJECT-TYPE
		SYNTAX			Integer32 (0..10000000)
		MAX-ACCESS		read-write
		STATUS			current
		DESCRIPTION
			"Overload detection condition lower threshold value."
		DEFVAL			{ 0 }
	::= { hm2PortMonitorConditionOvldDetIntfEntry 3 }


hm2PortMonitorConditionOvldDetUprTholdVal 	OBJECT-TYPE
		SYNTAX			Integer32 (0..10000000)
		MAX-ACCESS		read-write
		STATUS			current
		DESCRIPTION
			"Overload detection condition upper threshold value."
		DEFVAL			{ 0 }
	::= { hm2PortMonitorConditionOvldDetIntfEntry 4 }
			
hm2PortMonitorConditionOvldDetIntvl 		OBJECT-TYPE
		SYNTAX			Integer32(1..20)
		MAX-ACCESS		read-write
		STATUS			current
		DESCRIPTION
			"Measure interval in seconds (1-20s) for overload detection."
		DEFVAL			{ 1 }
	::= { hm2PortMonitorConditionOvldDetIntfEntry 5 }			
	

hm2PortMonitorConditionOvldDetPkgCntAll 	OBJECT-TYPE
		SYNTAX			Integer32
		MAX-ACCESS		read-only
		STATUS			current
		DESCRIPTION
			"All package count from last interval."
		DEFVAL			{ 0 }
	::= { hm2PortMonitorConditionOvldDetIntfEntry 6}


hm2PortMonitorConditionOvldDetPkgCntBC 	OBJECT-TYPE
		SYNTAX			Integer32
		MAX-ACCESS		read-only
		STATUS			current
		DESCRIPTION
			"Broadcast package count from last interval."
		DEFVAL			{ 0 }
	::= { hm2PortMonitorConditionOvldDetIntfEntry 7}
	
hm2PortMonitorConditionOvldDetPkgCntMC   	OBJECT-TYPE
		SYNTAX			Integer32
		MAX-ACCESS		read-only
		STATUS			current
		DESCRIPTION
			"Overload detection condition lower threshold value."
		DEFVAL			{ 0 }
	::= { hm2PortMonitorConditionOvldDetIntfEntry 8}	

hm2PortMonitorConditionOvldDetPkgCntKbit   	OBJECT-TYPE
		SYNTAX			Integer32
		MAX-ACCESS		read-only
		STATUS			current
		DESCRIPTION
			"Overload detection condition lower threshold value."
		DEFVAL			{ 0 }
	::= { hm2PortMonitorConditionOvldDetIntfEntry 9}		


hm2PortMonitorConditionSpeedDuplexGroup	OBJECT IDENTIFIER ::= { hm2PortMonitorConditionGroup 5 }


hm2PortMonitorConditionSpeedDuplexTable	OBJECT-TYPE
		SYNTAX	SEQUENCE OF Hm2PortMonitorConditionSpeedDuplexEntry
		MAX-ACCESS		not-accessible
		STATUS			current
		DESCRIPTION
			"Port condition speed-duplex interface table."
	::= { hm2PortMonitorConditionSpeedDuplexGroup 1 }

hm2PortMonitorConditionSpeedDuplexEntry	OBJECT-TYPE
		SYNTAX			Hm2PortMonitorConditionSpeedDuplexEntry
		MAX-ACCESS		not-accessible
		STATUS			current
		DESCRIPTION
				"Port condition speed-duplex interface entry."
		INDEX			{ ifIndex }
	::= { hm2PortMonitorConditionSpeedDuplexTable 1 }
	
	
Hm2PortMonitorConditionSpeedDuplexEntry ::= SEQUENCE {
	hm2PortMonitorConditionSpeedDuplexValue 			BITS
}
    
hm2PortMonitorConditionSpeedDuplexValue  	OBJECT-TYPE
	SYNTAX			BITS  {
						hdx-10(0),
						fdx-10(1),
						hdx-100(2),
						fdx-100(3),
						hdx-1000(4),
						fdx-1000(5),
						fdx-2500(6),
						fdx-10000(7)
						}
	MAX-ACCESS		read-write
	STATUS			current
	DESCRIPTION
		"Speed and duplex combination allowed by port-monitor."
	DEFVAL			{{ hdx-10, fdx-10, hdx-100, fdx-100, hdx-1000, fdx-1000, fdx-2500, fdx-10000 }}
::= { hm2PortMonitorConditionSpeedDuplexEntry 1} 
	
-- **************************************************************************
-- *																		*
-- *	System Resources including CPU, memory, network						*
-- *																		*
-- **************************************************************************

hm2DiagEnableMeasurement OBJECT-TYPE
	SYNTAX		HmEnabledStatus
	MAX-ACCESS  read-write
    STATUS  	current
    DESCRIPTION
            "Enable or disable the resources measurement If disabled, the
             task - needed for measurement - is also deleted."
	DEFVAL  { enable }
    ::= { hm2DiagResourcesGroup 1 }

-- 
-- ***********************************************************
-- 
--                  C P U    R E S O U R C E S 
-- 
-- *********************************************************** 
--
hm2DiagCpuResourcesGroup           	   OBJECT IDENTIFIER ::= { hm2DiagResourcesGroup 10 }

hm2DiagCpuUtilization OBJECT-TYPE
    SYNTAX      Integer32 (0..100)
    UNITS		"percent"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The current cpu utilization of the device in percent."

    ::= { hm2DiagCpuResourcesGroup 1 }

hm2DiagCpuAverageUtilization OBJECT-TYPE
    SYNTAX      Integer32 (0..100)
    UNITS		"percent"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The average cpu utilization of the device in percent,
             max. measured over the last 30 minutes."
 
    ::= { hm2DiagCpuResourcesGroup 2 }

hm2DiagCpuRunningProcesses OBJECT-TYPE
    SYNTAX      Integer32 (0..32768)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The current number of processes running."

    ::= { hm2DiagCpuResourcesGroup 3 }

hm2DiagCpuMaxRunningProcesses OBJECT-TYPE
    SYNTAX      Integer32 (0..32768)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The maximum number of processes running, max. since
             the last 30 minutes." 
 
    ::= { hm2DiagCpuResourcesGroup 4 }

-- 
-- ***********************************************************
-- 
--               M E M O R Y    R E S O U R C E S 
-- 
-- *********************************************************** 
--
hm2DiagMemoryResourcesGroup	           OBJECT IDENTIFIER ::= { hm2DiagResourcesGroup 11 }

hm2DiagMemoryRamAllocated OBJECT-TYPE
    SYNTAX      Integer32 (0..2147483647)
    UNITS		"kBytes"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The current allocated RAM of the device in kBytes."

    ::= { hm2DiagMemoryResourcesGroup 1 }

hm2DiagMemoryRamFree OBJECT-TYPE
    SYNTAX      Integer32 (0..2147483647)
    UNITS		"kBytes"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The current free RAM of the device in kBytes."
 
    ::= { hm2DiagMemoryResourcesGroup 2 }

hm2DiagMemoryRamAllocatedAverage OBJECT-TYPE
    SYNTAX      Integer32 (0..2147483647)
    UNITS		"kBytes"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The average allocated RAM of the device in kBytes,
             measured over the last 30 minutes."

    ::= { hm2DiagMemoryResourcesGroup 3 }

hm2DiagMemoryRamFreeAverage OBJECT-TYPE
    SYNTAX      Integer32 (0..2147483647)
    UNITS		"kBytes"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The average free RAM of the device in kBytes,
             measured over the last 30 minutes."
   
    ::= { hm2DiagMemoryResourcesGroup 4 }

hm2DiagMemoryRawFlashMainAllocated OBJECT-TYPE
    SYNTAX      Integer32 (0..2147483647)
    UNITS		"kBytes"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The current allocated flash memory for the main 
			 software image in kBytes."
   
    ::= { hm2DiagMemoryResourcesGroup 10 }
	
hm2DiagMemoryRawFlashMainFree OBJECT-TYPE
    SYNTAX      Integer32 (0..2147483647)
    UNITS		"kBytes"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The current free flash memory for the main 
			 software image in kBytes."
   
    ::= { hm2DiagMemoryResourcesGroup 11 }

hm2DiagMemoryFlashFileSystemAllocated OBJECT-TYPE
    SYNTAX      Integer32 (0..2147483647)
    UNITS		"kBytes"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The current allocated memory within the flash 
			 file system in kBytes."
   
    ::= { hm2DiagMemoryResourcesGroup 12 }
	
hm2DiagMemoryFlashFileSystemFree OBJECT-TYPE
    SYNTAX      Integer32 (0..2147483647)
    UNITS		"kBytes"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The current free memory within the flash 
			 file system in kBytes."
   
    ::= { hm2DiagMemoryResourcesGroup 13 }
	
-- 
-- ***********************************************************
-- 
--             N E T W O R K    R E S O U R C E S 
-- 
-- *********************************************************** 
--
hm2DiagNetworkResourcesGroup           OBJECT IDENTIFIER ::= { hm2DiagResourcesGroup 12 } 

hm2DiagNetworkCpuIfUtilization OBJECT-TYPE
    SYNTAX      Integer32 (0..100)
    UNITS		"precent"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The current network utilization of the internal cpu interface in percent."

    ::= { hm2DiagNetworkResourcesGroup 1 }

hm2DiagNetworkCpuIfAverageUtilization OBJECT-TYPE
    SYNTAX      Integer32 (0..100)
    UNITS		"precent"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The average network utilization of the internal cpu interface in percent,
             measured over the last 30 minutes."
 
    ::= { hm2DiagNetworkResourcesGroup 2 }  

-- 
-- ***********************************************************
-- hm2DiagnosticMibNotifications
-- ***********************************************************
--

hm2SigConStateChangeTrap NOTIFICATION-TYPE
		OBJECTS  { 
					hm2SigConID,
					hm2SigConOperState, 
					hm2SigConTrapCause, 
					hm2SigConTrapCauseIndex 
		  		 }
		STATUS  current
		DESCRIPTION
			"This trap is sent if the value of hm2SigConState changes its value."
		::= { hm2DiagnosticMibNotifications 1 }

hm2DevMonStateChangeTrap NOTIFICATION-TYPE
		OBJECTS  { 
					hm2DevMonID,
					hm2DevMonOperState, 
					hm2DevMonTrapCause, 
					hm2DevMonTrapCauseIndex 
				 }
		STATUS  current
		DESCRIPTION
			"This trap is sent if the value of hm2DevMonState changes its value."
		::= { hm2DiagnosticMibNotifications 2 }


hm2DevSecStateChangeTrap NOTIFICATION-TYPE
		OBJECTS {
					hm2DevSecOperState,
					hm2DevSecTrapCause,
					hm2DevSecTrapCauseIndex
				}
		STATUS  current
		DESCRIPTION
			"This trap is sent if the value of hm2DevSecState changes its value."
		::= { hm2DiagnosticMibNotifications 3 }

hm2DiagSelftestActionTrap NOTIFICATION-TYPE
		OBJECTS		{ hm2DiagSelftestActionCause }
		STATUS		current
		DESCRIPTION	
			"This trap is sent if a self-test action is performed and
			hm2DiagSelftestAction is configured to sendTrap(2)."
		::= { hm2DiagnosticMibNotifications 4 }

-- *************************************************************
-- hm2DiagIfaceUtilization notifications
-- *************************************************************
hm2DiagIfaceUtilizationTrap NOTIFICATION-TYPE
   OBJECTS { 
      hm2DiagIfaceUtilization,
      hm2DiagIfaceUtilizationAlarmCondition
      }
   STATUS  current
   DESCRIPTION "This trap is sent if the value of hm2DiagIfaceUtilization 
      exceeds or falls back below the interface utilization thresholds
      hm2DiagIfaceUtilizationAlarmConditionThreshold and 
      hm2DiagIfaceUtilizationAlarmRemovalThreshold."
   ::= { hm2DiagnosticMibNotifications 5 }
   
-- *************************************************************
-- hm2PortMonitorPortTrap 
-- *************************************************************

	hm2PortMonitorPortTrap NOTIFICATION-TYPE
	OBJECTS  { ifIndex, 
			   hm2PortMonitorConditionField
			 }
		STATUS current
		DESCRIPTION
		"This trap is sent if the a port has been disabled by port disable action by port monitor."
		::= { hm2DiagnosticMibNotifications 6 }   

-- *************************************************************
-- hm2DiagEgressIfaceUtilization notifications
-- *************************************************************
hm2DiagEgressIfaceUtilizationTrap NOTIFICATION-TYPE
   OBJECTS { 
      hm2DiagEgressIfaceUtilization,
      hm2DiagEgressIfaceUtilizationAlarmCondition
      }
   STATUS  current
   DESCRIPTION "This trap is sent if the value of hm2DiagEgressIfaceUtilizationAlarmCondition is true."
   ::= { hm2DiagnosticMibNotifications 7 }

--
-- ***********************************************************
-- hm2DiagnosticSNMPExtensionGroup
-- ***********************************************************
--

hm2PortMonitorSpeedDuplexErrorReturn OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "Indicates that the specified speed value is not supported by the port capabilities"
           ::= { hm2DiagnosticSNMPExtensionGroup 1 }
           
hm2PortMonitorCndOvldDetInconsistenTholdVal OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "Indicates that the configured upper and lower threshold values are inconsistent"
           ::= { hm2DiagnosticSNMPExtensionGroup 2 }
           
hm2DiagSelftestTaskInvlVal OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "Indicates that log-only and send-trap actions are unavailable for the task cause."
           ::= { hm2DiagnosticSNMPExtensionGroup 3 }
           
END

