
HM2-DEVMGMT-MIB DEFINITIONS ::= BEGIN

-- 
-- ***********************************************************
-- Hirschmann Device Management MIB
-- ***********************************************************
--


IMPORTS
    MODULE-IDENTITY, 
    OBJECT-TYPE, 
    Integer32,
    Unsigned32,
    NOTIFICATION-TYPE		    FROM SNMPv2-SMI
    TEXTUAL-CONVENTION, 
    DisplayString,
    TruthValue			        FROM SNMPv2-TC
    SnmpAdminString             FROM SNMP-FRAMEWORK-MIB
    ifIndex, 
    InterfaceIndexOrZero        FROM IF-MIB
    HmEnabledStatus,
    HmTimeSeconds1970,
    hm2ConfigurationMibs        FROM HM2-TC-MIB
	IANAifType                  FROM IANAifType-MIB;
      		 


hm2DeviceMgmtMib MODULE-IDENTITY
    LAST-UPDATED "201210100000Z" -- October 10, 2012
    ORGANIZATION "Hirschmann Automation and Control GmbH"
    CONTACT-INFO
        "Postal:     Stuttgarter Str. 45-51
                     72654 Neckartenzlingen
                     Germany
         Phone:      +49 7127 140
         E-mail:     hac.support@belden.com"
    DESCRIPTION
        "Hirschmann Device Management MIB.
         Copyright (C) 2012. All Rights Reserved."
    REVISION     "201210100000Z" -- October 10, 2012
    DESCRIPTION
        "hm2SfpThresholdTable table added to store
        SFP thresholds."
    REVISION     "201103160000Z" -- March 16, 2011
    DESCRIPTION
         "Initial version."
    ::= { hm2ConfigurationMibs 10 }


Hm2DeviceExtNVMType ::= TEXTUAL-CONVENTION
		STATUS       current
		DESCRIPTION
		"Type of an external non volatile memory device."
		REFERENCE
		"RFC3164 - 4.1.1: Table 2"
		SYNTAX  INTEGER {
        	 	 	 	 	none(0),
        	 	 	 	 	sd(1),
        	 	 	 	 	usb(2),
        	 	 	 	 	serial(3)
         	 	 	 	 }     

-- 
-- ***********************************************************
-- hm2DeviceMgmtMib
-- ***********************************************************
--

hm2DeviceMgmtMibNotifications			OBJECT IDENTIFIER ::= { hm2DeviceMgmtMib 0 }
hm2DeviceMgmtMibObjects					OBJECT IDENTIFIER ::= { hm2DeviceMgmtMib 1 }
-- hm2DeviceMgmtMibConformance				OBJECT IDENTIFIER ::= { hm2DeviceMgmtMib 2 }

hm2DeviceMgmtGroup						OBJECT IDENTIFIER ::= { hm2DeviceMgmtMibObjects 1 }

hm2DeviceMgmtActionGroup				OBJECT IDENTIFIER ::= { hm2DeviceMgmtMibObjects 2 }

hm2DeviceMgmtSoftwareGroup				OBJECT IDENTIFIER ::= { hm2DeviceMgmtMibObjects 3 }

hm2DeviceMgmtHardwareGroup				OBJECT IDENTIFIER ::= { hm2DeviceMgmtMibObjects 4 }

hm2DeviceMgmtTemperatureGroup			OBJECT IDENTIFIER ::= { hm2DeviceMgmtMibObjects 5 }

hm2IfaceGroup							OBJECT IDENTIFIER ::= { hm2DeviceMgmtMibObjects 6 }

hm2SfpGroup								OBJECT IDENTIFIER ::= { hm2DeviceMgmtMibObjects 7 }

hm2ExtNvmGroup							OBJECT IDENTIFIER ::= { hm2DeviceMgmtMibObjects 8 }

hm2AutoDisableGroup 					OBJECT IDENTIFIER ::= { hm2DeviceMgmtMibObjects 9 }

hm2UnitGroup							OBJECT IDENTIFIER ::= { hm2DeviceMgmtMibObjects 10 }

hm2ModuleGroup							OBJECT IDENTIFIER ::= { hm2DeviceMgmtMibObjects 11 }

hm2DeviceMgmtHumidityGroup			    OBJECT IDENTIFIER ::= { hm2DeviceMgmtMibObjects 12 }

-- 
-- ***********************************************************
-- hm2DeviceMgmtGroup
-- ***********************************************************
--
hm2DevMgmtProductId OBJECT-TYPE
		 SYNTAX   		OBJECT IDENTIFIER
		 MAX-ACCESS   	read-only							  
		 STATUS 	  	current
		 DESCRIPTION
				"Manufacturer-defined product identifier (product family + product ID).
				 Example:Objekt-ID 1.3.6.1.4.1.248.11.2.1.1 is the hm2ProductFamily EES and
				 Objekt-ID 1.3.6.1.4.1.248.11.2.1.1.2 is the Product ID for ees25-0600"
		 ::= { hm2DeviceMgmtGroup 1 }		

hm2DevMgmtProductDescr OBJECT-TYPE
		 SYNTAX   		DisplayString 
		 MAX-ACCESS   	read-only							  
		 STATUS 	  	current
		 DESCRIPTION
				"Manufacturer-defined product description."
		 ::= { hm2DeviceMgmtGroup 2 }
		 
hm2DevMgmtSerialNumber OBJECT-TYPE
		 SYNTAX   		DisplayString 
		 MAX-ACCESS   	read-only							  
		 STATUS 	  	current
		 DESCRIPTION
				"Manufacturer-defined serial number of the device."
		 ::= { hm2DeviceMgmtGroup 3 }

 

-- 
-- ***********************************************************
-- hm2DeviceMgmtActionGroup
-- ***********************************************************
--

hm2DevMgmtActionReset OBJECT-TYPE
	SYNTAX 		INTEGER
				{
				 other(1),
				 reset(2)
				} 
	MAX-ACCESS 	read-write							  
	STATUS 	  	current
	DESCRIPTION
		"Setting the object to 'reset' has the same effect as a power-on sequence (cold start)
		 Reading the object always returns 'other'."			
	::= { hm2DeviceMgmtActionGroup 1 }

hm2DevMgmtActionFlushFDB OBJECT-TYPE
	SYNTAX   	INTEGER
				{
				 other(1),
				 flushFDB(2)
				} 
	MAX-ACCESS  read-write							  
	STATUS 	  	current
	DESCRIPTION
		"Setting the object to 'flushFDB' will flush the forwarding database of the switch.
		 Reading the object always returns 'other'."			
	::= { hm2DeviceMgmtActionGroup 2 }

hm2DevMgmtActionFlushARP OBJECT-TYPE
	SYNTAX   	INTEGER
				{
				 other(1),
				 flushARP(2)
				} 
	MAX-ACCESS  read-write							  
	STATUS 	  	current
	DESCRIPTION
		"Setting the object to 'flushARP' will flush the ARP cache.
		 Reading the object always returns 'other'."			
	::= { hm2DeviceMgmtActionGroup 3 }

hm2DevMgmtActionFlushIGS OBJECT-TYPE
	SYNTAX   	INTEGER
				{
				 other(1),
				 flushIGS(2)
				} 
	MAX-ACCESS  read-write							  
	STATUS 	  	current
	DESCRIPTION
		"Setting the object to 'flushIGS' will flush all dynamically
		 learnt IGMP snooping entries.
		 Reading the object always returns 'other'."			
	::= { hm2DeviceMgmtActionGroup 4 }	

hm2DevMgmtActionFlushPortStats OBJECT-TYPE
	SYNTAX   	INTEGER
				{
				 other(1),
				 flushPortStats(2)
				} 
	MAX-ACCESS  read-write							  
	STATUS 	  	current
	DESCRIPTION
		"Setting the object to 'flushPortStats' will flush all port statistics.
		 Reading the object always returns 'other'."			
	::= { hm2DeviceMgmtActionGroup 5 }	

hm2DevMgmtActionFlushEmailLogStats OBJECT-TYPE
	SYNTAX   	INTEGER
				{
				 other(1),
				 flushEmailLogCounters(2)
				} 
	MAX-ACCESS  read-write							  
	STATUS 	  	current
	DESCRIPTION
		"Setting the object to 'flushEmailLogCounters' will flush all email logging statistics.
		 Reading the object always returns 'other'."			
	::= { hm2DeviceMgmtActionGroup 6 }	

hm2DevMgmtActionFlushMMRP OBJECT-TYPE
	SYNTAX   	INTEGER
				{
				 other(1),
				 flushMMRP(2)
				} 
	MAX-ACCESS  read-write							  
	STATUS 	  	current
	DESCRIPTION
		"Setting the object to 'flushMMRP' will flush all MMRP counters.
		 Reading the object always returns 'other'."			
	::= { hm2DeviceMgmtActionGroup 7 }

hm2DevMgmtActionFlushMVRP OBJECT-TYPE
	SYNTAX   	INTEGER
				{
				 other(1),
				 flushMVRP(2)
				} 
	MAX-ACCESS  read-write							  
	STATUS 	  	current
	DESCRIPTION
		"Setting the object to 'flushMVRP' will flush all MVRP counters.
		 Reading the object always returns 'other'."			
	::= { hm2DeviceMgmtActionGroup 8 }

hm2DevMgmtActionFlushMSRP OBJECT-TYPE
	SYNTAX   	INTEGER
				{
				 other(1),
				 flushMSRP(2)
				} 
	MAX-ACCESS  read-write							  
	STATUS 	  	current
	DESCRIPTION
		"Setting the object to 'flushMSRP' will flush all MSRP counters.
		 Reading the object always returns 'other'."			
	::= { hm2DeviceMgmtActionGroup 9 }
	
hm2DevMgmtActionFlushIeee8021AS OBJECT-TYPE
	SYNTAX   	INTEGER
				{
				 other(1),
				 flushIeee8021AS(2)
				} 
	MAX-ACCESS  read-write							  
	STATUS 	  	current
	DESCRIPTION
		"Setting the object to 'flushIeee8021AS' will flush all IEEE8021AS related counters.
		 Reading the object always returns 'other'."			
	::= { hm2DeviceMgmtActionGroup 10 }

hm2DevMgmtActionFlushDnsClientCache OBJECT-TYPE
	SYNTAX   	INTEGER
				{
				 other(1),
				 flushDnsClientCache(2)
				} 
	MAX-ACCESS  read-write							  
	STATUS 	  	current
	DESCRIPTION
		"Setting the object to 'flushDnsClientCache' will flush all DNS client cache records.
		 Reading the object always returns 'other'."			
	::= { hm2DeviceMgmtActionGroup 11 }
	
hm2DevMgmtActionFlushDnsCachingServerCache OBJECT-TYPE
	SYNTAX   	INTEGER
				{
				 other(1),
				 flushDnsCachingServerCache(2)
				} 
	MAX-ACCESS  read-write							  
	STATUS 	  	current
	DESCRIPTION
		"Setting the object to 'flushDnsCachingServerCache' will flush all DNS caching server cache records.
		 Reading the object always returns 'other'."			
	::= { hm2DeviceMgmtActionGroup 12 }
	
hm2DevMgmtActionFlushIpUdpHelperStats OBJECT-TYPE
	SYNTAX   	INTEGER
				{
				 other(1),
				 flushIpUdpHelperStats(2)
				} 
	MAX-ACCESS  read-write							  
	STATUS 	  	current
	DESCRIPTION
		"Setting the object to 'flushIpUdpHelperStats' will flush all ip udp helper statistics.
		 Reading the object always returns 'other'."			
	::= { hm2DeviceMgmtActionGroup 13 }	

hm2DevMgmtActionFlushAclStats OBJECT-TYPE
	SYNTAX   	INTEGER
				{
				 other(1),
				 flushAclStats(2),
				 flushAclMacStats(3)
				} 
	MAX-ACCESS  read-write							  
	STATUS 	  	current
	DESCRIPTION
		"Setting the object to 'flushAclStats' will flush all acl statistics from the AgentAclRuleTable.
		 Setting the object to 'flushAclMacStats' will flush all acl statistics from the AgentAclMacRuleTable.
		 Reading the object always returns 'other'."			
	::= { hm2DeviceMgmtActionGroup 14 }

hm2DevMgmtActionFlushLdapUserCache OBJECT-TYPE
	SYNTAX   	INTEGER
				{
				 other(1),
				 flushLdapUserCache(2)
				} 
	MAX-ACCESS  read-write							  
	STATUS 	  	current
	DESCRIPTION
		"Setting the object to 'flushLdapUserCache' will flush all cached users from LDAP queries to an 
		 Active Directory Server.
		 Reading the object always returns 'other'."			
	::= { hm2DeviceMgmtActionGroup 15 }	

hm2DevMgmtActionFlushMgmtAccessStatistics OBJECT-TYPE
	SYNTAX 		INTEGER
				{
		 		other(1),
		 		flushMgmtAccessStatistics(2)
				}
	MAX-ACCESS 	read-write
	STATUS 	  	current
	DESCRIPTION
		"Setting the object to 'flushMgmtAccessStatistics' will flush all management access statistics.
		Reading the object always returns 'other'."
	::= { hm2DeviceMgmtActionGroup 16 }
	
hm2DevMgmtActionFlushDiffServ OBJECT-TYPE
    SYNTAX      INTEGER
                {
                other(1),
                flushDiffServ(2)
                }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Setting the object to 'flushDiffServ' will flush all diffserv tables.
        Reading the object always returns 'other'."
    ::= { hm2DeviceMgmtActionGroup 17 }

hm2DevMgmtActionDelayPreset OBJECT-TYPE
	SYNTAX 		 Integer32 (0..2147483)
	MAX-ACCESS	 read-write
	STATUS 		 current	
	DESCRIPTION
		"Time in seconds until a reset that was triggered         
		 over the hm2DevMgmtActionReset object is executed. 
		 Writing a zero will cancel any scheduled reset."
	DEFVAL		 { 0 }
	::= { hm2DeviceMgmtActionGroup 100 }

hm2DevMgmtActionDelayCurrent OBJECT-TYPE
	SYNTAX 		 Integer32 (0..2147483)
	MAX-ACCESS	 read-only
	STATUS 		 current
	DESCRIPTION
		 "If a delayed reset is scheduled this object 
		  will decrement from the start value to zero."
	::= { hm2DeviceMgmtActionGroup 101 }


hm2DevMgmtActionLanBypass OBJECT-TYPE
	SYNTAX 		 HmEnabledStatus
	MAX-ACCESS	 read-write
	STATUS 		 current
	DESCRIPTION
		 "Enable/Disable run-time LAN Bypass mode upon 
		  software request. LAN bypass feature ensures that traffic 
		  pass freely between interface pairs in the event 
		  of device failure caused due to power outage, 
		  application failure or upon software request"
	DEFVAL		 { disable }
	::= { hm2DeviceMgmtActionGroup 102 }
-- 
-- ***********************************************************
-- hm2DeviceMgmtSoftwareVersionGroup
-- ***********************************************************
--
hm2DeviceMgmtSoftwareVersionGroup OBJECT IDENTIFIER ::= { hm2DeviceMgmtSoftwareGroup 1 }

		 
hm2DevMgmtSwVersBootcode	OBJECT-TYPE
			 SYNTAX 	DisplayString 			 
			 MAX-ACCESS	read-only
			 STATUS 	current
			 DESCRIPTION
				 "Software version of the boot code."
			 ::= { hm2DeviceMgmtSoftwareVersionGroup 1 }

hm2DevMgmtSwVersAllowUnsigned	OBJECT-TYPE
		SYNTAX		HmEnabledStatus
		MAX-ACCESS	read-write
		STATUS		current
		DESCRIPTION
			"Status Enable allows the update with an unsigned firmware
			 Status Disable blocks the update with an unsigned firmware."
		DEFVAL	{enable}
			::= { hm2DeviceMgmtSoftwareVersionGroup 2 }

hm2DevMgmtSwVersCertTable OBJECT-TYPE
		SYNTAX SEQUENCE OF Hm2DevMgmtSwVersCertEntry
		MAX-ACCESS	not-accessible
		STATUS		current
		DESCRIPTION
			"This table contains all information related
			to the stored certificates."
			::= { hm2DeviceMgmtSoftwareVersionGroup 7 }

hm2DevMgmtSwVersCertEntry	OBJECT-TYPE
		SYNTAX 		Hm2DevMgmtSwVersCertEntry
		MAX-ACCESS 	not-accessible
		STATUS 		current
		DESCRIPTION
			"Certificate table entry."
		INDEX { hm2DevMgmtSwVersCertIndex }
		::= { hm2DevMgmtSwVersCertTable 1 }

Hm2DevMgmtSwVersCertEntry 	::= SEQUENCE {
		hm2DevMgmtSwVersCertIndex		Integer32,
		hm2DevMgmtSwVersCertSerialNo	OCTET STRING,
		hm2DevMgmtSwVersCertSubject		DisplayString,
		hm2DevMgmtSwVersCertSigAlg		DisplayString,
		hm2DevMgmtSwVersCertType		INTEGER,
		hm2DevMgmtSwVersCertStatus		INTEGER,
		hm2DevMgmtSwVersCertFingerprint	OCTET STRING
			}

hm2DevMgmtSwVersCertIndex	OBJECT-TYPE
		SYNTAX		Integer32
		MAX-ACCESS	not-accessible
		STATUS		current
		DESCRIPTION
			"Certificate index."
		::= { hm2DevMgmtSwVersCertEntry 1 }

hm2DevMgmtSwVersCertSerialNo	OBJECT-TYPE
		SYNTAX		OCTET STRING
		MAX-ACCESS	read-only
		STATUS		current
		DESCRIPTION
			"Certificate serial number."
		::= { hm2DevMgmtSwVersCertEntry 2 }

hm2DevMgmtSwVersCertSubject	OBJECT-TYPE
		SYNTAX		DisplayString
		MAX-ACCESS	read-only
		STATUS		current
		DESCRIPTION
			"Certificate subject name."
		::= { hm2DevMgmtSwVersCertEntry 3 }

hm2DevMgmtSwVersCertSigAlg	OBJECT-TYPE
		SYNTAX		DisplayString
		MAX-ACCESS	read-only
		STATUS		current
		DESCRIPTION
			"Certificate signature algorithm."
		::= { hm2DevMgmtSwVersCertEntry 4 }

hm2DevMgmtSwVersCertType OBJECT-TYPE
		SYNTAX		INTEGER {
					production(1),
					development(2)
					}
		MAX-ACCESS	read-only
		STATUS		current
		DESCRIPTION
			"Certificate type used for image verification."
		::= { hm2DevMgmtSwVersCertEntry 5 }

hm2DevMgmtSwVersCertStatus	OBJECT-TYPE
		SYNTAX		INTEGER {
					revoked(1),
					valid(2)
					}
		MAX-ACCESS	read-only
		STATUS		current
		DESCRIPTION
			"Contains the revocation status of the Certificate."
		::= { hm2DevMgmtSwVersCertEntry 6 }

hm2DevMgmtSwVersCertFingerprint	OBJECT-TYPE
		SYNTAX		OCTET STRING
		MAX-ACCESS	read-only
		STATUS		current
		DESCRIPTION
			"SHA-256 certificate fingerprint."
		::= { hm2DevMgmtSwVersCertEntry 7 }

hm2DevMgmtSwVersTable	OBJECT-TYPE
			 SYNTAX 		 SEQUENCE OF Hm2DevMgmtSwVersEntry
			 MAX-ACCESS 	 not-accessible
			 STATUS 		 current
			 DESCRIPTION
				 "This table contains all information related to running 
				 and stored software versions on the device.
				 The limit are 24 firmware (*.bin) files in up to 5 directory levels."
			 ::= { hm2DeviceMgmtSoftwareVersionGroup 10 }

hm2DevMgmtSwVersEntry	OBJECT-TYPE
			 SYNTAX 		 Hm2DevMgmtSwVersEntry
			 MAX-ACCESS 	 not-accessible
			 STATUS 		 current
			 DESCRIPTION     "The entry of the hm2DevMgmtSwVersTable."
			 INDEX			 { hm2DevMgmtSwFileLocation, hm2DevMgmtSwFileType, hm2DevMgmtSwFileIdx}
			 ::= { hm2DevMgmtSwVersTable 1}

Hm2DevMgmtSwVersEntry ::= SEQUENCE {
			 hm2DevMgmtSwFileLocation	INTEGER,
			 hm2DevMgmtSwFileType		INTEGER,
			 hm2DevMgmtSwFileIdx		Integer32,
			 hm2DevMgmtSwFileName 		DisplayString,
			 hm2DevMgmtSwVersion		DisplayString,
			 hm2DevMgmtSwMajorRelNum   	Integer32,
			 hm2DevMgmtSwMinorRelNum   	Integer32,
			 hm2DevMgmtSwBugfixRelNum  	Integer32
			 }

hm2DevMgmtSwFileLocation	 OBJECT-TYPE
			 SYNTAX 		 INTEGER {
							 ram (1),
							 flash (2),
							 sd-card (3),
							 usb (4)
							 }
			 MAX-ACCESS 	 not-accessible
			 STATUS 		 current
			 DESCRIPTION
				 "Indicates the file location (ram, flash, sd-card or usb)."
			 ::= { hm2DevMgmtSwVersEntry 1 }

hm2DevMgmtSwFileType	 	 OBJECT-TYPE
			 SYNTAX 		 INTEGER {
							 firmware (1),
							 applet (2),
							 logic (3)
							 }
			 MAX-ACCESS 	 not-accessible
			 STATUS 		 current
			 DESCRIPTION
				 "Indicates the file type (firmware, applet, logic)."
			 ::= { hm2DevMgmtSwVersEntry 2 }

hm2DevMgmtSwFileIdx	 	 	 OBJECT-TYPE
			 SYNTAX			 Integer32 (1..25)
			 MAX-ACCESS 	 not-accessible
			 STATUS 		 current
			 DESCRIPTION
				 "Indicates the index.
				  For flash the index has the following meaning:
				  - flash.xxx.1 = bootable version in flash (ROM)
				  - flash.xxx.2 = backup version in flash (BAK)"
			 ::= { hm2DevMgmtSwVersEntry 3 }
			 			 
hm2DevMgmtSwFileName	 	 OBJECT-TYPE
			 SYNTAX 		 DisplayString
			 MAX-ACCESS		 read-only
			 STATUS 		 current
			 DESCRIPTION
				 "Indicates the file name."
			 ::= { hm2DevMgmtSwVersEntry 4 }

hm2DevMgmtSwVersion		OBJECT-TYPE
			 SYNTAX 		DisplayString
			 MAX-ACCESS		read-only
			 STATUS 		current
			 DESCRIPTION
				 "Version of the stored software."
			 ::= { hm2DevMgmtSwVersEntry 5 }

hm2DevMgmtSwMajorRelNum    		OBJECT-TYPE
               SYNTAX      		Integer32
               MAX-ACCESS  		read-only
               STATUS      		current
               DESCRIPTION
                    "Shows the major release number of the firmware."
               ::= { hm2DevMgmtSwVersEntry 6 }

hm2DevMgmtSwMinorRelNum       	OBJECT-TYPE
               SYNTAX         	Integer32
               MAX-ACCESS     	read-only
               STATUS           current
               DESCRIPTION
                    "Shows the minor release number of the firmware."
               ::= { hm2DevMgmtSwVersEntry 7 }

hm2DevMgmtSwBugfixRelNum      	OBJECT-TYPE
               SYNTAX          	Integer32
               MAX-ACCESS      	read-only
               STATUS          	current
               DESCRIPTION
                    "Shows the bug fix release number of the firmware."
               ::= { hm2DevMgmtSwVersEntry 8 }




-- 
-- ***********************************************************
-- hm2DeviceMgmtHardwareVersionGroup
-- ***********************************************************
--

hm2DevMgmtHwVersion	OBJECT-TYPE
			 SYNTAX 	DisplayString 			 
			 MAX-ACCESS	read-only
			 STATUS 	current
			 DESCRIPTION
				 "Version of the device hardware."
			 ::= { hm2DeviceMgmtHardwareGroup 1 }
			 
hm2DevMgmtSwitchingCoreVersion	OBJECT-TYPE
			 SYNTAX 	DisplayString 			 
			 MAX-ACCESS	read-only
			 STATUS 	current
			 DESCRIPTION
				 "Version of the device hardware."
			 ::= { hm2DeviceMgmtHardwareGroup 2 }
			 			 
-- 
-- ***********************************************************
-- hm2DeviceMgmtLogicVersionGroup
-- ***********************************************************
--

hm2DeviceMgmtLogicVersionGroup OBJECT IDENTIFIER ::= { hm2DeviceMgmtHardwareGroup 5 }

hm2DevMgmtLogicVersTable	OBJECT-TYPE
			 SYNTAX 		 SEQUENCE OF Hm2DevMgmtLogicVersEntry
			 MAX-ACCESS		 not-accessible
			 STATUS 		 current
			 DESCRIPTION "The table displays all versions of
				supported logic modules."
			 ::= { hm2DeviceMgmtLogicVersionGroup 1 }

hm2DevMgmtLogicVersEntry	OBJECT-TYPE
			 SYNTAX 		 Hm2DevMgmtLogicVersEntry
			 MAX-ACCESS 	 not-accessible
			 STATUS 		 current
			 DESCRIPTION     "The entry of the 
			 	hm2DevMgmtLogicVersTable."
			 INDEX			 { hm2DevMgmtLogicIdx }
			 ::= { hm2DevMgmtLogicVersTable 1}

Hm2DevMgmtLogicVersEntry ::= SEQUENCE {

			 hm2DevMgmtLogicIdx					Integer32,
			 hm2DevMgmtLogicAddress 			DisplayString,
			 hm2DevMgmtLogicVersion				DisplayString 
			 }

hm2DevMgmtLogicIdx 		     OBJECT-TYPE
			 SYNTAX			 Integer32 (1..32)
			 MAX-ACCESS      not-accessible
			 STATUS 		 current
			 DESCRIPTION
					"Index of the module to display."
			 ::= { hm2DevMgmtLogicVersEntry 1 }

hm2DevMgmtLogicAddress	    OBJECT-TYPE
			 SYNTAX 		DisplayString 			 
			 MAX-ACCESS		read-only
			 STATUS 		current
			 DESCRIPTION
				 "Address of the logic module in fpga."
			::= { hm2DevMgmtLogicVersEntry 2 }
			 
hm2DevMgmtLogicVersion	OBJECT-TYPE
			 SYNTAX 		DisplayString 			 
			 MAX-ACCESS		read-only
			 STATUS 		current
			 DESCRIPTION
				 "Version of the logic module in fpga."
			::= { hm2DevMgmtLogicVersEntry 3 }


-- 
-- ***********************************************************
-- hm2DeviceMgmtTemperatureGroup
-- ***********************************************************
--
hm2DevMgmtTemperature	OBJECT-TYPE
			 SYNTAX			Integer32
			 MAX-ACCESS		read-only
			 STATUS			current
			 DESCRIPTION
			    "This object is used to identify the temperature
				within a device in units of centigrade (Celsius)."
			 ::= { hm2DeviceMgmtTemperatureGroup 1 }

hm2DevMgmtTemperatureUpperLimit	 OBJECT-TYPE
			 SYNTAX			Integer32 (-99..99)
			 MAX-ACCESS		read-write
			 STATUS			current
			 DESCRIPTION
				"This object is used to define a maximum level for the
				temperature within a device. If the temperature rises above
				this upper limit, the management station will be notified by
				a hm2DevMonStateChangeTrap trap."
			 DEFVAL  {70 }				
			 ::= { hm2DeviceMgmtTemperatureGroup 2 }
 
hm2DevMgmtTemperatureLowerLimit	 OBJECT-TYPE
			 SYNTAX			Integer32 (-99..99)
			 MAX-ACCESS		read-write
			 STATUS			current
			 DESCRIPTION
				"This object is used to define a minimum level for the
				temperature within a device. If the temperature falls
				below this lower limit, the management station will be notified
				by a hm2DevMonStateChangeTrap trap."
			 DEFVAL  { 0 }				
			 ::= { hm2DeviceMgmtTemperatureGroup 3 }

--

--  hm2DevMgmtTemperatureExtTable

-- 

hm2DevMgmtTemperatureExtTable  OBJECT-TYPE
			SYNTAX         SEQUENCE OF Hm2DevMgmtTemperatureExtEntry
            MAX-ACCESS     not-accessible
            STATUS         current
            DESCRIPTION
                "This table is used to identify the temperature settings within a device."
            ::= { hm2DeviceMgmtTemperatureGroup 10 }

hm2DevMgmtTemperatureExtEntry  OBJECT-TYPE
			SYNTAX         Hm2DevMgmtTemperatureExtEntry
            MAX-ACCESS     not-accessible
            STATUS         current
            DESCRIPTION    
                "The entries of the temperature table per unit."
            INDEX  { hm2UnitIndex, hm2DevMgmtTemperatureExtType, hm2DevMgmtTemperatureExtSensorId}
            ::= { hm2DevMgmtTemperatureExtTable 1 }
 
Hm2DevMgmtTemperatureExtEntry ::= SEQUENCE {
            hm2DevMgmtTemperatureExtType                INTEGER,
			hm2DevMgmtTemperatureExtSensorId            Integer32,
            hm2DevMgmtTemperatureExt                    Integer32,
            hm2DevMgmtTemperatureExtUpperLimit          Integer32,
            hm2DevMgmtTemperatureExtLowerLimit          Integer32
            }

hm2DevMgmtTemperatureExtType  OBJECT-TYPE
           SYNTAX         INTEGER { mainboard(1), module(2), switch(3), cpu(4), phy(5), other(10) }
           MAX-ACCESS     not-accessible
           STATUS         current
           DESCRIPTION
               "This object is used to identify the type of the temperature sensor."
           ::= { hm2DevMgmtTemperatureExtEntry 1 }
		   
hm2DevMgmtTemperatureExtSensorId  OBJECT-TYPE
          SYNTAX         Integer32 (1..8)
          MAX-ACCESS     read-only
          STATUS         current
          DESCRIPTION
              "This object is used to identify the sensor Id."
		  ::= { hm2DevMgmtTemperatureExtEntry 2 }

 
hm2DevMgmtTemperatureExt  OBJECT-TYPE
          SYNTAX         Integer32
          MAX-ACCESS     read-only
          STATUS         current
          DESCRIPTION
              "This object is used to identify the temperature within a device in units of centigrade (Celsius)."
		  ::= { hm2DevMgmtTemperatureExtEntry 3 }

hm2DevMgmtTemperatureExtUpperLimit  OBJECT-TYPE
          SYNTAX         Integer32 (-99..99)
          MAX-ACCESS     read-write
          STATUS         current
          DESCRIPTION
              "This object is used to define a maximum level for the
               temperature within a device. If the temperature rises above
               this upper limit, the management station will be notified by
               a hm2DevMgmtTemperature trap."
          DEFVAL  {70 }                                                   
          ::= { hm2DevMgmtTemperatureExtEntry 4 }

hm2DevMgmtTemperatureExtLowerLimit  OBJECT-TYPE
          SYNTAX         Integer32 (-99..99)
          MAX-ACCESS     read-write
          STATUS         current
          DESCRIPTION
              "This object is used to define a minimum level for the
              temperature within a device. If the temperature falls
              below this lower limit, the management station will be notified
              by a hm2DevMgmtTemperature trap."
          DEFVAL  { 0 }                                                     
          ::= { hm2DevMgmtTemperatureExtEntry 5 }

-- ***********************************************************
-- hm2DeviceMgmtHumidityGroup
-- ***********************************************************
--
hm2DevMgmtHumidity	OBJECT-TYPE
			 SYNTAX			Unsigned32 (0..100)
			 UNITS 			"percent"
			 MAX-ACCESS		read-only
			 STATUS			current
			 DESCRIPTION
			    "This object is used to identify the humidity
				within a device."
			 ::= { hm2DeviceMgmtHumidityGroup 1 }

hm2DevMgmtHumidityUpperLimit	 OBJECT-TYPE
			 SYNTAX			Unsigned32 (0..100)
			 UNITS 			"percent"
			 MAX-ACCESS		read-write
			 STATUS			current
			 DESCRIPTION
				"This object is used to define a maximum level for the
				humidity within a device. If the humidity rises above
				this upper limit, the management station will be
				notified by a hm2DevMonStateChangeTrap trap."
			 DEFVAL  { 95 }
			 ::= { hm2DeviceMgmtHumidityGroup 2 }
 
hm2DevMgmtHumidityLowerLimit	 OBJECT-TYPE
			 SYNTAX			Unsigned32 (0..100)
			 UNITS 			"percent"
			 MAX-ACCESS		read-write
			 STATUS			current
			 DESCRIPTION
				"This object is used to define a minimum level for the
				humidity within a device. If the humidity falls
				below this lower limit, the management station
				will be notified by a hm2DevMonStateChangeTrap trap."
			 DEFVAL  { 5 }
			 ::= { hm2DeviceMgmtHumidityGroup 3 }

-- 
-- ***********************************************************
-- hm2IfaceGroup
-- ***********************************************************
--
hm2IfaceTable   OBJECT-TYPE
			 SYNTAX 	 	SEQUENCE OF Hm2IfaceEntry
			 MAX-ACCESS 	not-accessible
			 STATUS 		current
			 DESCRIPTION
				 "This table contains extended PHY capabilities and
				  configuration options."
			 ::= { hm2IfaceGroup 1 }

hm2IfaceEntry	 OBJECT-TYPE
			 SYNTAX 		 Hm2IfaceEntry
			 MAX-ACCESS 	 not-accessible
			 STATUS 		 current
			 DESCRIPTION     
			 	"Entry with the configuration options and supported
			 	 features of a port."
			 INDEX	 { hm2IfacePhysIndex }
			 ::= { hm2IfaceTable 1 }

Hm2IfaceEntry ::= SEQUENCE {
			 hm2IfacePhysIndex			Integer32,
			 hm2IfacePortCapabilityBits	BITS,
			 hm2IfaceCableCrossing  	INTEGER,
			 hm2IfacePowerState			HmEnabledStatus,
			 hm2IfaceAutoPowerDown  	INTEGER,
			 hm2IfaceOperAdminStatus	INTEGER
			 }

hm2IfacePhysIndex OBJECT-TYPE
			 SYNTAX 		 Integer32 
			 MAX-ACCESS 	 accessible-for-notify
			 STATUS 		 current
			 DESCRIPTION
				 "The index of the available physical interfaces." 
			 ::= { hm2IfaceEntry 1 }

			
hm2IfacePortCapabilityBits	OBJECT-TYPE
			SYNTAX 		 BITS 	{
							manual-mdix	(0),
							auto-mdix 	(1),
							auto-power-down (2),
							energy-efficient-ethernet (3),
							cable-test (4),
							poe (5),
							poe-plus (6),
							poe-ext (7)
						}
			MAX-ACCESS      read-only
			STATUS          current			 
			DESCRIPTION
			"manual-mdix - port supports MDIX and MDI
			auto-mdix    - port supports MDIX and Auto-MDIX
			auto-power-down - port can enter low power mode if no link is established
			energy-efficient-ethernet - port supports EEE
			cable-test - port supports cable testing
			poe - port supports PoE
			poe-plus - port supports PoE+
			poe-ext - port supports PoE Extender"
			::= { hm2IfaceEntry 2 }
			
hm2IfaceCableCrossing	OBJECT-TYPE
		 SYNTAX INTEGER
						{
						 mdi(1),
						 mdix(2),
						 auto-mdix(3),
						 unsupported(4)
						}
			MAX-ACCESS      read-write
			STATUS          current			 
			DESCRIPTION
			"This variable configures the cable crossing on twisted pair cables.
			When set to 'mdi', the device does not swap the send and receive line pairs of the TP cable for this port.
			When set to 'mdix', the device swaps the send and receive line pairs of the TP cable for this port.
			When set to 'auto-mdix', the port uses the auto crossover mode.
			'Unsupported' is shown, if a port does not support cable crossing or auto-negotiation is disabled.
			It is not possible to set 'unsupported' to any type of port."
			DEFVAL { mdix }
			::= { hm2IfaceEntry 3 } 
					
hm2IfacePowerState	OBJECT-TYPE
			SYNTAX HmEnabledStatus
			MAX-ACCESS      read-write
			STATUS          current			 
			DESCRIPTION
			"This variable configures the power on the interface.
			When set to 'enable' that means the interface-power is on (power up)
			When set to 'disable' that means the interface-power is off (power down)
			The interface power state settings have no effect if the interface admin state
			(ifAdminStatus) is enabled"
			DEFVAL { disable }
			::= { hm2IfaceEntry 4 }


			
hm2IfaceAutoPowerDown	OBJECT-TYPE
			SYNTAX INTEGER
							{
							auto-power-down (1),
							no-power-save (2),
							energy-efficient-ethernet (3),
							unsupported(4)
							}
			MAX-ACCESS      read-write
			STATUS          current			 
			DESCRIPTION
			"This variable configures the automatic power save mode on the interface.
			When set to 'auto-power-down', the port goes in a low power mode if no link is detected.
			When set to 'no-power-save', the port does not use the automatic power save mode.
			When set to 'energy-efficient-ethernet', the port uses energy-efficient-ethernet mode to save the power.
			'Unsupported' is shown, if a port does not support automatic power save mode."
			DEFVAL { no-power-save }
			::= { hm2IfaceEntry 5 }
			
			
hm2IfaceOperAdminStatus	OBJECT-TYPE
			SYNTAX INTEGER
							{
							up(1),
							down(2)
							}
			MAX-ACCESS      read-only
			STATUS          current			 
			DESCRIPTION
			"This variable shows the operational admin state of a specific interface.
			The operational state could be different to the ifAdminStatus if the interface is 
			forced to down by other means like hm2AutoDisableIntfOperState."
			
			::= { hm2IfaceEntry 6 }

-- 
-- ***********************************************************
-- hm2IfaceLayoutTable
-- ***********************************************************
--
hm2IfaceLayoutTable   OBJECT-TYPE
			 SYNTAX 	 	SEQUENCE OF Hm2IfaceLayoutEntry
			 MAX-ACCESS 	not-accessible
			 STATUS 		current
			 DESCRIPTION
				"This table does contain the layout of the interface modules or 
			 	blocks. It contains all possible physical and logical items. 
			 	This table can be used to determine any interface index according to 
			 	'IfEntry' that may exist and the name of this interface. "
			 ::= { hm2IfaceGroup 2 }


hm2IfaceLayoutEntry	 OBJECT-TYPE
			 SYNTAX 		 Hm2IfaceLayoutEntry
			 MAX-ACCESS 	 not-accessible
			 STATUS 		 current
			 DESCRIPTION     
			 	"An entry of a module or block of interfaces."
			 INDEX	 { hm2IfaceLayoutIndex }
			 ::= { hm2IfaceLayoutTable 1 }

Hm2IfaceLayoutEntry ::= SEQUENCE {
			 hm2IfaceLayoutIndex				Integer32,
			 hm2IfaceLayoutStartIfIndex			InterfaceIndexOrZero,
			 hm2IfaceLayoutEndIfIndex			InterfaceIndexOrZero,
			 hm2IfaceLayoutModuleCapacity		Unsigned32,
			 hm2IfaceLayoutModulePortCapacity   Unsigned32,
			 hm2IfaceLayoutFormat				SnmpAdminString,
			 hm2IfaceLayoutIfIndexType			IANAifType
			 }

hm2IfaceLayoutIndex OBJECT-TYPE
			 SYNTAX 		 Integer32 
			 MAX-ACCESS 	 not-accessible
			 STATUS 		 current
			 DESCRIPTION
				 "The index used for this table." 
			 ::= { hm2IfaceLayoutEntry 1 }

hm2IfaceLayoutStartIfIndex OBJECT-TYPE
			 SYNTAX 		 InterfaceIndexOrZero 
			 MAX-ACCESS 	 read-only
			 STATUS 		 current
			 DESCRIPTION
				 "It specifies the first interface index of this block or module." 
			 ::= { hm2IfaceLayoutEntry 2 }

hm2IfaceLayoutEndIfIndex OBJECT-TYPE
			 SYNTAX 		 InterfaceIndexOrZero 
			 MAX-ACCESS 	 read-only
			 STATUS 		 current
			 DESCRIPTION
				 "It specifies the last interface index of this block or module that 
				 can exist for this particular device. The amount of interfaces 
				 between first and last may not be equal than to the maximum 
				 interface per module." 
			 ::= { hm2IfaceLayoutEntry 3 }

hm2IfaceLayoutModuleCapacity OBJECT-TYPE
			 SYNTAX 		 Unsigned32 
			 MAX-ACCESS 	 read-only
			 STATUS 		 current
			 DESCRIPTION
				 "It is the Number of modules in that block. Currently not used and it is always 0." 
			 ::= { hm2IfaceLayoutEntry 4 }

hm2IfaceLayoutModulePortCapacity OBJECT-TYPE
			 SYNTAX 		 Unsigned32 
			 MAX-ACCESS 	 read-only
			 STATUS 		 current
			 DESCRIPTION
				 "Number of interfaces that one module can contain. Currently not used and it is always 0" 
			 ::= { hm2IfaceLayoutEntry 5 }

hm2IfaceLayoutFormat OBJECT-TYPE
			 SYNTAX 		 SnmpAdminString 
			 MAX-ACCESS 	 read-only
			 STATUS 		 current
			 DESCRIPTION
				 "This specifies a format string that can be used to determine the textual representation of an interface in this block.
					following wildcards are supported:
					%i the absolute interface number according to 'IfEntry'. 
					%p the relative number based on hm2IfaceLayoutStartIfIndex
					%s the block number from 'hm2IfaceLayoutIndex'
					%vid the vlan of the routing interface
					%lre the name of the redundancy port (prp or hsr)"
			 ::= { hm2IfaceLayoutEntry 6 }

hm2IfaceLayoutIfIndexType OBJECT-TYPE
			 SYNTAX 		 IANAifType
			 MAX-ACCESS 	 read-only
			 STATUS 		 current
			 DESCRIPTION
				 "Type of the interfaces in that block according to IANA-Type table." 
			 ::= { hm2IfaceLayoutEntry 7 }
			 
			 
			 -- 
-- ***********************************************************
-- hm2IfaceExtTable
-- ***********************************************************
--
hm2IfaceExtTable   OBJECT-TYPE
			 SYNTAX 	 	SEQUENCE OF Hm2IfaceExtEntry
			 MAX-ACCESS 	not-accessible
			 STATUS 		current
			 DESCRIPTION
				 "This table contains additional information about the interfaces."
			 ::= { hm2IfaceGroup 3 }

hm2IfaceExtEntry	 OBJECT-TYPE
			 SYNTAX 		 Hm2IfaceExtEntry
			 MAX-ACCESS 	 not-accessible
			 STATUS 		 current
			 DESCRIPTION     
			 	"."
			 INDEX	 { ifIndex }
			 ::= { hm2IfaceExtTable 1 }

Hm2IfaceExtEntry ::= SEQUENCE {
			 hm2IfaceExtIfRole			INTEGER
			 }

hm2IfaceExtIfRole OBJECT-TYPE
			 SYNTAX 		 INTEGER
			 		{
			 			ethernetCsmacd 		(6),
			 			softwareLoopback 	(24),
			 			l3ipvlan 			(136),
			 			ieee8023adLag 		(161),
			 			shdsl 				(169),
			 			ringPort 			(1001),
			 			subringPort 		(1002),
			 			couplingPort 		(1003),
			 			routerPort 			(1004),
			 			probePort 			(1005),
			 			cpuPort 			(1006),
			 			servicePort 		(1007),
			 			outOfBandMgmtPort	(1008),
			 			lagMember 			(1101),
			 			lreMember 			(1102),
			 			lreInterface 		(1201),
			 			ringLagInterface 	(1202)
			 		}
			 MAX-ACCESS 	 read-only
			 STATUS 		 current
			 DESCRIPTION
				 "The current role of the interface." 
			 ::= { hm2IfaceExtEntry 1 }

			 
-- 
-- ***********************************************************
-- hm2SfpGroup
-- ***********************************************************
--

hm2SfpInfoTable   OBJECT-TYPE
			 SYNTAX 	 	SEQUENCE OF Hm2SfpInfoEntry
			 MAX-ACCESS 	not-accessible
			 STATUS 		current
			 DESCRIPTION
				 "This table contains variables for each SFP."
			 ::= { hm2SfpGroup 1 }

hm2SfpInfoEntry	 OBJECT-TYPE
			 SYNTAX 		 Hm2SfpInfoEntry
			 MAX-ACCESS 	 not-accessible
			 STATUS 		 current
			 DESCRIPTION     
			 	"Entry for a detected SFP."
			 INDEX	 { ifIndex }
			 ::= { hm2SfpInfoTable 1 }

Hm2SfpInfoEntry ::= SEQUENCE {
			 hm2SfpModuleType		INTEGER,
			 hm2SfpMediaType		INTEGER,
			 hm2SfpConnector		INTEGER,
			 hm2SfpVendorName		SnmpAdminString,
			 hm2SfpVendorOUI		OCTET STRING,
			 hm2SfpPartNumber 		SnmpAdminString,
			 hm2SfpPartRev 			SnmpAdminString,
			 hm2SfpSerialNum		SnmpAdminString,
			 hm2SfpDateCode			SnmpAdminString,
			 hm2SfpInfoVersion		Integer32,
			 hm2SfpInfoPartNumber 	SnmpAdminString,
			 hm2SfpInfoPartId		SnmpAdminString,
			 hm2SfpBitRateNominal	Integer32,
			 hm2SfpBitRateMin		Integer32,
			 hm2SfpBitRateMax		Integer32,
			 hm2SfpMaxLength-fiber-9	Integer32,
			 hm2SfpMaxLength-fiber-50	Integer32,
			 hm2SfpMaxLength-fiber-e50	Integer32,
			 hm2SfpMaxLength-fiber-62-5	Integer32,
			 hm2SfpMaxLength-copper		Integer32,
			 hm2SfpWaveLength		Integer32,
 			 hm2SfpWaveLengthTolerance	Integer32,
			 hm2SfpEnhancedOptions		BITS,
			 hm2SfpSupported		TruthValue,
			 hm2SfpSupportedReason  INTEGER
			 }


hm2SfpModuleType OBJECT-TYPE
			 SYNTAX		INTEGER {
						sfp(3),
						xfp(6)
						}
			 MAX-ACCESS 		 read-only
			 STATUS 		 current
			 DESCRIPTION
				 "Type of the module. SFP or SFP+ (3), XFP (6)." 
			 ::= { hm2SfpInfoEntry 1 }

hm2SfpMediaType OBJECT-TYPE
			 SYNTAX		INTEGER {
						ge-1000-base-sx (1),
						ge-1000-base-lx (2),
						ge-1000-base-cx (4),
						fe-100base-lx (5),
						fe-100base-fx (6),
						ge-1000-base-t (8),
						unsupported (9),
						oc3-mm-sr (10),
						oc3-sm-ir (11),
						oc3-sm-lr (12),
						oc12-mm-sr (13),
						oc12-sm-ir (14),
						oc12-sm-lr (15),
						oc48-sr (16),
						oc48-ir (17),
						oc48-lr (18),
						xfp-10gbase-sr(30),
						xfp-10gbase-lr(31),
						xfp-10gbase-er(32),
						microfx(40),
						pof(41),
						m-sfp-2500(50)
						}
			 MAX-ACCESS 	 read-only
			 STATUS 		 current
			 DESCRIPTION
				 "The SFP's Media Type"
			 ::= { hm2SfpInfoEntry 2 }

hm2SfpConnector OBJECT-TYPE
			 SYNTAX 	INTEGER {
						nonSfp (1),
						fiberjack (6),
						lc (7),
						mtrj (8),
						opticalPigtail (11),
						copperPigtail (33),
						rj45 (34),
						vendorSpecific (128)
						}
			 MAX-ACCESS 		 read-only
			 STATUS 		 current
			 DESCRIPTION
				 "The SFP's Connector Type." 
			 ::= { hm2SfpInfoEntry 3 }

hm2SfpVendorName	 OBJECT-TYPE
			 SYNTAX 		 SnmpAdminString
			 MAX-ACCESS 		 read-only
			 STATUS 		 current
			 DESCRIPTION
				 "The SFP's vendor name (ASCII)."
			 ::= { hm2SfpInfoEntry 4 }

hm2SfpVendorOUI	OBJECT-TYPE
			 SYNTAX 		 OCTET STRING
			 MAX-ACCESS 		 read-only
			 STATUS 		 current
			 DESCRIPTION
				 "The vendor organizationally unique identifier field (OUI)."
			 ::= { hm2SfpInfoEntry 5 }

hm2SfpPartNumber	 OBJECT-TYPE
			 SYNTAX 		 SnmpAdminString 
			 MAX-ACCESS 		 read-only
			 STATUS 		 current
			 DESCRIPTION
				"The part number of the module (ASCII)."
			 ::= { hm2SfpInfoEntry 6 }

hm2SfpPartRev	 OBJECT-TYPE
			 SYNTAX 		 SnmpAdminString 
			 MAX-ACCESS 		 read-only
			 STATUS 		 current
			 DESCRIPTION
				"The revision number of the module (ASCII)."
			 ::= { hm2SfpInfoEntry 7 }

hm2SfpSerialNum	 OBJECT-TYPE
			 SYNTAX 		 SnmpAdminString 
			 MAX-ACCESS 		 read-only
			 STATUS 		 current
			 DESCRIPTION
				"The SFP's serial number provided by vendor (ASCII)."
			 ::= { hm2SfpInfoEntry 8 }

hm2SfpDateCode	 OBJECT-TYPE
			 SYNTAX 		 SnmpAdminString 
			 MAX-ACCESS 		 read-only
			 STATUS 		 current
			 DESCRIPTION
				"The SFP's vendor manufacturing date code. Format is YY:MM:DD."
			 ::= { hm2SfpInfoEntry 9 }

hm2SfpInfoVersion OBJECT-TYPE
			 SYNTAX 		 Integer32
			 MAX-ACCESS 		 read-only
			 STATUS 		 current
			 DESCRIPTION
				"Version of SFP's Hirschmann information. 
				Contains -1 in case of a device read error."
			 ::= { hm2SfpInfoEntry 10 }

hm2SfpInfoPartNumber	 OBJECT-TYPE
			 SYNTAX 		 SnmpAdminString (SIZE (0..11))
			 MAX-ACCESS 		 read-only
			 STATUS 		 current
			 DESCRIPTION
				"Part Number of SFP's Hirschmann information."
		 	 ::= { hm2SfpInfoEntry 11 }

hm2SfpInfoPartId		OBJECT-TYPE
			 SYNTAX 		 SnmpAdminString (SIZE (0..16))
			 MAX-ACCESS 		 read-only
			 STATUS 		 current
			 DESCRIPTION
				"Part Identifier of SFP's Hirschmann information."
			 ::= { hm2SfpInfoEntry 12 }
			 
hm2SfpBitRateNominal	 OBJECT-TYPE
			 SYNTAX 		 Integer32 
			 MAX-ACCESS 		 read-only
			 STATUS 		 current
			 DESCRIPTION
				 "The SFP's nominal bitrate in units of MBits/sec. 
				 Contains -1 in case of a device read error."
			 ::= { hm2SfpInfoEntry 13 }

hm2SfpBitRateMin	 OBJECT-TYPE
			 SYNTAX 		 Integer32 
			 MAX-ACCESS 		 read-only
			 STATUS 		 current
			 DESCRIPTION
					"The minimum bit rate is specified in
					units of 100 Megabits per second, rounded off
					to the nearest 100 Megabits per second.
					A value of 0 indicates that the minimum bit rate
					is not specified."
			 ::= { hm2SfpInfoEntry 14 }

hm2SfpBitRateMax	 OBJECT-TYPE
			 SYNTAX 		 Integer32 
			 MAX-ACCESS 		 read-only
			 STATUS 		 current
			 DESCRIPTION
					"The maximum bit rate is specified in
					units of 100 Megabits per second, rounded off
					to the nearest 100 Megabits per second.
					A value of 0 indicates that the maximum bit rate
					is not specified."
			 ::= { hm2SfpInfoEntry 15 }


hm2SfpMaxLength-fiber-9	OBJECT-TYPE
			 SYNTAX 		 Integer32
			 MAX-ACCESS 		 read-only
			 STATUS 		 current
			 DESCRIPTION
		           "Max. usable length for the cable type '9/125 micrometer fiber'
		            with this SFP in units of meters."
			 ::= { hm2SfpInfoEntry 16 }

hm2SfpMaxLength-fiber-50	OBJECT-TYPE
			 SYNTAX 		 Integer32
			 MAX-ACCESS 		 read-only
			 STATUS 		 current
			 DESCRIPTION
		           "Max. usable length for the cable type '50/125 micrometer fiber'
		            with this SFP in units of meters."
			 ::= { hm2SfpInfoEntry 17 }

hm2SfpMaxLength-fiber-e50	OBJECT-TYPE
			 SYNTAX 		 Integer32
			 MAX-ACCESS 		 read-only
			 STATUS 		 current
			 DESCRIPTION
		           "Max. usable length for the cable type 'EBW 50/125 micrometer fiber'
		            with this SFP in units of meters or -1 if not supported."
			 ::= { hm2SfpInfoEntry 18 }

hm2SfpMaxLength-fiber-62-5	OBJECT-TYPE
			 SYNTAX 		 Integer32
			 MAX-ACCESS 		 read-only
			 STATUS 		 current
			 DESCRIPTION
		           "Max. usable length for the cable type '62.5/125 micrometer fiber'
		            with this SFP in units of meters."
			 ::= { hm2SfpInfoEntry 19 }

hm2SfpMaxLength-copper	OBJECT-TYPE
			 SYNTAX 		 Integer32
			 MAX-ACCESS 		 read-only
			 STATUS 		 current
			 DESCRIPTION
		           "Max. usable length for the cable type 'copper'
		            with this SFP in units of meters."
			 ::= { hm2SfpInfoEntry 20 }

hm2SfpWaveLength	OBJECT-TYPE
			 SYNTAX 		 Integer32
			 MAX-ACCESS 		 read-only
			 STATUS 		 current
			 DESCRIPTION
		           "Nominal transmitter output wavelength at room temperature.
			   The laser wavelength in nm (units of 0.05nm)."
			 ::= { hm2SfpInfoEntry 21 }

hm2SfpWaveLengthTolerance	OBJECT-TYPE
			 SYNTAX 		 Integer32
			 MAX-ACCESS 	 read-only
			 STATUS 		 current
			 DESCRIPTION
				"The +/- range of transmitter output wavelength under normal operating conditions 
				or -1 if not supported."
			 ::= { hm2SfpInfoEntry 22 }

hm2SfpEnhancedOptions	OBJECT-TYPE
			 SYNTAX 		 BITS {
		            				none(0)
			 	 	 	 	 	  }
			 MAX-ACCESS 	 read-only
			 STATUS 		 current
			 DESCRIPTION
		           "Not supported."
			 ::= { hm2SfpInfoEntry 23 }

hm2SfpSupported OBJECT-TYPE
			 SYNTAX 	TruthValue
			 MAX-ACCESS read-only
			 STATUS 	current
			 DESCRIPTION
				 "The SFP is supported by the device (true) or not (false)." 
			 ::= { hm2SfpInfoEntry 24 }

hm2SfpSupportedReason OBJECT-TYPE
			 SYNTAX 	INTEGER{
					hirschmannID (1),
					whiteList (2),
					wrongSpeed (3),
					noneEthernet (4),
					tpSfpNotSupported (5),
					otnID (6)
					}
			 MAX-ACCESS 	read-only
			 STATUS 	current
			 DESCRIPTION
				 "The reason why this SFP is supported." 
			 ::= { hm2SfpInfoEntry 25 }

hm2SfpDiagTable   OBJECT-TYPE
			 SYNTAX 	 	SEQUENCE OF Hm2SfpDiagEntry
			 MAX-ACCESS 	not-accessible
			 STATUS 		current
			 DESCRIPTION
				 "This table contains variables for each SFP."
			 ::= { hm2SfpGroup 2 }

hm2SfpDiagEntry	 OBJECT-TYPE
			 SYNTAX 		 Hm2SfpDiagEntry
			 MAX-ACCESS 	 not-accessible
			 STATUS 		 current
			 DESCRIPTION     
			 	"Entry for a detected SFP."
			 INDEX	 { ifIndex }
			 ::= { hm2SfpDiagTable 1 }

Hm2SfpDiagEntry ::= SEQUENCE {
			 hm2SfpCurrentBitRate				Integer32,
			 hm2SfpCurrentTemperature			Integer32,
			 hm2SfpCurrentTxPower				Integer32,
			 hm2SfpCurrentRxPower				Integer32,
			 hm2SfpCurrentTxPowerdBm 			SnmpAdminString,
			 hm2SfpCurrentRxPowerdBm 			SnmpAdminString,
			 hm2SfpCurrentRxPowerState			INTEGER
			 }

hm2SfpCurrentBitRate	OBJECT-TYPE
			 SYNTAX 		 Integer32 
			 MAX-ACCESS 		 read-only
			 STATUS 		 current
			 DESCRIPTION
 	 			"The current bit rate in units of Megabits per second."
			 ::= { hm2SfpDiagEntry 1 }

hm2SfpCurrentTemperature	OBJECT-TYPE
			 SYNTAX 		 Integer32 
			 MAX-ACCESS 		 read-only
			 STATUS 		 current
			 DESCRIPTION
 	 			"This signed integer is used to identify
 				the temperature within the SFP in units of centigrade (Celsius). 
 				Contains -1000 in case of a device read error."
			 ::= { hm2SfpDiagEntry 2 }

hm2SfpCurrentTxPower	 OBJECT-TYPE
			 SYNTAX 		 Integer32 
			 MAX-ACCESS 		 read-only
			 STATUS 		 current
			 DESCRIPTION
 	 			"The SFP's internally measured Tx Power in units of 1/10 microwatt
 	 			or -1 if it is not supported."
	 		 ::= { hm2SfpDiagEntry 3}

hm2SfpCurrentRxPower	 OBJECT-TYPE
			 SYNTAX 		 Integer32 
			 MAX-ACCESS 		 read-only
			 STATUS 		 current
			 DESCRIPTION
  	 			"The SFP's internally measured Rx Power in units of 1/10 microWatts
  	 			or -10000 if not supportted."
			 ::= { hm2SfpDiagEntry 4}

hm2SfpCurrentTxPowerdBm	 OBJECT-TYPE
			 SYNTAX 		 SnmpAdminString 
			 MAX-ACCESS 		 read-only
			 STATUS 		 current
			 DESCRIPTION
 	 			"The SFP's internally measured Tx Power in units of dBm.
				(ASCII representation of a floating point number).
				- if not supported."
	 		 ::= { hm2SfpDiagEntry 5}

hm2SfpCurrentRxPowerdBm	 OBJECT-TYPE
			 SYNTAX 		 SnmpAdminString 
			 MAX-ACCESS 		 read-only
			 STATUS 		 current
			 DESCRIPTION
 	 			"The SFP's internally measured Rx Power in units of dBm.
				(ASCII representation of a floating point number).
				- if not supported."
			 ::= { hm2SfpDiagEntry 6}

hm2SfpCurrentRxPowerState  OBJECT-TYPE
           SYNTAX  INTEGER {
                   ok(1),
                   warning(2),
                   alarm(3),
                   unsupported(4)
           }
           MAX-ACCESS  read-only
           STATUS      current
           DESCRIPTION
           "The state of the SFP's internally measured Rx."
           ::= { hm2SfpDiagEntry 7}


hm2SfpWLGroup OBJECT IDENTIFIER ::= { hm2SfpGroup 3 }
			 
hm2SfpWLStatus OBJECT-TYPE
   			SYNTAX INTEGER
   			{
      			present(1),
      			absent(2),
      			not-supported(3)
		   	}
		   	MAX-ACCESS read-only
		   	STATUS     current
		   	DESCRIPTION
		   	"Status of the SFP White List.
		   	present(1): a white list is present on the device
		   	absent(2): no white list is present on the device
		   	not-supported(3): white list feature is not supported in this device"
		   	::= { hm2SfpWLGroup 1 }


hm2SfpThresholdTable   OBJECT-TYPE
             SYNTAX         SEQUENCE OF Hm2SfpThresholdEntry
             MAX-ACCESS     not-accessible
             STATUS         current
             DESCRIPTION
                 "This table contains the thresholds for each SFP."
             ::= { hm2SfpGroup 4 }

hm2SfpThresholdEntry  OBJECT-TYPE
             SYNTAX          Hm2SfpThresholdEntry
             MAX-ACCESS      not-accessible
             STATUS          current
             DESCRIPTION     
                "Entry for a detected SFP."
             INDEX   { ifIndex }
             ::= { hm2SfpThresholdTable 1 }

Hm2SfpThresholdEntry ::= SEQUENCE {
             hm2SfpTemperatureHighAlarm         Integer32,
             hm2SfpTemperatureHighWarning       Integer32,
             hm2SfpTemperatureLowAlarm          Integer32,
             hm2SfpTemperatureLowWarning        Integer32,
             hm2SfpTxPowerHighAlarm             Integer32,
             hm2SfpTxPowerHighWarning           Integer32,
             hm2SfpTxPowerLowAlarm              Integer32,
             hm2SfpTxPowerLowWarning            Integer32,
             hm2SfpRxPowerHighAlarm             Integer32,
             hm2SfpRxPowerHighWarning           Integer32,
             hm2SfpRxPowerLowAlarm              Integer32,
             hm2SfpRxPowerLowWarning            Integer32,
             hm2SfpTxPowerdBmHighAlarm          SnmpAdminString,
             hm2SfpTxPowerdBmHighWarning        SnmpAdminString,
             hm2SfpTxPowerdBmLowAlarm           SnmpAdminString,
             hm2SfpTxPowerdBmLowWarning         SnmpAdminString,
             hm2SfpRxPowerdBmHighAlarm          SnmpAdminString,
             hm2SfpRxPowerdBmHighWarning        SnmpAdminString,
             hm2SfpRxPowerdBmLowAlarm           SnmpAdminString,
             hm2SfpRxPowerdBmLowWarning         SnmpAdminString
             }

hm2SfpTemperatureHighAlarm         OBJECT-TYPE
             SYNTAX          Integer32 
             MAX-ACCESS      read-only
             STATUS          current
             DESCRIPTION
                "The SFP's Temperature High Alarm threshold in units of
                 centigrade (Celsius). It is -1000 if the SFP device does
                 not support it or in case of a device read error."
             ::= { hm2SfpThresholdEntry 1}

hm2SfpTemperatureHighWarning      OBJECT-TYPE
             SYNTAX          Integer32 
             MAX-ACCESS      read-only
             STATUS          current
             DESCRIPTION
                "The SFP's Temperature High Warning threshold in units of
                 centigrade (Celsius). It is -1000 if the SFP device does
                 not support it or in case of a device read error."
             ::= { hm2SfpThresholdEntry 2}

hm2SfpTemperatureLowAlarm      OBJECT-TYPE
             SYNTAX          Integer32 
             MAX-ACCESS      read-only
             STATUS          current
             DESCRIPTION
                "The SFP's Temperature Low Alarm threshold in units of
                 centigrade (Celsius). It is -1000 if the SFP device does
                 not support it or in case of a device read error."
             ::= { hm2SfpThresholdEntry 3}

hm2SfpTemperatureLowWarning      OBJECT-TYPE
             SYNTAX          Integer32 
             MAX-ACCESS      read-only
             STATUS          current
             DESCRIPTION
                "The SFP's Temperature Low Warning threshold in units of
                 centigrade (Celsius). It is -1000 if the SFP device does
                 not support it or in case of a device read error."
             ::= { hm2SfpThresholdEntry 4}

hm2SfpTxPowerHighAlarm         OBJECT-TYPE
             SYNTAX          Integer32 
             MAX-ACCESS      read-only
             STATUS          current
             DESCRIPTION
                "The SFP's Tx Power High Alarm threshold in units of
                 0.1uW. It is -10000 if the SFP device does
                 not support it or in case of a device read error."
             ::= { hm2SfpThresholdEntry 5}

hm2SfpTxPowerHighWarning      OBJECT-TYPE
             SYNTAX          Integer32 
             MAX-ACCESS      read-only
             STATUS          current
             DESCRIPTION
                "The SFP's Tx Power High Warning threshold in units of
                 0.1uW. It is -10000 if the SFP device does
                 not support it or in case of a device read error."
             ::= { hm2SfpThresholdEntry 6}

hm2SfpTxPowerLowAlarm      OBJECT-TYPE
             SYNTAX          Integer32 
             MAX-ACCESS      read-only
             STATUS          current
             DESCRIPTION
                "The SFP's Tx Power Low Alarm threshold in units of
                 0.1uW. It is -10000 if the SFP device does
                 not support it or in case of a device read error."
             ::= { hm2SfpThresholdEntry 7}

hm2SfpTxPowerLowWarning      OBJECT-TYPE
             SYNTAX          Integer32 
             MAX-ACCESS      read-only
             STATUS          current
             DESCRIPTION
                "The SFP's Tx Power Low Warning threshold in units of
                 0.1uW. It is -10000 if the SFP device does
                 not support it or in case of a device read error."
             ::= { hm2SfpThresholdEntry 8}

hm2SfpRxPowerHighAlarm         OBJECT-TYPE
             SYNTAX          Integer32 
             MAX-ACCESS      read-only
             STATUS          current
             DESCRIPTION
                "The SFP's Rx Power High Alarm threshold in units of
                 0.1uW. It is -10000 if the SFP device does
                 not support it or in case of a device read error."
             ::= { hm2SfpThresholdEntry 9}

hm2SfpRxPowerHighWarning      OBJECT-TYPE
             SYNTAX          Integer32 
             MAX-ACCESS      read-only
             STATUS          current
             DESCRIPTION
                "The SFP's Rx Power High Warning threshold in units of
                 0.1uW. It is -10000 if the SFP device does
                 not support it or in case of a device read error."
             ::= { hm2SfpThresholdEntry 10}

hm2SfpRxPowerLowAlarm      OBJECT-TYPE
             SYNTAX          Integer32 
             MAX-ACCESS      read-only
             STATUS          current
             DESCRIPTION
                "The SFP's Rx Power Low Alarm threshold in units of
                 0.1uW. It is -10000 if the SFP device does
                 not support it or in case of a device read error."
             ::= { hm2SfpThresholdEntry 11}

hm2SfpRxPowerLowWarning      OBJECT-TYPE
             SYNTAX          Integer32 
             MAX-ACCESS      read-only
             STATUS          current
             DESCRIPTION
                "The SFP's Rx Power Low Warning threshold in units of
                 0.1uW. It is -10000 if the SFP device does
                 not support it or in case of a device read error."
             ::= { hm2SfpThresholdEntry 12}

hm2SfpTxPowerdBmHighAlarm         OBJECT-TYPE
             SYNTAX          SnmpAdminString 
             MAX-ACCESS      read-only
             STATUS          current
             DESCRIPTION
                "The SFP's Tx Power High Alarm threshold in units of
                 dBm (ASCII representation of floating point number). 
                 It is N/A if the SFP device does not support it or
                 in case of a device read error."
             ::= { hm2SfpThresholdEntry 13}

hm2SfpTxPowerdBmHighWarning      OBJECT-TYPE
             SYNTAX          SnmpAdminString 
             MAX-ACCESS      read-only
             STATUS          current
             DESCRIPTION
                "The SFP's Tx Power High Warning threshold in units of
                 dBm (ASCII representation of floating point number). 
                 It is N/A if the SFP device does not support it or
                 in case of a device read error."
             ::= { hm2SfpThresholdEntry 14}

hm2SfpTxPowerdBmLowAlarm      OBJECT-TYPE
             SYNTAX          SnmpAdminString 
             MAX-ACCESS      read-only
             STATUS          current
             DESCRIPTION
                "The SFP's Tx Power Low Alarm threshold in units of
                 dBm (ASCII representation of floating point number). 
                 It is N/A if the SFP device does not support it or
                 in case of a device read error."
             ::= { hm2SfpThresholdEntry 15}

hm2SfpTxPowerdBmLowWarning      OBJECT-TYPE
             SYNTAX          SnmpAdminString 
             MAX-ACCESS      read-only
             STATUS          current
             DESCRIPTION
                "The SFP's Tx Power Low Warning threshold in units of
                 dBm (ASCII representation of floating point number). 
                 It is N/A if the SFP device does not support it or
                 in case of a device read error."
             ::= { hm2SfpThresholdEntry 16}

hm2SfpRxPowerdBmHighAlarm         OBJECT-TYPE
             SYNTAX          SnmpAdminString 
             MAX-ACCESS      read-only
             STATUS          current
             DESCRIPTION
                "The SFP's Rx Power High Alarm threshold in units of
                 dBm (ASCII representation of floating point number). 
                 It is N/A if the SFP device does not support it or
                 in case of a device read error."
             ::= { hm2SfpThresholdEntry 17}

hm2SfpRxPowerdBmHighWarning      OBJECT-TYPE
             SYNTAX          SnmpAdminString 
             MAX-ACCESS      read-only
             STATUS          current
             DESCRIPTION
                "The SFP's Rx Power High Warning threshold in units of
                 dBm (ASCII representation of floating point number). 
                 It is N/A if the SFP device does not support it or
                 in case of a device read error."
             ::= { hm2SfpThresholdEntry 18}

hm2SfpRxPowerdBmLowAlarm      OBJECT-TYPE
             SYNTAX          SnmpAdminString 
             MAX-ACCESS      read-only
             STATUS          current
             DESCRIPTION
                "The SFP's Rx Power Low Alarm threshold in units of
                 dBm (ASCII representation of floating point number). 
                 It is N/A if the SFP device does not support it or
                 in case of a device read error."
             ::= { hm2SfpThresholdEntry 19}

hm2SfpRxPowerdBmLowWarning      OBJECT-TYPE
             SYNTAX          SnmpAdminString 
             MAX-ACCESS      read-only
             STATUS          current
             DESCRIPTION
                "The SFP's Rx Power Low Warning threshold in units of
                 dBm (ASCII representation of floating point number). 
                 It is N/A if the SFP device does not support it or
                 in case of a device read error."
             ::= { hm2SfpThresholdEntry 20}


-- 
-- ***********************************************************
-- hm2ExtNvmGroup
-- ***********************************************************
--

hm2ExtNvmGeneralGroup OBJECT IDENTIFIER ::= { hm2ExtNvmGroup 1 }	

hm2ExtNvmChooseActive	OBJECT-TYPE
						 SYNTAX Hm2DeviceExtNVMType
						 MAX-ACCESS	read-write
						 STATUS			 current
						 DESCRIPTION
							 "The user can choose which external NV memory to use for file operations."
					     DEFVAL { sd }
						 ::= { hm2ExtNvmGeneralGroup 1 }
						 
hm2ExtNvmLogDevice		OBJECT-TYPE
						 SYNTAX Hm2DeviceExtNVMType
						 MAX-ACCESS	read-write
						 STATUS			 current
						 DESCRIPTION
							 "The user can choose which external NV memory to use for persistent logging."
					     DEFVAL { sd }
						 ::= { hm2ExtNvmGeneralGroup 2 }
						 
hm2ExtNvmAdminMode		OBJECT-TYPE
						 SYNTAX INTEGER {
						 					normal(1),
						 					compatibility(2)
						 				}
						 MAX-ACCESS	read-write
						 STATUS			 current
						 DESCRIPTION
							 "Switches the USB bus between High Speed (normal) and Full Speed (compatibility).
							 This setting only takes effect after a reboot."
					     DEFVAL { normal }
						 ::= { hm2ExtNvmGeneralGroup 3 }
						 
hm2ExtNvmOperMode		OBJECT-TYPE
						 SYNTAX INTEGER {
						 					normal(1),
						 					compatibility(2)
						 				}
						 MAX-ACCESS	read-only
						 STATUS			 current
						 DESCRIPTION
							 "Shows the USB mode the device is currently operating in."
						 ::= { hm2ExtNvmGeneralGroup 4 }
		
hm2ExtNvmTable		OBJECT-TYPE
			SYNTAX		SEQUENCE OF Hm2ExtNvmEntry
			MAX-ACCESS	not-accessible
			STATUS		current
			DESCRIPTION
				"This table contains variables for each nvram."
			::= { hm2ExtNvmGroup 2 }

hm2ExtNvmEntry		OBJECT-TYPE
			SYNTAX		Hm2ExtNvmEntry
			MAX-ACCESS	not-accessible
			STATUS		current
			DESCRIPTION
				"Entry for an external nvram."
			INDEX	{ hm2ExtNvmTableIndex }
			::= { hm2ExtNvmTable 1 }

Hm2ExtNvmEntry ::= SEQUENCE {
			hm2ExtNvmTableIndex					Hm2DeviceExtNVMType,
			hm2ExtNvmStatus						INTEGER,
			hm2ExtNvmManufacturerId				DisplayString,
			hm2ExtNvmHWRevision					DisplayString,
			hm2ExtNvmProductName				DisplayString,
			hm2ExtNvmVersion					DisplayString,
			hm2ExtNvmSerialNum					DisplayString,
			hm2ExtNvmAutomaticSoftwareLoad		HmEnabledStatus,
			hm2ExtNvmConfigLoadPriority			INTEGER,
			hm2ExtNvmConfigSave					HmEnabledStatus,
			hm2ExtNvmWritable					HmEnabledStatus,
			hm2ExtNvmAutomaticSshKeyLoad		HmEnabledStatus
}

hm2ExtNvmTableIndex		OBJECT-TYPE
			SYNTAX		Hm2DeviceExtNVMType
			MAX-ACCESS	not-accessible
			STATUS		current
			DESCRIPTION
				"Index"
			::= { hm2ExtNvmEntry 1 }

hm2ExtNvmStatus			OBJECT-TYPE
			SYNTAX INTEGER {
						notPresent(1),
						removed(2),
						ok(3),
						outOfMemory(4),
						genericErr(5)
						}
			MAX-ACCESS	read-only
			STATUS		current
			DESCRIPTION
				"Status of the external non-volatile memory.
				notPresent(1): external non-volatile memory has not been detected.
				removed(2): external non-volatile memory was removed in running mode of the agent.
				ok(3): external non-volatile memory is present and OK.
				outOfMemory(4): external non-volatile memory is full.
				genericErr(5): Any other failure, e.g. hardware malfunction."
			::= { hm2ExtNvmEntry 2 }
 
hm2ExtNvmManufacturerId	OBJECT-TYPE
			SYNTAX		DisplayString 
			MAX-ACCESS	read-only
			STATUS		current
			DESCRIPTION
				"The manufacturer ID."
			 ::= { hm2ExtNvmEntry 3 }

hm2ExtNvmHWRevision	OBJECT-TYPE
			SYNTAX		DisplayString 
			MAX-ACCESS	read-only
			STATUS		current
			DESCRIPTION
				"The application ID."
			 ::= { hm2ExtNvmEntry 4 }

hm2ExtNvmProductName	OBJECT-TYPE
			SYNTAX		DisplayString 
			MAX-ACCESS	read-only
			STATUS		current
			DESCRIPTION
				"The product name."
			 ::= { hm2ExtNvmEntry 5 }

hm2ExtNvmVersion		OBJECT-TYPE
			SYNTAX		DisplayString 
			MAX-ACCESS	read-only
			STATUS		current
			DESCRIPTION
				"The version."
			 ::= { hm2ExtNvmEntry 6 }

hm2ExtNvmSerialNum		OBJECT-TYPE
			SYNTAX		DisplayString 
			MAX-ACCESS	read-only
			STATUS		current
			DESCRIPTION
				"The serial number provided by vendor (ASCII)."
			 ::= { hm2ExtNvmEntry 7 }

hm2ExtNvmAutomaticSoftwareLoad OBJECT-TYPE
			SYNTAX		HmEnabledStatus
			MAX-ACCESS	read-write
			STATUS		current
			DESCRIPTION
				"Enable or disable Automatic loading of a software image
				from the external non-volatile memory. A file named 'startup.txt'
				must be present on the external non-volatile memory and contain the
				line 'autoUpdate=filename'."
			DEFVAL { enable }
			::= { hm2ExtNvmEntry 8 }

hm2ExtNvmConfigLoadPriority OBJECT-TYPE
			SYNTAX		INTEGER {
						disable(0),
						first(1),
						second(2),
						third(3)
						}
			MAX-ACCESS	read-write
			STATUS		current
			DESCRIPTION
				"Set the priority of this external non-volatile memory for
				loading the configuration while booting. The configuration
				on the device with the lowest priority is loaded.
				Setting this variable to 0 disables loading of a configuration
				from this device."
			::= { hm2ExtNvmEntry 9 }

hm2ExtNvmConfigSave OBJECT-TYPE
			SYNTAX		HmEnabledStatus
			MAX-ACCESS	read-write
			STATUS		current
			DESCRIPTION
				"Enable or disable Automatic saving of the configuration to the
				external non-volatile memory. If this is enabled, saving the
				configuration of the device to its internal nvram also stores
				in on this external nvram."
			DEFVAL { enable }
			::= { hm2ExtNvmEntry 10 }

hm2ExtNvmWritable OBJECT-TYPE
			SYNTAX		HmEnabledStatus
			MAX-ACCESS	read-only
			STATUS		current
			DESCRIPTION
				"Shows if writing to the device is possible, i.e. if it is
				write protected."
			::= { hm2ExtNvmEntry 11 }

hm2ExtNvmAutomaticSshKeyLoad OBJECT-TYPE
			SYNTAX      HmEnabledStatus
			MAX-ACCESS  read-write
			STATUS      current
			DESCRIPTION
				"Enable or disable automatic loading of a SSH key
				 from the external non-volatile memory. A file named 'startup.txt'
				 must be present on the external non-volatile memory and contain 
				 the line 'autoUpdateRSA=' and/or 'autoUpdateDSA='."
			DEFVAL { enable }
			::= { hm2ExtNvmEntry 12 }
			
-- 
-- ***********************************************************
-- hm2AutoDisableGroup
-- ***********************************************************
--	


		
hm2AutoDisableIntfTable	OBJECT-TYPE
					SYNTAX	SEQUENCE OF Hm2AutoDisableIntfEntry
					MAX-ACCESS	not-accessible
					STATUS		current
					DESCRIPTION
					"Port Auto Disable interface table."
					::= { hm2AutoDisableGroup 1 }

hm2AutoDisableIntfEntry	OBJECT-TYPE
					SYNTAX			Hm2AutoDisableIntfEntry
					MAX-ACCESS		not-accessible
					STATUS			current
					DESCRIPTION
					"Port Auto Disable interface entry."
					INDEX	{ ifIndex }
					::= { hm2AutoDisableIntfTable 1 }

Hm2AutoDisableIntfEntry ::=
					SEQUENCE		{									 
					hm2AutoDisableIntfRemainingTime 	Unsigned32,
					hm2AutoDisableIntfComponentName 	SnmpAdminString,
					hm2AutoDisableIntfErrorReason 		INTEGER,
					hm2AutoDisableIntfTimer 			Unsigned32,
					hm2AutoDisableIntfReset 			TruthValue,
					hm2AutoDisableIntfOperState 		INTEGER,	
					hm2AutoDisableIntfErrorTime 	    HmTimeSeconds1970		
					}


hm2AutoDisableIntfRemainingTime	OBJECT-TYPE
					SYNTAX		Unsigned32
				 	MAX-ACCESS	read-only
					STATUS		current
					DESCRIPTION
					"Remaining time in seconds until the re-activation of the port."
					DEFVAL		{0}
					::= { hm2AutoDisableIntfEntry 1}

hm2AutoDisableIntfComponentName
					OBJECT-TYPE
					SYNTAX		SnmpAdminString
				 	MAX-ACCESS	read-only
					STATUS		current
					DESCRIPTION
					"Name of the component that triggered the error"				
					::= { hm2AutoDisableIntfEntry 2}

hm2AutoDisableIntfErrorReason
					OBJECT-TYPE
					SYNTAX INTEGER {
									none(0), 
									link-flap(1), 
									crc-error(2),
									duplex-mismatch(3), 
									dhcp-snooping(4),
									arp-rate(5),
									bpdu-rate(6),
									mac-based-port-security(7),
									overload-detection(8),
									speed-duplex(9),
									loop-protection(10)
								   }
				 	MAX-ACCESS	read-only
					STATUS		current
					DESCRIPTION
					"Error disable reason"
					::= { hm2AutoDisableIntfEntry 3}
					
hm2AutoDisableIntfTimer OBJECT-TYPE
 					SYNTAX		Unsigned32 (0|30..4294967295) 
				 	MAX-ACCESS	read-write
					STATUS		current
					DESCRIPTION
					"Timer value in seconds after a deactivated port is activated again.
					Possible values are: 30-4294967295.
					A value of 0 disables the timer."
					DEFVAL	{0}
					::= {hm2AutoDisableIntfEntry 4}
					

hm2AutoDisableIntfReset	OBJECT-TYPE
					SYNTAX			TruthValue
					MAX-ACCESS		read-write
					STATUS			current
					DESCRIPTION
					"Port Auto Disable interface reset."
					DEFVAL			{ false }
					::= { hm2AutoDisableIntfEntry 5 }					
					
hm2AutoDisableIntfOperState OBJECT-TYPE
			SYNTAX		INTEGER {
						active(1),
						inactive(2)					
						}
			MAX-ACCESS	read-only
			STATUS		current
			DESCRIPTION
				"Status of Auto Disable interface admin state.
				Active means that a component has encountered an error 
				and Auto-Disable has turned off the interface. 
				Inactive means that currently there is no error"
				DEFVAL			{inactive}
			::= { hm2AutoDisableIntfEntry 6 }			
					

					
hm2AutoDisableIntfErrorTime OBJECT-TYPE
			SYNTAX		HmTimeSeconds1970 
		 	MAX-ACCESS	read-only
			STATUS		current
			DESCRIPTION
				"Local system time (hm2SystemLocalTime) when the error occured."
			::= {hm2AutoDisableIntfEntry 7}										
										

hm2AutoDisableReasonTable OBJECT-TYPE
					SYNTAX	SEQUENCE OF Hm2AutoDisableReasonEntry
					MAX-ACCESS	not-accessible
					STATUS		current
					DESCRIPTION
					"Possible reasons for Auto Disable"
					::= { hm2AutoDisableGroup 2 }

hm2AutoDisableReasonEntry	OBJECT-TYPE
					SYNTAX			Hm2AutoDisableReasonEntry
					MAX-ACCESS		not-accessible
					STATUS			current
					DESCRIPTION
					"Port Auto Disable interface entry."
					INDEX	{ hm2AutoDisableReasons }
					::= { hm2AutoDisableReasonTable 1 }

Hm2AutoDisableReasonEntry ::=
					SEQUENCE		{									 
					hm2AutoDisableReasons 			INTEGER,			
					hm2AutoDisableReasonOperation 	HmEnabledStatus,
					hm2AutoDisableReasonCategory 	INTEGER			 
					}
					
hm2AutoDisableReasons   OBJECT-TYPE
						SYNTAX INTEGER {
										link-flap(1), 
										crc-error(2),
										duplex-mismatch(3), 
										dhcp-snooping(4),
										arp-rate(5),
										bpdu-rate(6),
										mac-based-port-security(7),
										overload-detection(8),
										speed-duplex(9),
										loop-protection(10)
								   	   }
				     	MAX-ACCESS	not-accessible
					    STATUS		current
					    DESCRIPTION
					    "Reason for deactivation a port"
					    ::= { hm2AutoDisableReasonEntry 1}			
					    
hm2AutoDisableReasonOperation	OBJECT-TYPE
					SYNTAX			HmEnabledStatus
					MAX-ACCESS		read-write
					STATUS			current
					DESCRIPTION
					"Enables/disables recovery by resaon on this device."
					DEFVAL  		{ disable }
					::= { hm2AutoDisableReasonEntry 2 }					    		

hm2AutoDisableReasonCategory OBJECT-TYPE
					SYNTAX INTEGER {
									other(1), 
									port-monitor(2), 
									network-security(3), 
									l2-redundancy(4)
								   }
				 	MAX-ACCESS	read-only
					STATUS		current
					DESCRIPTION
					"Auto Disable Reason Category"
					::= { hm2AutoDisableReasonEntry 3}

-- 
-- ***********************************************************
-- hm2UnitGroup
-- ***********************************************************
--

-- Unit table
hm2UnitTable   OBJECT-TYPE
			SYNTAX		SEQUENCE OF Hm2UnitEntry
			MAX-ACCESS	not-accessible
			STATUS		current
			DESCRIPTION
			"This table contains unit capabilities and
			configuration options."
			::= { hm2UnitGroup 100 }

hm2UnitEntry	 OBJECT-TYPE
			SYNTAX		Hm2UnitEntry
			MAX-ACCESS	not-accessible
			STATUS		current
			DESCRIPTION
			"Entry with the configuration options and supported
			features of a unit."
			INDEX		{ hm2UnitIndex }
			::= { hm2UnitTable 1 }

Hm2UnitEntry ::= SEQUENCE {
			hm2UnitIndex					Integer32,
			hm2UnitMaxModuleCapacity 		Integer32,
			hm2UnitMaxModulePortCapacity	Integer32
			}

hm2UnitIndex OBJECT-TYPE
			SYNTAX		Integer32 
			MAX-ACCESS	accessible-for-notify
			STATUS		current
			DESCRIPTION
			"The index of the available unit." 
			::= { hm2UnitEntry 1 }

hm2UnitMaxModuleCapacity OBJECT-TYPE
			SYNTAX		Integer32 
			MAX-ACCESS	read-only
			STATUS		current
			DESCRIPTION
			"Maximum number of modules that this unit can
			contain in this system."
			::= { hm2UnitEntry 2 }

hm2UnitMaxModulePortCapacity OBJECT-TYPE
			SYNTAX 		Integer32 
			MAX-ACCESS	read-only
			STATUS 		current
			DESCRIPTION
			"Maximum number of ports that a module can 
			contain in this unit."
			::= { hm2UnitEntry 3 }
			
-- 
-- ***********************************************************
-- hm2ModuleGroup
-- ***********************************************************
--


-- Module table
hm2ModuleTable   OBJECT-TYPE
			SYNTAX		SEQUENCE OF Hm2ModuleEntry
			MAX-ACCESS	not-accessible
			STATUS		current
			DESCRIPTION
			"This table contains capabilities and
			configuration options of device modules."
			::= { hm2ModuleGroup 100 }

hm2ModuleEntry	 OBJECT-TYPE
			SYNTAX		Hm2ModuleEntry
			MAX-ACCESS	not-accessible
			STATUS		current
			DESCRIPTION
			"Entry with the configuration options and supported
			features of a device module."
			INDEX		{ hm2UnitIndex, hm2ModuleIndex }
			::= { hm2ModuleTable 1 }

Hm2ModuleEntry ::= SEQUENCE {
			hm2ModuleIndex				Integer32,
			hm2ModuleId					OBJECT IDENTIFIER,
			hm2ModuleDescription		SnmpAdminString,
			hm2ModuleProductCode		SnmpAdminString,
			hm2ModuleVersion			SnmpAdminString,
			hm2ModuleNumOfPorts			Integer32,
			hm2ModuleFirstMauIndex		Integer32,
			hm2ModuleStatus				INTEGER,
			hm2ModuleSerialNum			SnmpAdminString,
			hm2ModuleMinSWVersion		Integer32,
			hm2ModuleCapability			BITS,
			hm2ModuleInternalID			Integer32,
			hm2ModuleInternalIDVariant	Integer32,
			hm2ModuleFirstIfIndex		Integer32,
			hm2ModuleAdminState			HmEnabledStatus
			}

hm2ModuleIndex OBJECT-TYPE
			SYNTAX		Integer32 
			MAX-ACCESS	accessible-for-notify
			STATUS		current
			DESCRIPTION
			"The index of the available module." 
			::= { hm2ModuleEntry 1 }
		 
hm2ModuleId OBJECT-TYPE
			SYNTAX		OBJECT IDENTIFIER
			MAX-ACCESS	read-only
			STATUS		current
			DESCRIPTION
			"Manufacturer-defined product identifier (module family + product ID).
			Example: Object-ID 1.3.6.1.4.1.248.11.2.2.1 is the hm2ModuleFamily MSM and
			Object-ID 1.3.6.1.4.1.248.11.2.2.1.1 is the Product ID for msm-4tx"
			::= { hm2ModuleEntry 2 }
 
hm2ModuleDescription OBJECT-TYPE
			SYNTAX		SnmpAdminString
			MAX-ACCESS	read-write
			STATUS		current
			DESCRIPTION
			"Description of the module. This value cannot be written by external 
			entities (only for internal purposes)."
			::= { hm2ModuleEntry 3 }

hm2ModuleProductCode OBJECT-TYPE
			SYNTAX		SnmpAdminString
			MAX-ACCESS	read-only
			STATUS		current
			DESCRIPTION
			"Product Code of the module."
			::= { hm2ModuleEntry 4 }

hm2ModuleVersion OBJECT-TYPE
			SYNTAX		SnmpAdminString
			MAX-ACCESS	read-only
			STATUS		current
			DESCRIPTION
			"Version of the module."
			::= { hm2ModuleEntry 5 }

hm2ModuleNumOfPorts	 OBJECT-TYPE
			SYNTAX		Integer32
			MAX-ACCESS	read-only
			STATUS		current
			DESCRIPTION
			"The numberOfPorts is the number of ports contained within
			the module. Within each module, the ports are uniquely
			numbered in the range from 1 to numberOfPorts."
			::= { hm2ModuleEntry 6 }
 
hm2ModuleFirstMauIndex	OBJECT-TYPE
			SYNTAX		Integer32
			MAX-ACCESS	read-only
			STATUS		obsolete
			DESCRIPTION
			"Value of the first mauIndex used by the module.
			 **NOTE: This object is obsolete in favour of hm2ModuleFirstIfIndex.**"
			::= { hm2ModuleEntry 7 }

hm2ModuleStatus	OBJECT-TYPE
			SYNTAX		INTEGER {
						physical (1),
						configurable (2),
						remove (3),
						fix (4)
						}
			MAX-ACCESS	read-write
			STATUS		current
			DESCRIPTION
			"Status of the module.
			If the value is physical(1), then the module is plugged in,
			if the value is configurable, the ports can be configured,
			but the card is absent, with the value remove(3) written to
			the agent the card can be logically removed.
			The value fix(4) is for modules which cannot be removed."
			::= { hm2ModuleEntry 8 }

hm2ModuleSerialNum OBJECT-TYPE
			SYNTAX		SnmpAdminString
			MAX-ACCESS	read-only
			STATUS		current
			DESCRIPTION
			"The serial number provided by vendor (ASCII)."
			::= { hm2ModuleEntry 9 }

hm2ModuleMinSWVersion OBJECT-TYPE
			SYNTAX		Integer32
			MAX-ACCESS	read-only
			STATUS		current
			DESCRIPTION
			"The minimum software version required to support this module."
			::= { hm2ModuleEntry 10 }

hm2ModuleCapability OBJECT-TYPE
			SYNTAX		BITS 	{
						poe(0),
						fpga(1),
						ptp(2),
						io-module(3)
						}
			MAX-ACCESS	read-write
			STATUS		current
			DESCRIPTION
			"poe - module supports Power over Ethernet,
			fpga - module has a FPGA,
			ptp - module supports PTP,
			io-module - module is an IO module. 
			This value cannot be written by external entities (only for internal purposes)."
			::= { hm2ModuleEntry 11 }
			
hm2ModuleInternalID	 OBJECT-TYPE
			SYNTAX		Integer32
			MAX-ACCESS	read-write
			STATUS		current
			DESCRIPTION
			"An internal ID of the Module. This value cannot be written by external 
			entities (only for internal purposes)."
			DEFVAL  { 0 }
			::= { hm2ModuleEntry 12 }
			
hm2ModuleInternalIDVariant	OBJECT-TYPE
			SYNTAX		Integer32
			MAX-ACCESS	read-write
			STATUS		obsolete
			DESCRIPTION
			"An internal variant ID of the Module.
			 **NOTE: This object is obsolete.**"
			DEFVAL  { 0 }
			::= { hm2ModuleEntry 13 }
			
hm2ModuleFirstIfIndex	OBJECT-TYPE
			SYNTAX		Integer32
			MAX-ACCESS	read-only
			STATUS		current
			DESCRIPTION
			"Value of the first ifIndex used by the module."
			::= { hm2ModuleEntry 14 }

hm2ModuleAdminState		OBJECT-TYPE
		SYNTAX  HmEnabledStatus
		 MAX-ACCESS 	read-write
		 STATUS 	 	current
		 DESCRIPTION
			"Enable or disable the module. If disabled, module 
 plugged in this slot will not be activated. "
DEFVAL { enable }
	::= { hm2ModuleEntry 15 }

-- 
-- ***********************************************************
-- hm2DeviceMgmtMibNotifications
-- ***********************************************************
--

hm2SfpChangeTrap	NOTIFICATION-TYPE
		OBJECTS		{ ifIndex }
		STATUS  	current
		DESCRIPTION	
			"This trap is sent when a SFP has been added or removed.
			It is also sent for an otherwise unsupported SFP."
		::= { hm2DeviceMgmtMibNotifications 1 }	

hm2AutoDisablePortTrap	NOTIFICATION-TYPE
		OBJECTS  { ifIndex,
			   hm2IfaceOperAdminStatus,
			   hm2AutoDisableIntfErrorReason
			 }
		STATUS current
		DESCRIPTION
			"This trap is sent if the port has been disabled or enabled by auto disable feature."
		::= { hm2DeviceMgmtMibNotifications 2 }   		

hm2ModulePluggedTrap	NOTIFICATION-TYPE
	OBJECTS	{	hm2UnitIndex, 
				hm2ModuleIndex
			}
		STATUS current
		DESCRIPTION
		"This trap is sent if a module is plugged into a unit."
		::= { hm2DeviceMgmtMibNotifications 3 }

hm2ModuleRemovedTrap	NOTIFICATION-TYPE
	OBJECTS	{	hm2UnitIndex, 
				hm2ModuleIndex
			}
		STATUS current
		DESCRIPTION
		"This trap is sent if a module is removed from a unit."
		::= { hm2DeviceMgmtMibNotifications 4 }

hm2SFPRxPowerChangeTrap	NOTIFICATION-TYPE
		OBJECTS		{ hm2SfpCurrentRxPowerState }
		STATUS  	current
		DESCRIPTION	
			"This trap is sent when the state (hm2SfpCurrentRxPowerState) of the rx power of a SFP changes."
		::= { hm2DeviceMgmtMibNotifications 5 }	

END

