HM2-MGMTACCESS-MIB DEFINITIONS ::= BEGIN

--
-- *************************************************************
-- Hirschmann Management Access MIB
-- *************************************************************
--

IMPORTS
   NOTIFICATION-TYPE,
   MODULE-IDENTITY, 
   OBJECT-IDENTITY,
   OBJECT-TYPE,
   Integer32, Counter64    FROM SNMPv2-SMI -- RFC 2578
   DisplayString,
   TEXTUAL-CONVENTION,
   RowStatus               FROM SNMPv2-TC
   SnmpAdminString         FROM SNMP-FRAMEWORK-MIB
   InetAddressType,
   InetAddress,
   InetPortNumber,
   InetAddressPrefixLength FROM INET-ADDRESS-MIB
   hm2ConfigurationMibs,
   HmEnabledStatus,
   HmLargeDisplayString      FROM HM2-TC-MIB;

hm2MgmtAccessMib MODULE-IDENTITY
	LAST-UPDATED "201103160000Z" -- March 16, 2011
    ORGANIZATION "Hirschmann Automation and Control GmbH"
    CONTACT-INFO
        "Postal:     Stuttgarter Str. 45-51
                     72654 Neckartenzlingen
                     Germany
         Phone:      +49 7127 140
         E-mail:     hac.support@belden.com"
    DESCRIPTION
        "Hirschmann Management Access MIB.
         Copyright (C) 2012. All Rights Reserved."
    REVISION     "201103160000Z" -- March 16, 2011
    DESCRIPTION
         "Initial version."
    ::= { hm2ConfigurationMibs 25 }

--
-- *************************************************************
-- Textual Conventions
-- *************************************************************
--
Hm2RestartAction ::= TEXTUAL-CONVENTION
			STATUS			current
			DESCRIPTION		"."
			SYNTAX			INTEGER {
										other(1),
										restart(2)
									}

Hm2TlsVersions ::= TEXTUAL-CONVENTION
			STATUS			current
			DESCRIPTION		"The Transport Layer Security versions available on the device."
			SYNTAX			BITS {
									tlsv1-0(0),
									tlsv1-1(1), -- not implemented
									tlsv1-2(2)
								}

Hm2TlsCipherSuites ::= TEXTUAL-CONVENTION
			STATUS			current
			DESCRIPTION		"The Transport Layer Security ciphers available on the device."
			SYNTAX			BITS {
									tls-rsa-with-rc4-128-sha(0),
									tls-rsa-with-aes-128-cbc-sha(1),
									tls-dhe-rsa-with-aes-128-cbc-sha(2),
									tls-dhe-rsa-with-aes-256-cbc-sha(3),
									tls-ecdhe-rsa-with-aes-128-cbc-sha(4),
									tls-ecdhe-rsa-with-aes-256-cbc-sha(5),
									tls-ecdhe-rsa-with-aes-128-gcm-sha256(6),
									tls-ecdhe-rsa-with-aes-256-gcm-sha384(7)
								}

Hm2SshHmacAlgorithms ::= TEXTUAL-CONVENTION
      STATUS      current
      DESCRIPTION   "The Secure Shell algorithms for HMAC available on the device."
      SYNTAX      BITS {
                  hmac-sha1(0),
                  hmac-sha2-256(1),
                  hmac-sha2-512(2),
                  hmac-sha1-etm-at-openssh-com(3),
                  hmac-sha2-256-etm-at-openssh-com(4),
                  hmac-sha2-512-etm-at-openssh-com(5)
                }

Hm2SshKexAlgorithms ::= TEXTUAL-CONVENTION
      STATUS      current
      DESCRIPTION   "The Secure Shell algorithms for key exchange available on the device."
      SYNTAX      BITS {
                  diffie-hellman-group1-sha1(0),
                  diffie-hellman-group14-sha1(1),
                  diffie-hellman-group14-sha256(2),
                  diffie-hellman-group16-sha512(3),
                  diffie-hellman-group18-sha512(4),
                  diffie-hellman-group-exchange-sha256(5),
                  ecdh-sha2-nistp256(6),
                  ecdh-sha2-nistp384(7)
                }

Hm2SshEncryptionAlgorithms ::= TEXTUAL-CONVENTION
      STATUS      current
      DESCRIPTION   "The Secure Shell algorithms for encryption available on the device."
      SYNTAX      BITS {
                  aes128-ctr(0),
                  aes192-ctr(1),
                  aes256-ctr(2),
                  aes128-gcm-at-openssh-com(3),
                  aes256-gcm-at-openssh-com(4),
                  chacha20-poly1305-at-openssh-com(5)
                }

--
-- *************************************************************
-- hm2MgmtAccessMib
-- *************************************************************
--
hm2MgmtAccessMibNotifications			OBJECT IDENTIFIER ::= { hm2MgmtAccessMib 0 }
hm2MgmtAccessMibObjects					OBJECT IDENTIFIER ::= { hm2MgmtAccessMib 1 }
-- hm2MgmtAccessMibConformance					OBJECT IDENTIFIER ::= { hm2MgmtAccessMib 2 }
hm2MgmtAccessMibSNMPExtensionGroup 		OBJECT IDENTIFIER ::= { hm2MgmtAccessMib 3 }

--
-- *************************************************************
-- hm2MgmtAccessMib groups
-- *************************************************************
--
hm2MgmtAccessSnmpGroup 					OBJECT IDENTIFIER ::= { hm2MgmtAccessMibObjects 1 }
hm2MgmtAccessWebGroup 					OBJECT IDENTIFIER ::= { hm2MgmtAccessMibObjects 2 }
hm2MgmtAccessTelnetGroup				OBJECT IDENTIFIER ::= { hm2MgmtAccessMibObjects 3 }
hm2MgmtAccessSshGroup					OBJECT IDENTIFIER ::= { hm2MgmtAccessMibObjects 4 }
hm2MgmtAccessPreLoginBannerGroup		OBJECT IDENTIFIER ::= { hm2MgmtAccessMibObjects 5 }
hm2MgmtAccessCliGroup					OBJECT IDENTIFIER ::= { hm2MgmtAccessMibObjects 6 }
hm2RestrictedMgmtAccessGroup 			OBJECT IDENTIFIER ::= { hm2MgmtAccessMibObjects 7 }
hm2MgmtAccessStatisticsGroup 			OBJECT IDENTIFIER ::= { hm2MgmtAccessMibObjects 10 }

--
-- *************************************************************
-- hm2MgmtAccessSnmp
-- *************************************************************
--
hm2SnmpV1AdminStatus		OBJECT-TYPE
			SYNTAX HmEnabledStatus
			MAX-ACCESS	read-write
			STATUS	current
			DESCRIPTION
			"Enables/disables the SNMP version 1 protocol."
			DEFVAL  { disable }			
			::= { hm2MgmtAccessSnmpGroup 1 }

hm2SnmpV2AdminStatus 	OBJECT-TYPE
			SYNTAX HmEnabledStatus
			MAX-ACCESS	read-write
			STATUS	current
			DESCRIPTION
			"Enables/disables the SNMP version 2c protocol."						
			DEFVAL  { disable }
			::= { hm2MgmtAccessSnmpGroup 2 }

hm2SnmpV3AdminStatus 	OBJECT-TYPE
			SYNTAX HmEnabledStatus
			MAX-ACCESS	read-write
			STATUS	current
			DESCRIPTION
			"Enables/disables the SNMP version 3 protocol."						
			DEFVAL  { enable }
			::= { hm2MgmtAccessSnmpGroup 3 }

hm2SnmpPortNumber  	OBJECT-TYPE
			SYNTAX	InetPortNumber
			MAX-ACCESS	read-write
			STATUS	current
			DESCRIPTION
			"The port number of the snmp server.
			To activate the port number the device
			has to be restarted.
            Setting the port to zero is not allowed."						
			DEFVAL  { 161 }
			::= { hm2MgmtAccessSnmpGroup 4 }

hm2SnmpOver802AdminStatus OBJECT-TYPE
			SYNTAX HmEnabledStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION "Enables/disables SNMP over IEEE 802 networks."
			DEFVAL { disable }
			::= { hm2MgmtAccessSnmpGroup 5 }
			
hm2SnmpTrapServiceAdminStatus OBJECT-TYPE
			SYNTAX HmEnabledStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION "Enables/disables the SNMP trap sending service globally on the device."
			DEFVAL { enable }
			::= { hm2MgmtAccessSnmpGroup 6 }
			
--
-- *************************************************************
-- hm2MgmtAccessWeb
-- *************************************************************
--

hm2WebHttpAdminStatus OBJECT-TYPE
			SYNTAX			 HmEnabledStatus
			MAX-ACCESS		 read-write
			STATUS			 current
			DESCRIPTION
			"Enables/Disables HTTP access to the device."
			DEFVAL 		 	{ enable } 
			::= { hm2MgmtAccessWebGroup 1 }
		
hm2WebHttpsAdminStatus OBJECT-TYPE
			SYNTAX			 HmEnabledStatus
			MAX-ACCESS		 read-write
			STATUS			 current
			DESCRIPTION
				 "Enables/Disables HTTPS access to the device."
			 DEFVAL  { enable }	
			::= { hm2MgmtAccessWebGroup 2 }
			
hm2WebHttpPortNumber OBJECT-TYPE
			SYNTAX	InetPortNumber
			MAX-ACCESS		 read-write
			STATUS			 current
			DESCRIPTION
			"The port number of the HTTP web server.
                         Setting the port to zero is not allowed."
			DEFVAL			 { 80 }
			::= { hm2MgmtAccessWebGroup 3 }
					
hm2WebHttpsPortNumber OBJECT-TYPE
			SYNTAX	InetPortNumber
			MAX-ACCESS		 read-write
			STATUS			 current
			DESCRIPTION
			"The port number of the HTTPS web server.
                         Setting the port to zero is not allowed."
			DEFVAL { 443 }
			::= { hm2MgmtAccessWebGroup 4 }	

hm2WebHttpsCertPresent OBJECT-TYPE
		SYNTAX INTEGER {
		     pem(1),
		     none(2)
		     }
		MAX-ACCESS  read-only
		STATUS      current
		DESCRIPTION
		             "Indicates what HTTP certificate files are present on the device, if any."
		::= { hm2MgmtAccessWebGroup 5 }

hm2WebHttpsCertControl OBJECT-TYPE
     	SYNTAX INTEGER {
               noop(1),
               generate(2),
               delete(3)
                 }
	     MAX-ACCESS  read-write
	     STATUS      current
	     DESCRIPTION
                 "Controls HTTPS certificate generation and deletion. Always returns noop(1)."
     ::= { hm2MgmtAccessWebGroup 6 }
     
hm2WebHttpsCertOperStatus OBJECT-TYPE
        SYNTAX      INTEGER{
		     		generate(1),
		     		delete(2),
		     		none(3)
		     		}
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                    "Indicates what key files are currently being generated, if any."
        ::= { hm2MgmtAccessWebGroup 7 }

hm2WebIntfTimeOut OBJECT-TYPE
		   SYNTAX Integer32 (0..160)
		   MAX-ACCESS read-write
		   STATUS current
		   DESCRIPTION
		            "Web interface idle timeout value for this switch in minutes.
		    	     If the value is set to 0 the idle logout is disabled."
			DEFVAL { 5 }           
		   ::= { hm2MgmtAccessWebGroup 8 }

hm2WebTrapEnable  OBJECT-TYPE
    	SYNTAX      HmEnabledStatus
    	MAX-ACCESS  read-write
    	STATUS      current
    	DESCRIPTION
            	"Indicates whether login success, login failed or logout traps 
             	 should be generated for this application."
			DEFVAL { enable }             
    ::= { hm2MgmtAccessWebGroup 9 }

hm2WebLastLogoutUserName OBJECT-TYPE
        SYNTAX      SnmpAdminString (SIZE(0..32))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                    "User name of last logout for this application."
        ::= { hm2MgmtAccessWebGroup 10 }

hm2WebLastLoginUserName OBJECT-TYPE
        SYNTAX      SnmpAdminString (SIZE(0..32))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                    "User name of last login for this application."
        ::= { hm2MgmtAccessWebGroup 11 }

hm2WebLastLoginInetAddressType OBJECT-TYPE
        SYNTAX      InetAddressType 
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                    "InetAddressType of the last login used for this application."
        ::= { hm2MgmtAccessWebGroup 12 }

hm2WebLastLoginInetAddress OBJECT-TYPE
        SYNTAX      InetAddress 
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                    "IP address or DNS name specified in the last request for this application."
        ::= { hm2MgmtAccessWebGroup 13 }
        
hm2WebHttpsCertFingerPrintType OBJECT-TYPE 
       SYNTAX INTEGER { 
                   sha1(1), 
                   sha256(2) 
                   } 
      MAX-ACCESS  read-write 
      STATUS      current 
      DESCRIPTION 
          "Controls HTTPS certificate fingerprint generation. If set to 'sha1' hm2WebHttpsCertFingerPrint 
           will show the SHA1 fingerprint of the certificate." 
      DEFVAL { sha256 }  
     ::= { hm2MgmtAccessWebGroup  14 } 
      
hm2WebHttpsCertFingerPrint    OBJECT-TYPE 
      SYNTAX         DisplayString 
      MAX-ACCESS     read-only 
      STATUS         current 
      DESCRIPTION 
         "The HTTPS certificate fingerprint as hash. The type of the hash is defined with hm2WebHttpsCertFingerPrintType."                         
     ::= { hm2MgmtAccessWebGroup  15 }                  
        
hm2WebHttpsServerRestart     OBJECT-TYPE
      SYNTAX       Hm2RestartAction
      MAX-ACCESS   read-write
      STATUS       current
      DESCRIPTION
                   "Setting the object to restart will have the effect of restarting the HTTPS server.
                    The server will load the new settings."
      ::= { hm2MgmtAccessWebGroup  16 }

hm2WebHttpsServerTlsVersions OBJECT-TYPE
      SYNTAX       Hm2TlsVersions
      MAX-ACCESS   read-write
      STATUS       current
      DESCRIPTION
                   "The TLS version supported by the HTTPS server.
                    Changing the value has only effect after restarting the HTTPS Server."
      DEFVAL       {{ tlsv1-2 }}
      ::= { hm2MgmtAccessWebGroup  17 }

hm2WebHttpsServerTlsCipherSuites OBJECT-TYPE
      SYNTAX       Hm2TlsCipherSuites
      MAX-ACCESS   read-write
      STATUS       current
      DESCRIPTION
                   "The cipher suite used by the HTTPS server.
                    Changing the value has only effect after restarting the HTTPS server."
      DEFVAL       {{
                     tls-ecdhe-rsa-with-aes-128-gcm-sha256,
                     tls-ecdhe-rsa-with-aes-256-gcm-sha384
                   }}
      ::= { hm2MgmtAccessWebGroup  18 }

--
-- *************************************************************
-- hm2MgmtAccessTelnet
-- *************************************************************
--
hm2TelnetServerAdminStatus OBJECT-TYPE
   SYNTAX HmEnabledStatus
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Enable/Disable telnet operation. A (1) enables, a (2) disables.
      When disabled, no telnet sessions are allowed by the system."
   DEFVAL { disable }
   ::= { hm2MgmtAccessTelnetGroup 1 }
            
hm2TelnetServerPort OBJECT-TYPE
   SYNTAX InetPortNumber
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Telnet port operation. Default telnet port is 23.
       Setting the port to zero is not allowed."
   DEFVAL { 23 }           
   ::= { hm2MgmtAccessTelnetGroup 2 }

hm2TelnetServerSessionsCount OBJECT-TYPE
     SYNTAX      	Integer32
     MAX-ACCESS  	read-only
     STATUS      	current
     DESCRIPTION
                 "Current number of active telnet sessions on this switch."
     ::= { hm2MgmtAccessTelnetGroup 3 }
          
hm2TelnetServerMaxSessions OBJECT-TYPE
   SYNTAX Integer32 (1..5)
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Maximum number of telnet sessions.
      An integer value from 1 to 5 specifies 
      the maximum number of telnet sessions that can be established.
      The full range is not supported by all variants."
   DEFVAL { 5 }           
   ::= { hm2MgmtAccessTelnetGroup 4 }
      
hm2TelnetServerSessionsTimeOut OBJECT-TYPE
   SYNTAX Integer32 (0..160)
   MAX-ACCESS read-write
   STATUS current
   DESCRIPTION
      "Telnet login timeout (minutes)
      Config telnet timeout  will set the telnet session timeout value. 
      A session is active as long as the session has not remained idle for 
      the value set. Specify a value from 0 to 160.                     
      Note: Changing the timeout value for active 
      sessions does not become effective until the session is re-established."
   DEFVAL { 5 }           
   ::= { hm2MgmtAccessTelnetGroup 5 }

hm2TelnetTrapEnable  OBJECT-TYPE
    	SYNTAX      HmEnabledStatus
    	MAX-ACCESS  read-write
    	STATUS      current
    	DESCRIPTION
            	"Indicates whether login success, login failed or logout traps 
             	 should be generated for this application."
			DEFVAL { enable }             
    ::= { hm2MgmtAccessTelnetGroup 6 }

hm2TelnetLastLogoutUserName OBJECT-TYPE
        SYNTAX      SnmpAdminString (SIZE(0..32))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                    "User name of last logout for this application."
        ::= { hm2MgmtAccessTelnetGroup 7 }

hm2TelnetLastLoginUserName OBJECT-TYPE
        SYNTAX      SnmpAdminString (SIZE(0..32))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                    "User name of last login for this application."
        ::= { hm2MgmtAccessTelnetGroup 8 }

hm2TelnetLastLoginInetAddressType OBJECT-TYPE
        SYNTAX      InetAddressType 
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                    "InetAddressType of the last login used for this application."
        ::= { hm2MgmtAccessTelnetGroup 9 }

hm2TelnetLastLoginInetAddress OBJECT-TYPE
        SYNTAX      InetAddress 
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                    "IP address or DNS name specified in the last request for this application."
        ::= { hm2MgmtAccessTelnetGroup 10 }                  

--
-- *************************************************************
-- hm2MgmtAccessSsh
-- *************************************************************
--
hm2SshAdminStatus OBJECT-TYPE
        SYNTAX      	HmEnabledStatus
        MAX-ACCESS  	read-write
        STATUS      	current
        DESCRIPTION
			"Configures whether the SSH service is enabled on this switch.  The
            default value is enable(1)."
        DEFVAL { enable }
        ::= { hm2MgmtAccessSshGroup 1 }

hm2SshProtocolLevel OBJECT-TYPE
     SYNTAX      INTEGER {
                 ssh20(2) -- SSH 2.0
                 }
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
                 "Configures which protocol versions of SSH are enabled on this
      			  switch.  Currently only SSHv2 is supported."
     ::= { hm2MgmtAccessSshGroup 2 }

hm2SshPortNumber  	OBJECT-TYPE
   SYNTAX			InetPortNumber
   MAX-ACCESS 		read-write
   STATUS 			current
   DESCRIPTION 		"The port number of the SSH server.
                         Setting the port to zero is not allowed."
   DEFVAL 			{ 22 }           
   ::= { hm2MgmtAccessSshGroup 3 }


hm2SshSessionsCount OBJECT-TYPE
     SYNTAX      	Integer32
     MAX-ACCESS  	read-only
     STATUS      	current
     DESCRIPTION
                 "Current number of active SSH sessions on this switch."
     ::= { hm2MgmtAccessSshGroup 4 }

hm2SshMaxSessionsCount OBJECT-TYPE
	 SYNTAX       	Integer32 (1..5)
     MAX-ACCESS   	read-write
     STATUS       	current
     DESCRIPTION
                  "Max number of SSH sessions permitted on this switch.
                   The full range is not supported by all variants."
	 DEFVAL { 5 }                  
      ::= { hm2MgmtAccessSshGroup 5 }

hm2SshSessionTimeout OBJECT-TYPE
      SYNTAX       Integer32 (0..160)
      MAX-ACCESS   read-write
      STATUS       current
      DESCRIPTION
                  "SSH idle timeout value for this switch in minutes.
                   If the value is set to 0 the idle logout is disabled."
	  DEFVAL { 5 }                   
      ::= { hm2MgmtAccessSshGroup 6 }

hm2SshKeysPresent OBJECT-TYPE
     SYNTAX      INTEGER {
                 dsa(1),
                 rsa(2),
                 both(3),
                 none(4)
                 }
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
                 "Indicates what key files are present on the device, if any."
     ::= { hm2MgmtAccessSshGroup 7 }

hm2SshKeyOperStatus OBJECT-TYPE
        SYNTAX      INTEGER {
                    dsa(1),
                    rsa(2),
                    both(3),
                    none(4)
                    }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                    "Indicates what key files are currently being generated or deleted, if any."
        ::= { hm2MgmtAccessSshGroup 8 }

hm2SshRSAKeyControl OBJECT-TYPE
     SYNTAX      INTEGER {
                 noop(1),
                 generate(2),
                 delete(3)
                 }
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION
                 "Controls RSA key generation and deletion.  Always returns noop(1)."
     ::= { hm2MgmtAccessSshGroup 9 }

hm2SshDSAKeyControl OBJECT-TYPE
     SYNTAX      INTEGER {
                 noop(1),
                 generate(2),
                 delete(3)
                 }
     MAX-ACCESS  read-write
     STATUS      obsolete
     DESCRIPTION
                 "Controls DSA key generation and deletion.  Always returns noop(1)."
     ::= { hm2MgmtAccessSshGroup 10 }

hm2SshFingerPrintDSA  	OBJECT-TYPE
	 SYNTAX 		DisplayString (SIZE (0..128))
	 MAX-ACCESS		read-only
	 STATUS			obsolete
	 DESCRIPTION
		"The local DSA fingerprint for SSH connections."						
	 ::= { hm2MgmtAccessSshGroup 11 }

hm2SshFingerPrintRSA  	OBJECT-TYPE
	 SYNTAX 		DisplayString (SIZE (0..128))
	 MAX-ACCESS		read-only
	 STATUS			current
	 DESCRIPTION
		"The local RSA key fingerprint for SSH connections. The type of the hash is defined with hm2SshKeyFingerPrintType."
	 ::= { hm2MgmtAccessSshGroup 12 }

hm2SshTrapEnable  OBJECT-TYPE
    	SYNTAX      HmEnabledStatus
    	MAX-ACCESS  read-write
    	STATUS      current
    	DESCRIPTION
            	"Indicates whether login success, login failed or logout traps 
             	 should be generated for this application."
			DEFVAL { enable }             
    ::= { hm2MgmtAccessSshGroup 13 }

hm2SshLastLogoutUserName OBJECT-TYPE
        SYNTAX      SnmpAdminString (SIZE(0..32))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                    "User name of last logout for this application."
        ::= { hm2MgmtAccessSshGroup 14 }

hm2SshLastLoginUserName OBJECT-TYPE
        SYNTAX      SnmpAdminString (SIZE(0..32))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                    "User name of last login for this application."
        ::= { hm2MgmtAccessSshGroup 15 }

hm2SshLastLoginInetAddressType OBJECT-TYPE
        SYNTAX      InetAddressType 
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                    "InetAddressType of the last login used for this application."
        ::= { hm2MgmtAccessSshGroup 16 }

hm2SshLastLoginInetAddress OBJECT-TYPE
        SYNTAX      InetAddress 
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                    "IP address or DNS name specified in the last request for this application."
        ::= { hm2MgmtAccessSshGroup 17 }

hm2SshKeyFingerPrintType OBJECT-TYPE 
       SYNTAX INTEGER {
                   md5(1),
                   sha256(2)
                   }
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
          "Controls SSH key fingerprint display. If set to 'md5' SSH will show the MD5 fingerprint of a key."
      DEFVAL { sha256 }
     ::= { hm2MgmtAccessSshGroup 18 }

hm2SshHmacAlgorithms OBJECT-TYPE
      SYNTAX       Hm2SshHmacAlgorithms
      MAX-ACCESS   read-write
      STATUS       current
      DESCRIPTION
                   "The HMAC algorithms supported by the SSH server."
      DEFVAL       {{
      						hmac-sha1,
      						hmac-sha2-256,
      						hmac-sha1-etm-at-openssh-com,
      						hmac-sha2-256-etm-at-openssh-com
                   }}
      ::= { hm2MgmtAccessSshGroup 19 }

hm2SshKexAlgorithms OBJECT-TYPE
      SYNTAX       Hm2SshKexAlgorithms
      MAX-ACCESS   read-write
      STATUS       current
      DESCRIPTION
                   "The key exchange algorithms supported by the SSH server."
      DEFVAL       {{
      						diffie-hellman-group1-sha1,
							diffie-hellman-group14-sha1,
							diffie-hellman-group16-sha512,
							diffie-hellman-group18-sha512,
							diffie-hellman-group-exchange-sha256,
							ecdh-sha2-nistp256
                   }}
      ::= { hm2MgmtAccessSshGroup 20 }

hm2SshEncryptionAlgorithms OBJECT-TYPE
      SYNTAX       Hm2SshEncryptionAlgorithms
      MAX-ACCESS   read-write
      STATUS       current
      DESCRIPTION
                   "The encryption algorithms supported by the SSH server."
      DEFVAL       {{
      						aes128-ctr,
							aes128-gcm-at-openssh-com,
							chacha20-poly1305-at-openssh-com
                   }}
      ::= { hm2MgmtAccessSshGroup 21 }

-- *************************************************************
-- Outbound SSH client MIB objects
-- *************************************************************

hm2SshOutboundSessionsCount OBJECT-TYPE
     SYNTAX      	Integer32
     MAX-ACCESS  	read-only
     STATUS      	current
     DESCRIPTION
                 "Current number of active outbound SSH sessions from this switch."
     ::= { hm2MgmtAccessSshGroup 50 }
     
hm2SshOutboundMaxSessionsCount OBJECT-TYPE
	 SYNTAX       	Integer32 (1..5)
     MAX-ACCESS   	read-write
     STATUS       	current
     DESCRIPTION
                  "Max number of outbound SSH sessions permitted on this switch."
	 DEFVAL { 5 }                  
      ::= { hm2MgmtAccessSshGroup 51 }

hm2SshOutboundSessionTimeout OBJECT-TYPE
      SYNTAX       Integer32 (0..160)
      MAX-ACCESS   read-write
      STATUS       current
      DESCRIPTION
                  "SSH outbound idle timeout value for this switch in minutes.
                   If the value is set to 0 the idle logout is disabled."
	  DEFVAL { 5 }
        ::= { hm2MgmtAccessSshGroup 52 }

--
-- *************************************************************
-- hm2MgmtAccessPreLoginBannerGroup
-- *************************************************************
--

hm2PreLoginBannerAdminStatus	OBJECT-TYPE
	SYNTAX HmEnabledStatus
	MAX-ACCESS	read-write
	STATUS	current
	DESCRIPTION
				"Enables/disables the NERC CIP-005-1 R2.6 compliant use banner"
	DEFVAL  { disable }			
	::= { hm2MgmtAccessPreLoginBannerGroup 1 }
                                              
hm2PreLoginBannerText  OBJECT-TYPE
	 SYNTAX 		HmLargeDisplayString (SIZE (0..512))			 
	 MAX-ACCESS     read-write
	 STATUS			current
	 DESCRIPTION
	 			"The text added in this variable by the user will be displayed in
	 			 the system login page as banner before login into the CLI 
	 			 (local or remote) or before login into the web interface.
	 			 The default value is an empty string.
	 			 Special meaning have the sequences '\t' and '\n' which
	 			 allow the user to format the string with tabulator (\t) 
	 			 and newline (\n) format instructions. The use case is to provide a NERC 
	 			 CIP-005-1 R2.6 compliant use banner. The banner must be enabled using
	 			 hm2PreLoginBannerAdminStatus"
	 DEFVAL  { "" }                
	 ::= { hm2MgmtAccessPreLoginBannerGroup 2 }

--
-- *************************************************************
-- hm2MgmtAccessCliGroup
-- *************************************************************
--
hm2CliLoginPrompt OBJECT-TYPE
	SYNTAX 		DisplayString (SIZE(0..128))
	MAX-ACCESS 	read-write
	STATUS 		current
	DESCRIPTION 
	            "Prompt string for the command line interface."
	DEFVAL  { "" }				 
	::= { hm2MgmtAccessCliGroup 1 }

hm2CliLoginTimeoutSerial  OBJECT-TYPE
	SYNTAX 		Integer32 (0..160)
	MAX-ACCESS 	read-write
	STATUS 		current
	DESCRIPTION 
	            "Timeout for serial connections in minutes.
 	             If the value is set to 0, there will be 
 	             no idle logout at all."
	DEFVAL  { 5 }				 
	::= { hm2MgmtAccessCliGroup 3 }


hm2CliLoginBannerAdminStatus	OBJECT-TYPE
	SYNTAX HmEnabledStatus
	MAX-ACCESS	read-write
	STATUS	current
	DESCRIPTION
	"Enables/disables the display of the cli login banner text
	 instead of the standard login banner."
	DEFVAL  { disable }			
	::= { hm2MgmtAccessCliGroup 10  }


hm2CliLoginBannerText  OBJECT-TYPE
	 SYNTAX 		HmLargeDisplayString (SIZE (0..1024))			 
	 MAX-ACCESS     read-write
	 STATUS			current
	 DESCRIPTION
	 			"The text added in this variable by the user will be displayed in
	 			 the system login page (local or remote) instead of the systemoverview.
	 			 The default value is an empty string.
	 			 Special meaning have the sequences '\t' and '\n' which
	 			 allow the user to format the string with tabulator (\t) 
	 			 and newline (\n) format instructions.
	 			 The Banner must be enabled using CliLoginBannerAdminStatus."
	 DEFVAL  { "" }                
	 ::= { hm2MgmtAccessCliGroup 11 }

hm2ConsoleTrapEnable  OBJECT-TYPE
    	SYNTAX      HmEnabledStatus
    	MAX-ACCESS  read-write
    	STATUS      current
    	DESCRIPTION
            	"Indicates whether login success, login failed or logout traps 
             	 should be generated for console (V.24)."
			DEFVAL { enable }             
    ::= { hm2MgmtAccessCliGroup 12 }

hm2ConsoleLastLogoutUserName OBJECT-TYPE
        SYNTAX      SnmpAdminString (SIZE(0..32))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                    "User name of last logout for this application."
        ::= { hm2MgmtAccessCliGroup 13 }

hm2ConsoleLastLoginUserName OBJECT-TYPE
        SYNTAX      SnmpAdminString (SIZE(0..32))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                    "User name of last login for console (V.24)."
        ::= { hm2MgmtAccessCliGroup 14 }
        
hm2ConsoleServiceShellAdminState OBJECT-TYPE
        SYNTAX      HmEnabledStatus
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
                    "Admin State of service shell. (1=enable, 2=disable)."
        DEFVAL { enable }
        ::= { hm2MgmtAccessCliGroup 15 }

--
-- *************************************************************
-- hm2RestrictedMgmtAccessGroupTable
-- *************************************************************
--

hm2RmaTable OBJECT-TYPE
			SYNTAX SEQUENCE OF Hm2RmaEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION "A list of management access entries (rules) to increase security."
			::= { hm2RestrictedMgmtAccessGroup 1 }

hm2RmaEntry OBJECT-TYPE
			SYNTAX Hm2RmaEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION "An entry contains a rule for the management access."
			INDEX { hm2RmaIndex }
			::= { hm2RmaTable 1 }

Hm2RmaEntry ::= SEQUENCE {
				hm2RmaIndex 		Integer32,
				hm2RmaRowStatus 	RowStatus,
				hm2RmaIpAddrType 	InetAddressType,
				hm2RmaIpAddr 		InetAddress,
				hm2RmaPrefixLength	InetAddressPrefixLength,
				hm2RmaSrvHttp 		HmEnabledStatus,
				hm2RmaSrvHttps 		HmEnabledStatus,
				hm2RmaSrvSnmp 		HmEnabledStatus, 
				hm2RmaSrvTelnet 	HmEnabledStatus,
				hm2RmaSrvSsh 		HmEnabledStatus,
				hm2RmaSrvIEC61850   HmEnabledStatus,
				hm2RmaSrvModbusTcp  HmEnabledStatus,
				hm2RmaSrvEthernetIP HmEnabledStatus,
				hm2RmaSrvProfinetIO HmEnabledStatus 
			}

hm2RmaIndex OBJECT-TYPE
			SYNTAX Integer32 (1..16)
			MAX-ACCESS read-only
			STATUS current
			DESCRIPTION "The unique index used for each row in the RMA table."
			::= { hm2RmaEntry 1 }

hm2RmaRowStatus OBJECT-TYPE
			SYNTAX RowStatus
			MAX-ACCESS read-create
			STATUS current
			DESCRIPTION "Describes the status of a row in this table if it is active or not available."
			::= { hm2RmaEntry 2 }

hm2RmaIpAddrType OBJECT-TYPE
			SYNTAX InetAddressType
			MAX-ACCESS read-create
			STATUS current
			DESCRIPTION "Type of allowed IP address."
			DEFVAL { ipv4 }
			::= { hm2RmaEntry 3 }
			
hm2RmaIpAddr OBJECT-TYPE
			SYNTAX InetAddress
			MAX-ACCESS read-create
			STATUS current
			DESCRIPTION "Allowed IP address in IPv4 or IPv6 style."
			DEFVAL { '00000000'h }
			::= { hm2RmaEntry 4 }

hm2RmaPrefixLength OBJECT-TYPE
			SYNTAX InetAddressPrefixLength
			MAX-ACCESS read-create
			STATUS current
			DESCRIPTION "The length of the IP netmask."  
			DEFVAL { 0 }
			::= { hm2RmaEntry 5 }

hm2RmaSrvHttp OBJECT-TYPE
			SYNTAX HmEnabledStatus
			MAX-ACCESS read-create
			STATUS current
			DESCRIPTION "Enables/disables HTTP access."
			DEFVAL { enable }
			::= { hm2RmaEntry 6 }

hm2RmaSrvHttps OBJECT-TYPE
			SYNTAX HmEnabledStatus
			MAX-ACCESS read-create
			STATUS current
			DESCRIPTION "Enables/disables HTTPS access."
			DEFVAL { enable }
			::= { hm2RmaEntry 7 }

hm2RmaSrvSnmp OBJECT-TYPE
			SYNTAX HmEnabledStatus
			MAX-ACCESS read-create
			STATUS current
			DESCRIPTION "Enables/disbales SNMP access."
			DEFVAL { enable }
			::= { hm2RmaEntry 8 }

hm2RmaSrvTelnet OBJECT-TYPE
			SYNTAX HmEnabledStatus
			MAX-ACCESS read-create
			STATUS current
			DESCRIPTION "Enables/disables telnet access."
			DEFVAL { enable }
			::= { hm2RmaEntry 9 }

hm2RmaSrvSsh OBJECT-TYPE
			SYNTAX HmEnabledStatus
			MAX-ACCESS read-create
			STATUS current
			DESCRIPTION "Enables/disables SSH access."
			DEFVAL { enable }
			::= { hm2RmaEntry 10 }

hm2RmaSrvIEC61850 OBJECT-TYPE
			SYNTAX HmEnabledStatus
			MAX-ACCESS read-create
			STATUS current
			DESCRIPTION "Enables/disables IEC61850-MMS access."
			DEFVAL { enable }
			::= { hm2RmaEntry 11 }

hm2RmaSrvModbusTcp OBJECT-TYPE
			SYNTAX HmEnabledStatus
			MAX-ACCESS read-create
			STATUS current
			DESCRIPTION "Enables/disables Modbus/TCP access."
			DEFVAL { enable }
			::= { hm2RmaEntry 12 }

hm2RmaSrvEthernetIP OBJECT-TYPE
			SYNTAX HmEnabledStatus
			MAX-ACCESS read-create
			STATUS current
			DESCRIPTION "Enables/disables EtherNet/IP access."
			DEFVAL { enable }
			::= { hm2RmaEntry 13 }

hm2RmaSrvProfinetIO OBJECT-TYPE
			SYNTAX HmEnabledStatus
			MAX-ACCESS read-create
			STATUS current
			DESCRIPTION "Enables/disables PROFINET access."
			DEFVAL { enable }
			::= { hm2RmaEntry 14 }

--
-- *************************************************************
-- hm2RestrictedMgmtAccessGroup Objects
-- *************************************************************
--

hm2RmaOperation OBJECT-TYPE
			SYNTAX HmEnabledStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION "Enables/disables management access globally."
			DEFVAL { disable }
			::= { hm2RestrictedMgmtAccessGroup 2 }

--
-- *************************************************************
-- hm2MgmtAccessStatisticsGroup
-- *************************************************************
--

hm2HttpPacketsSent				OBJECT-TYPE
    		SYNTAX      Counter64
    		MAX-ACCESS  read-only
    		STATUS      current
    		DESCRIPTION
            		"Number of HTTP management packets sent."
    		::= { hm2MgmtAccessStatisticsGroup 1 }

hm2HttpPacketsReceived			OBJECT-TYPE
    		SYNTAX      Counter64
    		MAX-ACCESS  read-only
    		STATUS      current
    		DESCRIPTION
            		"Number of HTTP management packets received."
    		::= { hm2MgmtAccessStatisticsGroup 2 }

hm2HttpsPacketsSent				OBJECT-TYPE
    		SYNTAX      Counter64
    		MAX-ACCESS  read-only
    		STATUS      current
    		DESCRIPTION
            		"Number of HTTPS management packets sent."
    		::= { hm2MgmtAccessStatisticsGroup 3 }

hm2HttpsPacketsReceived			OBJECT-TYPE
    		SYNTAX      Counter64
    		MAX-ACCESS  read-only
    		STATUS      current
    		DESCRIPTION
            		"Number of HTTPS management packets received."
    		::= { hm2MgmtAccessStatisticsGroup 4 }

hm2TelnetPacketsSent			OBJECT-TYPE
    		SYNTAX      Counter64
    		MAX-ACCESS  read-only
    		STATUS      current
    		DESCRIPTION
            		"Number of Telnet management packets sent."
    		::= { hm2MgmtAccessStatisticsGroup 5 }

hm2TelnetPacketsReceived		OBJECT-TYPE
    		SYNTAX      Counter64
    		MAX-ACCESS  read-only
    		STATUS      current
    		DESCRIPTION
            		"Number of Telnet management packets received."
    		::= { hm2MgmtAccessStatisticsGroup 6 }

hm2SshPacketsSent				OBJECT-TYPE
    		SYNTAX      Counter64
    		MAX-ACCESS  read-only
    		STATUS      current
    		DESCRIPTION
            		"Number of SSH management packets sent."
    		::= { hm2MgmtAccessStatisticsGroup 7 }

hm2SshPacketsReceived			OBJECT-TYPE
    		SYNTAX      Counter64
    		MAX-ACCESS  read-only
    		STATUS      current
    		DESCRIPTION
            		"Number of SSH management packets received."
    		::= { hm2MgmtAccessStatisticsGroup 8 }

-- *************************************************************
-- hm2MgmtAccessMibNotifications 
-- *************************************************************
--
	hm2WebLoginSuccessTrap NOTIFICATION-TYPE
		OBJECTS	{ hm2WebLastLoginUserName, hm2WebLastLoginInetAddressType, hm2WebLastLoginInetAddress}
		STATUS  current
		DESCRIPTION "This trap is sent if a user successfully grants access via web to the device. 
		             hm2WebLastLoginInetAddress contains the IP address or DNS name of the login request. 
		             hm2WebLastLoginUserName contains the user name of the last user who logged in 
					 into the device."
		::= { hm2MgmtAccessMibNotifications 1 }
	
	hm2WebLoginFailedTrap NOTIFICATION-TYPE
		OBJECTS	{ hm2WebLastLoginUserName, hm2WebLastLoginInetAddressType, hm2WebLastLoginInetAddress}
		STATUS  current
		DESCRIPTION "This trap is sent if a user tried to grant access via web to the device. 
					 hm2WebLastLoginInetAddress contains the IP address or the DNS name of the login request.
					 hm2WebLastLoginUserName contains the user name of the user who tried to 
					 login into the device."
		::= { hm2MgmtAccessMibNotifications 2 }
		
	hm2WebLogoutTrap NOTIFICATION-TYPE
		OBJECTS	{ hm2WebLastLogoutUserName }
		STATUS  current
		DESCRIPTION "This trap is sent when a user logs out a web session.
					 hm2WebLastLogoutUserName contains the user name of the last user who logged out of the device."
		::= { hm2MgmtAccessMibNotifications 3 }		

	hm2TelnetLoginSuccessTrap NOTIFICATION-TYPE
		OBJECTS	{ hm2TelnetLastLoginUserName, hm2TelnetLastLoginInetAddressType, hm2TelnetLastLoginInetAddress}
		STATUS  current
		DESCRIPTION "This trap is sent if a user successfully grants access via telnet to the device. 
		             hm2TelnetLoginLastInetAddress contains the IP address	or DNS name of the login request. 
		             hm2TelnetLastLoginUserName contains the user name of the last user who logged in 
					 into the device."
		::= { hm2MgmtAccessMibNotifications 4 }
	
	hm2TelnetLoginFailedTrap NOTIFICATION-TYPE
		OBJECTS	{ hm2TelnetLastLoginUserName, hm2TelnetLastLoginInetAddressType, hm2TelnetLastLoginInetAddress}
		STATUS  current
		DESCRIPTION "This trap is sent if a user tried to grant access via telnet to the device. 
					 hm2TelnetLastLoginInetAddress contains the IP address or the DNS name of the login request.
					 hm2TelnetLastLoginUserName contains the user name of the last user who tried to 
					 log in into the device."
		::= { hm2MgmtAccessMibNotifications 5 }
		
	hm2TelnetLogoutTrap NOTIFICATION-TYPE
		OBJECTS	{ hm2TelnetLastLogoutUserName }
		STATUS  current
		DESCRIPTION "This trap is sent when a user logs out a telnet session.
					 hm2TelnetLastLogoutUserName contains the user name of the last user who logged out of the device."
		::= { hm2MgmtAccessMibNotifications 6 }		

	hm2SshLoginSuccessTrap NOTIFICATION-TYPE
		OBJECTS	{ hm2SshLastLoginUserName, hm2SshLastLoginInetAddressType, hm2SshLastLoginInetAddress}
		STATUS  current
		DESCRIPTION "This trap is sent if a user successfully grants access via SSH to the device. 
		             hm2SshLastLoginInetAddress contains the IP address or DNS name of the login request. 
		             hm2SshLastLoginUserName contains the user name of the last user logged in  
					 into the device."
		::= { hm2MgmtAccessMibNotifications 7 }
	
	hm2SshLoginFailedTrap NOTIFICATION-TYPE
		OBJECTS	{ hm2SshLastLoginUserName, hm2SshLastLoginInetAddressType, hm2SshLastLoginInetAddress}
		STATUS  current
		DESCRIPTION "This trap is sent if a user tried to grant access via SSH to the device. 
					 hm2SshLastLoginInetAddress contains the IP address or the DNS name of the login request.
					 hm2SshLastLoginUserName contains the user name of the last user who tried to 
					 login into the device."
		::= { hm2MgmtAccessMibNotifications 8 }
		
	hm2SshLogoutTrap NOTIFICATION-TYPE
		OBJECTS	{ hm2SshLastLogoutUserName }
		STATUS  current
		DESCRIPTION "This trap is sent when a user logs out a SSH session.
					 hm2SshLastLogoutUserName contains the user name of the last user who logged out of the device."
		::= { hm2MgmtAccessMibNotifications 9 }				

	hm2ConsoleLoginSuccessTrap NOTIFICATION-TYPE
		OBJECTS	{ hm2ConsoleLastLoginUserName }
		STATUS  current
		DESCRIPTION "This trap is sent if a user successfully grants access via console (V.24) to the device. 
		             hm2ConsoleLastLoginUserName contains the user name of the last user who logged in  
					 into the device."
		::= { hm2MgmtAccessMibNotifications 10 }
	
	hm2ConsoleLoginFailedTrap NOTIFICATION-TYPE
		OBJECTS	{ hm2ConsoleLastLoginUserName }
		STATUS  current
		DESCRIPTION "This trap is sent if a user tried to grant access via console (V.24) to the device. 
					 hm2ConsoleLastLoginUserName contains the user name of the last user who tried to login  
					 into the device."
		::= { hm2MgmtAccessMibNotifications 11 }
		
	hm2ConsoleLogoutTrap NOTIFICATION-TYPE
		OBJECTS	{ hm2ConsoleLastLogoutUserName }
		STATUS  current
		DESCRIPTION "This trap is sent when a user logs out a console (V.24) session.
					 hm2ConsoleLastLogoutUserName contains the user name of the last user who logged out of the device."
		::= { hm2MgmtAccessMibNotifications 12 }				

-- ***********************************************************
-- hm2MgmtAccessMibSNMPExtensionGroup
-- ***********************************************************
hm2MgmtAccessSnmpSESGroup 			OBJECT IDENTIFIER ::= { hm2MgmtAccessMibSNMPExtensionGroup 1 }
hm2MgmtAccessWebSESGroup 			OBJECT IDENTIFIER ::= { hm2MgmtAccessMibSNMPExtensionGroup 2 }
hm2MgmtAccessTelnetSESGroup	 		OBJECT IDENTIFIER ::= { hm2MgmtAccessMibSNMPExtensionGroup 3 }
hm2MgmtAccessSshSESGroup	 		OBJECT IDENTIFIER ::= { hm2MgmtAccessMibSNMPExtensionGroup 4 }
hm2MgmtAccessPreLoginBannerSESGroup	OBJECT IDENTIFIER ::= { hm2MgmtAccessMibSNMPExtensionGroup 5 }
hm2MgmtAccessCliSESGroup	 		OBJECT IDENTIFIER ::= { hm2MgmtAccessMibSNMPExtensionGroup 6 }
hm2RestrictedMgmtAccessSESGroup	 	OBJECT IDENTIFIER ::= { hm2MgmtAccessMibSNMPExtensionGroup 7 }

-- ***********************************************************
-- hm2MgmtAccessWebSESGroup
-- ***********************************************************
hm2MgmtAccessWebSESCertGenInProgress OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION 
           		"Indicates that the certificate generation is already in progress."
           ::= { hm2MgmtAccessWebSESGroup 1 }

hm2MgmtAccessWebSESCertNotPresent OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION 
           		"Indicates that no certificate is available."
           ::= { hm2MgmtAccessWebSESGroup 2 }

-- ***********************************************************
-- hm2MgmtAccessSshSESGroup
-- ***********************************************************
hm2MgmtAccessSshSESServerEnabled OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION 
           		"Indicates that the SSH server is running."
           ::= { hm2MgmtAccessSshSESGroup 1 }

hm2MgmtAccessSshSESKeyGenInProgress OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION 
           		"Indicates that the SSH key generation is in progress."
           ::= { hm2MgmtAccessSshSESGroup 2 }

hm2MgmtAccessSshSESKeyNotAvailable  OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION 
           		"Indicates that the SSH key is not available."
           ::= { hm2MgmtAccessSshSESGroup 3 }           

END
