
HM2-TC-MIB DEFINITIONS ::= BEGIN

--
-- *************************************************************
-- Hirschmann TEXTUAL-CONVENTIONs MIB
-- *************************************************************
--

IMPORTS
    MODULE-IDENTITY, enterprises, Unsigned32
        FROM SNMPv2-SMI -- RFC 2578
    TEXTUAL-CONVENTION
        FROM SNMPv2-TC; -- RFC 2579

hm2TcMib MODULE-IDENTITY
	LAST-UPDATED "201103160000Z" -- March 16, 2011
    ORGANIZATION "Hirschmann Automation and Control GmbH"
    CONTACT-INFO
        "Postal:     Stuttgarter Str. 45-51
                     72654 Neckartenzlingen
                     Germany
         Phone:      +49 7127 140
         E-mail:     hac.support@belden.com"
    DESCRIPTION
        "Textual conventions used throughout the various Hirschmann MIB modules.
         Copyright (C) 2011. All Rights Reserved."
    REVISION     "201103160000Z" -- March 16, 2011
    DESCRIPTION
         "Initial version."
    ::= { hm2ConfigurationMibs 1 }

hirschmann					  OBJECT IDENTIFIER ::= { enterprises 248 }
hm2ConfigurationMibs 		  OBJECT IDENTIFIER ::= { hirschmann 11 }
hm2PlatformMibs	 		  	  OBJECT IDENTIFIER ::= { hirschmann 12 }

--
-- *************************************************************
-- Textual Conventions
-- *************************************************************
--

HmEnabledStatus ::= TEXTUAL-CONVENTION
    STATUS       current
    DESCRIPTION  "Status of a feature"
    SYNTAX       INTEGER { 
					        enable(1),      -- feature is enabled
        					disable(2)      -- feature is disabled
        				 }

HmActionValue ::= TEXTUAL-CONVENTION
    STATUS       current
    DESCRIPTION  "Trigger a action on the device.
    			  Reading the variable normally returns noop.
    			  The processing state and the termination result can be monitored with SNMP Protocol Extension MIB."
    SYNTAX       INTEGER { 
					        noop(1),        -- no operation ongoing
        					action(2)       -- trigger the action specified by the variable
        				 }

HmTimeHHMM24 ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "5a"    
    STATUS       current
    DESCRIPTION  "The time in hh:mm format:
                   range for hh: 0 to 23
                   range for mm: 0 to 59"
    SYNTAX       OCTET STRING (SIZE(0..5))

HmTimeSeconds1970 ::= TEXTUAL-CONVENTION
    STATUS       current
    DESCRIPTION  "Time in seconds since Jan, 1st, 1970."
    SYNTAX       Unsigned32
    
HmLargeDisplayString ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "1024a"
    STATUS       current
    DESCRIPTION
            "Represents textual information taken from the NVT ASCII
            character set, as defined in pages 4, 10-11 of RFC 854.

            To summarize RFC 854, the NVT ASCII repertoire specifies:

              - the use of character codes 0-127 (decimal)

              - the graphics characters (32-126) are interpreted as
                US ASCII

              - NUL, LF, CR, BEL, BS, HT, VT and FF have the special
                meanings specified in RFC 854

              - the other 25 codes have no standard interpretation

              - the sequence 'CR LF' means newline

              - the sequence 'CR NUL' means carriage-return

              - an 'LF' not preceded by a 'CR' means moving to the
                same column on the next line.

              - the sequence 'CR x' for any x other than LF or NUL is
                illegal.  (Note that this also means that a string may
                end with either 'CR LF' or 'CR NUL', but not with CR.)

            Any object defined using this syntax may not exceed 2048
            characters in length."
    SYNTAX       OCTET STRING (SIZE (0..1024))
    
HmAccessLevel ::= TEXTUAL-CONVENTION
    STATUS        current
    DESCRIPTION   "Access level for the item."
    SYNTAX        INTEGER {
                            readWrite (1),
                            readOnly (2)
                          }

END

