HM2-TRACKING-MIB   DEFINITIONS ::= BEGIN

IMPORTS
	hm2ConfigurationMibs, 
	HmTimeSeconds1970,
	HmEnabledStatus						FROM HM2-TC-MIB
    MODULE-IDENTITY,
    OBJECT-TYPE, NOTIFICATION-TYPE,
    Integer32							FROM SNMPv2-SMI    
    InetAddress, InetAddressType        FROM INET-ADDRESS-MIB                        
    RowStatus							FROM SNMPv2-TC
    SnmpAdminString     				FROM SNMP-FRAMEWORK-MIB
    inetCidrRouteEntry					FROM IP-FORWARD-MIB
    InterfaceIndexOrZero			    FROM IF-MIB;



hm2TrackingMib MODULE-IDENTITY
        LAST-UPDATED "201309031200Z" -- 3 Sep 2013 12:00:00 GMT
        ORGANIZATION "Hirschmann Automation and Control GmbH"
        CONTACT-INFO
          "Customer Support
           Postal: 
           Hirschmann Automation and Control GmbH
           Stuttgarter Str. 45-51
           72654 Neckartenzlingen
           Germany
           Tel: +49 7127 14 1981
           Web: http://www.hicomcenter.com/
           E-Mail: hicomcenter@hirschmann.com"
        DESCRIPTION
          "The Hirschmann Private Tracking MIB definitions for Platform devices."

        -- Revision history.
        REVISION
          "201309031200Z" -- 3 Sep 2013 12:00:00 GMT
        DESCRIPTION
          "Initial Version"     
        ::= { hm2ConfigurationMibs 115 }


--
-- *************************************************************
-- hm2TrackingMib
-- *************************************************************
--        

hm2TrackingMibNotifications   OBJECT IDENTIFIER ::= { hm2TrackingMib 0 }
hm2TrackingMibObjects   OBJECT IDENTIFIER ::= { hm2TrackingMib 1 }


--
-- *************************************************************
-- hm2TrackingMibNotifications
-- *************************************************************
--  


hm2TrackStatusChangeEvent NOTIFICATION-TYPE
	OBJECTS	{hm2TrackType, hm2TrackId, hm2TrackStatus, hm2TrackOperState }
	STATUS  current
    DESCRIPTION
         "Sent when the state of a tracking instance changes between up and down."
	::= { hm2TrackingMibNotifications 1 }

            

--
-- *************************************************************
-- hm2TrackingMib groups
-- *************************************************************
--


hm2TrackingConfigGroup   		OBJECT IDENTIFIER ::= { hm2TrackingMibObjects 1 }
hm2TrackingInterfaceGroup   	OBJECT IDENTIFIER ::= { hm2TrackingMibObjects 2 }
hm2TrackingPingGroup   			OBJECT IDENTIFIER ::= { hm2TrackingMibObjects 3 }
hm2TrackingLogicalGroup   		OBJECT IDENTIFIER ::= { hm2TrackingMibObjects 4 }
hm2TrackingApplicationGroup   	OBJECT IDENTIFIER ::= { hm2TrackingMibObjects 5 }
hm2TrackingStaticRouteGroup   	OBJECT IDENTIFIER ::= { hm2TrackingMibObjects 6 }
hm2TrackingSNMPExtensionGroup 	OBJECT IDENTIFIER ::= { hm2TrackingMibObjects 7 }

--
-- *************************************************************
-- hm2TrackingConfigGroup
-- *************************************************************
--

hm2TrackingConfigTable OBJECT-TYPE
                SYNTAX          SEQUENCE OF Hm2TrackingConfigEntry
                MAX-ACCESS      not-accessible
                STATUS          current
                DESCRIPTION     "Tracking configuration table.
                				 This table provides the interface to setup a 
                				 specific tracking instance in the tracking database."
                ::= { hm2TrackingConfigGroup 1 }

hm2TrackingConfigEntry OBJECT-TYPE
                SYNTAX          Hm2TrackingConfigEntry
                MAX-ACCESS      not-accessible
                STATUS          current
                DESCRIPTION     "The entry of the hm2TrackingConfigTable."
                INDEX           { hm2TrackType, hm2TrackId }
                ::= { hm2TrackingConfigTable 1 }

Hm2TrackingConfigEntry ::= SEQUENCE {
				hm2TrackType		        	INTEGER,
                hm2TrackId 						Integer32,
                hm2TrackName					SnmpAdminString,
                hm2TrackDescription				SnmpAdminString,
                hm2TrackOperState				INTEGER,
                hm2TrackNumberOfChanges			Integer32,
                hm2TrackTimeLastChange			HmTimeSeconds1970,
                hm2TrackSendStateChangeTrap 	HmEnabledStatus,
                hm2TrackStatus					RowStatus
}

hm2TrackType	OBJECT-TYPE
                SYNTAX          INTEGER {
                					interface(1),
                					ping(2),
                					logical(3)
                				}
                MAX-ACCESS      accessible-for-notify
                STATUS          current
                DESCRIPTION     "The kind of an object being tracked."
                ::= { hm2TrackingConfigEntry 1 }


hm2TrackId		OBJECT-TYPE
                SYNTAX          Integer32 (1..256)
                MAX-ACCESS      accessible-for-notify
                STATUS          current
                DESCRIPTION     "The id of an object being tracked."
                ::= { hm2TrackingConfigEntry 2 }


hm2TrackName	OBJECT-TYPE
                SYNTAX          SnmpAdminString
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION     "The name of an object being tracked."
                ::= { hm2TrackingConfigEntry 3 }

hm2TrackDescription		OBJECT-TYPE
                SYNTAX          SnmpAdminString
                MAX-ACCESS      read-create
                STATUS          current
                DESCRIPTION     "The name of an object being tracked."
                ::= { hm2TrackingConfigEntry 4 }
                              
hm2TrackOperState	OBJECT-TYPE
                SYNTAX          INTEGER {
                					up(1),
                					down(2),
                					notReady(3)
                				}
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION     "Shows if the tracked object is currently up(1), down(2) or notReady(3).
                				 in case the state indicates notReady, the corresponding configuration
                				 is missing or invalid."
                DEFVAL			{ notReady }
                ::= { hm2TrackingConfigEntry 5 }
                
                
hm2TrackNumberOfChanges
				OBJECT-TYPE
                SYNTAX          Integer32
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION     "The number of state changes after an object being
								tracked, entered its operational state.
								If the current state was entered prior to the last
                      			re-initialization of the local network management
                      			subsystem, then this object contains a zero
                      			value."
                ::= { hm2TrackingConfigEntry 6 }                

hm2TrackTimeLastChange
				OBJECT-TYPE
                SYNTAX          HmTimeSeconds1970
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION     "The time of the last state change of an object being
                      			tracked, measured in seconds since 00:00:00, January 1, 1970.
                      			If the current state was entered prior to the last
                      			re-initialization of the local network management
                      			subsystem, then this object contains the time the system was re-initialized. 
                      			value."
                ::= { hm2TrackingConfigEntry 7 }
 
hm2TrackSendStateChangeTrap	OBJECT-TYPE
                SYNTAX          HmEnabledStatus
                MAX-ACCESS      read-create
                STATUS          current
                DESCRIPTION     "Enables or disables the sending of a trap when hm2TrackStatus changes"
                DEFVAL			{ disable }
                ::= { hm2TrackingConfigEntry 8 }
 
                
hm2TrackStatus
				OBJECT-TYPE
                SYNTAX          RowStatus
                MAX-ACCESS      read-create
                STATUS          current
                DESCRIPTION     "Defines the status of the tracking database entry.
                				 Set to createAndWait(5) to create a new row.
                				 Set to destroy(6) to delete an entry.
                				 Reads as active(1) if the tracked object exists and is trackable,
                				 notReady(3) otherwise."
                ::= { hm2TrackingConfigEntry 9 }
                
--
-- *************************************************************
-- hm2TrackingInterfaceGroup
-- *************************************************************
--

hm2TrackingInterfaceTable OBJECT-TYPE
                SYNTAX          SEQUENCE OF Hm2TrackingInterfaceEntry
                MAX-ACCESS      not-accessible
                STATUS          current
                DESCRIPTION     "Interface tracking configuration table.
                				 This table provides the interface to setup the parameters
                				 for an interface tracking object."  
                ::= { hm2TrackingInterfaceGroup 1 }

hm2TrackingInterfaceEntry OBJECT-TYPE
                SYNTAX          Hm2TrackingInterfaceEntry
                MAX-ACCESS      not-accessible
                STATUS          current
                DESCRIPTION     "The entry of the hm2TrackingInterfaceTable."
                INDEX           { hm2TrackInterfaceId }
                ::= { hm2TrackingInterfaceTable 1 }

Hm2TrackingInterfaceEntry ::= SEQUENCE {
                hm2TrackInterfaceId 			Integer32,
                hm2TrackIfNumber        		InterfaceIndexOrZero,
                hm2TrackIfLinkUpDelay    		Integer32,
                hm2TrackIfLinkDownDelay  		Integer32
				}

hm2TrackInterfaceId
				OBJECT-TYPE
                SYNTAX          Integer32 
                MAX-ACCESS      not-accessible
                STATUS          current
                DESCRIPTION     "The identifier of the interface object being tracked."
                ::= { hm2TrackingInterfaceEntry 1 }

hm2TrackIfNumber
				OBJECT-TYPE
                SYNTAX          InterfaceIndexOrZero
                MAX-ACCESS      read-write
                STATUS          current
                DESCRIPTION     "The number of the interface being tracked."
                DEFVAL			{ 0 }
                ::= { hm2TrackingInterfaceEntry 2 }
                

hm2TrackIfLinkUpDelay		
				OBJECT-TYPE
                SYNTAX          Integer32 (0..255)
                UNITS			"seconds"
                MAX-ACCESS      read-write
                STATUS          current
                DESCRIPTION     "If a link-up recovers within this delay,
								the tracked object is not considered as up."
				DEFVAL			{ 0 }
                ::= { hm2TrackingInterfaceEntry 3 }
                
                
hm2TrackIfLinkDownDelay		
				OBJECT-TYPE
                SYNTAX          Integer32 (0..255)
                UNITS			"seconds"
                MAX-ACCESS      read-write
                STATUS          current
                DESCRIPTION     "If a link-down recovers within this delay,
								the tracked object is not considered as down."
				DEFVAL			{ 0 }
                ::= { hm2TrackingInterfaceEntry 4 }


--
-- *************************************************************
-- hm2TrackingPingGroup
-- *************************************************************
--

hm2TrackingPingTable OBJECT-TYPE
                SYNTAX          SEQUENCE OF Hm2TrackingPingEntry
                MAX-ACCESS      not-accessible
                STATUS          current
                DESCRIPTION     "Ping tracking configuration table.
                				 This table provides the interface to setup the parameters
                				 for a ping tracking object."  
                ::= { hm2TrackingPingGroup 1 }

hm2TrackingPingEntry OBJECT-TYPE
                SYNTAX          Hm2TrackingPingEntry
                MAX-ACCESS      not-accessible
                STATUS          current
                DESCRIPTION     "The entry of the hm2TrackingPingTable."
                INDEX           { hm2TrackPingId }
                ::= { hm2TrackingPingTable 1 }

Hm2TrackingPingEntry ::= SEQUENCE {
                hm2TrackPingId 					Integer32,
                hm2TrackPingIfNumber      		InterfaceIndexOrZero,
                hm2TrackPingInetAddrType 		InetAddressType,
                hm2TrackPingInetAddr   			InetAddress,
                hm2TrackPingInterval     		Integer32,
                hm2TrackPingMiss         		Integer32,
                hm2TrackPingSuccess     		Integer32,
                hm2TrackPingTimeout      		Integer32,
                hm2TrackPingTTL					Integer32,
                hm2TrackPingBestRouteIfNumber 	InterfaceIndexOrZero
}

hm2TrackPingId
				OBJECT-TYPE
                SYNTAX          Integer32 
                MAX-ACCESS      not-accessible
                STATUS          current
                DESCRIPTION     "The identifier of the ping object being tracked."
                ::= { hm2TrackingPingEntry 1 }

hm2TrackPingIfNumber
				OBJECT-TYPE
                SYNTAX          InterfaceIndexOrZero
                MAX-ACCESS      read-write
                STATUS          current
                DESCRIPTION     "The number of the source interface, the ping packets are sent.
                				 A value of Zero (0) indicates that no interface is configured."
                DEFVAL			{ 0 }
                ::= { hm2TrackingPingEntry 2 }

hm2TrackPingInetAddrType
				OBJECT-TYPE
                SYNTAX          InetAddressType
                MAX-ACCESS      read-write
                STATUS          current
                DESCRIPTION     "The address type of the router being monitored."
                ::= { hm2TrackingPingEntry 3 }

hm2TrackPingInetAddr
				OBJECT-TYPE
                SYNTAX          InetAddress
                MAX-ACCESS      read-write
                STATUS          current
                DESCRIPTION     "The address of the router being monitored."
                ::= { hm2TrackingPingEntry 4 }

                
hm2TrackPingInterval
				OBJECT-TYPE
                SYNTAX          Integer32 (100..20000)
                UNITS			"milliseconds"
                MAX-ACCESS      read-write
                STATUS          current
                DESCRIPTION     "The number of milliseconds between the pings to the
								target router address."
				DEFVAL			{ 1000 }
                ::= { hm2TrackingPingEntry 5 }

hm2TrackPingMiss
				OBJECT-TYPE
                SYNTAX          Integer32 (1..10)
                MAX-ACCESS      read-write
                STATUS          current
                DESCRIPTION     "This specifies the number of consecutive ping
								misses until the tracked object is considered
								to be down."
				DEFVAL			{ 3 }
                ::= { hm2TrackingPingEntry 6 }

                
hm2TrackPingSuccess
				OBJECT-TYPE
                SYNTAX          Integer32 (1..10)
                MAX-ACCESS      read-write
                STATUS          current
                DESCRIPTION     "This specifies the number of consecutive ping
								successes until the tracked object is considered
								to be up."
				DEFVAL			{ 2 }
                ::= { hm2TrackingPingEntry 7 }
                
hm2TrackPingTimeout
				OBJECT-TYPE
                SYNTAX          Integer32 (10..10000)
                UNITS			"milliseconds"
                MAX-ACCESS      read-write
                STATUS          current
                DESCRIPTION     "This specifies the timeout in milliseconds for
                				 a ping reply. After the timeout the ping reply
                				 is considered as lost."
				DEFVAL			{ 100 }
                ::= { hm2TrackingPingEntry 8 }

hm2TrackPingTTL
				OBJECT-TYPE
                SYNTAX          Integer32 (1..255)
                MAX-ACCESS      read-write
                STATUS          current
                DESCRIPTION     "This specifies the time to live for a ping request
                				 packet."
				DEFVAL			{ 128 }
                ::= { hm2TrackingPingEntry 9 }

hm2TrackPingBestRouteIfNumber
				OBJECT-TYPE
                SYNTAX          InterfaceIndexOrZero
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION     "This shows the number of the interface which
                				 belongs to the best route. The interface number
                				 is zero if the best route is not used to send
                				 ping packets."
                ::= { hm2TrackingPingEntry 10 }



--
-- *************************************************************
-- hm2TrackingLogicalGroup
-- *************************************************************
--

hm2TrackLogicalInstanceTable
				OBJECT-TYPE
                SYNTAX          SEQUENCE OF Hm2TrackLogicalInstanceEntry
                MAX-ACCESS      not-accessible
                STATUS          current
                DESCRIPTION     "This table contains the configuration of the tracking
                				 instances that are combined into logical
                				 tracking instances."
                ::= { hm2TrackingLogicalGroup 1 }


hm2TrackLogicalInstanceEntry 
				OBJECT-TYPE
                SYNTAX          Hm2TrackLogicalInstanceEntry
                MAX-ACCESS      not-accessible
                STATUS          current
                DESCRIPTION     "The entry of the hm2TrackLogicalInstanceTable."
                INDEX           { hm2TrackLogicalId}
                ::= { hm2TrackLogicalInstanceTable 1 }


Hm2TrackLogicalInstanceEntry ::= SEQUENCE {
                hm2TrackLogicalId				Integer32,
                hm2TrackLogicalOperandNameA		SnmpAdminString,
                hm2TrackLogicalOperandNameB		SnmpAdminString,
                hm2TrackLogicalOperator			INTEGER
                }

hm2TrackLogicalId
				OBJECT-TYPE
                SYNTAX          Integer32
                MAX-ACCESS      not-accessible
                STATUS          current
                DESCRIPTION     "The identifier of the logical object being tracked."
                ::= { hm2TrackLogicalInstanceEntry 1 }

hm2TrackLogicalOperandNameA	OBJECT-TYPE
                SYNTAX          SnmpAdminString
                MAX-ACCESS      read-write
                STATUS          current
                DESCRIPTION     "The name of the tracking object to be used as operand A in the logical operation: A operator B."
                ::= { hm2TrackLogicalInstanceEntry 2 }
                
hm2TrackLogicalOperandNameB	OBJECT-TYPE
                SYNTAX          SnmpAdminString
                MAX-ACCESS      read-write
                STATUS          current
                DESCRIPTION     "The name of the tracking object to be used as operand B in the logical operation: A operator B."
                ::= { hm2TrackLogicalInstanceEntry 3 }                

hm2TrackLogicalOperator	OBJECT-TYPE
                SYNTAX          INTEGER {
                					and(1),
                					or(2)
                				}
                MAX-ACCESS      read-write
                STATUS          current
                DESCRIPTION     "Defines the logical operation performed on the configured operands A and B."
                DEFVAL			{ or }
                ::= { hm2TrackLogicalInstanceEntry 4 }


--
-- *************************************************************
-- hm2TrackingApplicationGroup
-- *************************************************************
--

hm2TrackingApplicationTable
				OBJECT-TYPE
                SYNTAX          SEQUENCE OF Hm2TrackingApplicationEntry
                MAX-ACCESS      not-accessible
                STATUS          current
                DESCRIPTION     "This table contains information about registered
                				 applications, for each object being tracked."
                ::= { hm2TrackingApplicationGroup 1 }


hm2TrackingApplicationEntry 
				OBJECT-TYPE
                SYNTAX          Hm2TrackingApplicationEntry
                MAX-ACCESS      not-accessible
                STATUS          current
                DESCRIPTION     "The entry of the hm2TrackingApplicationTable."
                INDEX           { hm2TrackAppId, hm2TrackType, hm2TrackId }
                ::= { hm2TrackingApplicationTable 1 }


Hm2TrackingApplicationEntry ::= SEQUENCE {
                hm2TrackAppId			Integer32,
                hm2TrackAppName			SnmpAdminString,
                hm2TrackAppObjectName	SnmpAdminString
                }
                
hm2TrackAppId	
				OBJECT-TYPE
                SYNTAX          Integer32
                MAX-ACCESS      not-accessible
                STATUS          current
                DESCRIPTION     "The id of an application which tracks an object."
                ::= { hm2TrackingApplicationEntry 1 }           
                
hm2TrackAppName		
				OBJECT-TYPE
                SYNTAX          SnmpAdminString
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION     "The name of the registered application."
                ::= { hm2TrackingApplicationEntry 4 }
                
hm2TrackAppObjectName		
				OBJECT-TYPE
                SYNTAX          SnmpAdminString
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION     "The name of the tracking object the application registered for."
                ::= { hm2TrackingApplicationEntry 5 }


--
-- *************************************************************
-- hm2TrackStaticRouteTable
-- *************************************************************
--
hm2TrackStaticRouteTable OBJECT-TYPE
         SYNTAX   	 SEQUENCE OF Hm2TrackStaticRouteEntry
         MAX-ACCESS  not-accessible
         STATUS   	 current
         DESCRIPTION
           			 "."
       ::= { hm2TrackingStaticRouteGroup 1 }

    hm2TrackStaticRouteEntry OBJECT-TYPE
         SYNTAX   	 Hm2TrackStaticRouteEntry
         MAX-ACCESS  not-accessible
         STATUS   	 current
         DESCRIPTION
           			 "."
         AUGMENTS { inetCidrRouteEntry }
         ::= { hm2TrackStaticRouteTable 1 }

    Hm2TrackStaticRouteEntry ::=
         SEQUENCE 
         {
             hm2TrackStaticRouteTrackId		SnmpAdminString,
             hm2TrackStaticRouteTrackState  INTEGER
         }

	hm2TrackStaticRouteTrackId OBJECT-TYPE
         SYNTAX          SnmpAdminString
         MAX-ACCESS      read-create
         STATUS          current
         DESCRIPTION     "Associate and dissociate the tracking instance to a static route.
         				  To dissociate, pass an empty string."
         ::= { hm2TrackStaticRouteEntry 1 }

	hm2TrackStaticRouteTrackState	OBJECT-TYPE
         SYNTAX          INTEGER {
             					up(1),
               					down(2),
               					notReady(3)
               				}
         MAX-ACCESS      read-only
         STATUS          current
         DESCRIPTION     "Shows if the tracked object is currently up(1), down(2) or notReady(3).
           				 in case the state indicates notReady, the corresponding configuration
           				 is missing or invalid."
         DEFVAL			{ notReady }
         ::= { hm2TrackStaticRouteEntry 2 }

   --**************************************************************************************
   --  hm2TrackingSNMPExtensionGroup - SNMP Extension Group
   --**************************************************************************************

   hm2TrackingInvalidTrackID OBJECT-IDENTITY
          STATUS      current
          DESCRIPTION "Indicates that the entry for track id is invalid."
          ::= { hm2TrackingSNMPExtensionGroup 1 }

   hm2TrackingTrackNameRegistrationErrorReturn OBJECT-IDENTITY
          STATUS      current
          DESCRIPTION "Indicates that the track name registeration is unsuccessful."
          ::= { hm2TrackingSNMPExtensionGroup 2 }

   hm2TrackingTrackNameDeregisterationErrorReturn OBJECT-IDENTITY
          STATUS      current
          DESCRIPTION "Indicates that the track name deregisteration is unsuccessful."
          ::= { hm2TrackingSNMPExtensionGroup 3 }

END
