
            S O F T W A R E - R E L E A S E - D O C U M E N T

                 Hirschmann Automation and Control GmbH
              
            	     MSP40 Release 10.0.00
            		
                            2024/08/31
             		
                          C O N T E N T S
                          ===============


    1.   Limitations of the release MSP40 10.0.00
    2.   Supported Hardware
    3.   History of Changes

   

This document is delivered with the software in the file 
"Readme_MSP40.10.0.00.txt".

 

.-----------------------------------------------------------------------------.
| For superior functions like software update,                                |
| supported web browser and limitations of the platform release 10.0.00       | 
| please read the document Readme_10.0.00.txt.                                |
'-----------------------------------------------------------------------------'



1. Limitations of the release MSP40 10.0.00
=============================================
- Twisted-Pair SFPs are not supported on MSM60 media module.

Prerequisite for the update to a HiOS version 09.1.00 or higher is that the 
device is running HiOS version 09.0.02 or higher. For an update of versions 
before 09.0.02, an update to HiOS 09.0.02 or higher is required first. 

Caution:
- With the update to HiOS 09.1.00 the bootloader is also replaced.
  Make sure that there is no power interruption during the update.
- The first boot after the update to HiOS 09.1.00 will take significantly longer.
- When downgrading from 09.1.00 to an earlier version, the device does not adopt 
  the configuration profile and the certificates automatically. Therefore, save 
  the configuration before the downgrade. Import this configuration profile after 
  the downgrade.


2. Supported Hardware
=====================
This platform software release 10.0.00 is released exclusively for the 
following hardware:

HiOS-MSP40-10000.bin:
- MSP40-00120               (Since SW 06.2.00)
- MSP40-00200               (Since SW 06.2.00)
- MSP40-00280               (Since SW 06.2.00)
- MSP42-00120               (Since SW 06.2.00)
- MSP42-00200               (Since SW 06.2.00)
- MSP42-00280               (Since SW 06.2.00)

Supported Software Level / Packages:
- 2A
- 3A (Unicast Routing)

For information on supported accessories, refer to the "User Manual Installation".
You will find the manuals under "https://www.doc.hirschmann.com".

3. History of Changes
=====================

Software Release 06.2.00
------------------------
First Version

Software Release 07.0.00
------------------------
Bugfixes (see Issue List)

New Functions:
- HTML5-based Graphical User Interface
- Backup the Config on a Remote Server
- Clear Config Keep IP
- MAC Authentication Bypass Format Options
- Port Mirroring N:2

Software Level 3A:
- ACD for Router Interfaces
- Source-Routing can be activated/deactivated

Software Release 07.0.04
------------------------
Bugfixes (see Issue List)

Changed Functions:
- Import / Export CLI scripts via grafical user interface.
- SSH: support for new ciphers.
- SSH: DSA auth. key support removed.

Software Release 07.5.01
------------------------
Bugfixes (see Issue List)

New Functions:
- Support for MSM60 media module

Software Release 08.0.00
------------------------
Bugfixes (see Issue List)

New Functions:
- Automatic login by HiVision
- CLI script load on boot 
- Changed defaults: SNMPv1/v2 and telnet are disabled.

Software Release 07.1.00 and 08.1.00
------------------------------------
Bugfixes (see Issue List)

New Functions:
- Password change on first login
  Protocols that require a login (e.g. SNMPv3) remain deactivated until the password is changed. 

Software Release 08.4.01
------------------------
Bugfixes (see Issue List)

New Functions:
- Maximum number of configurable static routes increased from 512 to 1280.
- BOOTP/DHCP options (DHCP client) can be switched off.
- Display differences to default configuration in the graphical user interface.
- Display delivered PoE current in mA (additional to the power in W).
- New parameter "index" in the CLI for adding and deleting ACL rules. 
- Private VLAN

Software Release 08.6.00
------------------------
Bugfixes (see Issue List)

New Functions:
- OPC UA Server
- Protocol packet statistics

Software Release 08.7.00
------------------------------------
Bugfixes (see Issue List)

New Functions: 
Software Level 2A/3A:
- Loop-Protection function

Software Release 09.0.00
------------------------
Bugfixes (see Issue List)

New Functions:
- Responsive GUI

Software Level 2A/3A:
- Double VLAN Tagging 

Software Release 09.1.00
------------------------
Bugfixes (see Issue List)

Attention: 	The HiOS 09.1.00 release only supports 2A Software Level. 
			Updating devices running Software Level 3A, will remove the 3A functionality.

New Functions:
- Update 802.1X to Version 2010
- Profinet Combined family GSDML
- Profinet new stack , spec 2.41 compliant
- VLAN configuration for EtherNet/IP
- IPv6-Management
- LLDP IPv6 Support

Software Release 09.2.00
------------------------
Bugfixes (see Issue List)

New Functions:
- Signed Firmware Images
- SNMPv3 Traps

Software Level 2A:
- SNMPv1/v2 Read-Only
- Interface Shutdown via Tracking

Software Release 09.4.00
------------------------
Bugfixes (see Issue List)

New Functions:
- SNMPv3 Traps (GUI)

Software Level 3A:
- L3A UR

Software Release 10.0.00
------------------------
Bugfixes (see Issue List)

New Functions:
- SSH Known Host verification

Software Level 2A/3S:
- Certificates/CRLs validation (LDAP, Email Logging, Syslog over TLS)
- Service Discovery (with ITxPT Module Inventory)
- RSPAN with dedicated destination port 

Software Release 10.0.00
------------------------
Bugfixes (see Issue List)
