HM2-PLATFORM-ROUTING-MIB DEFINITIONS ::= BEGIN

-- 
-- ***********************************************************
-- Hirschmann Platform Routing MIB
-- ***********************************************************
--

	IMPORTS
		hm2PlatformMibs, HmEnabledStatus
			FROM HM2-TC-MIB
		ifIndex, InterfaceIndex, InterfaceIndexOrZero
			FROM IF-MIB
		InetAddress, InetAddressType, InetAddressIPv4
			FROM INET-ADDRESS-MIB
		ospfIfEntry, ospfNbrEntry, ospfVirtIfEntry, ospfAreaEntry, ospfIfMetricEntry, RouterID
    		FROM OSPF-MIB
    	VlanId
			FROM Q-BRIDGE-MIB
		vrrpOperVrId
		    FROM VRRP-MIB			
		PhysAddress
			FROM RFC1213-MIB
		rip2IfConfEntry
			FROM RIPv2-MIB
		TimeTicks, Integer32, Gauge32, 
		IpAddress, Counter32, Unsigned32, MODULE-IDENTITY,
		OBJECT-IDENTITY, OBJECT-TYPE
			FROM SNMPv2-SMI
		DisplayString, RowStatus, TruthValue
			FROM SNMPv2-TC
		SnmpAdminString     	
			FROM SNMP-FRAMEWORK-MIB;

--
-- Node definitions
--
	 
	hm2PlatformRouting MODULE-IDENTITY
		LAST-UPDATED "201109080000Z"		-- September 8, 2011 at 00:00 GMT (201109080000Z)
		ORGANIZATION
			"Hirschmann Automation and Control GmbH"
		CONTACT-INFO
			"Postal:     Stuttgarter Str. 45-51
			72654 Neckartenzlingen
			Germany
			Phone:      +49 7127 140
			E-mail:     hac.support@belden.com"
		DESCRIPTION
			"The Hirschmann Platform2 MIB for Layer3 Switching.
			Copyright (C) 2011. All Rights Reserved."
		REVISION "201109080000Z"		-- September 8, 2011 at 00:00 GMT (201109080000Z)
		DESCRIPTION
			"Initial version."
	::= { hm2PlatformMibs 2 }

--
-- hm2AgentSwitchArpGroup
--	 
	hm2AgentSwitchArpGroup OBJECT IDENTIFIER ::= { hm2PlatformRouting 1 }
	 
	hm2AgentSwitchArpAgeoutTime OBJECT-TYPE
		SYNTAX Integer32 (15..21600)
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"HiOS: Configures the exact ARP entry age-out time in seconds.
			 HiSecOS: Configures the average ARP entry age-out time in seconds, with each
			   entry aging out after a random time between 0.5*hm2AgentSwitchArpAgeoutTime
			   and 1.5*hm2AgentSwitchArpAgeoutTime."
		DEFVAL { 1200 } 
	::= { hm2AgentSwitchArpGroup 1 }

	 
	hm2AgentSwitchArpResponseTime OBJECT-TYPE
		SYNTAX Integer32 (1..10)
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"Configures the ARP request response timeout in seconds.
			Allowable range: 1-10"
		DEFVAL	{ 1 }
	::= { hm2AgentSwitchArpGroup 2 }

	 
	hm2AgentSwitchArpMaxRetries OBJECT-TYPE
		SYNTAX Integer32 (0..10)
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"Configures the ARP count of maximum request for retries.
			Allowable range: 0-10"
		DEFVAL	{ 4 }
	::= { hm2AgentSwitchArpGroup 3 }

	 
	hm2AgentSwitchArpCacheSize OBJECT-TYPE
		SYNTAX Integer32
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"Configures the ARP maximum number of entries in the cache.
			Allowable range is platform specific."
	::= { hm2AgentSwitchArpGroup 4 }

	 
	hm2AgentSwitchArpDynamicRenew OBJECT-TYPE
		SYNTAX HmEnabledStatus
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"This indicates the current setting of ARP dynamic renew mode."
		DEFVAL { disable }
	::= { hm2AgentSwitchArpGroup 5 }

	 
	hm2AgentSwitchArpTotalEntryCountCurrent OBJECT-TYPE
		SYNTAX Gauge32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"Current number of entries in the ARP cache."
	::= { hm2AgentSwitchArpGroup 6 }

	 
	hm2AgentSwitchArpTotalEntryCountPeak OBJECT-TYPE
		SYNTAX Gauge32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"Peak number of entries recorded in the ARP cache over
			time.  This value is restarted whenever the ARP cache
			size is changed."
	::= { hm2AgentSwitchArpGroup 7 }

	 
	hm2AgentSwitchArpStaticEntryCountCurrent OBJECT-TYPE
		SYNTAX Gauge32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"Current number of configured static ARP entries."
	::= { hm2AgentSwitchArpGroup 8 }

	 
	hm2AgentSwitchArpStaticEntryCountMax OBJECT-TYPE
		SYNTAX Integer32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"Maximum number of configurable static ARP entries."
	::= { hm2AgentSwitchArpGroup 9 }

	 
	hm2AgentSwitchLocalProxyArpTable OBJECT-TYPE
		SYNTAX SEQUENCE OF Hm2AgentSwitchLocalProxyArpEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"This table contains the per-interface configuration
			parameters for local proxy ARP."
	::= { hm2AgentSwitchArpGroup 11 }

	 
	hm2AgentSwitchLocalProxyArpEntry OBJECT-TYPE
		SYNTAX Hm2AgentSwitchLocalProxyArpEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"Represents a logical row in the
			hm2AgentSwitchLocalProxyArpTable."
		INDEX { ifIndex } 
	::= { hm2AgentSwitchLocalProxyArpTable 1 }


	Hm2AgentSwitchLocalProxyArpEntry ::= SEQUENCE
		{
		hm2AgentSwitchLocalProxyArpMode INTEGER
		}

	 
	hm2AgentSwitchLocalProxyArpMode OBJECT-TYPE
		SYNTAX HmEnabledStatus
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"The local proxy ARP mode for the interface."
		DEFVAL	{ disable }
	::= { hm2AgentSwitchLocalProxyArpEntry 1 }

	 
	hm2AgentSwitchIntfArpTable OBJECT-TYPE
		SYNTAX SEQUENCE OF Hm2AgentSwitchIntfArpEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"This table augments the MIB-II ipNetToMediaTable by providing
			per-interface ARP entry information."
	::= { hm2AgentSwitchArpGroup 12 }

	 
	hm2AgentSwitchIntfArpEntry OBJECT-TYPE
		SYNTAX Hm2AgentSwitchIntfArpEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"This table augments the MIB-II ipNetToMediaTable by providing
			per-interface ARP entry information."
		INDEX { hm2AgentSwitchIntfArpIpAddress, hm2AgentSwitchIntfArpIfIndex } 
	::= { hm2AgentSwitchIntfArpTable 1 }


	Hm2AgentSwitchIntfArpEntry ::= SEQUENCE
		{
		hm2AgentSwitchIntfArpIpAddress 		IpAddress,
		hm2AgentSwitchIntfArpIfIndex 		InterfaceIndex,
		hm2AgentSwitchIntfArpAge 			TimeTicks,
		hm2AgentSwitchIntfArpMacAddress 	PhysAddress,
		hm2AgentSwitchIntfArpType 			INTEGER,
		hm2AgentSwitchIntfArpStatus 		RowStatus
		}

	 
	hm2AgentSwitchIntfArpIpAddress OBJECT-TYPE
		SYNTAX IpAddress
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"The Type of Address assigned to this interface."
	::= { hm2AgentSwitchIntfArpEntry 1 }

	 
	hm2AgentSwitchIntfArpIfIndex OBJECT-TYPE
		SYNTAX InterfaceIndex
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"The Associated IfIndex which identified the ARP Entry.
			This value must be specified for static ARP entries on an
			unnumbered interface"
	::= { hm2AgentSwitchIntfArpEntry 2 }

	 
	hm2AgentSwitchIntfArpAge OBJECT-TYPE
		SYNTAX TimeTicks
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"This defines the time (in seconds) since the ARP entry 
			was last refreshed.  This value is 0 for ARP entries of
			type local(1) or static(3), since these entries are 
			not subject to aging."
	::= { hm2AgentSwitchIntfArpEntry 3 }

	 
	hm2AgentSwitchIntfArpMacAddress OBJECT-TYPE
		SYNTAX PhysAddress
		MAX-ACCESS read-create
		STATUS current
		DESCRIPTION
			"The hardware MAX Address that each interface maps to."
	::= { hm2AgentSwitchIntfArpEntry 4 }

	 
	hm2AgentSwitchIntfArpType OBJECT-TYPE
		SYNTAX INTEGER
		{
			local(1),
			gateway(2),
			static(3),
			dynamic(4)
		}
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The type of ARP entry."
	::= { hm2AgentSwitchIntfArpEntry 5 }

	 
	hm2AgentSwitchIntfArpStatus OBJECT-TYPE
		SYNTAX RowStatus
		MAX-ACCESS read-create
		STATUS current
		DESCRIPTION
			"The status of this ARP entry.  Setting this object destroy will remove the entry."
	::= { hm2AgentSwitchIntfArpEntry 6 }

	 
	hm2AgentSwitchArpSparseLearn OBJECT-TYPE
		SYNTAX HmEnabledStatus
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"This indicates the current setting of ARP sparse learn mode. "
		DEFVAL { enable }
	::= { hm2AgentSwitchArpGroup 100 }

	 
	hm2AgentSwitchArpCacheClear OBJECT-TYPE
		SYNTAX INTEGER
		{
			other(1),
			flushARP(2),
			flushARPWithGateway(3)
		}
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"Setting the object to 'flushARP' will flush the ARP cache.
			Setting the object to 'flushARPWithGateway' will also flush
			the ARP cache but includes the ARP entries that are used by
			gateways of routes.
			Reading the object always returns 'other'."
	::= { hm2AgentSwitchArpGroup 101 }

	hm2AgentSwitchProxyArpMaxResponseDelay OBJECT-TYPE
		SYNTAX Integer32 (0|1..1000)
		UNITS       "milli-seconds"
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"Configures the maximum time in ms to wait before a proxy
			response is sent. Setting this to 0 determines a response
			to be sent immediately."
		DEFVAL { 800 }
	::= { hm2AgentSwitchArpGroup 248 }

--
-- hm2AgentSwitchIpGroup
--	 
	hm2AgentSwitchIpGroup OBJECT IDENTIFIER ::= { hm2PlatformRouting 2 }

	 
	hm2AgentSwitchIpRoutingMode OBJECT-TYPE
		SYNTAX HmEnabledStatus
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"Administratively enables/disables routing on the switch."
		DEFVAL { disable }
	::= { hm2AgentSwitchIpGroup 1 }

		 
	hm2AgentSwitchIpDefaultGateway OBJECT-TYPE
		SYNTAX IpAddress
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"Specifies the default gateway manually configured."
	::= { hm2AgentSwitchIpGroup 2 }

	 
	hm2AgentSwitchIpInterfaceTable OBJECT-TYPE
		SYNTAX SEQUENCE OF Hm2AgentSwitchIpInterfaceEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"IP interface table."
	::= { hm2AgentSwitchIpGroup 3 }

	 
	hm2AgentSwitchIpInterfaceEntry OBJECT-TYPE
		SYNTAX Hm2AgentSwitchIpInterfaceEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"IP interface entry."
		INDEX { hm2AgentSwitchIpInterfaceIfIndex } 
	::= { hm2AgentSwitchIpInterfaceTable 1 }


	Hm2AgentSwitchIpInterfaceEntry ::= SEQUENCE
		{
		hm2AgentSwitchIpInterfaceIfIndex 			InterfaceIndex,
		hm2AgentSwitchIPAddressConfigMethod 		INTEGER,
		hm2AgentSwitchIpInterfaceIpAddress 			IpAddress,
		hm2AgentSwitchIpInterfaceNetMask 			IpAddress,
		hm2AgentSwitchIpInterfaceClearIp 			HmEnabledStatus,
		hm2AgentSwitchIpInterfaceRoutingMode 		HmEnabledStatus,
		hm2AgentSwitchIpInterfaceProxyARPMode 		HmEnabledStatus,
		hm2AgentSwitchIpInterfaceMtuValue 			Unsigned32,
		hm2AgentSwitchIpInterfaceBandwidth 			Unsigned32,
		hm2AgentSwitchIpInterfaceUnnumberedIfIndex 	InterfaceIndexOrZero,
		hm2AgentSwitchIpInterfaceIcmpUnreachables 	HmEnabledStatus,
		hm2AgentSwitchIpInterfaceIcmpRedirects 		HmEnabledStatus,
		hm2AgentSwitchDhcpOperation 				INTEGER,
		hm2AgentSwitchIpInterfaceSuppressed 		INTEGER,
		hm2AgentSwitchIpInterfaceNumberOfFlaps		Unsigned32,
		hm2AgentSwitchIpInterfaceCurrentPenalty 	Unsigned32,
		hm2AgentSwitchIpInterfaceReUseTime 			Unsigned32,
		hm2AgentSwitchIpInterfaceNetdirectedBCMode 	HmEnabledStatus
		}

	 
	hm2AgentSwitchIpInterfaceIfIndex OBJECT-TYPE
		SYNTAX InterfaceIndex
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The IfIndex associated with this instance."
	::= { hm2AgentSwitchIpInterfaceEntry 1 }

	 
	hm2AgentSwitchIPAddressConfigMethod OBJECT-TYPE
		SYNTAX INTEGER
		{
			none(0),
			manual(1),
			dhcp(2)
		}
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"The source of the IP address. User can set the object to none(0) or dhcp(2).
			Option dhcp(2) enables DHCP client on the interface.
			Option none(0) disables DHCP client on the interface.
			Get on this object returns manual(1) only when the interface has a manually configured address."
	::= { hm2AgentSwitchIpInterfaceEntry 2 }

	 
	hm2AgentSwitchIpInterfaceIpAddress OBJECT-TYPE
		SYNTAX IpAddress
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"The IP address assigned to this interface. When setting this value,
			the value of hm2AgentSwitchIpInterfaceNetMask must be set at the same time."
	::= { hm2AgentSwitchIpInterfaceEntry 3 }

	 
	hm2AgentSwitchIpInterfaceNetMask OBJECT-TYPE
		SYNTAX IpAddress
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"The netmask assigned to this interface. When setting this value, the 
			value of hm2AgentSwitchIpInterfaceIpAddress must be set at the same time."
	::= { hm2AgentSwitchIpInterfaceEntry 4 }

	 
	hm2AgentSwitchIpInterfaceClearIp OBJECT-TYPE
		SYNTAX HmEnabledStatus
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"When setting this object to 'enable(1)' the interfaces IP address and netmask will
			be set back to 0.0.0.0. Reading this object always returns 'disable(2)."
	::= { hm2AgentSwitchIpInterfaceEntry 5 }

	 
	hm2AgentSwitchIpInterfaceRoutingMode OBJECT-TYPE
		SYNTAX HmEnabledStatus
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"Enables or disables routing for this interface."
		DEFVAL	{ disable }
	::= { hm2AgentSwitchIpInterfaceEntry 6 }

	 
	hm2AgentSwitchIpInterfaceProxyARPMode OBJECT-TYPE
		SYNTAX HmEnabledStatus
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"Enables or disables proxy ARP for this interface."
		DEFVAL	{ disable }
	::= { hm2AgentSwitchIpInterfaceEntry 7 }

	 
	hm2AgentSwitchIpInterfaceMtuValue OBJECT-TYPE
		SYNTAX Unsigned32 (0 | 68..12266)
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"Configures the MTU value for this interface. The applicable range is 
			68 to the <interface MTU value - 18>, in bytes. Get of this object 
			returns the effective MTU value on the interface. Set of this object 
			with a value of 0 resets the MTU to the default IP MTU value on the 
			interface. If a packet is received where the size exceeds the mtu
			value, an icmp destination unreachable message is sent back to the
			sender with the current mtu."
	::= { hm2AgentSwitchIpInterfaceEntry 8 }

	 
	hm2AgentSwitchIpInterfaceBandwidth OBJECT-TYPE
		SYNTAX Unsigned32 (0..10000000)
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"Configures the bandwidth value for this interface. If the returned value is 0,
			bandwidth for this interface is not configured."
	::= { hm2AgentSwitchIpInterfaceEntry 9 }

	 
	hm2AgentSwitchIpInterfaceUnnumberedIfIndex OBJECT-TYPE
		SYNTAX InterfaceIndexOrZero
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"If this object is non-zero, it indicates that the interface is unnumbered
			and specifies which interface the address is borrowed from."
	::= { hm2AgentSwitchIpInterfaceEntry 10 }

	 
	hm2AgentSwitchIpInterfaceIcmpUnreachables OBJECT-TYPE
		SYNTAX HmEnabledStatus
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"If this object is enabled, it indicates that ICMP unreachables can be sent on this
			interface."
		DEFVAL	{ enable }
	::= { hm2AgentSwitchIpInterfaceEntry 11 }

	 
	hm2AgentSwitchIpInterfaceIcmpRedirects OBJECT-TYPE
		SYNTAX HmEnabledStatus
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"If this object is enabled and hm2AgentSwitchIpIcmpRedirectsMode is also enabled, ICMP redirects
			can be sent on this interface."
		DEFVAL	{ enable }
	::= { hm2AgentSwitchIpInterfaceEntry 12 }

	 
	hm2AgentSwitchDhcpOperation OBJECT-TYPE
		SYNTAX INTEGER
		{
			renew(1),
			release(2),
			none(3)
		}
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"Renew or release the IP address learned through DHCP.
			Get on this object always gives none. None means no operation is performed on DHCP."
	::= { hm2AgentSwitchIpInterfaceEntry 13 }

	 
	hm2AgentSwitchIpInterfaceSuppressed OBJECT-TYPE
		SYNTAX INTEGER
		{
			unsuppressed(0),
			suppressed(1)
		}
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			" This mib variable contains the following values, which has the meaning as:
			'unsuppressed'     - The interface is not suppressed
			'suppressed'         - The interface is suppressed
			"
	::= { hm2AgentSwitchIpInterfaceEntry 14 }

	 
	hm2AgentSwitchIpInterfaceNumberOfFlaps OBJECT-TYPE
		SYNTAX Unsigned32 (0..4294967295)
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"This mib variable displays the number of flaps occurred on the interface"
	::= { hm2AgentSwitchIpInterfaceEntry 15 }

	 
	hm2AgentSwitchIpInterfaceCurrentPenalty OBJECT-TYPE
		SYNTAX Unsigned32 (0..20000)
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"This mib variable displays the current penalty of an interface"
	::= { hm2AgentSwitchIpInterfaceEntry 16 }

	 
	hm2AgentSwitchIpInterfaceReUseTime OBJECT-TYPE
		SYNTAX Unsigned32 (0..255)
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"This mib variable displays the number of seconds until the interface is  
			allowed to come up "
	::= { hm2AgentSwitchIpInterfaceEntry 17 }

	 
	hm2AgentSwitchIpInterfaceNetdirectedBCMode OBJECT-TYPE
		SYNTAX HmEnabledStatus
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"Enables or disables netdirected broadcasts for this interface."
		DEFVAL { disable }
	::= { hm2AgentSwitchIpInterfaceEntry 248 }

	 
	hm2AgentSwitchIpRouterDiscoveryTable OBJECT-TYPE
		SYNTAX SEQUENCE OF Hm2AgentSwitchIpRouterDiscoveryEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"There is no global administrative flag for router discovery.  The global
			routing flag (hm2AgentSwitchIpRoutingMode) will be used for this purpose.  If routing
			is disabled, router discovery is disabled as well."
	::= { hm2AgentSwitchIpGroup 4 }

	 
	hm2AgentSwitchIpRouterDiscoveryEntry OBJECT-TYPE
		SYNTAX Hm2AgentSwitchIpRouterDiscoveryEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"."
		INDEX { hm2AgentSwitchIpRouterDiscoveryIfIndex } 
	::= { hm2AgentSwitchIpRouterDiscoveryTable 1 }


	Hm2AgentSwitchIpRouterDiscoveryEntry ::= SEQUENCE
		{
		hm2AgentSwitchIpRouterDiscoveryIfIndex 					Integer32,
		hm2AgentSwitchIpRouterDiscoveryAdvertiseMode 			INTEGER,
		hm2AgentSwitchIpRouterDiscoveryMaxAdvertisementInterval Integer32,
		hm2AgentSwitchIpRouterDiscoveryMinAdvertisementInterval Integer32,
		hm2AgentSwitchIpRouterDiscoveryAdvertisementLifetime 	Integer32,
		hm2AgentSwitchIpRouterDiscoveryPreferenceLevel 			Integer32,
		hm2AgentSwitchIpRouterDiscoveryAdvertisementAddress 	IpAddress
		}

	 
	hm2AgentSwitchIpRouterDiscoveryIfIndex OBJECT-TYPE
		SYNTAX Integer32 (0..2147483647)
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"Interface Number to configure Router Discovery on."
	::= { hm2AgentSwitchIpRouterDiscoveryEntry 1 }

	 
	hm2AgentSwitchIpRouterDiscoveryAdvertiseMode OBJECT-TYPE
		SYNTAX HmEnabledStatus
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"Enable or disable router discovery on the interface."
		DEFVAL { disable }
	::= { hm2AgentSwitchIpRouterDiscoveryEntry 2 }

	 
	hm2AgentSwitchIpRouterDiscoveryMaxAdvertisementInterval OBJECT-TYPE
		SYNTAX Integer32 (4..1800)
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"Maximum time allowed between sending router advertisements 
			from the interface."
		DEFVAL { 600 } 
	::= { hm2AgentSwitchIpRouterDiscoveryEntry 3 }

	 
	hm2AgentSwitchIpRouterDiscoveryMinAdvertisementInterval OBJECT-TYPE
		SYNTAX Integer32 (3..1800)
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"Minimum time allowed between sending router advertisements from the interface.
			
			This value must be less than or equal to 
			hm2AgentSwitchIpRouterDiscoveryMaxAdvertisementInterval."
		DEFVAL { 450 } 
	::= { hm2AgentSwitchIpRouterDiscoveryEntry 4 }

	 
	hm2AgentSwitchIpRouterDiscoveryAdvertisementLifetime OBJECT-TYPE
		SYNTAX Integer32 (4..9000)
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"Value of lifetime field of router advertsisement sent from 
			the interface.
			
			This value must be greater than or equal to 
			hm2AgentSwitchIpRouterDiscoveryMaxAdvertisementInterval."
		DEFVAL { 1800 } 
	::= { hm2AgentSwitchIpRouterDiscoveryEntry 5 }

	 
	hm2AgentSwitchIpRouterDiscoveryPreferenceLevel OBJECT-TYPE
		SYNTAX Integer32
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"Preferability of the address as a default router address,
			related to other addresses on the same subnet.  This is defined
			as the larger the number, the higher the preference."
		DEFVAL { 0 } 
	::= { hm2AgentSwitchIpRouterDiscoveryEntry 6 }

	 
	hm2AgentSwitchIpRouterDiscoveryAdvertisementAddress OBJECT-TYPE
		SYNTAX IpAddress
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"Address used when sending router advertisements from the interface."
		DEFVAL { 'E0000001'h } 
	::= { hm2AgentSwitchIpRouterDiscoveryEntry 7 }

	 
	hm2AgentSwitchIpVlanTable OBJECT-TYPE
		SYNTAX SEQUENCE OF Hm2AgentSwitchIpVlanEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"A static VLAN for which routing can be enabled/disabled."
	::= { hm2AgentSwitchIpGroup 5 }

	 
	hm2AgentSwitchIpVlanEntry OBJECT-TYPE
		SYNTAX Hm2AgentSwitchIpVlanEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"A static VLAN for which routing can be enabled/disabled."
		INDEX { hm2AgentSwitchIpVlanId } 
	::= { hm2AgentSwitchIpVlanTable 1 }


	Hm2AgentSwitchIpVlanEntry ::= SEQUENCE
		{
		hm2AgentSwitchIpVlanId VlanId,
		hm2AgentSwitchIpVlanIfIndex InterfaceIndex,
		hm2AgentSwitchIpVlanRoutingStatus RowStatus
		}

	 
	hm2AgentSwitchIpVlanId OBJECT-TYPE
		SYNTAX VlanId
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The VLAN's ID."
	::= { hm2AgentSwitchIpVlanEntry 1 }

	 
	hm2AgentSwitchIpVlanIfIndex OBJECT-TYPE
		SYNTAX InterfaceIndex
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"The IfIndex associated with this VLAN."
	::= { hm2AgentSwitchIpVlanEntry 2 }

	 
	hm2AgentSwitchIpVlanRoutingStatus OBJECT-TYPE
		SYNTAX RowStatus
		MAX-ACCESS read-create
		STATUS current
		DESCRIPTION
			"Status of Routing mode per VLAN.
			active(1)       - VLAN is enabled for routing
			createAndGo(4)  - Adds VLAN entry for routing
			createAndWait(5)  - Adds VLAN entry for routing
			destroy(6)      - Removes VLAN from routing"
	::= { hm2AgentSwitchIpVlanEntry 3 }

	 
	hm2AgentSwitchSecondaryAddressTable OBJECT-TYPE
		SYNTAX SEQUENCE OF Hm2AgentSwitchSecondaryAddressEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"Contains a list of secondary IP addresses associated with an interface."
	::= { hm2AgentSwitchIpGroup 6 }

	 
	hm2AgentSwitchSecondaryAddressEntry OBJECT-TYPE
		SYNTAX Hm2AgentSwitchSecondaryAddressEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"A secondary IP address for a given interface. This IP address must not 
			conflict with the IP address configured in the hm2AgentSwitchIpInterfaceTable."
		INDEX { hm2AgentSwitchIpInterfaceIfIndex, hm2AgentSwitchSecondaryIpAddress } 
	::= { hm2AgentSwitchSecondaryAddressTable 1 }


	Hm2AgentSwitchSecondaryAddressEntry ::= SEQUENCE
		{
		hm2AgentSwitchSecondaryIpAddress 	IpAddress,
		hm2AgentSwitchSecondaryNetMask 		IpAddress,
		hm2AgentSwitchSecondaryStatus 		RowStatus
		}

	 
	hm2AgentSwitchSecondaryIpAddress OBJECT-TYPE
		SYNTAX IpAddress
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"The secondary IP address assigned to this interface."
	::= { hm2AgentSwitchSecondaryAddressEntry 1 }

	 
	hm2AgentSwitchSecondaryNetMask OBJECT-TYPE
		SYNTAX IpAddress
		MAX-ACCESS read-create
		STATUS current
		DESCRIPTION
			"The secondary netmask assigned to this interface. This value must be
			set during creation and can not be changed."
	::= { hm2AgentSwitchSecondaryAddressEntry 2 }

	 
	hm2AgentSwitchSecondaryStatus OBJECT-TYPE
		SYNTAX RowStatus
		MAX-ACCESS read-create
		STATUS current
		DESCRIPTION
			"Creates a new entry in the secondary address table.
			Allowed values are:
			createAndGo(4)  - Creates an entry in this table, associating the address
					  with a given interface.  The hm2AgentSwitchSecondaryNetMask
					  object must be set during creation.
			
			destroy(6)      - Removes the associated address from the interface."
	::= { hm2AgentSwitchSecondaryAddressEntry 3 }

--
-- hm2AgentSwitchIpIcmpControlGroup
--	 
	hm2AgentSwitchIpIcmpControlGroup OBJECT IDENTIFIER ::= { hm2AgentSwitchIpGroup 8 }
    hm2AgentSwitchIpIcmpEchoReplyMode OBJECT-TYPE
				 SYNTAX      HmEnabledStatus
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "Sets the administrative Echo Reply Mode."
         DEFVAL 	{ enable }
         ::= { hm2AgentSwitchIpIcmpControlGroup 1 }

    hm2AgentSwitchIpIcmpRedirectsMode OBJECT-TYPE
         SYNTAX      HmEnabledStatus
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION 
                     "Sets the administrative Mode for sending Redirects. "
         DEFVAL 	{ enable }
         ::= { hm2AgentSwitchIpIcmpControlGroup 2 }

    hm2AgentSwitchIpIcmpRateLimitInterval OBJECT-TYPE
         SYNTAX      Integer32 (0..2147483647)
         UNITS       "milli-seconds"
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "HiOS: Specifies the time interval between tokens being placed in the bucket
                      for ICMP Ratelimit.
                     HiSecOS: Specifies the average minimum time between subsequent ICMP packets for
                      each destination, using a token bucket algorithm. In times without ICMP packets,
                      the tokens accumulate to allow for bursts of up to
                      hm2AgentSwitchIpIcmpRateLimitBurstSize packets."
         DEFVAL 	{ 1000 }
         ::= { hm2AgentSwitchIpIcmpControlGroup 3 }

    hm2AgentSwitchIpIcmpRateLimitBurstSize OBJECT-TYPE
         SYNTAX      Integer32 (1..200)
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "HiOS: Specifies the number of tokens to be placed after timeout.
                     HiSecOS: The size of the token bucket, fixed at 6 tokens."
         DEFVAL 	{ 100 }
         ::= { hm2AgentSwitchIpIcmpControlGroup 4 }


	hm2AgentSwitchIntfIpHelperAddressTable OBJECT-TYPE
		SYNTAX SEQUENCE OF Hm2AgentSwitchIntfIpHelperAddressEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"Contains a list of IP helper addresses associated with an interface."
	::= { hm2AgentSwitchIpGroup 10 }

	 
	hm2AgentSwitchIpFirstActiveAddressType OBJECT-TYPE
		SYNTAX InetAddressType 
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The type of hm2AgentSwitchIpFirstActiveAddress."
	::= { hm2AgentSwitchIpGroup 248 }
	 
    hm2AgentSwitchIpFirstActiveAddress OBJECT-TYPE
       	SYNTAX InetAddress (SIZE(4|16))
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The lowest ip address of any active routing interface."
	::= { hm2AgentSwitchIpGroup 249 }
	 
	hm2AgentSwitchIpStaticDefaultPref OBJECT-TYPE
       	SYNTAX Integer32 (1..255)
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"The default preference for static routes."
		DEFVAL 	{ 1 }
	::= { hm2AgentSwitchIpGroup 250 }

		hm2AgentSwitchIpRouteCount OBJECT-TYPE
        	SYNTAX      Unsigned32
        	MAX-ACCESS  read-only
        	STATUS      current
        	DESCRIPTION
                     "Number of routes configured on the switch."
        ::= { hm2AgentSwitchIpGroup 251 }

    	hm2AgentSwitchIpBestRouteCount OBJECT-TYPE
        	SYNTAX      Unsigned32
        	MAX-ACCESS  read-only
        	STATUS      current
        	DESCRIPTION
                     "Number of best routes active on the switch."
        ::= { hm2AgentSwitchIpGroup 252 }
        
        hm2AgentSwitchIpSourceRoutingMode OBJECT-TYPE
			SYNTAX HmEnabledStatus
			MAX-ACCESS read-write
			STATUS current
			DESCRIPTION
				"Administratively enables/disables source routing on the switch."
			DEFVAL { disable }
		::= { hm2AgentSwitchIpGroup 253 }

	 
	hm2AgentSwitchIntfIpHelperAddressEntry OBJECT-TYPE
		SYNTAX Hm2AgentSwitchIntfIpHelperAddressEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"An IP helper address for a given interface."
		INDEX { hm2AgentSwitchIpInterfaceIfIndex, hm2AgentSwitchIntfIpHelperUdpPort, 
		hm2AgentSwitchIntfIpHelperIpAddress } 
	::= { hm2AgentSwitchIntfIpHelperAddressTable 1 }


	Hm2AgentSwitchIntfIpHelperAddressEntry ::= SEQUENCE
		{
		hm2AgentSwitchIntfIpHelperUdpPort 		Unsigned32,
		hm2AgentSwitchIntfIpHelperIpAddress 	IpAddress,
		hm2AgentSwitchIntfIpHelperHitCount 		Unsigned32,
		hm2AgentSwitchIntfIpHelperStatus 		RowStatus
		}

	 
	hm2AgentSwitchIntfIpHelperUdpPort OBJECT-TYPE
		SYNTAX Unsigned32 (0..65535)
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"UDP port number. Received packets with this destination UDP port
			number are forwarded to the helper address in this entry.
			A relay entry with port 0 allows dhcp, time, winnameserver, tacacs,
			dns, tftp, netbios-ns and netbios-dgm relay."
	::= { hm2AgentSwitchIntfIpHelperAddressEntry 1 }

	 
	hm2AgentSwitchIntfIpHelperIpAddress OBJECT-TYPE
		SYNTAX IpAddress
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"An IP helper address for packets received on this interface. 
			An address of 0.0.0.0 identifies the entry as a discard entry.
			Packets that match a discard entry are dropped."
	::= { hm2AgentSwitchIntfIpHelperAddressEntry 2 }

	 
	hm2AgentSwitchIntfIpHelperHitCount OBJECT-TYPE
		SYNTAX Unsigned32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The number of times a packet has been forwarded or discarded according to this entry."
	::= { hm2AgentSwitchIntfIpHelperAddressEntry 4 }

	 
	hm2AgentSwitchIntfIpHelperStatus OBJECT-TYPE
		SYNTAX RowStatus
		MAX-ACCESS read-create
		STATUS current
		DESCRIPTION
			"Creates a new entry in the Helper Address table.
			Allowed values are:
			
			createAndGo(4)  - Creates an IP helper entry in this table.
			
			destroy(6)      - Removes the IP helper entry."
	::= { hm2AgentSwitchIntfIpHelperAddressEntry 5 }

    hm2AgentSwitchClearIpDefaultGateway OBJECT-TYPE
         SYNTAX      INTEGER {
                        enable(1),
                        disable(2)
                       }
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                   "Resets the Global Default Gateway address."
       ::= { hm2AgentSwitchIpGroup 11 }


--
-- hm2AgentRouterRipConfigGroup
--	 
	hm2AgentRouterRipConfigGroup OBJECT IDENTIFIER ::= { hm2PlatformRouting 3 }

    hm2AgentRouterRipAdminState OBJECT-TYPE
         SYNTAX      HmEnabledStatus
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "Sets the administrative mode of RIP in the router."
         DEFVAL { disable }
         ::= { hm2AgentRouterRipConfigGroup 1 }
         
    hm2AgentRouterRipSplitHorizonMode OBJECT-TYPE
         SYNTAX      INTEGER 
         			 {
                     	none(1),
                     	simple(2),
                     	poisonReverse(3)
                  	 }
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "Sets the RIP split horizon operating mode in the router.
                      A value of none(1) means split horizon processing is
                      disabled.  When set to simple(2), the simple split 
                      horizon technique is used.  When set to poisonReverse(3),
                      the split horizon with poison reverse technique is used.
                      The default split horizon mode is simple(2)."
         DEFVAL { simple }
         ::= { hm2AgentRouterRipConfigGroup 2 }
         
    hm2AgentRouterRipAutoSummaryMode OBJECT-TYPE
         SYNTAX      HmEnabledStatus
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "Sets the RIP auto summarization mode in the router.
                      A value of enable(1) means that routes advertized by
                      this RIP router are combined, or summarized, whenever
                      possible into aggregates. When set to disable(2),
                      routes are not aggregated in RIP updates generated
                      by this router.  The default auto summary mode is 
                      enable(1)."
         DEFVAL { enable }
         ::= { hm2AgentRouterRipConfigGroup 3 }
         
    hm2AgentRouterRipHostRoutesAcceptMode OBJECT-TYPE
         SYNTAX      HmEnabledStatus
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "Sets the RIP host route acceptance mode in the router.
                      A value of enable(1) means that host routes advertized
                      to this RIP router will be accepted (learned) into its
                      routing table.  When set to disable(2), host routes 
                      advertized in RIP updates from neighboring routers
                      are ignored.  The default host routes accept mode is
                      enable(1)."
         DEFVAL { enable }
         ::= { hm2AgentRouterRipConfigGroup 4 }
         
    --************************************************************************************  
    hm2AgentRouterRipDefaultMetric  OBJECT-TYPE
    	 SYNTAX      Integer32 (0|1..15)
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
               		 "Default metric of redistributed routes, when RIP redistributes 
                	  from other protocols. {0} indicates that the parameter is not configured,
                	  this value should not be set. Valid range for set is (1..15)."
         DEFVAL { 0 }
         ::= { hm2AgentRouterRipConfigGroup 5 }

    hm2AgentRouterRipDefaultMetricConfigured OBJECT-TYPE
         SYNTAX      TruthValue
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
               		 "Flag to determine whether RIP default-metric is configured or not.
                	  Set to 'false' to unconfigure the default route metric. Set to 'true' is
                	  not allowed."
         DEFVAL { false }
         ::= { hm2AgentRouterRipConfigGroup 6 } 
            
    hm2AgentRouterRipDefaultInfoOriginate  OBJECT-TYPE
       	 SYNTAX      TruthValue
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
               		 "Flag to determine, whether RIP can advertise a default-route learned
                	  from another protocol." 
       	 DEFVAL { false }
         ::= { hm2AgentRouterRipConfigGroup 7 }   
                                
    -- Agent RIP Route-redistribution table.  This table contains, one entry per
    -- source(bgp, ospf, static, connected) from which BGP redistributes routes. 
        
    hm2AgentRipRouteRedistTable OBJECT-TYPE
         SYNTAX      SEQUENCE OF Hm2AgentRipRouteRedistEntry
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION 
                     "This table contains the MIB objects required to configure 
                      route-redistribution for RIP. Here, RIP is the Destination
                      protocol and the source protocols can be any of : BGP, OSPF,
                      Static, Connected."
         ::= { hm2AgentRouterRipConfigGroup 8 }

    hm2AgentRipRouteRedistEntry OBJECT-TYPE
         SYNTAX      Hm2AgentRipRouteRedistEntry
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION 
                     "The entries of the table."
         INDEX       { hm2AgentRipRouteRedistSource }
         ::= { hm2AgentRipRouteRedistTable 1 }
         
    Hm2AgentRipRouteRedistEntry ::= SEQUENCE {         
          hm2AgentRipRouteRedistSource
              INTEGER,
          hm2AgentRipRouteRedistMode
              INTEGER,
          hm2AgentRipRouteRedistMetric
              Integer32,
          hm2AgentRipRouteRedistMetricConfigured
              TruthValue,
          hm2AgentRipRouteRedistMatchInternal
              INTEGER,
          hm2AgentRipRouteRedistMatchExternal1
              INTEGER, 
          hm2AgentRipRouteRedistMatchExternal2
              INTEGER,
          hm2AgentRipRouteRedistMatchNSSAExternal1
              INTEGER, 
          hm2AgentRipRouteRedistMatchNSSAExternal2
              INTEGER,
          hm2AgentRipRouteRedistDistList
              Unsigned32,
          hm2AgentRipRouteRedistDistListConfigured
              TruthValue
          } 
         
    hm2AgentRipRouteRedistSource OBJECT-TYPE
         SYNTAX      INTEGER
         			 {
                     	connected(1),
                     	static(2),                     
                     	ospf(3),
                     	bgp(4)                                        
                     }         
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Source route, from which RIP can redistribute routes.
                      This object also acts as the identifier for  the 
                      RIP redistribution Table entry."
         ::= { hm2AgentRipRouteRedistEntry 1 }
                                                   
    hm2AgentRipRouteRedistMode OBJECT-TYPE
         SYNTAX      HmEnabledStatus
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "User enabels/disables route-redistribution for a particular source
                      protocol."
         DEFVAL { disable }
         ::= { hm2AgentRipRouteRedistEntry 2 }
     
    hm2AgentRipRouteRedistMetric OBJECT-TYPE
         SYNTAX      Integer32 (0|1..15)
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "Metric used for redistributing a particular source protocol route
                      into RIP. {0} indicates that the parameter is not configured, this value
                      should not be set. Valid range for set is (1..15)."
         DEFVAL { 0 }
         ::= { hm2AgentRipRouteRedistEntry 3 } 
         
    hm2AgentRipRouteRedistMetricConfigured OBJECT-TYPE
         SYNTAX      TruthValue
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "Flag to determine whether RIP redistribute-metric is configured
                      or not. Set to 'false' to unconfigure redistribute metric. Set to 'true'
                      is not allowed."
         DEFVAL { false }
         ::= { hm2AgentRipRouteRedistEntry 4 } 

    hm2AgentRipRouteRedistMatchInternal OBJECT-TYPE
         SYNTAX      INTEGER 
         			 {
                      	true(1),
                      	false(2),
                      	not-applicable(3)
                     }
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "If this flag is true, RIP redistributes OSPF internal routes.
                      It will be non-applicable, when source protocol is other than ospf."
         ::= { hm2AgentRipRouteRedistEntry 5 }
         
    hm2AgentRipRouteRedistMatchExternal1 OBJECT-TYPE
         SYNTAX      INTEGER 
         			 {
                      	true(1),
                      	false(2),
                      	not-applicable(3)
                     }
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "If this flag is true, RIP redistributes OSPF External1 routes.
                      It will be non-applicable, when source protocol is other than ospf."
         ::= { hm2AgentRipRouteRedistEntry 6 }
         
    hm2AgentRipRouteRedistMatchExternal2 OBJECT-TYPE
         SYNTAX      INTEGER 
         			 {
                      	true(1),
                      	false(2),
                      	not-applicable(3)
                     }
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "If this flag is true, RIP redistributes OSPF External2 routes.
                      It will be non-applicable, when source protocol is other than ospf."
         ::= { hm2AgentRipRouteRedistEntry 7 } 
         
    hm2AgentRipRouteRedistMatchNSSAExternal1 OBJECT-TYPE
         SYNTAX      INTEGER 
         			 {
                      	true(1),
                      	false(2),
                      	not-applicable(3)
                     }
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "If this flag is true, RIP redistributes OSPF NSSA-External1 routes.
                      It will be non-applicable, when source protocol is other than ospf."
         ::= { hm2AgentRipRouteRedistEntry 8 }
         
    hm2AgentRipRouteRedistMatchNSSAExternal2 OBJECT-TYPE
         SYNTAX      INTEGER {
                      true(1),
                      false(2),
                      not-applicable(3)
                     }
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "If this flag is true, RIP redistributes OSPF NSSA-External2 routes.
                      It will be non-applicable, when source protocol is other than ospf."
         ::= { hm2AgentRipRouteRedistEntry 9 } 
         
    hm2AgentRipRouteRedistDistList OBJECT-TYPE
         SYNTAX      Unsigned32 (0|1000..1099)
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "Access-list number of the access-list, which filters routes received
                      from a source-protocol."
         ::= { hm2AgentRipRouteRedistEntry 10 } 
         
     hm2AgentRipRouteRedistDistListConfigured OBJECT-TYPE
         SYNTAX      TruthValue
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "Flag to determine whether Access-list is configured or not."
         ::= { hm2AgentRipRouteRedistEntry 11 }
      
    -- The RIP Interface Configuration Table (augmented information).

    hm2AgentRip2IfConfTable OBJECT-TYPE
         SYNTAX   	 SEQUENCE OF Hm2AgentRip2IfConfEntry
         MAX-ACCESS  not-accessible
         STATUS   	 current
         DESCRIPTION
           			 "A list of subnets which require separate
           			  configuration in RIP.  Augments rip2IfConfTable
           			  in the RIPv2-MIB."
       ::= { hm2AgentRouterRipConfigGroup 9 }

    hm2AgentRip2IfConfEntry OBJECT-TYPE
         SYNTAX   	 Hm2AgentRip2IfConfEntry
         MAX-ACCESS  not-accessible
         STATUS   	 current
         DESCRIPTION
           			 "A Single Routing Domain in a single Subnet.
           			  Augments rip2IfConfEntry in RIPv2-MIB."
         AUGMENTS { rip2IfConfEntry }
         ::= { hm2AgentRip2IfConfTable 1 }

    Hm2AgentRip2IfConfEntry ::=
         SEQUENCE 
         {
             hm2AgentRip2IfConfAuthKeyId
             	 Integer32
         }

    hm2AgentRip2IfConfAuthKeyId OBJECT-TYPE
         SYNTAX      Integer32 (0..255)
         MAX-ACCESS  read-create
         STATUS      current
         DESCRIPTION
           			 "The identifier for the authentication key used
            		  on this interface.  This field is only meaningful 
           			  when the RIPv2-MIB rip2IfConfAuthType is md5(3); 
           			  otherwise, the value is not used."
      	 ::= { hm2AgentRip2IfConfEntry 1 }  

     hm2AgentRouterRipRoutePref OBJECT-TYPE
         SYNTAX   	 Integer32 (1..255)
         MAX-ACCESS  read-write
         STATUS   	 current
         DESCRIPTION
           			 "The route preference, sometimes called administrative distance, for RIP routes.
           			  A route with a preference of 255 is considered unreachable."
         DEFVAL { 120 }
      	 ::= { hm2AgentRouterRipConfigGroup 10 }

     hm2AgentRouterRipUpdateTimerInterval OBJECT-TYPE
         SYNTAX      Integer32 (1..1000)
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "Sets the RIP update timer interval in the router.
		 		      This is the time in seconds between two full routing table
		      		  update packets."
         DEFVAL { 30 }
         ::= { hm2AgentRouterRipConfigGroup 248 }
         
--
-- hm2AgentRouterOspfConfigGroup
--	 
	hm2AgentRouterOspfConfigGroup OBJECT IDENTIFIER ::= { hm2PlatformRouting 4 }

	 
	hm2AgentOspfDefaultMetric OBJECT-TYPE
		SYNTAX Integer32 (0 | 1..16777214)
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"Default metric of redistributed routes, when OSPF redistributes 
			from other protocols. {0} indicates that the parameter is not configured,
			this value should not be set. Valid range for set is (1..16777214)."
		DEFVAL { 0 } 
	::= { hm2AgentRouterOspfConfigGroup 1 }

	 
	hm2AgentOspfDefaultMetricConfigured OBJECT-TYPE
		SYNTAX TruthValue
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"Flag to determine whether OSPF default-metric is configured or not.
			Set to 'false' to unconfigure the OSPF default-metric. Set to 'true' is
			not allowed."
		DEFVAL { false }
	::= { hm2AgentRouterOspfConfigGroup 2 }

	 
	hm2AgentOspfDefaultInfoOriginate OBJECT-TYPE
		SYNTAX TruthValue
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"Flag to determine, whether OSPF can advertise a default-route learned
			from another protocol."
		DEFVAL { false }
	::= { hm2AgentRouterOspfConfigGroup 3 }

	 
	hm2AgentOspfDefaultInfoOriginateAlways OBJECT-TYPE
		SYNTAX TruthValue
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"When this flag is true, the router advertises 0.0.0.0/0.0.0.0 always.
			Without this option, OSPF will only advertise 0.0.0.0/0.0.0.0 if the
			router's forwarding table contains a default route."
		DEFVAL { false }
	::= { hm2AgentRouterOspfConfigGroup 4 }

	 
	hm2AgentOspfDefaultInfoOriginateMetric OBJECT-TYPE
		SYNTAX Integer32 (0 | 1..16777214)
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"Metric of the default route, which OSPF advertises when learned from
			other protocol.
			(0) indicates that the parameter is not configured, this value should not be set.
			Valid range for set is (1..16777214)."
		DEFVAL { 0 } 
	::= { hm2AgentRouterOspfConfigGroup 5 }

	 
	hm2AgentOspfDefaultInfoOriginateMetricConfigured OBJECT-TYPE
		SYNTAX TruthValue
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"Flag to determine whether OSPF default-info originate metric 
			is configured or not. Setting to false unconfigures the 
			default route metric. Setting to true is not allowed."
	::= { hm2AgentRouterOspfConfigGroup 6 }

	 
	hm2AgentOspfDefaultInfoOriginateMetricType OBJECT-TYPE
		SYNTAX INTEGER
		{
			externalType1(1),
			externalType2(2)
		}
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"Metric Type of the default route,which OSPF advertises when learned from
			other protocol. It can be 1(external type 1) or 2(external type 2)."
		DEFVAL { 2 } 
	::= { hm2AgentRouterOspfConfigGroup 7 }

	 
	hm2AgentOspfRouteRedistTable OBJECT-TYPE
		SYNTAX SEQUENCE OF Hm2AgentOspfRouteRedistEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"This table contains the MIB objects required to configure 
			route-redistribution for OSPF. Here, OSPF is the Destination
			protocol and the source protocols can be any of : BGP, RIP,
			Static, Connected."
	::= { hm2AgentRouterOspfConfigGroup 8 }

	 
	hm2AgentOspfRouteRedistEntry OBJECT-TYPE
		SYNTAX Hm2AgentOspfRouteRedistEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"The entries of the table."
		INDEX { hm2AgentOspfRouteRedistSource } 
	::= { hm2AgentOspfRouteRedistTable 1 }


	Hm2AgentOspfRouteRedistEntry ::= SEQUENCE
		{
		hm2AgentOspfRouteRedistSource 				INTEGER,
		hm2AgentOspfRouteRedistMode 				INTEGER,
		hm2AgentOspfRouteRedistMetric 				Integer32,
		hm2AgentOspfRouteRedistMetricConfigured 	TruthValue,
		hm2AgentOspfRouteRedistMetricType 			INTEGER,
		hm2AgentOspfRouteRedistTag 					Unsigned32,
		hm2AgentOspfRouteRedistSubnets 				TruthValue,
		hm2AgentOspfRouteRedistDistList 			Unsigned32,
		hm2AgentOspfRouteRedistDistListConfigured 	TruthValue
		}

	 
	hm2AgentOspfRouteRedistSource OBJECT-TYPE
		SYNTAX INTEGER
		{
			connected(1),
			static(2),
			rip(3),
			bgp(4)
		}
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"Source protocol, from which OSPF can redistribute routes.
			This object also acts as the identifier for  the 
			OSPF redistribution Table entry."
	::= { hm2AgentOspfRouteRedistEntry 1 }

	 
	hm2AgentOspfRouteRedistMode OBJECT-TYPE
		SYNTAX HmEnabledStatus
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"User enables/disables route-redistribution for a particular source
			protocol."
		DEFVAL { disable }
	::= { hm2AgentOspfRouteRedistEntry 2 }

	 
	hm2AgentOspfRouteRedistMetric OBJECT-TYPE
		SYNTAX Integer32 (0..16777214)
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"Metric used for redistributing a particular source protocol route
			into OSPF."
	::= { hm2AgentOspfRouteRedistEntry 3 }

	 
	hm2AgentOspfRouteRedistMetricConfigured OBJECT-TYPE
		SYNTAX TruthValue
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"Flag to determine whether OSPF redistribute-metric is configured or not."
	::= { hm2AgentOspfRouteRedistEntry 4 }

	 
	hm2AgentOspfRouteRedistMetricType OBJECT-TYPE
		SYNTAX INTEGER
		{
			externalType1(1),
			externalType2(2)
		}
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"Metric Type of routes,which OSPF redistributes from other source protocols.
			It can be 1(external type 1) or 2(external type 2)."
		DEFVAL { externalType2 }
	::= { hm2AgentOspfRouteRedistEntry 5 }

	hm2AgentOspfRouteRedistTag OBJECT-TYPE
		SYNTAX Unsigned32
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"It specifies the tag field in routes redistributed by OSPF."
	::= { hm2AgentOspfRouteRedistEntry 6 }

	 
	hm2AgentOspfRouteRedistSubnets OBJECT-TYPE
		SYNTAX TruthValue
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"If this value is false, then OSPF will not redistribute subnetted routes."
		DEFVAL { true }
	::= { hm2AgentOspfRouteRedistEntry 7 }

	 
	hm2AgentOspfRouteRedistDistList OBJECT-TYPE
		SYNTAX Unsigned32 (0|1..10000)
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"Access-list number of the access-list, which filters routes received
			from a source-protocol.
			  HiOS: Valid access list numbers are between 1000 and 1099.
			  HiSecOS: Valid access list numbers are between 1 and 10000."
	::= { hm2AgentOspfRouteRedistEntry 8 }

	 
	hm2AgentOspfRouteRedistDistListConfigured OBJECT-TYPE
		SYNTAX TruthValue
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"Flag to determine whether Access-list is configured or not."
	::= { hm2AgentOspfRouteRedistEntry 9 }

	 
	hm2AgentOspfIfTable OBJECT-TYPE
		SYNTAX SEQUENCE OF Hm2AgentOspfIfEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"The OSPF Interface Table describes the  inter-
			faces from the viewpoint of OSPF.  Augments 
			ospfIfTable from the OSPF-MIB."
	::= { hm2AgentRouterOspfConfigGroup 9 }

	 
	hm2AgentOspfIfEntry OBJECT-TYPE
		SYNTAX Hm2AgentOspfIfEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"The OSPF Interface Entry describes one  inter-
			face from the viewpoint of OSPF.  Augments
			ospfIfEntry in OSPF-MIB."
		AUGMENTS { ospfIfEntry } 
	::= { hm2AgentOspfIfTable 1 }


	Hm2AgentOspfIfEntry ::= SEQUENCE
		{
		hm2AgentOspfIfAuthKeyId 			Integer32,
		hm2AgentOspfIfIpMtuIgnoreFlag 		INTEGER,
		hm2AgentOspfIfPassiveMode 			TruthValue,
		hm2AgentOspfIfAdvertiseSecondaries 	INTEGER,
		hm2AgentOspfIfFastHelloMode			INTEGER
		}

	 
	hm2AgentOspfIfAuthKeyId OBJECT-TYPE
		SYNTAX Integer32 (0..255)
		MAX-ACCESS read-create
		STATUS current
		DESCRIPTION
			"The identifier for the authentication key used
			on this interface.  This field is only meaningful 
			when the OSPF-MIB ospfIfAuthType is md5(2); 
			otherwise, the value is not used."
	::= { hm2AgentOspfIfEntry 1 }

	 
	hm2AgentOspfIfIpMtuIgnoreFlag OBJECT-TYPE
		SYNTAX HmEnabledStatus
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"Configures the IP MTU Ignore Flag value for this OSPF interface."
	::= { hm2AgentOspfIfEntry 2 }

	 
	hm2AgentOspfIfPassiveMode OBJECT-TYPE
		SYNTAX TruthValue
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"Flag to determine whether the interface is passive.
			A passive interface will not participate in the OSPF
			adjacency formation."
		DEFVAL { false }
	::= { hm2AgentOspfIfEntry 3 }

	 
	hm2AgentOspfIfAdvertiseSecondaries OBJECT-TYPE
		SYNTAX HmEnabledStatus
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"Configures the advertisability of the secondary addresses
			configured on this interface."
	::= { hm2AgentOspfIfEntry 4 }
	

	hm2AgentOspfIfFastHelloMode OBJECT-TYPE
		SYNTAX HmEnabledStatus
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"Configures the fast hello mode on this interface.
			 If enabled, hello packets are sent every 250ms,
			 ospfIfHelloInterval is ignored. The dead interval and spf delay
			 need to be re-configured accordingly for faster convergence."
		DEFVAL { disable }
	::= { hm2AgentOspfIfEntry 248 }
	 


	hm2AgentOspfVirtIfTable OBJECT-TYPE
		SYNTAX SEQUENCE OF Hm2AgentOspfVirtIfEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"Information about this router's virtual inter-
			faces.  Augments ospfVirtIfTable from the OSPF-MIB."
	::= { hm2AgentRouterOspfConfigGroup 10 }

	 
	hm2AgentOspfVirtIfEntry OBJECT-TYPE
		SYNTAX Hm2AgentOspfVirtIfEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"Information about a single Virtual Interface.
			Augments ospfVirtIfEntry in OSPF-MIB."
		AUGMENTS { ospfVirtIfEntry } 
	::= { hm2AgentOspfVirtIfTable 1 }


	Hm2AgentOspfVirtIfEntry ::= SEQUENCE
		{
		hm2AgentOspfVirtIfAuthKeyId Integer32
		}

	 
	hm2AgentOspfVirtIfAuthKeyId OBJECT-TYPE
		SYNTAX Integer32 (0..255)
		MAX-ACCESS read-create
		STATUS current
		DESCRIPTION
			"The identifier for the authentication key used
			on this virtual interface.  This field is only meaningful 
			when the OSPF-MIB ospfVirtIfAuthType is md5(2); 
			otherwise, the value is not used."
	::= { hm2AgentOspfVirtIfEntry 1 }

	 
	hm2AgentRouterOspfRFC1583CompatibilityMode OBJECT-TYPE
		SYNTAX HmEnabledStatus
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"From RFC2328: 
			Controls the preference rules used in Section 16.4 when
			choosing among multiple AS-external-LSAs advertising the
			same destination. When set to 'enabled', the preference
			rules remain those specified by RFC 1583 ([Ref9]). When set
			to 'disabled', the preference rules are those stated in
			
			Section 16.4.1, which prevent routing loops when AS-
			external-LSAs for the same destination have been originated
			from different areas. Set to 'enabled' by default.
			
			In order to minimize the chance of routing loops, all OSPF
			routers in an OSPF routing domain should have
			RFC1583Compatibility set identically. When there are routers
			present that have not been updated with the functionality
			specified in Section 16.4.1 of this memo, all routers should
			have RFC1583Compatibility set to 'enabled'. Otherwise, all
			routers should have RFC1583Compatibility set to 'disabled',
			preventing all routing loops."
		DEFVAL { enable }
	::= { hm2AgentRouterOspfConfigGroup 11 }

	 
	hm2AgentOspfSpfDelayTime OBJECT-TYPE
		SYNTAX Integer32 (0..65535)
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"Delay time (in seconds) between when OSPF
			receives a topology change and when it
			starts an SPF calculation. It can be an
			integer from 0 to 65535. The default
			time is 5 seconds. A value of 0 means
			that there is no delay; that is, the
			SPF calculation is started immediately."
		DEFVAL { 5 } 
	::= { hm2AgentRouterOspfConfigGroup 12 }

	 
	hm2AgentOspfSpfHoldTime OBJECT-TYPE
		SYNTAX Integer32 (0..65535)
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"Minimum time (in seconds) between two
			consecutive SPF calculations. It can
			be an integer from 0 to 65535. The
			default time is 10 seconds. A value
			of 0 means that there is no delay;
			that is, two SPF calculations can
			be done, one immediately after the
			other."
		DEFVAL { 10 } 
	::= { hm2AgentRouterOspfConfigGroup 13 }

	 
	hm2AgentOspfAutoCostRefBw OBJECT-TYPE
		SYNTAX Unsigned32 (1..4294967)
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"Auto cost reference bandwidth of the 
			router interfaces for ospf metric calculations.
			It can be an integer from 1 to 4294967. The
			default reference bandwidth is 100 Mbps."
		DEFVAL { 100 } 
	::= { hm2AgentRouterOspfConfigGroup 14 }

	 
	hm2AgentOspfOpaqueLsaSupport OBJECT-TYPE
		SYNTAX TruthValue
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"The router's support for Opaque LSA types. 
			This object is persistent and when written 
			the entity SHOULD save the change to non-volatile
			storage."
		REFERENCE 
			"The OSPF Opaque LSA Option"
	::= { hm2AgentRouterOspfConfigGroup 15 }

	 
	hm2AgentOspfAreaOpaqueLsdbTable OBJECT-TYPE
		SYNTAX SEQUENCE OF Hm2AgentOspfAreaOpaqueLsdbEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"The OSPF Process's Area Link State Database (LSDB). 
			The LSDB contains type-10 Link State Advertisements 
			from throughout the areas that the device is attached to."
		REFERENCE 
			"OSPF Version 2, Section 12 Link State Advertisements"
	::= { hm2AgentRouterOspfConfigGroup 16 }

	 
	hm2AgentOspfAreaOpaqueLsdbEntry OBJECT-TYPE
		SYNTAX Hm2AgentOspfAreaOpaqueLsdbEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"A single AreaOpaque Link State Advertisement."
		INDEX { hm2AgentOspfAreaOpaqueLsdbAreaId, hm2AgentOspfAreaOpaqueLsdbType, 
		hm2AgentOspfAreaOpaqueLsdbLsid, hm2AgentOspfAreaOpaqueLsdbRouterId } 
	::= { hm2AgentOspfAreaOpaqueLsdbTable 1 }


	Hm2AgentOspfAreaOpaqueLsdbEntry ::= SEQUENCE
		{
		hm2AgentOspfAreaOpaqueLsdbAreaId 			IpAddress,
		hm2AgentOspfAreaOpaqueLsdbType 				INTEGER,
		hm2AgentOspfAreaOpaqueLsdbLsid 				IpAddress,
		hm2AgentOspfAreaOpaqueLsdbRouterId 			RouterID,
		hm2AgentOspfAreaOpaqueLsdbSequence 			Integer32,
		hm2AgentOspfAreaOpaqueLsdbAge 				Integer32,
		hm2AgentOspfAreaOpaqueLsdbChecksum 			Integer32,
		hm2AgentOspfAreaOpaqueLsdbAdvertisement 	OCTET STRING
		}

	 
	hm2AgentOspfAreaOpaqueLsdbAreaId OBJECT-TYPE
		SYNTAX IpAddress
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The 32 bit identifier of the Area from which 
			the LSA was received."
		REFERENCE 
			"OSPF Version 2, Appendix C.2 Area parameters"
	::= { hm2AgentOspfAreaOpaqueLsdbEntry 1 }

	 
	hm2AgentOspfAreaOpaqueLsdbType OBJECT-TYPE
		SYNTAX INTEGER
		{
			areaOpaqueLink(10)
		}
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The type of the link state advertisement. 
			Each link state type has a separate advertisement 
			format."
		REFERENCE 
			"OSPF Version 2, Appendix A.4.1 The  Link  State 
			Advertisement header"
	::= { hm2AgentOspfAreaOpaqueLsdbEntry 2 }

	 
	hm2AgentOspfAreaOpaqueLsdbLsid OBJECT-TYPE
		SYNTAX IpAddress
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The Link State ID is an LS Type Specific field 
			containing either a Router ID or an IP Address; 
			it identifies the piece of the routing domain 
			that is being described by the advertisement."
		REFERENCE 
			"OSPF Version 2, Section 12.1.4 Link State ID"
	::= { hm2AgentOspfAreaOpaqueLsdbEntry 3 }

	 
	hm2AgentOspfAreaOpaqueLsdbRouterId OBJECT-TYPE
		SYNTAX RouterID
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The 32 bit number that uniquely identifies the 
			originating router in the Autonomous System."
		REFERENCE 
			"OSPF Version 2, Appendix C.1 Global parameters"
	::= { hm2AgentOspfAreaOpaqueLsdbEntry 4 }

	 
	hm2AgentOspfAreaOpaqueLsdbSequence OBJECT-TYPE
		SYNTAX Integer32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The sequence number field is a signed 32-bit 
			integer. It starts with the value '80000001'h, 
			or -'7FFFFFFF'h, and increments until '7FFFFFFF'h. 
			Thus, a typical sequence number will be very negative. 
			It is used to detect old and duplicate link state 
			advertisements. The space of sequence numbers is linearly 
			ordered. The larger the sequence number the more recent 
			the advertisement."
		REFERENCE 
			"OSPF Version 2, Section 12.1.6 LS sequence 
			number"
	::= { hm2AgentOspfAreaOpaqueLsdbEntry 5 }

	 
	hm2AgentOspfAreaOpaqueLsdbAge OBJECT-TYPE
		SYNTAX Integer32
		UNITS
			"seconds"
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"This field is the age of the link state advertisement 
			in seconds."
		REFERENCE 
			"OSPF Version 2, Section 12.1.1 LS age"
	::= { hm2AgentOspfAreaOpaqueLsdbEntry 6 }

	 
	hm2AgentOspfAreaOpaqueLsdbChecksum OBJECT-TYPE
		SYNTAX Integer32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"This field is the checksum of the complete contents of
			the advertisement, excepting the age field. The age field
			is excepted so that an advertisement's age can be 
			incremented without updating the checksum. The checksum
			used is the same that is used for ISO connectionless
			datagrams; it is commonly referred to as the Fletcher 
			checksum."
		REFERENCE 
			"OSPF Version 2, Section 12.1.7 LS checksum"
	::= { hm2AgentOspfAreaOpaqueLsdbEntry 7 }

	 
	hm2AgentOspfAreaOpaqueLsdbAdvertisement OBJECT-TYPE
		SYNTAX OCTET STRING (SIZE (1..65535))
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The entire Link State Advertisement, including 
			its header. 
			Note that for variable length LSAs, SNMP agents 
			may not be able to return the largest string size"
		REFERENCE 
			"OSPF Version 2, Section 12 Link State Advertisements"
	::= { hm2AgentOspfAreaOpaqueLsdbEntry 8 }

	 
	hm2AgentOspfLocalLsdbTable OBJECT-TYPE
		SYNTAX SEQUENCE OF Hm2AgentOspfLocalLsdbEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"The OSPF Process's Link-Local Link State Database 
			for non-virtual links. 
			This table is identical to the OSPF LSDB Table 
			in format, but contains only Link-Local Link State 
			Advertisements for non-virtual links. The purpose is 
			to allow Link-Local LSAs to be displayed for each 
			non-virtual interface. This table is implemented to 
			support type-9 LSAs which are defined 
			in 'The OSPF Opaque LSA Option'."
		REFERENCE 
			"OSPF Version 2, Section 12 Link State 
			Advertisements and The OSPF Opaque LSA Option"
	::= { hm2AgentRouterOspfConfigGroup 17 }

	 
	hm2AgentOspfLocalLsdbEntry OBJECT-TYPE
		SYNTAX Hm2AgentOspfLocalLsdbEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"A single Link State Advertisement."
		INDEX { hm2AgentOspfLocalLsdbIpAddress, hm2AgentOspfLocalLsdbAddressLessIf, 
		hm2AgentOspfLocalLsdbType, hm2AgentOspfLocalLsdbLsid, 
		hm2AgentOspfLocalLsdbRouterId } 
	::= { hm2AgentOspfLocalLsdbTable 1 }


	Hm2AgentOspfLocalLsdbEntry ::= SEQUENCE
		{
		hm2AgentOspfLocalLsdbIpAddress 		IpAddress,
		hm2AgentOspfLocalLsdbAddressLessIf 	InterfaceIndexOrZero,
		hm2AgentOspfLocalLsdbType 			INTEGER,
		hm2AgentOspfLocalLsdbLsid 			IpAddress,
		hm2AgentOspfLocalLsdbRouterId 		RouterID,
		hm2AgentOspfLocalLsdbSequence	 	Integer32,
		hm2AgentOspfLocalLsdbAge 			Integer32,
		hm2AgentOspfLocalLsdbChecksum 		Integer32,
		hm2AgentOspfLocalLsdbAdvertisement 	OCTET STRING
		}

	 
	hm2AgentOspfLocalLsdbIpAddress OBJECT-TYPE
		SYNTAX IpAddress
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The IP Address of the interface from 
			which the LSA was received if the interface is 
			numbered."
		REFERENCE 
			"OSPF Version 2, Appendix C.3 Interface parameters"
	::= { hm2AgentOspfLocalLsdbEntry 1 }

	 
	hm2AgentOspfLocalLsdbAddressLessIf OBJECT-TYPE
		SYNTAX InterfaceIndexOrZero
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The Interface Index of the interface from 
			which the LSA was received if the interface is 
			unnumbered."
		REFERENCE 
			"OSPF Version 2, Appendix C.3 Interface parameters"
	::= { hm2AgentOspfLocalLsdbEntry 2 }

	 
	hm2AgentOspfLocalLsdbType OBJECT-TYPE
		SYNTAX INTEGER
		{
			localOpaqueLink(9)
		}
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The type of the link state advertisement. 
			Each link state type has a separate advertise- 
			ment format."
		REFERENCE 
			"OSPF Version 2, Appendix A.4.1 The  Link  State 
			Advertisement header and "
	::= { hm2AgentOspfLocalLsdbEntry 3 }

	 
	hm2AgentOspfLocalLsdbLsid OBJECT-TYPE
		SYNTAX IpAddress
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The Link State ID is an LS Type Specific field 
			containing a 32 bit identifier in IP address format; 
			it identifies the piece of the routing domain 
			that is being described by the advertisement."
		REFERENCE 
			"OSPF Version 2, Section 12.1.4 Link State ID"
	::= { hm2AgentOspfLocalLsdbEntry 4 }

	 
	hm2AgentOspfLocalLsdbRouterId OBJECT-TYPE
		SYNTAX RouterID
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The 32 bit number that uniquely identifies the 
			originating router in the Autonomous System."
		REFERENCE 
			"OSPF Version 2, Appendix C.1 Global parameters"
	::= { hm2AgentOspfLocalLsdbEntry 5 }

	 
	hm2AgentOspfLocalLsdbSequence OBJECT-TYPE
		SYNTAX Integer32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The sequence number field is a signed 32-bit 
			integer. It starts with the value '80000001'h, 
			or -'7FFFFFFF'h, and increments until '7FFFFFFF'h. 
			Thus, a typical sequence number will be very negative. 
			It is used to detect old and duplicate link state 
			advertisements. The space of sequence numbers is linearly 
			ordered. The larger the sequence number the more recent 
			the advertisement."
		REFERENCE 
			"OSPF Version 2, Section 12.1.6 LS sequence 
			number"
	::= { hm2AgentOspfLocalLsdbEntry 6 }

	 
	hm2AgentOspfLocalLsdbAge OBJECT-TYPE
		SYNTAX Integer32
		UNITS
			"seconds"
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"This field is the age of the link state adver- 
			tisement in seconds."
		REFERENCE 
			"OSPF Version 2, Section 12.1.1 LS age"
	::= { hm2AgentOspfLocalLsdbEntry 7 }

	 
	hm2AgentOspfLocalLsdbChecksum OBJECT-TYPE
		SYNTAX Integer32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"This field is the checksum of the complete 
			contents of the advertisement, excepting the 
			age field. The age field is excepted so that 
			an advertisement's age can be incremented 
			without updating the checksum. The checksum 
			used is the same that is used for ISO connec- 
			tionless datagrams; it is commonly referred  to 
			as the Fletcher checksum."
		REFERENCE 
			"OSPF Version 2, Section 12.1.7 LS checksum"
	::= { hm2AgentOspfLocalLsdbEntry 8 }

	 
	hm2AgentOspfLocalLsdbAdvertisement OBJECT-TYPE
		SYNTAX OCTET STRING (SIZE (1..65535))
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The entire Link State Advertisement, including 
			its header. 
			
			Note that for variable length LSAs, SNMP agents 
			may not be able to return the largest string size."
		REFERENCE 
			"OSPF Version 2, Section 12 Link State Adver- 
			tisements"
	::= { hm2AgentOspfLocalLsdbEntry 9 }

	 
	hm2AgentOspfAsLsdbTable OBJECT-TYPE
		SYNTAX SEQUENCE OF Hm2AgentOspfAsLsdbEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"The OSPF Process's AS-scope LSA Link State Database. 
			The Database contains the AS-scope Link State 
			Advertisements from throughout the areas that 
			the device is attached to. 
			
			This table is identical to the OSPF LSDB Table 
			in format, but contains only AS-scope Link State 
			Advertisements.  The purpose is to allow AS-scope 
			LSAs to be displayed once for the router rather 
			than once in each non-stub area."
		REFERENCE 
			"OSPF Version 2, Section 12 Link State Adver- 
			tisements"
	::= { hm2AgentRouterOspfConfigGroup 18 }

	 
	hm2AgentOspfAsLsdbEntry OBJECT-TYPE
		SYNTAX Hm2AgentOspfAsLsdbEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"A single Link State Advertisement."
		INDEX { hm2AgentOspfAsLsdbType, hm2AgentOspfAsLsdbLsid, 
		hm2AgentOspfAsLsdbRouterId } 
	::= { hm2AgentOspfAsLsdbTable 1 }


	Hm2AgentOspfAsLsdbEntry ::= SEQUENCE
		{
		hm2AgentOspfAsLsdbType 			INTEGER,
		hm2AgentOspfAsLsdbLsid 			IpAddress,
		hm2AgentOspfAsLsdbRouterId 		RouterID,
		hm2AgentOspfAsLsdbSequence 		Integer32,
		hm2AgentOspfAsLsdbAge 			Integer32,
		hm2AgentOspfAsLsdbChecksum 		Integer32,
		hm2AgentOspfAsLsdbAdvertisement OCTET STRING
		}

	 
	hm2AgentOspfAsLsdbType OBJECT-TYPE
		SYNTAX INTEGER
		{
			asOpaqueLink(11)
		}
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The type of the link state advertisement. 
			Each link state type has a separate advertise- 
			ment format."
		REFERENCE 
			"OSPF Version 2, Appendix A.4.1 The  Link  State 
			Advertisement header"
	::= { hm2AgentOspfAsLsdbEntry 1 }

	 
	hm2AgentOspfAsLsdbLsid OBJECT-TYPE
		SYNTAX IpAddress
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The Link State ID is an LS Type Specific field 
			containing either a Router ID or an IP Address; 
			it identifies the piece of the routing domain 
			that is being described by the advertisement."
		REFERENCE 
			"OSPF Version 2, Section 12.1.4 Link State ID"
	::= { hm2AgentOspfAsLsdbEntry 2 }

	 
	hm2AgentOspfAsLsdbRouterId OBJECT-TYPE
		SYNTAX RouterID
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The 32 bit number that uniquely identifies the 
			originating router in the Autonomous System."
		REFERENCE 
			"OSPF Version 2, Appendix C.1 Global parameters"
	::= { hm2AgentOspfAsLsdbEntry 3 }

	 
	hm2AgentOspfAsLsdbSequence OBJECT-TYPE
		SYNTAX Integer32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The sequence number field is a signed 32-bit 
			integer. It starts with the value '80000001'h, 
			or -'7FFFFFFF'h, and increments until '7FFFFFFF'h. 
			Thus, a typical sequence number will be very negative. 
			It is used to detect old and duplicate link state 
			advertisements. The space of sequence numbers is linearly 
			ordered. The larger the sequence number the more recent 
			the advertisement."
		REFERENCE 
			"OSPF Version  2,  Section  12.1.6  LS  sequence 
			number"
	::= { hm2AgentOspfAsLsdbEntry 4 }

	 
	hm2AgentOspfAsLsdbAge OBJECT-TYPE
		SYNTAX Integer32
		UNITS
			"seconds"
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"This field is the age of the link state adver- 
			tisement in seconds."
		REFERENCE 
			"OSPF Version 2, Section 12.1.1 LS age"
	::= { hm2AgentOspfAsLsdbEntry 5 }

	 
	hm2AgentOspfAsLsdbChecksum OBJECT-TYPE
		SYNTAX Integer32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"This field is the checksum of the complete 
			contents of the advertisement, excepting the 
			age field. The age field is excepted so that 
			an advertisement's age can be incremented 
			without updating the checksum. The checksum 
			used is the same that is used for ISO connec- 
			tionless datagrams; it is commonly referred  to 
			as the Fletcher checksum."
		REFERENCE 
			"OSPF Version 2, Section 12.1.7 LS checksum"
	::= { hm2AgentOspfAsLsdbEntry 6 }

	 
	hm2AgentOspfAsLsdbAdvertisement OBJECT-TYPE
		SYNTAX OCTET STRING (SIZE (1..65535))
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The entire Link State Advertisement, including 
			its header."
		REFERENCE 
			"OSPF Version 2, Section 12  Link  State  Adver- 
			tisements. 
			Note that for variable length LSAs, SNMP agents 
			may not be able to return the largest string size."
	::= { hm2AgentOspfAsLsdbEntry 7 }

	 
	hm2AgentOspfDefaultPassiveMode OBJECT-TYPE
		SYNTAX TruthValue
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"Flag to determine, whether all the interfaces are passive interfaces
			by default. A passive interface will not participate in the OSPF
			adjacency formation."
		DEFVAL { false }
	::= { hm2AgentRouterOspfConfigGroup 19 }

	 
	hm2AgentOspfRoutePrefIntraArea OBJECT-TYPE
		SYNTAX Integer32 (1..255)
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"The route preference, sometimes called administrative distance, for intra-area OSPFv2 routes.
			A route with a preference of 255 is considered unreachable."
		DEFVAL { 110 } 
	::= { hm2AgentRouterOspfConfigGroup 20 }

	 
	hm2AgentOspfRoutePrefInterArea OBJECT-TYPE
		SYNTAX Integer32 (1..255)
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"The route preference, sometimes called administrative distance, for inter-area OSPFv2 routes.
			A route with a preference of 255 is considered unreachable."
		DEFVAL { 110 } 
	::= { hm2AgentRouterOspfConfigGroup 21 }

	 
	hm2AgentOspfRoutePrefExternal OBJECT-TYPE
		SYNTAX Integer32 (1..255)
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"The route preference, sometimes called administrative distance, for external OSPFv2 routes.
			A route with a preference of 255 is considered unreachable."
		DEFVAL { 110 } 
	::= { hm2AgentRouterOspfConfigGroup 22 }

--
-- hm2AgentOspfAreaNSSAEntry
--	 
	hm2AgentOspfAreaNSSATable OBJECT-TYPE
		SYNTAX SEQUENCE OF Hm2AgentOspfAreaNSSAEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"Information about all the configured Not-So-Stubby-Area(NSSAs) in OSPF.  
			Augments ospfAreaTable from the OSPF-MIB."
	::= { hm2AgentRouterOspfConfigGroup 248 }
	 
	hm2AgentOspfAreaNSSAEntry OBJECT-TYPE
		SYNTAX Hm2AgentOspfAreaNSSAEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"Information about a single Not-So-Stubby-Area(NSSA).
			Augments ospfAreaEntry in OSPF-MIB."
		AUGMENTS { ospfAreaEntry } 
	::= { hm2AgentOspfAreaNSSATable 1 }

	Hm2AgentOspfAreaNSSAEntry ::= SEQUENCE
		{
			hm2AgentOspfAreaNSSAImportSummaries				HmEnabledStatus,
			hm2AgentOspfAreaNSSARedistribute 				HmEnabledStatus,
			hm2AgentOspfAreaNSSADefaultInfoOriginate		TruthValue,
			hm2AgentOspfAreaNSSADefaultMetric				Integer32,
			hm2AgentOspfAreaNSSADefaultMetricType			INTEGER
		}

	hm2AgentOspfAreaNSSAImportSummaries OBJECT-TYPE
		SYNTAX HmEnabledStatus
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"When set to enabled, OSPF's summary routes are imported into 
			 the NSSA as Type-3 summary-LSAs.  
			 When set to disabled, summary routes are not imported 
			 into the NSSA.  
			 The default setting is enabled."
		DEFVAL { enable }
	::= { hm2AgentOspfAreaNSSAEntry 1 }

	hm2AgentOspfAreaNSSARedistribute OBJECT-TYPE
		SYNTAX HmEnabledStatus
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"When set to enabled NSSA ASBRs will not redistribute external
             routes into the NSSA and they will cease to originate Type-7
             external LSAs for external routes."
		DEFVAL { enable }
	::= { hm2AgentOspfAreaNSSAEntry 2 }
	 
	hm2AgentOspfAreaNSSADefaultInfoOriginate OBJECT-TYPE                                         
		SYNTAX TruthValue
		MAX-ACCESS read-write
		STATUS current
        DESCRIPTION                                                         
            "Determines if the router will originate a Type-7 default LSA    
             into the NSSA.  This command will cause a default LSA to be     
             originated only if the router is an NSSA ABR or ASBR."          
		DEFVAL { false }
	::= { hm2AgentOspfAreaNSSAEntry 3 }

	hm2AgentOspfAreaNSSADefaultMetric OBJECT-TYPE                                         
		SYNTAX Integer32 (1..16777214)
		MAX-ACCESS read-write
		STATUS current
        DESCRIPTION                                                         
            "Defines the metric value advertised in the Type-7 default LSA 
             originated by this router"          
		DEFVAL { 10 }
	::= { hm2AgentOspfAreaNSSAEntry 4 }

	hm2AgentOspfAreaNSSADefaultMetricType OBJECT-TYPE                                         
		SYNTAX INTEGER
				{
				    ospfMetric (1),
                    comparable (2),
                    nonComparable (3)
				}
		MAX-ACCESS read-write
		STATUS current
        DESCRIPTION                                                         
            "Defines the metric type advertised in the Type-7 default LSA 
             originated by this router"          
		DEFVAL { nonComparable }
	::= { hm2AgentOspfAreaNSSAEntry 5 }


--
-- hm2AgentOspfIfMetricTable
--	 
	hm2AgentOspfIfMetricTable OBJECT-TYPE
		SYNTAX SEQUENCE OF Hm2AgentOspfIfMetricEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"Information about interface metrics."
	::= { hm2AgentRouterOspfConfigGroup 249 }
	 
	hm2AgentOspfIfMetricEntry OBJECT-TYPE
		SYNTAX Hm2AgentOspfIfMetricEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"Information about interface metrics."
		AUGMENTS { ospfIfMetricEntry } 
	::= { hm2AgentOspfIfMetricTable 1 }

	Hm2AgentOspfIfMetricEntry ::= SEQUENCE
		{
			hm2AgentOspfIfMetricCalculatedCost			Integer32
		}

	hm2AgentOspfIfMetricCalculatedCost OBJECT-TYPE                                         
		SYNTAX Integer32 (1..'FFFF'h)
		MAX-ACCESS read-only
		STATUS current
        DESCRIPTION                                                         
            "Returns the actual cost value used by OSPF for
             this interface."
	::= { hm2AgentOspfIfMetricEntry 1 }


--
-- hm2AgentSnmpTrapFlagsConfigGroupLayer3
--	 
	hm2AgentSnmpTrapFlagsConfigGroupLayer3 OBJECT IDENTIFIER ::= { hm2PlatformRouting 5 }

	hm2AgentSnmpVRRPNewMasterTrapFlag OBJECT-TYPE
		SYNTAX HmEnabledStatus
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"This flag enables the sending of VRRP new master notification
			traps."
		DEFVAL		{ disable }
	::= { hm2AgentSnmpTrapFlagsConfigGroupLayer3 1 }

	 
	hm2AgentSnmpVRRPAuthFailureTrapFlag OBJECT-TYPE
		SYNTAX HmEnabledStatus
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"This flag enables the sending of VRRP authentication failure
			notification traps."
		DEFVAL		{ disable }
	::= { hm2AgentSnmpTrapFlagsConfigGroupLayer3 2 }

--
-- hm2AgentBootpDhcpRelayGroup
--	 
	hm2AgentBootpDhcpRelayGroup OBJECT IDENTIFIER ::= { hm2PlatformRouting 6 }

	 
	hm2AgentBootpDhcpRelayMaxHopCount OBJECT-TYPE
		SYNTAX Integer32 (1..16)
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"The BOOTP/DHCP Max Hop Count.
			The relay agent silently discards BOOTREQUEST messages whose hops field exceeds the value 16 
			assuming that the request is looped through the intermediate agents. The default value is 4."
		DEFVAL { 4 } 
	::= { hm2AgentBootpDhcpRelayGroup 1 }

	 
	hm2AgentBootpDhcpRelayMinWaitTime OBJECT-TYPE
		SYNTAX Integer32 (0..100)
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"The BOOTP/DHCP Minimum Wait Time. 
			When the BOOTP relay agent receives a BOOTREQUEST message, it MAY use the value of the 'secs' 
			(seconds since client began booting) field of the request as a factor in deciding whether to 
			relay the request or not."
	::= { hm2AgentBootpDhcpRelayGroup 4 }

	 
	hm2AgentBootpDhcpRelayCircuitIdOptionMode OBJECT-TYPE
		SYNTAX HmEnabledStatus
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"The BOOTP/DHCP Circuit ID Option Mode. 
			This flag is set to enable/disable the network element to add/remove the DHCP Relay agent
			Circuit ID sub-options."
	::= { hm2AgentBootpDhcpRelayGroup 5 }

--
-- hm2AgentECMPGroup
--	 
	hm2AgentECMPGroup OBJECT IDENTIFIER ::= { hm2PlatformRouting 7 }

	 
	hm2AgentECMPOspfMaxPaths OBJECT-TYPE
		SYNTAX Integer32
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"It sets the number of paths that OSPF can report for a given destination 
			where maxpaths is platform-dependent."
	::= { hm2AgentECMPGroup 1 }

--
-- hm2AgentRouterVrrpConfigGroup
--	 
	hm2AgentRouterVrrpConfigGroup OBJECT IDENTIFIER ::= { hm2PlatformRouting 8 }
	 
	hm2AgentRouterVrrpAdminState OBJECT-TYPE
		SYNTAX HmEnabledStatus
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"Sets the administrative mode of VRRP in the router."
	::= { hm2AgentRouterVrrpConfigGroup 1 }


--
-- hm2AgentRouterVrrpOperTable
--
	hm2AgentVrrpOperations    OBJECT IDENTIFIER ::= { hm2PlatformRouting 9 }

	hm2AgentRouterVrrpOperTable OBJECT-TYPE
	   SYNTAX      SEQUENCE OF Hm2AgentRouterVrrpOperEntry
	   MAX-ACCESS   not-accessible
	   STATUS       obsolete
	   DESCRIPTION
		   "Operations table for a VRRP router which consists of a
			sequence (i.e., one or more conceptual rows) of
			`hm2AgentRouterVrrpOperEntry' items."
	   ::= { hm2AgentVrrpOperations 1 }
   
	hm2AgentRouterVrrpOperEntry OBJECT-TYPE
	   SYNTAX Hm2AgentRouterVrrpOperEntry
	   MAX-ACCESS   not-accessible 
	   STATUS       obsolete
	   DESCRIPTION 
		   "An entry in the table contains operational priority that is 
			associated with a virtual router."
	   INDEX    { ifIndex, vrrpOperVrId }
	   ::= { hm2AgentRouterVrrpOperTable 1 }

	Hm2AgentRouterVrrpOperEntry ::=
	  SEQUENCE {
		   hm2AgentRouterVrrpOperPriority 
			  Integer32
		  }
		
	hm2AgentRouterVrrpOperPriority  OBJECT-TYPE 
	 	 SYNTAX       Integer32 (0..255)
	 	 MAX-ACCESS   read-only
	 	 STATUS       obsolete
	 	 DESCRIPTION 
		 	 "This object specifies the operational priority of the VRRP router.
		 	 This value will be afftected by both the tracking process and the
		 	 configured priority set by the vrrpOperPriority object."
		 ::= {  hm2AgentRouterVrrpOperEntry 1 }


	hm2AgentRouterVrrpNumberOfFastInst  OBJECT-TYPE 
		SYNTAX       Integer32 (0..16)
	 	 MAX-ACCESS   read-only
	 	 STATUS       current
	 	 DESCRIPTION 
		 	 "Number of VRRP instances with advertisement interval less
		 	 than one second."
		 ::= { hm2AgentVrrpOperations 248 }
	
--
-- hm2AgentIpHelperGroup
--	 
	hm2AgentIpHelperGroup OBJECT IDENTIFIER ::= { hm2PlatformRouting 11 }

	 
	hm2AgentIpHelperAdminMode OBJECT-TYPE
		SYNTAX HmEnabledStatus
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"Administratively enable or disable IP helper."
	::= { hm2AgentIpHelperGroup 1 }

	 
	hm2AgentDhcpClientMsgsReceived OBJECT-TYPE
		SYNTAX Counter32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The Number of DHCP Requests Received. 
			Total number of DHCP requests received from all clients."
	::= { hm2AgentIpHelperGroup 2 }

	 
	hm2AgentDhcpClientMsgsRelayed OBJECT-TYPE
		SYNTAX Counter32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The Number of DHCP Requests Forwarded. 
			Total number of DHCP requests relayed to a server."
	::= { hm2AgentIpHelperGroup 3 }

	 
	hm2AgentDhcpServerMsgsReceived OBJECT-TYPE
		SYNTAX Counter32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The number of DHCP messages received from a server."
	::= { hm2AgentIpHelperGroup 4 }

	 
	hm2AgentDhcpServerMsgsRelayed OBJECT-TYPE
		SYNTAX Counter32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The number of DHCP messages relayed to a server."
	::= { hm2AgentIpHelperGroup 5 }

	 
	hm2AgentUdpClientMsgsReceived OBJECT-TYPE
		SYNTAX Counter32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The number of UDP messages received from all clients."
	::= { hm2AgentIpHelperGroup 6 }

	 
	hm2AgentUdpClientMsgsRelayed OBJECT-TYPE
		SYNTAX Counter32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The number of UDP messages relayed to a server."
	::= { hm2AgentIpHelperGroup 7 }

	 
	hm2AgentSwitchIpHelperAddressTable OBJECT-TYPE
		SYNTAX SEQUENCE OF Hm2AgentSwitchIpHelperAddressEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"Contains a list of IP helper addresses configured globally."
	::= { hm2AgentIpHelperGroup 8 }

	 
	hm2AgentSwitchIpHelperAddressEntry OBJECT-TYPE
		SYNTAX Hm2AgentSwitchIpHelperAddressEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"An IP Helper address that applies to packets received on any interface."
		INDEX { hm2AgentSwitchIpHelperUdpPort, hm2AgentSwitchIpHelperAddress } 
	::= { hm2AgentSwitchIpHelperAddressTable 1 }


	Hm2AgentSwitchIpHelperAddressEntry ::= SEQUENCE
		{
		hm2AgentSwitchIpHelperUdpPort 	Unsigned32,
		hm2AgentSwitchIpHelperAddress 	IpAddress,
		hm2AgentSwitchIpHelperHitCount 	Unsigned32,
		hm2AgentSwitchIpHelperStatus 	RowStatus
		}

	 
	hm2AgentSwitchIpHelperUdpPort OBJECT-TYPE
		SYNTAX Unsigned32 (0..65535)
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"UDP port number. A relay entry with port 0 allows dhcp, time,
			 winnameserver, tacacs, dns, tftp, netbios-ns and netbios-dgm relay."
	::= { hm2AgentSwitchIpHelperAddressEntry 1 }

	 
	hm2AgentSwitchIpHelperAddress OBJECT-TYPE
		SYNTAX IpAddress
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"The IP Helper address assigned to this interface."
	::= { hm2AgentSwitchIpHelperAddressEntry 2 }

	 
	hm2AgentSwitchIpHelperHitCount OBJECT-TYPE
		SYNTAX Unsigned32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The number of times a packet has been forwarded or discarded according to this entry."
	::= { hm2AgentSwitchIpHelperAddressEntry 3 }

	 
	hm2AgentSwitchIpHelperStatus OBJECT-TYPE
		SYNTAX RowStatus
		MAX-ACCESS read-create
		STATUS current
		DESCRIPTION
			"Creates a new entry in the global IP Helper address table.
			Allowed values are:
			
			 createAndGo(4)  - Creates an IP helper entry in this table.
			 destroy(6)      - Removes the IP helper entry."
	::= { hm2AgentSwitchIpHelperAddressEntry 4 }

	 
	hm2AgentUdpClientMsgsTtlExpired OBJECT-TYPE
		SYNTAX Counter32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The number of UDP messages received with an expired TTL."
	::= { hm2AgentIpHelperGroup 9 }

	 
	hm2AgentUdpClientMsgsDiscarded OBJECT-TYPE
		SYNTAX Counter32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The number of UDP messages that matched a discard entry."
	::= { hm2AgentIpHelperGroup 10 }

--
-- hm2AgentInternalVlanGroup
--
	hm2AgentInternalVlanGroup OBJECT IDENTIFIER ::= { hm2PlatformRouting 12 }

	hm2AgentInternalVlanBase OBJECT-TYPE
		SYNTAX VlanId
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"The VLAN ID internally assigned to the first port-based routing interface."
		DEFVAL { 4093 } 
	::= { hm2AgentInternalVlanGroup 1 }

	 
	hm2AgentInternalVlanPolicy OBJECT-TYPE
		SYNTAX INTEGER
		{
			ascending(0),
			descending(1)
		}
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"Whether to search up or down from the base VLAN ID for a free VLAN ID to
			assign to a port-based routing interface."
		DEFVAL { descending }
	::= { hm2AgentInternalVlanGroup 2 }

	 
	hm2AgentSwitchInternalVlanTable OBJECT-TYPE
		SYNTAX SEQUENCE OF Hm2AgentSwitchInternalVlanEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"Contains a list of VLAN IDs used internally for port-based routing interfaces."
	::= { hm2AgentInternalVlanGroup 3 }

	 
	hm2AgentSwitchInternalVlanEntry OBJECT-TYPE
		SYNTAX Hm2AgentSwitchInternalVlanEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"A VLAN ID internally assigned to a port-based routing interface."
		INDEX { hm2AgentSwitchInternalVlanId } 
	::= { hm2AgentSwitchInternalVlanTable 1 }


	Hm2AgentSwitchInternalVlanEntry ::= SEQUENCE
		{
		hm2AgentSwitchInternalVlanId VlanId,
		hm2AgentSwitchInternalVlanIfIndex InterfaceIndex
		}

	 
	hm2AgentSwitchInternalVlanId OBJECT-TYPE
		SYNTAX VlanId
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"A VLAN ID internally assigned to a port-based routing interface."
	::= { hm2AgentSwitchInternalVlanEntry 1 }

	 
	hm2AgentSwitchInternalVlanIfIndex OBJECT-TYPE
		SYNTAX InterfaceIndex
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"Interface index of port-based routing interface using this VLAN ID."
	::= { hm2AgentSwitchInternalVlanEntry 2 }

--
-- hm2AgentOspfQueueGroup
--
	hm2AgentOspfQueueGroup OBJECT IDENTIFIER ::= { hm2PlatformRouting 13 }
	 
	hm2AgentOspfQueueTable OBJECT-TYPE
		SYNTAX SEQUENCE OF Hm2AgentOspfQueueEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"Table lists information about OSPFv2 message queue utilization."
	::= { hm2AgentOspfQueueGroup 1 }

	 
	hm2AgentOspfQueueEntry OBJECT-TYPE
		SYNTAX Hm2AgentOspfQueueEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"Information on a specific OSPFv2 message queue."
		INDEX { hm2AgentOspfQueueIndex } 
	::= { hm2AgentOspfQueueTable 1 }


	Hm2AgentOspfQueueEntry ::= SEQUENCE
		{
		hm2AgentOspfQueueIndex 	Unsigned32,
		hm2AgentOspfQueueName 	DisplayString,
		hm2AgentOspfQueueLength Gauge32,
		hm2AgentOspfQueueHigh 	Gauge32,
		hm2AgentOspfQueueDrops 	Counter32,
		hm2AgentOspfQueueLimit 	Unsigned32
		}

	 
	hm2AgentOspfQueueIndex OBJECT-TYPE
		SYNTAX Unsigned32
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"Index value for this message queue."
	::= { hm2AgentOspfQueueEntry 1 }

	 
	hm2AgentOspfQueueName OBJECT-TYPE
		SYNTAX DisplayString
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"Name of an OSPFv2 message queue."
	::= { hm2AgentOspfQueueEntry 2 }

	 
	hm2AgentOspfQueueLength OBJECT-TYPE
		SYNTAX Gauge32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The number of messages currently in the message queue."
	::= { hm2AgentOspfQueueEntry 3 }

	 
	hm2AgentOspfQueueHigh OBJECT-TYPE
		SYNTAX Gauge32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The high water mark of the number of messages in the message queue."
	::= { hm2AgentOspfQueueEntry 4 }

	 
	hm2AgentOspfQueueDrops OBJECT-TYPE
		SYNTAX Counter32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The number of items dropped because the message queue was full."
	::= { hm2AgentOspfQueueEntry 5 }

	 
	hm2AgentOspfQueueLimit OBJECT-TYPE
		SYNTAX Unsigned32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The maximum number of messages this queue can hold."
	::= { hm2AgentOspfQueueEntry 6 }

--
-- hm2AgentOspfPacketStatsGroup
--	 
	hm2AgentOspfPacketStatsGroup OBJECT IDENTIFIER ::= { hm2PlatformRouting 14 }

	hm2AgentOspfCountersCleared OBJECT-TYPE
		SYNTAX Unsigned32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The time since OSPFv2 counters were last cleared, in seconds."
	::= { hm2AgentOspfPacketStatsGroup 1 }

	 
	hm2AgentOspfLsaRetxCount OBJECT-TYPE
		SYNTAX Counter32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The total number of LSAs retransmitted since OSPF counters were last cleared. 
			If the same LSA is retransmitted to multiple neighbors, the count is incremented 
			for each neighbor."
	::= { hm2AgentOspfPacketStatsGroup 2 }

	 
	hm2AgentOspfHellosRx OBJECT-TYPE
		SYNTAX Counter32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The total number of OSPFv2 Hello packets received since OSPF counters were last cleared."
	::= { hm2AgentOspfPacketStatsGroup 3 }

	 
	hm2AgentOspfHellosTx OBJECT-TYPE
		SYNTAX Counter32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The total number of OSPFv2 Hello packets transmitted since OSPF counters were last cleared."
	::= { hm2AgentOspfPacketStatsGroup 4 }

	 
	hm2AgentOspfDdRx OBJECT-TYPE
		SYNTAX Counter32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The total number of OSPFv2 Database Description packets received since OSPF counters were last cleared."
	::= { hm2AgentOspfPacketStatsGroup 5 }

	 
	hm2AgentOspfDdTx OBJECT-TYPE
		SYNTAX Counter32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The total number of OSPFv2 Database Description packets transmitted since OSPF counters were last cleared."
	::= { hm2AgentOspfPacketStatsGroup 6 }

	 
	hm2AgentOspfLsReqRx OBJECT-TYPE
		SYNTAX Counter32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The total number of OSPFv2 LS Request packets received since OSPF counters were last cleared."
	::= { hm2AgentOspfPacketStatsGroup 7 }

	 
	hm2AgentOspfLsReqTx OBJECT-TYPE
		SYNTAX Counter32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The total number of OSPFv2 LS Request packets transmitted since OSPF counters were last cleared."
	::= { hm2AgentOspfPacketStatsGroup 8 }

	 
	hm2AgentOspfLsUpdatesRx OBJECT-TYPE
		SYNTAX Counter32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The total number of OSPFv2 LS Update packets received since OSPF counters 
			were last cleared."
	::= { hm2AgentOspfPacketStatsGroup 9 }

	 
	hm2AgentOspfLsUpdatesTx OBJECT-TYPE
		SYNTAX Counter32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The total number of OSPFv2 LS Update packets transmitted since OSPF counters 
			were last cleared."
	::= { hm2AgentOspfPacketStatsGroup 10 }

	 
	hm2AgentOspfLsAckRx OBJECT-TYPE
		SYNTAX Counter32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The total number of OSPFv2 LS Acknowledgement packets received since OSPF counters were last cleared."
	::= { hm2AgentOspfPacketStatsGroup 11 }

	 
	hm2AgentOspfLsAckTx OBJECT-TYPE
		SYNTAX Counter32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The total number of OSPFv2 LS Acknowledgement packets transmitted since OSPF counters were last cleared."
	::= { hm2AgentOspfPacketStatsGroup 12 }

	 
	hm2AgentOspfLsUpdatesRxMax OBJECT-TYPE
		SYNTAX Gauge32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The maximum rate of OSPFv2 LS Update packets received over any 5-second 
			interval since OSPF counters were last cleared. The rate is given in packets 
			per second (that is, the number of packets received during the 5-second 
			interval, divided by 5)."
	::= { hm2AgentOspfPacketStatsGroup 13 }

	 
	hm2AgentOspfLsUpdatesTxMax OBJECT-TYPE
		SYNTAX Gauge32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The maximum rate of OSPFv2 LS Update packets transmitted over any 5-second 
			interval since OSPF counters were last cleared. The rate is given in packets 
			per second (that is, the number of packets transmitted during the 5-second 
			interval, divided by 5)."
	::= { hm2AgentOspfPacketStatsGroup 14 }

	 
	hm2AgentOspfType1LsasRx OBJECT-TYPE
		SYNTAX Counter32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The number of type 1 (router) LSAs received since OSPF counters 
			were last cleared."
	::= { hm2AgentOspfPacketStatsGroup 15 }

	 
	hm2AgentOspfType2LsasRx OBJECT-TYPE
		SYNTAX Counter32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The number of type 2 (network) LSAs received since OSPF counters 
			were last cleared."
	::= { hm2AgentOspfPacketStatsGroup 16 }

	 
	hm2AgentOspfType3LsasRx OBJECT-TYPE
		SYNTAX Counter32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The number of type 3 (network summary) LSAs received since OSPF counters 
			were last cleared."
	::= { hm2AgentOspfPacketStatsGroup 17 }

	 
	hm2AgentOspfType4LsasRx OBJECT-TYPE
		SYNTAX Counter32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The number of type 4 (ASBR summary) LSAs received since OSPF counters 
			were last cleared."
	::= { hm2AgentOspfPacketStatsGroup 18 }

	 
	hm2AgentOspfType5LsasRx OBJECT-TYPE
		SYNTAX Counter32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The number of type 5 (external) LSAs received since OSPF counters 
			were last cleared."
	::= { hm2AgentOspfPacketStatsGroup 19 }

	 
	hm2AgentOspfType7LsasRx OBJECT-TYPE
		SYNTAX Counter32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The number of type 7 (NSSA external) LSAs received since OSPF counters 
			were last cleared."
	::= { hm2AgentOspfPacketStatsGroup 20 }

	 
	hm2AgentOspfType9LsasRx OBJECT-TYPE
		SYNTAX Counter32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The number of type 9 (Link Opaque) LSAs received since OSPF counters 
			were last cleared."
	::= { hm2AgentOspfPacketStatsGroup 21 }

	 
	hm2AgentOspfType10LsasRx OBJECT-TYPE
		SYNTAX Counter32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The number of type 10 (Area Opaque) LSAs received since OSPF counters 
			were last cleared."
	::= { hm2AgentOspfPacketStatsGroup 22 }

	 
	hm2AgentOspfType11LsasRx OBJECT-TYPE
		SYNTAX Counter32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The number of type 11 (AS Opaque) LSAs received since OSPF counters 
			were last cleared."
	::= { hm2AgentOspfPacketStatsGroup 23 }

--
-- hm2AgentOspfSpfStatsTable
--
	hm2AgentOspfSpfStatsTable OBJECT-TYPE
		SYNTAX SEQUENCE OF Hm2AgentOspfSpfStatsEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"Contains statistics for the twenty most recent SPF runs. 
			Statistics are reported from the oldest SPF first to the most recent."
	::= { hm2PlatformRouting 15 }

	hm2AgentOspfSpfStatsEntry OBJECT-TYPE
		SYNTAX Hm2AgentOspfSpfStatsEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"Statistics for a single SPF run."
		INDEX { hm2AgentOspfSpfIndex } 
	::= { hm2AgentOspfSpfStatsTable 1 }


	Hm2AgentOspfSpfStatsEntry ::= SEQUENCE
		{
		hm2AgentOspfSpfIndex 			Unsigned32,
		hm2AgentOspfSpfStatsDeltaT 		Unsigned32,
		hm2AgentOspfSpfStatsIntra 		Unsigned32,
		hm2AgentOspfSpfStatsSumm 		Unsigned32,
		hm2AgentOspfSpfStatsExt 		Unsigned32,
		hm2AgentOspfSpfStatsSpfTotal 	Unsigned32,
		hm2AgentOspfSpfStatsRibUpdate 	Unsigned32,
		hm2AgentOspfSpfStatsReason 		DisplayString
		}

	 
	hm2AgentOspfSpfIndex OBJECT-TYPE
		SYNTAX Unsigned32
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"Integer that uniquely identifies an SPF run. This value is 
			incremented each time OSPF runs a full routing table calculation."
	::= { hm2AgentOspfSpfStatsEntry 1 }

	 
	hm2AgentOspfSpfStatsDeltaT OBJECT-TYPE
		SYNTAX Unsigned32
		UNITS
			"seconds"
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"How long since this routing table calculation ran. The time is 
			given in seconds."
	::= { hm2AgentOspfSpfStatsEntry 2 }

	 
	hm2AgentOspfSpfStatsIntra OBJECT-TYPE
		SYNTAX Unsigned32
		UNITS
			"milli-seconds"
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"Number of milliseconds to compute intra-area routes."
	::= { hm2AgentOspfSpfStatsEntry 3 }

	 
	hm2AgentOspfSpfStatsSumm OBJECT-TYPE
		SYNTAX Unsigned32
		UNITS
			"milli-seconds"
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"Number of milliseconds to compute inter-area routes."
	::= { hm2AgentOspfSpfStatsEntry 4 }

	 
	hm2AgentOspfSpfStatsExt OBJECT-TYPE
		SYNTAX Unsigned32
		UNITS
			"milli-seconds"
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"Number of milliseconds to compute external routes."
	::= { hm2AgentOspfSpfStatsEntry 5 }

	 
	hm2AgentOspfSpfStatsSpfTotal OBJECT-TYPE
		SYNTAX Unsigned32
		UNITS
			"milli-seconds"
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"Number of milliseconds for entire routing table calculation."
	::= { hm2AgentOspfSpfStatsEntry 6 }

	 
	hm2AgentOspfSpfStatsRibUpdate OBJECT-TYPE
		SYNTAX Unsigned32
		UNITS
			"milli-seconds"
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"Number of milliseconds to update the common routing table."
	::= { hm2AgentOspfSpfStatsEntry 7 }

	 
	hm2AgentOspfSpfStatsReason OBJECT-TYPE
		SYNTAX DisplayString
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"Reasons why a routing table calculation was required. 
			R - new router LSA, 
			         N - new Network LSA, 
			         SN - new network summary LSA, 
			         SA - new ASBR summary LSA, 
			         X - new external LSA."
	::= { hm2AgentOspfSpfStatsEntry 8 }

    --****************************************************************
    -- hm2AgentRoutingHeapGroup
    --
    --****************************************************************
 
    hm2AgentRoutingHeapGroup    OBJECT IDENTIFIER ::= { hm2PlatformRouting 16 }

    hm2AgentRoutingHeapSize OBJECT-TYPE
      SYNTAX     Unsigned32
      MAX-ACCESS read-only
      STATUS     current
      DESCRIPTION
        "The size of the routing heap, in bytes.  Unicast routing protocols
        and ARP allocate memory from the routing heap."
    ::= { hm2AgentRoutingHeapGroup 1 }

    hm2AgentRoutingHeapInUse OBJECT-TYPE
      SYNTAX     Gauge32
      MAX-ACCESS read-only
      STATUS     current
      DESCRIPTION
        "The number of bytes currently allocated from the routing heap."
    ::= { hm2AgentRoutingHeapGroup 2 }

    hm2AgentRoutingHeapHigh OBJECT-TYPE
      SYNTAX     Gauge32
      MAX-ACCESS read-only
      STATUS     current
      DESCRIPTION
        "High water mark for the number of bytes allocated from the routing heap."
    ::= { hm2AgentRoutingHeapGroup 3 }

    --****************************************************************
    -- hm2AgentRoutingTableSummaryGroup
    --
    --****************************************************************

    hm2AgentRoutingTableSummaryGroup    OBJECT IDENTIFIER ::= { hm2PlatformRouting 17 }

    hm2AgentConnectedRoutes OBJECT-TYPE
      SYNTAX     Gauge32
      MAX-ACCESS read-only
      STATUS     current
      DESCRIPTION
        "The number of connected routes in the IPv4 routing table."
    ::= { hm2AgentRoutingTableSummaryGroup 1 }

    hm2AgentStaticRoutes OBJECT-TYPE
      SYNTAX     Gauge32
      MAX-ACCESS read-only
      STATUS     current
      DESCRIPTION
        "The number of static routes in the IPv4 routing table."
    ::= { hm2AgentRoutingTableSummaryGroup 2 }

    hm2AgentRipRoutes OBJECT-TYPE
      SYNTAX     Gauge32
      MAX-ACCESS read-only
      STATUS     current
      DESCRIPTION
        "The number of RIP routes in the IPv4 routing table."
    ::= { hm2AgentRoutingTableSummaryGroup 3 }

    hm2AgentOspfRoutes OBJECT-TYPE
      SYNTAX     Gauge32
      MAX-ACCESS read-only
      STATUS     current
      DESCRIPTION
        "The number of OSPFv2 routes in the IPv4 routing table."
    ::= { hm2AgentRoutingTableSummaryGroup 4 }

    hm2AgentOspfIntraRoutes OBJECT-TYPE
      SYNTAX     Gauge32
      MAX-ACCESS read-only
      STATUS     current
      DESCRIPTION
        "The number of OSPFv2 intra-area routes in the IPv4 routing table."
    ::= { hm2AgentRoutingTableSummaryGroup 5 }

    hm2AgentOspfInterRoutes OBJECT-TYPE
      SYNTAX     Gauge32
      MAX-ACCESS read-only
      STATUS     current
      DESCRIPTION
        "The number of OSPFv2 inter-area routes in the IPv4 routing table."
    ::= { hm2AgentRoutingTableSummaryGroup 6 }

    hm2AgentOspfExt1Routes OBJECT-TYPE
      SYNTAX     Gauge32
      MAX-ACCESS read-only
      STATUS     current
      DESCRIPTION
        "The number of OSPFv2 external type 1 routes in the IPv4 routing table."
    ::= { hm2AgentRoutingTableSummaryGroup 7 }

    hm2AgentOspfExt2Routes OBJECT-TYPE
      SYNTAX     Gauge32
      MAX-ACCESS read-only
      STATUS     current
      DESCRIPTION
        "The number of OSPFv2 external type 2 routes in the IPv4 routing table."
    ::= { hm2AgentRoutingTableSummaryGroup 8 }

    hm2AgentBgpRoutes OBJECT-TYPE
      SYNTAX     Gauge32
      MAX-ACCESS read-only
      STATUS     current
      DESCRIPTION
        "The number of BGP routes in the IPv4 routing table."
    ::= { hm2AgentRoutingTableSummaryGroup 9 }

    hm2AgentEbgpRoutes OBJECT-TYPE
      SYNTAX     Gauge32
      MAX-ACCESS read-only
      STATUS     current
      DESCRIPTION
        "The number of external BGP routes in the IPv4 routing table."
    ::= { hm2AgentRoutingTableSummaryGroup 10 }

    hm2AgentIbgpRoutes OBJECT-TYPE
      SYNTAX     Gauge32
      MAX-ACCESS read-only
      STATUS     current
      DESCRIPTION
        "The number of internal BGP routes in the IPv4 routing table."
    ::= { hm2AgentRoutingTableSummaryGroup 11 }

    hm2AgentLocalBgpRoutes OBJECT-TYPE
      SYNTAX     Gauge32
      MAX-ACCESS read-only
      STATUS     current
      DESCRIPTION
        "The number of local BGP routes in the IPv4 routing table."
    ::= { hm2AgentRoutingTableSummaryGroup 12 }

    hm2AgentRejectRoutes OBJECT-TYPE
      SYNTAX     Gauge32
      MAX-ACCESS read-only
      STATUS     current
      DESCRIPTION
        "The number of reject routes in the IPv4 routing table."
    ::= { hm2AgentRoutingTableSummaryGroup 13 }

    hm2AgentTotalRoutes OBJECT-TYPE
      SYNTAX     Gauge32
      MAX-ACCESS read-only
      STATUS     current
      DESCRIPTION
        "The number of routes in the IPv4 routing table."
    ::= { hm2AgentRoutingTableSummaryGroup 14 }

    hm2AgentBestRoutes OBJECT-TYPE
      SYNTAX     Gauge32
      MAX-ACCESS read-only
      STATUS     current
      DESCRIPTION
        "The number of IPv4 routes in the forwarding table."
    ::= { hm2AgentRoutingTableSummaryGroup 15 }

    hm2AgentBestRoutesHigh OBJECT-TYPE
      SYNTAX     Gauge32
      MAX-ACCESS read-only
      STATUS     current
      DESCRIPTION
        "The highest number of IPv4 routes in the forwarding table."
    ::= { hm2AgentRoutingTableSummaryGroup 16 }

    hm2AgentAlternateRoutes OBJECT-TYPE
      SYNTAX     Gauge32
      MAX-ACCESS read-only
      STATUS     current
      DESCRIPTION
        "The number of alternate routes in the IPv4 routing table.
         An alternate route is less preferred than the best route and is not used for forwarding."
    ::= { hm2AgentRoutingTableSummaryGroup 17 }

    hm2AgentRouteAdds OBJECT-TYPE
      SYNTAX     Counter32
      MAX-ACCESS read-only
      STATUS     current
      DESCRIPTION
        "The number of routes added to the IPv4 routing table."
    ::= { hm2AgentRoutingTableSummaryGroup 18 }

    hm2AgentRouteModifies OBJECT-TYPE
      SYNTAX     Counter32
      MAX-ACCESS read-only
      STATUS     current
      DESCRIPTION
        "The number of routes changed in the IPv4 routing table."
    ::= { hm2AgentRoutingTableSummaryGroup 19 }

    hm2AgentRouteDeletes OBJECT-TYPE
      SYNTAX     Counter32
      MAX-ACCESS read-only
      STATUS     current
      DESCRIPTION
        "The number of routes removed from the IPv4 routing table."
    ::= { hm2AgentRoutingTableSummaryGroup 20 }

    hm2AgentUnresolvedRouteAdds OBJECT-TYPE
      SYNTAX     Counter32
      MAX-ACCESS read-only
      STATUS     current
      DESCRIPTION
        "The number of IPv4 route adds that failed because none of the route's next hops were on a local subnet."
    ::= { hm2AgentRoutingTableSummaryGroup 21 }

    hm2AgentInvalidRouteAdds OBJECT-TYPE
      SYNTAX     Counter32
      MAX-ACCESS read-only
      STATUS     current
      DESCRIPTION
        "The number of IPv4 routes adds that failed because the route was invalid."
    ::= { hm2AgentRoutingTableSummaryGroup 22 }

    hm2AgentFailedRouteAdds OBJECT-TYPE
      SYNTAX     Counter32
      MAX-ACCESS read-only
      STATUS     current
      DESCRIPTION
        "The number of IPv4 routes adds that failed because of a resource limitation in the routing table"
    ::= { hm2AgentRoutingTableSummaryGroup 23 }

    hm2AgentReservedLocals OBJECT-TYPE
      SYNTAX     Gauge32
      MAX-ACCESS read-only
      STATUS     current
      DESCRIPTION
        "The number of IPv4 routing table entries reserved for a local subnet on a routing interface that is down. "
    ::= { hm2AgentRoutingTableSummaryGroup 24 }

    hm2AgentUniqueNextHops OBJECT-TYPE
      SYNTAX     Gauge32
      MAX-ACCESS read-only
      STATUS     current
      DESCRIPTION
        "The number of distinct next hops used among all IPv4 routes currently in the routing table.
         These include local interfaces for local routes and neighbors for indirect routes."
    ::= { hm2AgentRoutingTableSummaryGroup 25 }

    hm2AgentUniqueNextHopsHigh OBJECT-TYPE
      SYNTAX     Gauge32
      MAX-ACCESS read-only
      STATUS     current
      DESCRIPTION
        "The highest count of unique next hops since counters were last cleared."
    ::= { hm2AgentRoutingTableSummaryGroup 26 }

    hm2AgentNextHopGroups OBJECT-TYPE
      SYNTAX     Gauge32
      MAX-ACCESS read-only
      STATUS     current
      DESCRIPTION
        "The current number of next hop groups in use by one or more routes.
         Each next hop group includes one or more next hops."
    ::= { hm2AgentRoutingTableSummaryGroup 27 }

    hm2AgentNextHopGroupsHigh OBJECT-TYPE
      SYNTAX     Gauge32
      MAX-ACCESS read-only
      STATUS     current
      DESCRIPTION
        "The highest count of next hop groups since counters were last cleared."
    ::= { hm2AgentRoutingTableSummaryGroup 28 }

    hm2AgentEcmpGroups OBJECT-TYPE
      SYNTAX     Gauge32
      MAX-ACCESS read-only
      STATUS     current
      DESCRIPTION
        "The number of next hop groups with multiple next hops."
    ::= { hm2AgentRoutingTableSummaryGroup 29 }

    hm2AgentEcmpGroupsHigh OBJECT-TYPE
      SYNTAX     Gauge32
      MAX-ACCESS read-only
      STATUS     current
      DESCRIPTION
        "The high water mark of the number of ECMP groups."
    ::= { hm2AgentRoutingTableSummaryGroup 30 }

    hm2AgentEcmpRoutes OBJECT-TYPE
      SYNTAX     Gauge32
      MAX-ACCESS read-only
      STATUS     current
      DESCRIPTION
        "The current number of IPv4 routes with multiple next hops."
    ::= { hm2AgentRoutingTableSummaryGroup 31 }

    hm2AgentTruncEcmpRoutes OBJECT-TYPE
      SYNTAX     Gauge32
      MAX-ACCESS read-only
      STATUS     current
      DESCRIPTION
        "The number of ECMP routes that are currently installed in the forwarding table
         with just one next hop. The forwarding table may limit the number of ECMP
         routes or the number of ECMP groups. When an ECMP route cannot be installed
         because such a limit is reached, the route is installed with a single next hop."
    ::= { hm2AgentRoutingTableSummaryGroup 32 }

    hm2AgentEcmpRetries OBJECT-TYPE
      SYNTAX     Counter32
      MAX-ACCESS read-only
      STATUS     current
      DESCRIPTION
        "The number of ECMP routes that have been installed in the forwarding table
         after initially being installed with a single next hop."
    ::= { hm2AgentRoutingTableSummaryGroup 33 }

    --****************************************************************
    -- hm2AgentEcmpCountTable
    --
    --************************************************************

    hm2AgentEcmpCountTable OBJECT-TYPE
         SYNTAX      SEQUENCE OF Hm2AgentEcmpCountEntry
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION
                     "A count of the number of routes with each number of ECMP next hops."
         ::= { hm2PlatformRouting 18}

    hm2AgentEcmpCountEntry OBJECT-TYPE
         SYNTAX      Hm2AgentEcmpCountEntry
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION
                     "Number of IPv4 routes with a given number of next hops."
         INDEX       { hm2AgentEcmpNextHopCount }
         ::= { hm2AgentEcmpCountTable 1 }

    Hm2AgentEcmpCountEntry ::= SEQUENCE {
         hm2AgentEcmpNextHopCount
            Unsigned32,
         hm2AgentEcmpRouteCount
            Gauge32
       }

    hm2AgentEcmpNextHopCount OBJECT-TYPE
         SYNTAX      Unsigned32 (0..128)
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION
                     "The number of next hops in a route. From 0 to the maximum number of
                      next hops in an ECMP route. The maximum varies by platform."
         ::= { hm2AgentEcmpCountEntry 1 }

    hm2AgentEcmpRouteCount OBJECT-TYPE
         SYNTAX      Gauge32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "The number of IPv4 routes with agentEcmpNextHopCount next hops."
         ::= { hm2AgentEcmpCountEntry 2 }

 
    --****************************************************************
    -- hm2AgentOspfStubRouterGroup
    --
    --****************************************************************
    hm2AgentOspfStubRouterGroup    OBJECT IDENTIFIER ::= { hm2PlatformRouting 19 }

   hm2AgentOspfStubRouterAdvertisement OBJECT-TYPE
       SYNTAX       INTEGER {
                    doNotAdvertise(1),
                    advertise(2)
                    }
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
           "Specifies how the router LSAs are advertised by the router.
           The value doNotAdvertise indicates the advertisement of a
           standard router LSA and is the default value.  The value
           advertise indicates the advertisement of a stub router LSA."
       ::= { hm2AgentOspfStubRouterGroup 1 }

   hm2AgentOspfStubRouterReason OBJECT-TYPE
      SYNTAX     INTEGER {
                 configured(0),
                 startup(1),
                 resource-limitation(2)
                 }
      MAX-ACCESS read-only
      STATUS     current
      DESCRIPTION
        "This indicates the reason because of which the router is in Stub mode.
        This is valid only if the agentOspfStubRouterMode is 'active'."
    ::= { hm2AgentOspfStubRouterGroup 2 }

   hm2AgentOspfStubRouterStartupTimeRemaining OBJECT-TYPE
      SYNTAX     Unsigned32
      MAX-ACCESS read-only
      STATUS     current
      DESCRIPTION
        "The time remaining (in seconds) for the router to come out of the
        stub mode. This is valid only if the agentOspfStubRouterReason is
        'startup'."
    ::= { hm2AgentOspfStubRouterGroup 3 }

   hm2AgentOspfStubRouterDuration OBJECT-TYPE
      SYNTAX     Unsigned32
      MAX-ACCESS read-only
      STATUS     current
      DESCRIPTION
        "Time elapsed (in seconds) since the router last entered the stub
        router mode.  This is valid only if the agentOspfStubRouterMode is
        'active' and agentOspfStubRouterReason is 'resource-limitation'."
    ::= { hm2AgentOspfStubRouterGroup 4 }

-- 
-- hm2AgentOspfNbrTable
-- 

	hm2AgentOspfNbrTable OBJECT-TYPE
		SYNTAX   	SEQUENCE OF Hm2AgentOspfNbrEntry
		MAX-ACCESS  not-accessible
		STATUS   	current
		DESCRIPTION
		           "Information about this router's neighbors.
			    	Augments ospfNbrTable from the OSPF-MIB."
		::= { hm2PlatformRouting 249 }

	hm2AgentOspfNbrEntry OBJECT-TYPE
		SYNTAX   	Hm2AgentOspfNbrEntry
		MAX-ACCESS  not-accessible
		STATUS   	current
		DESCRIPTION
		           "Information about a single neighbor.
		            Augments ospfNbrEntry in OSPF-MIB."
		AUGMENTS { ospfNbrEntry }
		::= { hm2AgentOspfNbrTable 1 }

	Hm2AgentOspfNbrEntry ::= SEQUENCE {
		hm2AgentOspfNbrDeadTime       TimeTicks
	}

	hm2AgentOspfNbrDeadTime OBJECT-TYPE
		SYNTAX   	TimeTicks
		MAX-ACCESS  read-only
		STATUS   	current
		DESCRIPTION
		           "The neighbor's Dead Time is the amount of remaining time 
		           since the last OSPF hello packet received, before 
		           declaring the neighbor status as down."
		::= { hm2AgentOspfNbrEntry 1 }


-- 
--  hm2AgentOspfRouteTable
-- 

	hm2AgentOspfRouteTable OBJECT-TYPE
		SYNTAX   	SEQUENCE OF Hm2AgentOspfRouteEntry
		MAX-ACCESS  not-accessible
		STATUS   	current
		DESCRIPTION
		           "Information about this router's OSPF routes."
		::= { hm2PlatformRouting 250 }

	hm2AgentOspfRouteEntry OBJECT-TYPE
		SYNTAX   	Hm2AgentOspfRouteEntry
		MAX-ACCESS  not-accessible
		STATUS   	current
		DESCRIPTION
		           "Information about a single route."
		INDEX { hm2AgentOspfRouteNet, hm2AgentOspfRouteMask }  
		::= { hm2AgentOspfRouteTable 1 }

	Hm2AgentOspfRouteEntry ::= SEQUENCE {
		hm2AgentOspfRouteNet			InetAddressIPv4,
		hm2AgentOspfRouteMask			InetAddressIPv4,
		hm2AgentOspfRouteCost			Integer32,
		hm2AgentOspfRouteProtoType		INTEGER
	}

	hm2AgentOspfRouteNet OBJECT-TYPE
		SYNTAX      InetAddressIPv4
		MAX-ACCESS  not-accessible
		STATUS      current
		DESCRIPTION
			 "The IP Address of the Net or Subnet  indicated
			  by the route."
	   ::= { hm2AgentOspfRouteEntry 1 }
	
	hm2AgentOspfRouteMask OBJECT-TYPE
		SYNTAX      InetAddressIPv4
		MAX-ACCESS  not-accessible
		STATUS      current
		DESCRIPTION
				"The Subnet Mask that pertains to  the  Net  or
			  Subnet."
	 ::= { hm2AgentOspfRouteEntry 2 }		
		
	hm2AgentOspfRouteCost OBJECT-TYPE
		SYNTAX   	Integer32
		MAX-ACCESS  read-only
		STATUS   	current
		DESCRIPTION
		           "The route cost calculated in the SPF algorithm to reach the network."
		::= { hm2AgentOspfRouteEntry 3 }

	hm2AgentOspfRouteProtoType OBJECT-TYPE
		SYNTAX   	INTEGER { 
		                intra (1),
						inter (2),
						ext-type1 (3),
						ext-type2 (4),
						nssa-type1 (5),
						nssa-type2 (6)
						} 
		MAX-ACCESS  read-only
		STATUS   	current
		DESCRIPTION
		           "The type of route that was learned from OSPF."
		::= { hm2AgentOspfRouteEntry 4 }	
	
--
-- hm2AgentVrrpExtGroup
--	 
	hm2AgentVrrpExtGroup OBJECT IDENTIFIER ::= { hm2PlatformRouting 260 }


--
-- hm2AgentVrrpTrackingTable
--	 

	hm2AgentVrrpTrackingTable OBJECT-TYPE
		SYNTAX SEQUENCE OF Hm2AgentVrrpTrackingEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"This table contains variables to define
			an entry in the VRRP Tracking database."
	::= { hm2AgentVrrpExtGroup 1 }

	 
	hm2AgentVrrpTrackingEntry OBJECT-TYPE
		SYNTAX Hm2AgentVrrpTrackingEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"The entries of the table."
		INDEX { hm2AgentVrrpTrackIfIndex, hm2AgentVrrpTrackVrid, IMPLIED hm2AgentVrrpTrackId } 
	::= { hm2AgentVrrpTrackingTable 1 }


	Hm2AgentVrrpTrackingEntry ::= SEQUENCE
		{
		hm2AgentVrrpTrackIfIndex 	Integer32,
		hm2AgentVrrpTrackVrid 		Integer32,
		hm2AgentVrrpTrackId 		SnmpAdminString,
		hm2AgentVrrpTrackDecrement 	Integer32,
		hm2AgentVrrpTrackOperStatus INTEGER,
		hm2AgentVrrpTrackRowStatus 	RowStatus
		}

	 
	hm2AgentVrrpTrackIfIndex OBJECT-TYPE
		SYNTAX Integer32
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"DURABLE: { 1:all }
			The interface number of the virtual router"
	::= { hm2AgentVrrpTrackingEntry 1 }

	 
	hm2AgentVrrpTrackVrid OBJECT-TYPE
		SYNTAX Integer32 (1..255)
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"DURABLE: { 1:all }
			The virtual router id for this virtual router"
	::= { hm2AgentVrrpTrackingEntry 2 }

	 
	hm2AgentVrrpTrackId OBJECT-TYPE
		SYNTAX SnmpAdminString
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"DURABLE: { 1:all }
			The id of the object being tracked"
	::= { hm2AgentVrrpTrackingEntry 3 }

	 
	hm2AgentVrrpTrackDecrement OBJECT-TYPE
		SYNTAX Integer32 (1..253)
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"DURABLE: { 1:all }
			The value by wich the current priority of the virtual router
			is decremented when the tracked object goes DOWN."
	::= { hm2AgentVrrpTrackingEntry 4 }

	 
	hm2AgentVrrpTrackOperStatus OBJECT-TYPE
		SYNTAX INTEGER
		{
			up(1),
			down(2),
			notReady(3)
		}
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"Shows if the tracked object is currently UP or DOWN or NOT-READY"
	::= { hm2AgentVrrpTrackingEntry 5 }

	 
	hm2AgentVrrpTrackRowStatus OBJECT-TYPE
		SYNTAX RowStatus
		MAX-ACCESS read-create
		STATUS current
		DESCRIPTION
			"DURABLE: { 1:all }
			Defines the status of a vrrp tracking database entry.
			Set to createAndGo(4) to create a new row.
			Set to destroy(6) to delete an entry.
			Reads as active(1) if the tracked object exists and is trackable,
			notReady(3) otherwise."
	::= { hm2AgentVrrpTrackingEntry 6 }

--
-- hm2AgentVrrpExtTable
--	 

	hm2AgentVrrpExtTable OBJECT-TYPE
		SYNTAX SEQUENCE OF Hm2AgentVrrpExtEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"This table contains variables to define
			an entry in the VRRP enhancements database."
	::= { hm2AgentVrrpExtGroup 2 }

	 
	hm2AgentVrrpExtEntry OBJECT-TYPE
		SYNTAX Hm2AgentVrrpExtEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"The entry of the hm2AgentVrrpExtTable."
		INDEX { hm2AgentVrrpExtIfIndex, hm2AgentVrrpExtVrid } 
	::= { hm2AgentVrrpExtTable 1 }


	Hm2AgentVrrpExtEntry ::= SEQUENCE
		{
		hm2AgentVrrpExtIfIndex 			Integer32,
		hm2AgentVrrpExtVrid 			Integer32,
		hm2AgentVrrpExtDomainId 		Integer32,
		hm2AgentVrrpExtDomainRole 		INTEGER,
		hm2AgentVrrpExtDomainStatus 	INTEGER,
		hm2AgentVrrpExtAdvertAddress 	IpAddress,
		hm2AgentVrrpExtAdvertTimer 		Integer32,
		hm2AgentVrrpExtCfgPriority	 	Integer32,
		hm2AgentVrrpExtNotifyAddress 	IpAddress,
		hm2AgentVrrpExtNotifyLinkdown 	INTEGER,
		hm2AgentVrrpExtPreemptionDelay 	Integer32,
		hm2AgentVrrpPrimaryVirtualAddress 	IpAddress,
		hm2AgentVrrpExtMethod			INTEGER
		}

	 
	hm2AgentVrrpExtIfIndex OBJECT-TYPE
		SYNTAX Integer32
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"The interface number of the virtual router"
	::= { hm2AgentVrrpExtEntry 1 }

	 
	hm2AgentVrrpExtVrid OBJECT-TYPE
		SYNTAX Integer32 (1..255)
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"The virtual router id for this virtual router"
	::= { hm2AgentVrrpExtEntry 2 }

	 
	hm2AgentVrrpExtDomainId OBJECT-TYPE
		SYNTAX Integer32 (0..8)
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"The domain this virtual router is a member of. If set to
			0, the virtual router is not a member of any domain."
		DEFVAL { 0 }
	::= { hm2AgentVrrpExtEntry 3 }

	 
	hm2AgentVrrpExtDomainRole OBJECT-TYPE
		SYNTAX INTEGER
		{
			none(1),
			member(2),
			supervisor(3)
		}
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"The role of this virtual router in its domain. This is none(1) if 
			the virtual router is not member of a domain, supervisor(3) if it
			is the supervisor of its domain, member(2) otherwise."
		DEFVAL { none }
	::= { hm2AgentVrrpExtEntry 4 }

	 
	hm2AgentVrrpExtDomainStatus OBJECT-TYPE
		SYNTAX INTEGER
		{
			noError(1),
			noSupervisor(2),
			supervisorDown(3)
		}
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"Shows if the domain configuration is correct for this virtual router"
	::= { hm2AgentVrrpExtEntry 5 }

	 
	hm2AgentVrrpExtAdvertAddress OBJECT-TYPE
		SYNTAX IpAddress
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"The IP address advertisements of the virtual router are sent to"
		DEFVAL { 'E0000012'h } 
	::= { hm2AgentVrrpExtEntry 6 }

	 
	hm2AgentVrrpExtAdvertTimer OBJECT-TYPE
		SYNTAX Integer32 (100..255000)
		UNITS
			"milli-seconds"
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"This is used to set the interval between advertisements in
			milliseconds. This accesses the same value as
			vrrpOperAdvertisementInterval."
		DEFVAL { 1000 } 
	::= { hm2AgentVrrpExtEntry 7 }

	 
	hm2AgentVrrpExtCfgPriority OBJECT-TYPE
		SYNTAX Integer32 (1..254)
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"The configured priority of the virtual router. This can be
			different from the operating priority if tracked objects are down
			or the virtual router is the ip address owner"
		DEFVAL { 100 }
	::= { hm2AgentVrrpExtEntry 8 }

	 
	hm2AgentVrrpExtNotifyAddress OBJECT-TYPE
		SYNTAX IpAddress
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"The IP address notifications of the virtual router are sent to"
		DEFVAL  { '00000000'H } -- 0.0.0.0
	::= { hm2AgentVrrpExtEntry 9 }

	 
	hm2AgentVrrpExtNotifyLinkdown OBJECT-TYPE
		SYNTAX HmEnabledStatus
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"Enables or disables sending of notification messages if the
			virtual router's interface goes down."
		DEFVAL { disable }
	::= { hm2AgentVrrpExtEntry 10 }

	 
	hm2AgentVrrpExtPreemptionDelay OBJECT-TYPE
		SYNTAX Integer32 (0..65535)
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"Time (in seconds) after startup of the virtual router by which the
			preemption of a Master with a lower priority is delayed."
		DEFVAL { 0 } 
	::= { hm2AgentVrrpExtEntry 11 }

	hm2AgentVrrpPrimaryVirtualAddress OBJECT-TYPE
		SYNTAX IpAddress
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The virtual IP address in the subnet of the primary ip address on
			the interface. If no match is found, an unspecified virtual address
			is returned. If no virtual address is configured, 0.0.0.0 is returned."
	::= { hm2AgentVrrpExtEntry 12 }
	
	hm2AgentVrrpExtMethod  OBJECT-TYPE
   		SYNTAX      INTEGER
   		{
                    none (1),
                    config (2),
                    ttdp (3)
   		}
   		MAX-ACCESS  read-write
   		STATUS      current
   		DESCRIPTION
          		"The source of the VRRP instance. User can set the object to none(1), config(2), ttdp(3)."
		DEFVAL { none }
   	::= { hm2AgentVrrpExtEntry 13 }


--
-- hm2AgentVrrpDomainTable
--	 
	 
	hm2AgentVrrpDomainTable OBJECT-TYPE
		SYNTAX SEQUENCE OF Hm2AgentVrrpDomainEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"This table contains variables to define
			an entry in the VRRP domain database."
	::= { hm2AgentVrrpExtGroup 3 }

	 
	hm2AgentVrrpDomainEntry OBJECT-TYPE
		SYNTAX Hm2AgentVrrpDomainEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"The entries of the table."
		INDEX { hm2AgentVrrpDomainId } 
	::= { hm2AgentVrrpDomainTable 1 }


	Hm2AgentVrrpDomainEntry ::= SEQUENCE
		{
		hm2AgentVrrpDomainId 					Integer32,
		hm2AgentVrrpDomainMemberSendAdv 		INTEGER,
		hm2AgentVrrpDomainStatus 				INTEGER,
		hm2AgentVrrpDomainSupervisorIfIndex 	Integer32,
		hm2AgentVrrpDomainSupervisorVrid 		Integer32,
		hm2AgentVrrpDomainOperPriority 			Integer32,
		hm2AgentVrrpDomainSupervisorOperState 	INTEGER
		}

	 
	hm2AgentVrrpDomainId OBJECT-TYPE
		SYNTAX Integer32 (0..8)
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"The domain ID."
	::= { hm2AgentVrrpDomainEntry 1 }

	 
	hm2AgentVrrpDomainMemberSendAdv OBJECT-TYPE
		SYNTAX HmEnabledStatus
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"DURABLE: { 1:all }
			Determines if the members of this domain send advertisement packets.
			If set to disabled(2), only the supervisor of the domain sends packets."
		DEFVAL { disable }
	::= { hm2AgentVrrpDomainEntry 2 }

	 
	hm2AgentVrrpDomainStatus OBJECT-TYPE
		SYNTAX INTEGER
		{
			noError(1),
			noSupervisor(2),
			supervisorDown(3)
		}
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"Shows if the configuration of the domain is complete."
	::= { hm2AgentVrrpDomainEntry 3 }

	 
	hm2AgentVrrpDomainSupervisorIfIndex OBJECT-TYPE
		SYNTAX Integer32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The interface number of the supervisor of the domain"
	::= { hm2AgentVrrpDomainEntry 4 }

	 
	hm2AgentVrrpDomainSupervisorVrid OBJECT-TYPE
		SYNTAX Integer32 (0..255)
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The virtual router id of the supervisor of the domain. 0 if unconfigured"
	::= { hm2AgentVrrpDomainEntry 5 }

	 
	hm2AgentVrrpDomainOperPriority OBJECT-TYPE
		SYNTAX Integer32 (0..255)
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The current operating priority of the domain. This can be
			different from the configured priority if tracked objects are down.
			For domain members this is the priority of the supervisor of that
			Domain if the supervisor is configured and up."
	::= { hm2AgentVrrpDomainEntry 6 }

	 
	hm2AgentVrrpDomainSupervisorOperState OBJECT-TYPE
		SYNTAX INTEGER
		{
			initialize(1),
			backup(2),
			master(3),
			unknown(4)
		}
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"Shows the current operational state of the domain supervisor."
	::= { hm2AgentVrrpDomainEntry 7 }

--
-- hm2AgentNeighbourGroup
--
	hm2AgentNeighbourGroup OBJECT IDENTIFIER ::= { hm2PlatformRouting 270 }

--
-- hm2AgentStaticNeighbourTable
--		
	hm2AgentStaticNeighbourTable OBJECT-TYPE
		SYNTAX SEQUENCE OF Hm2AgentStaticNeighbourEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"."
	::= { hm2AgentNeighbourGroup 10 }

	 
	hm2AgentStaticNeighbourEntry OBJECT-TYPE
		SYNTAX Hm2AgentStaticNeighbourEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"."
		INDEX { hm2AgentStaticNeighbourAddressType, hm2AgentStaticNeighbourAddress } 
	::= { hm2AgentStaticNeighbourTable 1 }


	Hm2AgentStaticNeighbourEntry ::= SEQUENCE
		{
		hm2AgentStaticNeighbourAddressType 	InetAddressType,
		hm2AgentStaticNeighbourAddress 		InetAddress,
		hm2AgentStaticNeighbourPhysAddress 	PhysAddress,
		hm2AgentStaticNeighbourIfIndex		InterfaceIndexOrZero,
		hm2AgentStaticNeighbourRowStatus 	RowStatus
		}

	 
	hm2AgentStaticNeighbourAddressType OBJECT-TYPE
		SYNTAX InetAddressType 
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"."
	::= { hm2AgentStaticNeighbourEntry 1 }

	 
	hm2AgentStaticNeighbourAddress OBJECT-TYPE
		SYNTAX InetAddress (SIZE(4|16))
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"."
	::= { hm2AgentStaticNeighbourEntry 2 }

	 
	hm2AgentStaticNeighbourPhysAddress OBJECT-TYPE
		SYNTAX PhysAddress (SIZE(0..65535))
		MAX-ACCESS read-create
		STATUS current
		DESCRIPTION
			"."
	::= { hm2AgentStaticNeighbourEntry 3 }

	hm2AgentStaticNeighbourIfIndex OBJECT-TYPE
		SYNTAX InterfaceIndexOrZero
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"."
	::= { hm2AgentStaticNeighbourEntry 4 }
	 
	hm2AgentStaticNeighbourRowStatus OBJECT-TYPE
		SYNTAX RowStatus
		MAX-ACCESS read-create
		STATUS current
		DESCRIPTION
			"The status of this entry. Setting this object destroy will remove the entry."
	::= { hm2AgentStaticNeighbourEntry 5 }

--
-- hm2AgentDynamicNeighbourTable
--		
	hm2AgentDynamicNeighbourTable OBJECT-TYPE
		SYNTAX SEQUENCE OF Hm2AgentDynamicNeighbourEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"."
	::= { hm2AgentNeighbourGroup 11 }

	 
	hm2AgentDynamicNeighbourEntry OBJECT-TYPE
		SYNTAX Hm2AgentDynamicNeighbourEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"."
		INDEX { hm2AgentDynamicNeighbourAddressType, hm2AgentDynamicNeighbourAddress } 
	::= { hm2AgentDynamicNeighbourTable 1 }

	Hm2AgentDynamicNeighbourEntry ::= SEQUENCE
		{
		hm2AgentDynamicNeighbourAddressType 	InetAddressType,
		hm2AgentDynamicNeighbourAddress 		InetAddress,
		hm2AgentDynamicNeighbourPhysAddress 	PhysAddress,
		hm2AgentDynamicNeighbourIfIndex			InterfaceIndexOrZero,
		hm2AgentDynamicNeighbourAction	 		INTEGER
		}

	 
	hm2AgentDynamicNeighbourAddressType OBJECT-TYPE
		SYNTAX InetAddressType 
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"."
	::= { hm2AgentDynamicNeighbourEntry 1 }

	 
	hm2AgentDynamicNeighbourAddress OBJECT-TYPE
		SYNTAX InetAddress (SIZE(4|16))
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"."
	::= { hm2AgentDynamicNeighbourEntry 2 }

	 
	hm2AgentDynamicNeighbourPhysAddress OBJECT-TYPE
		SYNTAX PhysAddress (SIZE(0..65535))
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"."
	::= { hm2AgentDynamicNeighbourEntry 3 }

	hm2AgentDynamicNeighbourIfIndex OBJECT-TYPE
		SYNTAX InterfaceIndexOrZero
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"."
	::= { hm2AgentDynamicNeighbourEntry 4 }
	 
	hm2AgentDynamicNeighbourAction OBJECT-TYPE
		SYNTAX INTEGER {
						 other(1),
						 delete(2),
						 static(3)
					   }
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"."
	::= { hm2AgentDynamicNeighbourEntry 5 }                                          
                                          
--
-- hm2AgentRoutingSNMPExtensionGroup
--	 
	hm2AgentRoutingSNMPExtensionGroup OBJECT IDENTIFIER ::= { hm2PlatformRouting 280 }

	hm2AgentIpHelperTableFullErrorReturn OBJECT-IDENTITY
		STATUS current
		DESCRIPTION
			"The maximum number of IP helper entries has been reached"
	::= { hm2AgentRoutingSNMPExtensionGroup 1 }

    hm2AgentIpHelperInvalidServerAddrErrorReturn OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "Invalid IP server address."
    ::= { hm2AgentRoutingSNMPExtensionGroup 2 }
    
    hm2AgentRouterOspfDependenciesNotMet OBJECT-IDENTITY
    	STATUS      current
    	DESCRIPTION "Cannot modify OSPF admin state on this interface. Set primary IP address."
    ::= { hm2AgentRoutingSNMPExtensionGroup 3 }
    
    hm2AgentRouterOspfRangeTableFullErrorReturn OBJECT-IDENTITY
    	STATUS      current
    	DESCRIPTION "The maximum number of area-range entries has been reached."
    ::= { hm2AgentRoutingSNMPExtensionGroup 4 }
    
    hm2AgentRouterOspfVirtNbrTableFullErrorReturn OBJECT-IDENTITY
    	STATUS      current
    	DESCRIPTION "The maximum number of virtual neighbor entries has been reached."
    ::= { hm2AgentRoutingSNMPExtensionGroup 5 }
    
    hm2AgentRouterRIPDependenciesNotMet OBJECT-IDENTITY
    	STATUS      current
    	DESCRIPTION "Cannot modify RIP admin state on this interface. Set primary IP address."
    ::= { hm2AgentRoutingSNMPExtensionGroup 8 }
    
    hm2AgentIpHelperInvalidUdpPortErrorReturn OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "Invalid UDP port."
    ::= { hm2AgentRoutingSNMPExtensionGroup 9 }

     hm2AgentStaticNeighbourTableFullErrorReturn OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "Static Neighbour Table is full."
    ::= { hm2AgentRoutingSNMPExtensionGroup 10 }

    hm2AgentSecondaryAddrNoPrimaryErrorReturn OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "Cannot add the secondary IP address because the interface has no primary IP address."
    ::= { hm2AgentRoutingSNMPExtensionGroup 11 }

    hm2AgentSecondaryAddrDifferentPrimaryErrorReturn OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The secondary IP address must be different from the primary IP address."
    ::= { hm2AgentRoutingSNMPExtensionGroup 12 }

    hm2AgentSecondaryAddrWrongIpClassErrorReturn OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The network number of the secondary IP address is not valid to be used on a routing interface."
    ::= { hm2AgentRoutingSNMPExtensionGroup 13 }

    hm2AgentSecondaryAddrWrongSubnetErrorReturn OBJECT-IDENTITY
           STATUS      obsolete
           DESCRIPTION "All IP addresses on the interface must be from different subnets."
    ::= { hm2AgentRoutingSNMPExtensionGroup 14 }

    hm2AgentSecondaryAddrMaxIntfEntriesErrorReturn OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The maximum number of secondary IP addresses on the interface has been reached."
    ::= { hm2AgentRoutingSNMPExtensionGroup 15 }

    hm2AgentSecondaryAddrMaxSystemEntriesErrorReturn OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The maximum number of IP addresses on the system has been reached."
    ::= { hm2AgentRoutingSNMPExtensionGroup 16 }

    hm2AgentSecondaryAddrStaticRouteErrorReturn OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The secondary IP address is same as the next hop address of a static route."
    ::= { hm2AgentRoutingSNMPExtensionGroup 17 }

    hm2AgentSecondaryAddrStaticARPErrorReturn OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The secondary IP address is same as a static ARP entry."
    ::= { hm2AgentRoutingSNMPExtensionGroup 18 }

    hm2AgentSecondaryAddrAbsentEntryErrorReturn OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The secondary IP address is not configured on the interface."
    ::= { hm2AgentRoutingSNMPExtensionGroup 19 }

    hm2AgentPrimaryAddrWrongIpClassErrorReturn OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The primary IP address is out of the allowed IP class."
    ::= { hm2AgentRoutingSNMPExtensionGroup 20 }

    hm2AgentPrimaryAddrConflictErrorReturn OBJECT-IDENTITY
           STATUS      obsolete
           DESCRIPTION "The primary IP address conflicts with another IP address on a routing interface."
    ::= { hm2AgentRoutingSNMPExtensionGroup 21 }

   hm2AgentPrimaryAddrStaticRouteErrorReturn OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The primary IP address is same as the next hop address of a static route."
    ::= { hm2AgentRoutingSNMPExtensionGroup 22 }

   hm2AgentPrimaryAddrStaticARPErrorReturn OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The primary IP address is same as a static ARP entry."
    ::= { hm2AgentRoutingSNMPExtensionGroup 23 }

   hm2AgentPrimaryAddrExistingSecondaryErrorReturn OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The primary IP address cannot be changed because the interface has secondary IP addresses configured."
    ::= { hm2AgentRoutingSNMPExtensionGroup 24 }

   hm2AgentPrimaryAddrNetworkConflictErrorReturn OBJECT-IDENTITY
           STATUS      obsolete
           DESCRIPTION "The primary IP address conflicts with the management IP address."
    ::= { hm2AgentRoutingSNMPExtensionGroup 25 }

   hm2AgentPrimaryAddrRoutingTableFullErrorReturn OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The primary IP address cannot be added because there are no free entries in the routing table."
    ::= { hm2AgentRoutingSNMPExtensionGroup 26 }

   hm2AgentDstAddrHostBitSetErrorReturn OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The route cannot be added. Host bits must not be set in the destination. Network address is {0}."
    ::= { hm2AgentRoutingSNMPExtensionGroup 27 }
    
   hm2AgentSamePrefRouteErrorReturn OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "Route cannot be added because reject route and next hop route cannot share the same preference."
    ::= { hm2AgentRoutingSNMPExtensionGroup 28 }
    
	hm2AgentVrrpAssoIpAddrRowStatusInconsistentAddress OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The virtual address does not matching the current interface address configuration."
    ::= { hm2AgentRoutingSNMPExtensionGroup 29 }

	hm2AgentVrrpAssoIpAddrRowStatusInvalidAddress OBJECT-IDENTITY
	       STATUS      current
           DESCRIPTION "The virtual address is not valid with the current interface address configuration."
    ::= { hm2AgentRoutingSNMPExtensionGroup 30 }
	
	hm2AgentVrrpAssoIpAddrRowStatusUnknownVRID OBJECT-IDENTITY
	       STATUS      current
           DESCRIPTION "Unknown virtual router id."
    ::= { hm2AgentRoutingSNMPExtensionGroup 31 }
    
	hm2AgentSwitchIpRouterDiscMinMaxAdvtIntErrorRtrn OBJECT-IDENTITY
	       STATUS      current
           DESCRIPTION "Min advertisement interval is  bigger then max advertisement interval."
    ::= { hm2AgentRoutingSNMPExtensionGroup 32 }
    
	hm2AgentSwitchIpRouterDiscLifeTimeMaxAdvIntErrorRtrn OBJECT-IDENTITY
	       STATUS      current
           DESCRIPTION "Max advertisement interval is bigger then advertisement life time."
    ::= { hm2AgentRoutingSNMPExtensionGroup 33 }    

    hm2AgentSwitchIpIcmpRateLimitExceedingRatioErrorReturn OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "Rate limit ratio exceeds 100 packets per second."
    ::= { hm2AgentRoutingSNMPExtensionGroup 34 }

    hm2AgentRouterOspfMaxAreaErrorReturn OBJECT-IDENTITY
    	STATUS      current
    	DESCRIPTION "The maximum number of OSPF areas has been reached."
    ::= { hm2AgentRoutingSNMPExtensionGroup 35 }
    
    hm2AgentospfRouterIdChange OBJECT-IDENTITY
    	STATUS      current
    	DESCRIPTION "OSPF must be disabled to change the router ID."
    ::= { hm2AgentRoutingSNMPExtensionGroup 36 }
    
    hm2AgentOspfRedistDistList OBJECT-IDENTITY
    	STATUS      current
    	DESCRIPTION "Please add a redistribute list."
    ::= { hm2AgentRoutingSNMPExtensionGroup 37 }
    
    hm2AgentOspfDefaultAreaDeleteErrorReturn OBJECT-IDENTITY
    	STATUS      current
    	DESCRIPTION "The default area cannot be deleted."
    ::= { hm2AgentRoutingSNMPExtensionGroup 38 }
    
    hm2AgentLocalArpDeleteErrorReturn OBJECT-IDENTITY
    	STATUS      current
    	DESCRIPTION "Local ARP entries cannot be deleted."
    ::= { hm2AgentRoutingSNMPExtensionGroup 39 }

    hm2AgentDynamicVlanRoutingErrorReturn OBJECT-IDENTITY
    	STATUS      current
    	DESCRIPTION "Dynamic VLANs cannot be used for routing interfaces."
    ::= { hm2AgentRoutingSNMPExtensionGroup 40 }

	hm2AgentVlanUnawareRoutingErrorReturn OBJECT-IDENTITY
    	STATUS      current
    	DESCRIPTION "Routing cannot be used together with the vlan unaware mode."
    ::= { hm2AgentRoutingSNMPExtensionGroup 41 }

    hm2AgentRoutingInvalidNetworkAddress OBJECT-IDENTITY
          STATUS      current
          DESCRIPTION "Indicates that the routing table entry contains an invalid value for 
                       network address that cannot be processed."
          ::= { hm2AgentRoutingSNMPExtensionGroup 42 }

    hm2AgentRoutingTypeInvalidValue OBJECT-IDENTITY
          STATUS      current
          DESCRIPTION "Indicates that the type is invalid."
          ::= { hm2AgentRoutingSNMPExtensionGroup 43 }

    hm2AgentRoutingLocalRoutePreference OBJECT-IDENTITY
          STATUS      current
          DESCRIPTION "Indicates that the local type and local protocol should have the preference
                       value zero."
          ::= { hm2AgentRoutingSNMPExtensionGroup 44 }

    hm2AgentRoutingMetricInvalid OBJECT-IDENTITY
          STATUS      current
          DESCRIPTION "Indicates that the routing table entry contains an invalid value for
                        metric that cannot be processed."
          ::= { hm2AgentRoutingSNMPExtensionGroup 45 }

    hm2AgentRoutingMetricNotSupported OBJECT-IDENTITY
          STATUS      current
          DESCRIPTION "Indicates that the route metric except 1 is not supported and cannot be set."
          ::= { hm2AgentRoutingSNMPExtensionGroup 46 }

    hm2AgentRoutingNexthopAtLocalInterface OBJECT-IDENTITY
          STATUS      current
          DESCRIPTION "Indicates that the entry has Nexthop address that is set on a local interface."
          ::= { hm2AgentRoutingSNMPExtensionGroup 47 }

    hm2AgentRoutingNexthopInvalid OBJECT-IDENTITY
          STATUS      current
          DESCRIPTION "Indicates that the routing table entry contains an invalid value for
                        next hop IP address that cannot be processed."
          ::= { hm2AgentRoutingSNMPExtensionGroup 48 }

    hm2AgentRoutingMaxEntryCountReached OBJECT-IDENTITY
          STATUS      current
          DESCRIPTION "Indicates that the route entry cannot be added as maximum count has reached."
          ::= { hm2AgentRoutingSNMPExtensionGroup 49 }

    hm2AgentRoutingNoPreferenceUpdate OBJECT-IDENTITY
          STATUS      current
          DESCRIPTION "Indicates that the preference value cannot be updated."
          ::= { hm2AgentRoutingSNMPExtensionGroup 50 }

    hm2AgentRoutingPortInvalid OBJECT-IDENTITY
          STATUS      current
          DESCRIPTION "Indicates that the routing table entry contains an invalid value for
                        port that cannot be processed."
          ::= { hm2AgentRoutingSNMPExtensionGroup 51 }

    hm2AgentRoutingStaticRoutePreference OBJECT-IDENTITY
          STATUS      current
          DESCRIPTION "Indicates that the remote type and netmgmt protocol should have the preference
                       value in range 1..255."
          ::= { hm2AgentRoutingSNMPExtensionGroup 52 }

    hm2AgentRoutingSameNetworkAddrErrorReturn OBJECT-IDENTITY
          STATUS      current
          DESCRIPTION "Indicates that the entry with same network address already exists."
          ::= { hm2AgentRoutingSNMPExtensionGroup 53 }

    hm2AgentRoutingTypeInvalid OBJECT-IDENTITY
          STATUS      current
          DESCRIPTION "Indicates that the routing table entry contains an invalid value for
                        route type that cannot be processed."
          ::= { hm2AgentRoutingSNMPExtensionGroup 54 }

    hm2AgentRoutingMacAddressInvalid OBJECT-IDENTITY
          STATUS      current
          DESCRIPTION "Indicates that the entry contains an invalid value for MAC address that
                        cannot be processed."
          ::= { hm2AgentRoutingSNMPExtensionGroup 55 }

    hm2AgentRoutingIPAddressExist OBJECT-IDENTITY
          STATUS      current
          DESCRIPTION "Indicates that IP address already exists."
          ::= { hm2AgentRoutingSNMPExtensionGroup 56 }

    hm2AgentRoutingPingPortInvalid OBJECT-IDENTITY
          STATUS      current
          DESCRIPTION "Indicates that the ping port contains an invalid value
                       that cannot be processed."
          ::= { hm2AgentRoutingSNMPExtensionGroup 57 }

    hm2AgentRoutingIntervalTimeInvalid OBJECT-IDENTITY
          STATUS      current
          DESCRIPTION "Indicates that the tracking configuration entry contains invalid
                       characters or is out of range for ping interval time that cannot
                       be processed. The allowed range is 100..20000."
          ::= { hm2AgentRoutingSNMPExtensionGroup 58 }

    hm2AgentRoutingPingLoseTimeInvalid OBJECT-IDENTITY
          STATUS      current
          DESCRIPTION "Indicates that the tracking configuration entry contains invalid
                       characters or is out of range for ping replies to lose time
                       that cannot be processed. The allowed range is 1..10."
          ::= { hm2AgentRoutingSNMPExtensionGroup 59 }

    hm2AgentRoutingPingReceiveTimeInvalid OBJECT-IDENTITY
          STATUS      current
          DESCRIPTION "Indicates that the tracking configuration entry contains invalid
                       characters or is out of range for ping replies to receive time
                       that cannot be processed. The allowed range is 1..10."
          ::= { hm2AgentRoutingSNMPExtensionGroup 60 }

    hm2AgentRoutingPingTimeoutInvalid OBJECT-IDENTITY
          STATUS      current
          DESCRIPTION "Indicates that the tracking configuration entry contains invalid
                       characters or is out of range for ping timeout that cannot be
                       processed. The allowed range is 10..10000."
          ::= { hm2AgentRoutingSNMPExtensionGroup 61 }

    hm2AgentRoutingPingTTLInvalid OBJECT-IDENTITY
          STATUS      current
          DESCRIPTION "Indicates that the tracking configuration entry contains invalid
                       characters or is out of range for ping TTL that cannot be
                       processed. The allowed range is 1..125."
          ::= { hm2AgentRoutingSNMPExtensionGroup 62 }

    hm2AgentRoutingLogicalOperandInvalid OBJECT-IDENTITY
          STATUS      current
          DESCRIPTION "Indicates that the tracking configuration entry contains an
                       invalid value for logical operand A|B that cannot be processed."
          ::= { hm2AgentRoutingSNMPExtensionGroup 63 }

    hm2AgentRoutingOperatorInvalid OBJECT-IDENTITY
          STATUS      current
          DESCRIPTION "Indicates that the tracking configuration entry contains an invalid
                       value for operator that cannot be processed. Possible values
                       'and' and 'or'."
          ::= { hm2AgentRoutingSNMPExtensionGroup 64 }

    hm2AgentRoutingLinkDelayInvalid OBJECT-IDENTITY
          STATUS      current
          DESCRIPTION "Indicates that the tracking configuration entry contains an invalid
                       value for link up/down delay which is out of range and cannot be
                       processed. The allowed range is 0..255."
          ::= { hm2AgentRoutingSNMPExtensionGroup 65 }

    hm2AgentRoutingL3RelayFunctionInvalid OBJECT-IDENTITY
          STATUS      current
          DESCRIPTION "Indicates that the L3 relay function contains an invalid value
                       that cannot be processed."
          ::= { hm2AgentRoutingSNMPExtensionGroup 66 }

    hm2AgentRoutingBootpDhcpHopsInvalid OBJECT-IDENTITY
          STATUS      current
          DESCRIPTION "Indicates that L3 configuration entry contains invalid characters
                       or is out of range for bootp/dhcp hops (max.) that cannot be
                       processed. The allowed range is 1..16."
          ::= { hm2AgentRoutingSNMPExtensionGroup 67 }

    hm2AgentRoutingBootpDhcpWaitTimeInvalid OBJECT-IDENTITY
          STATUS      current
          DESCRIPTION "Indicates that L3 configuration entry contains invalid characters
                       or is out of range for bootp/dhcp wait time (min.) that cannot be
                       processed. The allowed range is 0..100."
          ::= { hm2AgentRoutingSNMPExtensionGroup 68 }

    hm2AgentRoutingCircuitIDInvalid OBJECT-IDENTITY
          STATUS      current
          DESCRIPTION "Indicates that the tracking configuration entry contains
                       an invalid value for circuit ID that cannot be processed."
          ::= { hm2AgentRoutingSNMPExtensionGroup 69 }

    hm2AgentRoutingTrackTypeEnableError OBJECT-IDENTITY
          STATUS      current
          DESCRIPTION "Indicates that the process of enabling tracking instance {0} has
                       failed because track type is invalid."
          ::= { hm2AgentRoutingSNMPExtensionGroup 70 }

    hm2AgentRoutingTrackingEnableErrorReturn OBJECT-IDENTITY
          STATUS      current
          DESCRIPTION "Indicates that the process of enabling tracking instance {0}
                       admin state has failed."
          ::= { hm2AgentRoutingSNMPExtensionGroup 71 }

    hm2AgentRoutingTrackingDisableErrorReturn OBJECT-IDENTITY
          STATUS      current
          DESCRIPTION "Indicates that the process of disabling tracking instance {0}
                       admin state has failed."
          ::= { hm2AgentRoutingSNMPExtensionGroup 72 }

    hm2AgentRoutingTrackTypeDisableError OBJECT-IDENTITY
          STATUS      current
          DESCRIPTION "Indicates that the process of disabling tracking instance {0} has
                       failed because track type is invalid."
          ::= { hm2AgentRoutingSNMPExtensionGroup 73 }

    hm2AgentRoutingTrackIDCreateError OBJECT-IDENTITY
          STATUS      current
          DESCRIPTION "Indicates that the creation of tracking instance {0} has failed
                       because track ID is invalid."
          ::= { hm2AgentRoutingSNMPExtensionGroup 74 }

    hm2AgentRoutingTrackTypeCreateError OBJECT-IDENTITY
          STATUS      current
          DESCRIPTION "Indicates that the creation of tracking instance {0} has failed
                       because track type is invalid."
          ::= { hm2AgentRoutingSNMPExtensionGroup 75 }

END