
HM2-DNS-MIB DEFINITIONS ::= BEGIN

--
-- ************************************************************* 
-- Hirschmann DNS Management MIB
-- *************************************************************
-- 

IMPORTS
   MODULE-IDENTITY,
   OBJECT-IDENTITY, 
   Integer32,
   OBJECT-TYPE                          FROM SNMPv2-SMI -- RFC 2578
   RowStatus                            FROM SNMPv2-TC
   SnmpAdminString						FROM SNMP-FRAMEWORK-MIB
   hm2ConfigurationMibs,
   HmActionValue,
   HmEnabledStatus                      FROM HM2-TC-MIB
   InetAddressType, InetAddress         FROM INET-ADDRESS-MIB; -- RFC4001  


hm2DnsMib MODULE-IDENTITY
    LAST-UPDATED "201106170000Z" -- June 17, 2011
    ORGANIZATION "Hirschmann Automation and Control GmbH"
    CONTACT-INFO
        "Postal:     Stuttgarter Str. 45-51
                     72654 Neckartenzlingen
                     Germany
         Phone:      +49 7127 140
         E-mail:     hac.support@belden.com"
    DESCRIPTION
        "Hirschmann DNS MIB for DNS client, DNS client cache and DNS caching server.
         Copyright (C) 2011. All Rights Reserved."
    REVISION     "201106170000Z" -- June 17, 2011
    DESCRIPTION
         "Initial version."
    ::= { hm2ConfigurationMibs 90 }


--
-- *************************************************************
-- hm2DnsMib
-- *************************************************************
--
hm2DnsMibNotifications      OBJECT IDENTIFIER ::= { hm2DnsMib 0 }
hm2DnsMibObjects            OBJECT IDENTIFIER ::= { hm2DnsMib 1 }
-- hm2DnsMibConformance		OBJECT IDENTIFIER ::= { hm2DnsMib 2 }
hm2DnsMibSNMPExtensionGroup OBJECT IDENTIFIER ::= { hm2DnsMib 3 }

--
-- *************************************************************
-- hm2DnsMib groups
-- *************************************************************
--
hm2DnsClientGroup           OBJECT IDENTIFIER ::= { hm2DnsMibObjects 1 }
hm2DnsCacheGroup            OBJECT IDENTIFIER ::= { hm2DnsMibObjects 2 } -- deprecated 
hm2DnsCachingServerGroup    OBJECT IDENTIFIER ::= { hm2DnsMibObjects 3 }

--
-- *************************************************************
-- hm2DnsClient
-- *************************************************************
--

hm2DnsClientAdminState OBJECT-TYPE
            SYNTAX           HmEnabledStatus
            MAX-ACCESS       read-write
            STATUS           current
            DESCRIPTION
            "The operational status of DNS client. If disabled, no host name
            lookups will be done for names entered on the CLI and in the
            configuration of services e.g. NTP."
            DEFVAL          { disable } 
            ::= { hm2DnsClientGroup 1 }

hm2DnsClientConfigSource    OBJECT-TYPE
            SYNTAX          INTEGER {
                            user(1),
                            mgmt-dhcp(2),
                            provider(3)
                            }
            MAX-ACCESS      read-write
            STATUS          current
            DESCRIPTION
                "DNS client server source.
                 If the value is set to user(1), 
                 the variables from hm2DnsClientServerCfgTable
                 will be used.
                 If the value is set to mgmt-dhcp(2), the DNS servers received
                 by DHCP on the management interface will be used.
                 If the value is set to provider(3),
                 the DNS configuration will be taken from DHCP, PPP or PPPoE on
                 the primary WAN link."
            DEFVAL { mgmt-dhcp }
            ::= { hm2DnsClientGroup 2 }

--
-- DNS Client Configuration Table
--
hm2DnsClientServerCfgTable OBJECT-TYPE
            SYNTAX SEQUENCE OF Hm2DnsClientServerCfgEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION "The table that contains the DNS Servers entries configured by the user in the system."
            ::= { hm2DnsClientGroup 3 }

hm2DnsClientServerCfgEntry OBJECT-TYPE
            SYNTAX Hm2DnsClientServerCfgEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION "An entry contains the IP address of a DNS server configured in the system."
            INDEX { hm2DnsClientServerIndex }
            ::= { hm2DnsClientServerCfgTable 1 }

            
Hm2DnsClientServerCfgEntry ::= SEQUENCE {
                hm2DnsClientServerIndex   Integer32,
                hm2DnsClientServerAddressType InetAddressType,
                hm2DnsClientServerAddress  InetAddress,
                hm2DnsClientServerRowStatus   RowStatus
            }

hm2DnsClientServerIndex OBJECT-TYPE
            SYNTAX Integer32 (1..4)
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION "The unique index used for each server added in the DNS servers table."
            ::= { hm2DnsClientServerCfgEntry 1 }

hm2DnsClientServerAddressType OBJECT-TYPE
           SYNTAX     InetAddressType
           MAX-ACCESS read-write
           STATUS     current
           DESCRIPTION
               "Address type for DNS server.
                Currently, only ipv4 and ipv6 are supported."
           DEFVAL { ipv4 }         
           ::= { hm2DnsClientServerCfgEntry 2 }
                    
hm2DnsClientServerAddress OBJECT-TYPE
           SYNTAX     InetAddress
           MAX-ACCESS read-write
           STATUS     current
           DESCRIPTION "The IP address of the DNS server."
           DEFVAL { '00000000'H }
           ::= { hm2DnsClientServerCfgEntry 3 }

hm2DnsClientServerRowStatus OBJECT-TYPE
            SYNTAX RowStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION "Describes the status of a row in the table."
            ::= { hm2DnsClientServerCfgEntry 4 }
-- end of DNS Client Configuration Table

--
-- DNS Client Diagnostics Table - contains the list of used DNS servers
--
hm2DnsClientServerDiagTable OBJECT-TYPE
            SYNTAX SEQUENCE OF Hm2DnsClientServerDiagEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION "The table that contains the DNS Servers entries configured and used in the system."
            ::= { hm2DnsClientGroup 4 }

hm2DnsClientServerDiagEntry OBJECT-TYPE
            SYNTAX Hm2DnsClientServerDiagEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION "An entry contains the IP address of a DNS server used in the system."
            INDEX { hm2DnsClientServerDiagIndex }
            ::= { hm2DnsClientServerDiagTable 1 }

Hm2DnsClientServerDiagEntry ::= SEQUENCE {
                hm2DnsClientServerDiagIndex   		Integer32,
                hm2DnsClientServerDiagAddressType 	InetAddressType,
                hm2DnsClientServerDiagAddress  		InetAddress
            }

hm2DnsClientServerDiagIndex OBJECT-TYPE
            SYNTAX Integer32 (1..4)
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION "The unique index used for each server added in the DNS servers table."
            ::= { hm2DnsClientServerDiagEntry 1 }

hm2DnsClientServerDiagAddressType OBJECT-TYPE
           SYNTAX     InetAddressType
           MAX-ACCESS read-only
           STATUS     current
           DESCRIPTION
               "Address type for DNS server used.
                Currently, only ipv4 and ipv6 are supported."
           ::= { hm2DnsClientServerDiagEntry 2 }
                    
hm2DnsClientServerDiagAddress OBJECT-TYPE
           SYNTAX     InetAddress
           MAX-ACCESS read-only
           STATUS     current
           DESCRIPTION "The IP address of the DNS server used by the system.
                        The entry can be configured by the provider, e.g. 
                        through DHCP client or PPPoE client."
           ::= { hm2DnsClientServerDiagEntry 3 }

-- end of DNS Client Diagnostics Table

--
-- DNS Client Global Group
--
hm2DnsClientGlobalGroup OBJECT IDENTIFIER ::= { hm2DnsClientGroup 5 }
hm2DnsClientDefaultDomainName OBJECT-TYPE
       SYNTAX      SnmpAdminString (SIZE (0..255))
       MAX-ACCESS  read-write
       STATUS      current
       DESCRIPTION
               "The default domain name for unqualified hostnames."
       DEFVAL { "" }
       ::= { hm2DnsClientGlobalGroup 1 }
       
hm2DnsClientRequestTimeout OBJECT-TYPE
       SYNTAX  Integer32 (0..3600)
       MAX-ACCESS  read-write
       STATUS      current
       DESCRIPTION
               "The timeout before retransmitting a request to the server. The 
                timeout value is configured and displayed in seconds."
       DEFVAL { 3 }
       ::= { hm2DnsClientGlobalGroup 2 }

hm2DnsClientRequestRetransmits OBJECT-TYPE
       SYNTAX  Integer32 (0..100)
       MAX-ACCESS  read-write
       STATUS      current
       DESCRIPTION
               "The number of times the request is retransmitted. The request
                is retransmitted provided the maximum timeout value allows
                this many number of retransmits."
       DEFVAL { 2 }
       ::= { hm2DnsClientGlobalGroup 3 }

hm2DnsClientCacheAdminState OBJECT-TYPE
	   SYNTAX           HmEnabledStatus
	   MAX-ACCESS       read-write
	   STATUS           current
	   DESCRIPTION
	   "Enables/Disables DNS client cache functionality of the device."
	   DEFVAL          { enable } 
	   ::= { hm2DnsClientGlobalGroup 4 }
	   
--
-- DNS Client Static Host Table
--
hm2DnsClientStaticHostConfigTable OBJECT-TYPE
       SYNTAX      SEQUENCE OF Hm2DnsClientStaticHostConfigEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
               "Static table of DNS hostname to IP address table"
       ::= {hm2DnsClientGroup 6 }

hm2DnsClientStaticHostConfigEntry OBJECT-TYPE
       SYNTAX      Hm2DnsClientStaticHostConfigEntry 
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
               "An entry in the static DNS hostname IP address list.
               Rows may be created or deleted at any time by the DNS
               resolver and by SNMP SET requests."
       INDEX     { hm2DnsClientStaticIndex } 
       ::= {hm2DnsClientStaticHostConfigTable 1 }

Hm2DnsClientStaticHostConfigEntry ::=
       SEQUENCE {
          hm2DnsClientStaticIndex
               Integer32,
          hm2DnsClientStaticHostName
               SnmpAdminString,
          hm2DnsClientStaticHostAddressType
               InetAddressType,
          hm2DnsClientStaticHostIPAddress
               InetAddress,
          hm2DnsClientStaticHostStatus
               RowStatus
       }

hm2DnsClientStaticIndex OBJECT-TYPE
       SYNTAX      Integer32 (1..64)
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
               "The index of the entry."
       ::= {hm2DnsClientStaticHostConfigEntry 1 }

hm2DnsClientStaticHostName OBJECT-TYPE
       SYNTAX      SnmpAdminString (SIZE (0 .. 255))
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
               "The static hostname."
       ::= {hm2DnsClientStaticHostConfigEntry 2 }

hm2DnsClientStaticHostAddressType OBJECT-TYPE
       SYNTAX     InetAddressType
       MAX-ACCESS read-create
       STATUS     current
       DESCRIPTION
               "Address type for static hosts used.
                Currently, only ipv4 and ipv6 are supported."
       ::= { hm2DnsClientStaticHostConfigEntry 3 }
           
hm2DnsClientStaticHostIPAddress OBJECT-TYPE
       SYNTAX      InetAddress
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
               "The IP address of the static host."
       ::= {hm2DnsClientStaticHostConfigEntry 4 }

hm2DnsClientStaticHostStatus OBJECT-TYPE
       SYNTAX      RowStatus
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
               "Describes the status of a row in the table."
       ::= { hm2DnsClientStaticHostConfigEntry 5 }

--
-- hm2DnsCachingServerGroup
--
hm2DnsCachingServerGlobalGroup OBJECT IDENTIFIER ::= { hm2DnsCachingServerGroup 1 }

hm2DnsCachingServerAdminState OBJECT-TYPE
            SYNTAX           HmEnabledStatus
            MAX-ACCESS       read-write
            STATUS           current
            DESCRIPTION
            "Enables/Disables DNS caching server functionality of the device."
            DEFVAL { enable } 
            ::= { hm2DnsCachingServerGlobalGroup 1 }

--
-- hm2DnsCache - deprecated
--
hm2DnsCacheAdminState OBJECT-TYPE
            SYNTAX           HmEnabledStatus
            MAX-ACCESS       read-write
            STATUS           deprecated
            DESCRIPTION
            "Enables/Disables DNS cache functionality of the device.
             **NOTE: this object is deprecated and replaced by hm2DnsClientCacheAdminState/hm2DnsCachingServerAdminState**."
            DEFVAL { enable } 
            ::= { hm2DnsCacheGroup 1 }

hm2DnsCacheFlushAction OBJECT-TYPE
            SYNTAX           HmActionValue
            MAX-ACCESS       read-write
            STATUS           deprecated
            DESCRIPTION
            "Setting this value to action will flush the DNS cache. After flushing the cache, 
             it will be set to noop automatically.
             **NOTE: this object is deprecated and replaced by hm2DevMgmtActionFlushDnsClientCache/hm2DevMgmtActionFlushDnsCachingServerCache**."
            DEFVAL          { noop } 
            ::= { hm2DnsCacheGroup 2 }

hm2DnsCHHostNameAlreadyExistsSESError OBJECT-IDENTITY
	STATUS      current
	DESCRIPTION "The host name entered exists and is associated with an IP. The change attempt was canceled."
	::= { hm2DnsMibSNMPExtensionGroup 1 }

hm2DnsCHBadIpNotAcceptedSESError OBJECT-IDENTITY
	STATUS      current
	DESCRIPTION "The Ip Adress entered is not a valid one for a host. The change attempt was canceled."
	::= { hm2DnsMibSNMPExtensionGroup 2 }

hm2DnsCHBadRowCannotBeActivatedSESError OBJECT-IDENTITY
	STATUS      current
	DESCRIPTION "The instance cannot be activated due to compliance issues. Please modify the entry and try again."
	::= { hm2DnsMibSNMPExtensionGroup 3 }

END
