HM2-L2REDUNDANCY-LRE-MIB DEFINITIONS ::= BEGIN

--
-- *************************************************************
-- Hirschmann Layer 2 Redundancy LRE MIB
-- *************************************************************
--

IMPORTS 
    MODULE-IDENTITY,
    OBJECT-TYPE,
    Unsigned32, 	
    Counter32                       FROM SNMPv2-SMI
    TruthValue                      FROM SNMPv2-TC
    InterfaceIndex                  FROM IF-MIB
    hm2L2RedundancyMibObjects       FROM HM2-L2REDUNDANCY-MIB
    lreInterfaceConfigIndex,
    lreInterfaceStatsIndex          FROM IEC-62439-3-MIB;

hm2LreMibGroup			MODULE-IDENTITY 
    LAST-UPDATED "201207020000Z"
    ORGANIZATION "Hirschmann Automation and Control GmbH"
    CONTACT-INFO
        "Postal:     Stuttgarter Str. 45-51
                     72654 Neckartenzlingen
                     Germany
         Phone:      +49 7127 140
         E-mail:     hac.support@belden.com"
    DESCRIPTION
        "Hirschmann Layer 2 Redundancy LRE MIB.
         Copyright (C) 2012. All Rights Reserved."
    REVISION "201207020000Z"
    DESCRIPTION
        "Initial version."
    ::= { hm2L2RedundancyMibObjects 2 }

-- ****************************************************************************
-- Objects of the LRE Network Management
-- ****************************************************************************

hm2LreEntityNotifications 	OBJECT IDENTIFIER ::={ hm2LreMibGroup 0 }
hm2LreEntityObjects 		OBJECT IDENTIFIER ::={ hm2LreMibGroup 1 }
hm2LreEntityConformance 	OBJECT IDENTIFIER ::={ hm2LreMibGroup 2 }

hm2LreConfiguration 		OBJECT IDENTIFIER ::={ hm2LreEntityObjects 1 }
hm2LreStatistics 			OBJECT IDENTIFIER ::={ hm2LreEntityObjects 2 }

hm2LreConfigurationGeneralGroup 	OBJECT IDENTIFIER ::={ hm2LreConfiguration 1 }
hm2LreConfigurationInterfaceGroup 	OBJECT IDENTIFIER ::={ hm2LreConfiguration 2 }

hm2LreStatisticsInterfaceGroup 		OBJECT IDENTIFIER ::={ hm2LreStatistics 1 }

-- ****************************************************************************
-- Objects for lreConfigurationInterfacesGroup
-- ****************************************************************************

hm2LreConfigurationInterfaces OBJECT IDENTIFIER 
 ::= { hm2LreConfigurationInterfaceGroup 1 }


-- *************************************
-- ***Begin InterfaceConfigTable***
-- *************************************
hm2LreInterfaceConfigTable OBJECT-TYPE
  SYNTAX SEQUENCE OF HM2LREInterfaceConfigEntry
  MAX-ACCESS 		not-accessible
  STATUS 			current
  DESCRIPTION
    "List of PRP/HSR interfaces. Each entry corresponds
    to one PRP/HSR Link Redundancy Entity (LRE), each representing a
    pair of LAN adapters A and B. A basic device supporting PRP/HSR might
    have only one LRE and thus one entry in the table, while more complex
    devices might have several entries for multiple LRE's."
  ::= { hm2LreConfigurationInterfaces 1 }


hm2LreInterfaceConfigEntry OBJECT-TYPE
  SYNTAX HM2LREInterfaceConfigEntry
  MAX-ACCESS 	not-accessible
  STATUS 		current
  DESCRIPTION
    "Each entry contains management information applicable to a
     particular LRE."
  INDEX { lreInterfaceConfigIndex }
::= { hm2LreInterfaceConfigTable 1 }

HM2LREInterfaceConfigEntry ::=
  SEQUENCE {
  hm2LreInterfaceA                  InterfaceIndex,
  hm2LreInterfaceB                  InterfaceIndex,
  hm2LreProxyNodeTableSize          Unsigned32,
  hm2LreSupervisionTxEnable         TruthValue,
  hm2LreSupervisionVDANsTxEnable    TruthValue,
  hm2LreStatisticsClear             INTEGER,
  hm2LreMaxFrameSizeLimit           Unsigned32,
  hm2LreMaxFrameSize                Unsigned32,
  hm2LreSpeed						INTEGER,
  hm2LreDuplicateDetectionAging     Unsigned32,
  hm2LreProxyNodeTableAging         Unsigned32
  }


hm2LreInterfaceA OBJECT-TYPE
  SYNTAX 		InterfaceIndex
  MAX-ACCESS 	read-only
  STATUS 		current
  DESCRIPTION 
  	"Physical interface in LAN_A."
::= { hm2LreInterfaceConfigEntry 1 }

hm2LreInterfaceB OBJECT-TYPE
  SYNTAX 		InterfaceIndex
  MAX-ACCESS 	read-only
  STATUS 		current
  DESCRIPTION 
  	"Physical interface in LAN_B."
::= { hm2LreInterfaceConfigEntry 2 }

hm2LreProxyNodeTableSize OBJECT-TYPE
  SYNTAX 		Unsigned32
  MAX-ACCESS 	read-only
  STATUS 		current
  DESCRIPTION 
  	"Size of the proxy node table."
::= { hm2LreInterfaceConfigEntry 3 }

hm2LreSupervisionTxEnable OBJECT-TYPE
  SYNTAX        TruthValue
  MAX-ACCESS    read-write
  STATUS        current
  DESCRIPTION 
  "True if the LRE sends supervision frames. False if it
  does not send supervision frames.
  Note: LREs are required to send supervision frames"
  DEFVAL      { true } 
::= { hm2LreInterfaceConfigEntry 4 }

hm2LreSupervisionVDANsTxEnable OBJECT-TYPE
  SYNTAX        TruthValue
  MAX-ACCESS    read-write
  STATUS        current
  DESCRIPTION 
  "True if the LRE sends a supervision for each VDAN. False if it
  does not send supervision frames for each VDAN.
  If supervision transmission for each VDAN is disabled but supervision transmission in general is enabled,
  only one supervision frame from LRE management is send."
  DEFVAL      { true } 
::= { hm2LreInterfaceConfigEntry 5 }

hm2LreStatisticsClear   OBJECT-TYPE
  SYNTAX                INTEGER
                        {
  noOp (0),
  clearStatistics (1)
  }
  MAX-ACCESS read-write
  STATUS current
  DESCRIPTION           
  "specifies that the statistics counters are to be cleared"
::= { hm2LreInterfaceConfigEntry 6 }

hm2LreMaxFrameSizeLimit OBJECT-TYPE
  SYNTAX      Unsigned32
  MAX-ACCESS  read-only
  STATUS      current
  DESCRIPTION
             "This object identifies the largest value that can be
             configured for hm2LreMaxFrameSize."
 ::= { hm2LreInterfaceConfigEntry 7 }
         
hm2LreMaxFrameSize OBJECT-TYPE
  SYNTAX      Unsigned32
  MAX-ACCESS  read-write
  STATUS      current
  DESCRIPTION
             "This object identifies the currently configured maximum frame size
              value for this port. The maximum value that this object can be set
              to is the value of hm2LreMaxFrameSizeLimit."
 ::= { hm2LreInterfaceConfigEntry 8 }

hm2LreSpeed OBJECT-TYPE
  SYNTAX      INTEGER
  			{
  				lreSpeed100Mbps (1),
  				lreSpeed1Gbps (2)
  			}
  MAX-ACCESS  read-write
  STATUS      current
  DESCRIPTION
             "Specifies the speed of the LRE interfaces.
             If the device does not support 1Gbps(2), a set to this value will 
             return an error."
  DEFVAL { lreSpeed100Mbps }
 ::= { hm2LreInterfaceConfigEntry 9 }

hm2LreDuplicateDetectionAging OBJECT-TYPE
  SYNTAX      Unsigned32 (10..5000)
  MAX-ACCESS  read-write
  STATUS      current
  DESCRIPTION
             "Specifies the aging time in miliseconds for the duplicate detection."
  DEFVAL { 400 }
 ::= { hm2LreInterfaceConfigEntry 10 }

hm2LreProxyNodeTableAging OBJECT-TYPE
  SYNTAX      Unsigned32 (10..300)
  MAX-ACCESS  read-write
  STATUS      current
  DESCRIPTION
             "Specifies the aging time in seconds for the proxy node table."
  DEFVAL { 60 }
 ::= { hm2LreInterfaceConfigEntry 11 }

-- *************************************
-- ***  End InterfaceConfigTable  ***
-- *************************************


-- ****************************************************************************
-- Objects for lreStatisticsInterfacesGroup
-- ****************************************************************************

hm2LreStatisticsInterfaces OBJECT IDENTIFIER
::= { hm2LreStatisticsInterfaceGroup 1 }

-- *************************************
-- ***Begin LRE InterfacesStatsTable ***
-- *************************************

hm2LreInterfaceStatsTable OBJECT-TYPE
  SYNTAX SEQUENCE OF HM2LREInterfaceStatsEntry
  MAX-ACCESS 	not-accessible
  STATUS 		current
  DESCRIPTION
  	"A list of PRP/HSR redundant interfaces. Each entry corresponds
   	 to one redundant PRP/HSR Link Redundancy Entity (LRE) with a
   	 LAN connector A and B each. A basic device supporting PRP/HSR might
   	 have only one LRE and thus one entry in the table, while more complex
   	 devices might have several entries for multiple LRE's."
  ::= { hm2LreStatisticsInterfaces 1 }


hm2LreInterfaceStatsEntry OBJECT-TYPE
  SYNTAX HM2LREInterfaceStatsEntry
  MAX-ACCESS    not-accessible
  STATUS        current
  DESCRIPTION
    "An entry containing management information applicable to a
     particular LRE."
  INDEX { lreInterfaceStatsIndex }
::= { hm2LreInterfaceStatsTable 1 }

HM2LREInterfaceStatsEntry ::=
  SEQUENCE {
            hm2LreProxyNodeTableEntries Unsigned32,
            hm2LreRxAError              Counter32,
            hm2LreRxACrcError           Counter32,
            hm2LreRxBError              Counter32,
            hm2LreRxBCrcError           Counter32,
            hm2LreRxIError              Counter32,
            hm2LreRxICrcError           Counter32,
            hm2LreRxAWrongLan           Counter32,
            hm2LreRxBWrongLan           Counter32,
            hm2LreRxAllFrameA           Counter32,
            hm2LreRxAllFrameB           Counter32,
            hm2LreRxAllFrameIl          Counter32,
            hm2LreRxShortFrameA         Counter32,
            hm2LreRxShortFrameB         Counter32,
            hm2LreRxLongFrameA          Counter32,
            hm2LreRxLongFrameB          Counter32,
            hm2LreRxADiscard            Counter32,
            hm2LreRxBDiscard            Counter32,
            hm2LreRxIlDiscard           Counter32,
            hm2LreRxCpuDiscard          Counter32,
            hm2LreTxARct                Counter32,
            hm2LreTxAHsr                Counter32,
            hm2LreTxAWithoutRct         Counter32,
            hm2LreTxBRct                Counter32,
            hm2LreTxBHsr                Counter32,
            hm2LreTxBWithoutRct         Counter32,
            hm2LreTxIlRct               Counter32,
            hm2LreTxIlWithoutRct        Counter32
  }


hm2LreProxyNodeTableEntries OBJECT-TYPE
  SYNTAX 		Unsigned32
  MAX-ACCESS 	read-only
  STATUS 		current
  DESCRIPTION
  	"Entries in the proxy node table.
   	 Initial value = 0."
::= { hm2LreInterfaceStatsEntry 1 }

hm2LreRxAError              OBJECT-TYPE
  SYNTAX        Counter32
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
    "number of phy receive errors on port A.
     Initial value = 0."
::= { hm2LreInterfaceStatsEntry 2 }

hm2LreRxACrcError           OBJECT-TYPE
  SYNTAX        Counter32
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
    "number of frames received with FCS error,
     fragments and symbol error on port A.
     Initial value = 0."
::= { hm2LreInterfaceStatsEntry 3 }

hm2LreRxBError              OBJECT-TYPE
  SYNTAX        Counter32
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
    "number of phy receive errors on port B.
     Initial value = 0."
::= { hm2LreInterfaceStatsEntry 4 }

hm2LreRxBCrcError           OBJECT-TYPE
  SYNTAX        Counter32
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
    "number of frames received with FCS error,
     fragments and symbol error on port B.
     Initial value = 0."
::= { hm2LreInterfaceStatsEntry 5 }

hm2LreRxIError              OBJECT-TYPE
  SYNTAX        Counter32
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
    "number of phy receive errors on interlink port.
     Initial value = 0."
::= { hm2LreInterfaceStatsEntry 6 }

hm2LreRxICrcError           OBJECT-TYPE
  SYNTAX        Counter32
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
    "number of frames received with FCS error,
     fragments and symbol error on interlink port.
     Initial value = 0."
::= { hm2LreInterfaceStatsEntry 7 }

hm2LreRxAWrongLan           OBJECT-TYPE
  SYNTAX        Counter32
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
    "number of frames with a wrong LAN identifier received on port A.
     Initial value = 0."
::= { hm2LreInterfaceStatsEntry 8 }

hm2LreRxBWrongLan           OBJECT-TYPE
  SYNTAX        Counter32
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
    "number of frames with a wrong LAN identifier received on port B.
     Initial value = 0."
::= { hm2LreInterfaceStatsEntry 9 }

hm2LreRxAllFrameA           OBJECT-TYPE
  SYNTAX        Counter32
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
    "number of frames received on port A.
     Initial value = 0."
::= { hm2LreInterfaceStatsEntry 10 }

hm2LreRxAllFrameB           OBJECT-TYPE
  SYNTAX        Counter32
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
    "number of frames received on port B.
     Initial value = 0."
::= { hm2LreInterfaceStatsEntry 11 }

hm2LreRxAllFrameIl          OBJECT-TYPE
  SYNTAX        Counter32
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
    "number of frames received on interlink port.
     Initial value = 0."
::= { hm2LreInterfaceStatsEntry 12 }

hm2LreRxShortFrameA         OBJECT-TYPE
  SYNTAX        Counter32
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
    "number of short frames received on port A.
    These frames are not forwarded.
    Initial value = 0."
::= { hm2LreInterfaceStatsEntry 13 }

hm2LreRxShortFrameB         OBJECT-TYPE
  SYNTAX        Counter32
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
    "number of short frames received on port B.
    These frames are not forwarded.
    Initial value = 0."
::= { hm2LreInterfaceStatsEntry 14 }

hm2LreRxLongFrameA          OBJECT-TYPE
  SYNTAX        Counter32
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
    "number of long frames received on port A.
    These frames are not forwarded.
    Initial value = 0."
::= { hm2LreInterfaceStatsEntry 15 }

hm2LreRxLongFrameB          OBJECT-TYPE
  SYNTAX        Counter32
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
    "number of long frames received on port B.
    These frames are not forwarded.
    Initial value = 0."
::= { hm2LreInterfaceStatsEntry 16 }

hm2LreRxADiscard            OBJECT-TYPE
  SYNTAX        Counter32
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
    "number of frames received on port A which are discarded in internal switch.
     Initial value = 0."
::= { hm2LreInterfaceStatsEntry 17 }

hm2LreRxBDiscard            OBJECT-TYPE
  SYNTAX        Counter32
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
    "number of frames received on port B which are discarded in internal switch.
     Initial value = 0."
::= { hm2LreInterfaceStatsEntry 18 }

hm2LreRxIlDiscard           OBJECT-TYPE
  SYNTAX        Counter32
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
    "number of frames received on interlink port which are discarded in internal switch.
     Initial value = 0."
::= { hm2LreInterfaceStatsEntry 19 }

hm2LreRxCpuDiscard          OBJECT-TYPE
  SYNTAX        Counter32
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
    "number of frames received on CPU port which are discarded in internal switch.
     Initial value = 0."
::= { hm2LreInterfaceStatsEntry 20 }

hm2LreTxARct                OBJECT-TYPE
  SYNTAX        Counter32
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
    "number of frames transmitted on port A with redundancy control trailer (RCT).
     Initial value = 0."
::= { hm2LreInterfaceStatsEntry 21 }

hm2LreTxAHsr                OBJECT-TYPE
  SYNTAX        Counter32
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
    "number of frames transmitted on port A with HSR tag.
     Initial value = 0."
::= { hm2LreInterfaceStatsEntry 22 }

hm2LreTxAWithoutRct         OBJECT-TYPE
  SYNTAX        Counter32
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
    "number of frames transmitted on port A without redundancy control trailer (RCT).
     Initial value = 0."
::= { hm2LreInterfaceStatsEntry 23 }

hm2LreTxBRct                OBJECT-TYPE
  SYNTAX        Counter32
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
    "number of frames transmitted on port B with redundancy control trailer (RCT).
     Initial value = 0."
::= { hm2LreInterfaceStatsEntry 24 }

hm2LreTxBHsr                OBJECT-TYPE
  SYNTAX        Counter32
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
    "number of frames transmitted on port B with HSR tag.
     Initial value = 0."
::= { hm2LreInterfaceStatsEntry 25 }

hm2LreTxBWithoutRct         OBJECT-TYPE
  SYNTAX        Counter32
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
    "number of frames transmitted on port B without redundancy control trailer (RCT).
     Initial value = 0."
::= { hm2LreInterfaceStatsEntry 26 }

hm2LreTxIlRct               OBJECT-TYPE
  SYNTAX        Counter32
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
    "number of frames transmitted on interlink port with redundancy control trailer (RCT).
     Initial value = 0."
::= { hm2LreInterfaceStatsEntry 27 }

hm2LreTxIlWithoutRct        OBJECT-TYPE
  SYNTAX        Counter32
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
    "number of frames transmitted on interlink port without redundancy control trailer (RCT).
     Initial value = 0."
::= { hm2LreInterfaceStatsEntry 28 }


-- *************************************
-- ***  End LRE InterfacesStatsTable ***
-- *************************************

END

