HM2-DHCPS-MIB DEFINITIONS ::= BEGIN

--
-- ***********************************************************
-- Hirschmann DHCP Server MIB
-- ***********************************************************
--

IMPORTS
	OBJECT-IDENTITY,
    MODULE-IDENTITY,
    OBJECT-TYPE,
	Integer32,
	Counter32,  
	Unsigned32, 
	IpAddress                   FROM SNMPv2-SMI -- RFC 2578
    RowStatus, 
	DisplayString, 
	MacAddress	                FROM SNMPv2-TC
    hm2ConfigurationMibs,
    HmEnabledStatus             FROM HM2-TC-MIB
    InterfaceIndex              FROM IF-MIB;


hm2DhcpsMib MODULE-IDENTITY
	LAST-UPDATED "201203160000Z" -- March 16, 2012
    ORGANIZATION "Hirschmann Automation and Control GmbH"
    CONTACT-INFO
        "Postal:     Stuttgarter Str. 45-51
                     72654 Neckartenzlingen
                     Germany
         Phone:      +49 7127 140
         E-mail:     hac.support@belden.com"
    DESCRIPTION
        "Hirschmann DHCP server MIB.
         Copyright (C) 2012. All Rights Reserved."
    REVISION     "201203160000Z" -- March 16, 2012
    DESCRIPTION
         "Initial version."
    ::= { hm2ConfigurationMibs 91 }

-- 
-- DHCP Server MIB
--
hm2DHCPServerMibNotifications			OBJECT IDENTIFIER ::= { hm2DhcpsMib 0 }
hm2DHCPServerMibObjects					OBJECT IDENTIFIER ::= { hm2DhcpsMib 1 }
-- hm2DHCPServerMibConformance				OBJECT IDENTIFIER ::= { hm2DhcpsMib 2 }
hm2DHCPServerSNMPExtensionGroup 		OBJECT IDENTIFIER ::= { hm2DhcpsMib 3 }

-- 
-- DHCP Server Group
--

hm2DHCPServerGroup  			OBJECT IDENTIFIER ::= { hm2DHCPServerMibObjects 1 }
hm2DHCPServerConfigGroup     	OBJECT IDENTIFIER ::= { hm2DHCPServerGroup 1 }
hm2DHCPServerLeaseGroup      	OBJECT IDENTIFIER ::= { hm2DHCPServerGroup 2 }
hm2DHCPServerInterfaceGroup  	OBJECT IDENTIFIER ::= { hm2DHCPServerGroup 3 }
hm2DHCPServerCounterGroup    	OBJECT IDENTIFIER ::= { hm2DHCPServerGroup 4 }


--   
-- DHCP Server Config Group
--
hm2DHCPServerMode  OBJECT-TYPE 
   SYNTAX      HmEnabledStatus
   MAX-ACCESS  read-write 
   STATUS      current 
   DESCRIPTION 
      "Enable or disable DHCP server global." 
   DEFVAL  { disable } 
   ::= { hm2DHCPServerConfigGroup 1 }

hm2DHCPServerMaxPoolEntries  OBJECT-TYPE 
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only 
   STATUS      current 
   DESCRIPTION 
      "Maximum possible entries in hm2DHCPServerPoolTable."
   ::= { hm2DHCPServerConfigGroup 2 }

hm2DHCPServerMaxLeaseEntries  OBJECT-TYPE 
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only 
   STATUS      current
   DESCRIPTION 
      "Maximum possible entries in hm2DHCPServerLeaseTable."
   ::= { hm2DHCPServerConfigGroup 3 }

hm2DHCPServerAddrProbe  OBJECT-TYPE
   SYNTAX      HmEnabledStatus
   MAX-ACCESS  read-write
   STATUS      current
   DESCRIPTION
      "If set to enable the DHCP server probes the allocated address
      with an ICMP Echo Request before offering to the client."
   DEFVAL  { enable }
   ::= { hm2DHCPServerConfigGroup 4 }

-- DHCP Pool
hm2DHCPServerPoolTable  OBJECT-TYPE 
   SYNTAX      SEQUENCE OF Hm2DHCPServerPoolEntry 
   MAX-ACCESS  not-accessible 
   STATUS      current 
   DESCRIPTION 
      "A table containing the DHCP server pools."
   ::= { hm2DHCPServerConfigGroup 5 } 
 
hm2DHCPServerPoolEntry  OBJECT-TYPE 
   SYNTAX      Hm2DHCPServerPoolEntry 
   MAX-ACCESS  not-accessible 
   STATUS      current 
   DESCRIPTION 
      "A logical row in the hm2DHCPServerPoolTable." 
   INDEX { 
      hm2DHCPServerPoolIndex 
   } 
   ::= { hm2DHCPServerPoolTable 1}
 
Hm2DHCPServerPoolEntry ::= SEQUENCE { 
   hm2DHCPServerPoolIndex              Unsigned32,
   hm2DHCPServerPoolStartIpAddress     IpAddress,
   hm2DHCPServerPoolEndIpAddress       IpAddress,
   hm2DHCPServerPoolLeaseTime          Unsigned32,
   hm2DHCPServerPoolFlags              BITS,
   hm2DHCPServerPoolIfIndex            Integer32,
   hm2DHCPServerPoolMacAddress         MacAddress,
   hm2DHCPServerPoolGateway            IpAddress,
   hm2DHCPServerPoolClientId           OCTET STRING,
   hm2DHCPServerPoolRemoteId           OCTET STRING,
   hm2DHCPServerPoolCircuitId          OCTET STRING,
   hm2DHCPServerPoolHirschmannClient   HmEnabledStatus,
   hm2DHCPServerPoolVlanId             Integer32,
   hm2DHCPServerPoolOptionConfFileName DisplayString,
   hm2DHCPServerPoolOptionGateway      IpAddress,
   hm2DHCPServerPoolOptionNetmask      IpAddress,
   hm2DHCPServerPoolOptionWINS         IpAddress,
   hm2DHCPServerPoolOptionDNS          IpAddress,
   hm2DHCPServerPoolOptionHostname     DisplayString,
   hm2DHCPServerPoolMethod			   INTEGER,
   hm2DHCPServerPoolErrorStatus        Unsigned32,
   hm2DHCPServerPoolRowStatus          RowStatus
}

hm2DHCPServerPoolIndex  OBJECT-TYPE 
   SYNTAX      Unsigned32 (1..128)
   MAX-ACCESS  read-only
   STATUS      current 
   DESCRIPTION 
      "The index of hm2DHCPServerPoolTable." 
   ::= { hm2DHCPServerPoolEntry 1 }

hm2DHCPServerPoolStartIpAddress  OBJECT-TYPE 
   SYNTAX      IpAddress
   MAX-ACCESS  read-create
   STATUS      current 
   DESCRIPTION 
      "The IPv4 address of the first address in the range.  The 
      value of hm2DHCPServerPoolStartIpAddress MUST be less than or 
      equal to the value of hm2DHCPServerPoolEndIpAddress." 
   ::= { hm2DHCPServerPoolEntry 2 }

hm2DHCPServerPoolEndIpAddress  OBJECT-TYPE 
   SYNTAX      IpAddress
   MAX-ACCESS  read-create
   STATUS      current 
   DESCRIPTION 
      "The IPv4 address of the last address in the range.  The value 
      of hm2DHCPServerPoolEndIpAddress MUST be greater than or equal 
      to the value of hm2DHCPServerPoolStartIpAddress."
   ::= { hm2DHCPServerPoolEntry 3 }

hm2DHCPServerPoolLeaseTime  OBJECT-TYPE 
   SYNTAX      Unsigned32
   MAX-ACCESS  read-create
   STATUS      current 
   DESCRIPTION 
      "The pools lease time in number of seconds. 
      A value of 4294967295 SHOULD be used for leases that  
      have a lease time which is 'infinite' and for BOOTP leases." 
   DEFVAL  { 86400 }      
   ::= { hm2DHCPServerPoolEntry 4 }
      
hm2DHCPServerPoolFlags  OBJECT-TYPE 
   SYNTAX      BITS {
                  interface(0),
                  mac(1),
                  gateway(2),
                  clientid(3),
                  remoteid(4),
                  circuitid(5),
                  dynamic(6),
                  vlanid(7)
               }
   MAX-ACCESS  read-create
   STATUS      current 
   DESCRIPTION 
      "This object shows the parameters
      that are used to lease the IP Address."
   ::= { hm2DHCPServerPoolEntry 5 }

hm2DHCPServerPoolIfIndex  OBJECT-TYPE 
   SYNTAX      Integer32
   MAX-ACCESS  read-create
   STATUS      current 
   DESCRIPTION 
      "The index of the interface." 
   ::= { hm2DHCPServerPoolEntry 6 }
    
hm2DHCPServerPoolMacAddress  OBJECT-TYPE 
   SYNTAX      MacAddress
   MAX-ACCESS  read-create
   STATUS      current 
   DESCRIPTION 
      "The MAC Address of the  entry
      that is used to lease the IP Address."    
   ::= { hm2DHCPServerPoolEntry 7 }

hm2DHCPServerPoolGateway  OBJECT-TYPE 
   SYNTAX      IpAddress
   MAX-ACCESS  read-create
   STATUS      current 
   DESCRIPTION 
      "The IPv4 address of the Gatewayinterface
      that is used to lease the IP Address." 
   ::= { hm2DHCPServerPoolEntry 8 }

hm2DHCPServerPoolClientId  OBJECT-TYPE 
   SYNTAX      OCTET STRING
   MAX-ACCESS  read-create
   STATUS      current 
   DESCRIPTION 
      "The Client Identifier of the entry
      that is used to lease the IP Address."
   ::= { hm2DHCPServerPoolEntry 9 }
    
hm2DHCPServerPoolRemoteId  OBJECT-TYPE 
   SYNTAX      OCTET STRING
   MAX-ACCESS  read-create
   STATUS      current 
   DESCRIPTION 
      "The Remote Identifier of the  entry
      that is used to lease the IP Address.
      The Remote Identifier must be send in
      Option 82 as defined in RFC 3046."
   ::= { hm2DHCPServerPoolEntry 10 }

hm2DHCPServerPoolCircuitId  OBJECT-TYPE 
   SYNTAX      OCTET STRING
   MAX-ACCESS  read-create
   STATUS      current 
   DESCRIPTION 
      "The Cicuit Identifier of the  entry
      that is used to lease the IP Address.
      The Circuit Identifier must be send in
      Option 82 as defined in RFC 3046."
   ::= { hm2DHCPServerPoolEntry 11 }

hm2DHCPServerPoolHirschmannClient  OBJECT-TYPE 
   SYNTAX      HmEnabledStatus
   MAX-ACCESS  read-create 
   STATUS      current 
   DESCRIPTION 
      "Enable or disable Hirschmann Multicast." 
   DEFVAL  { disable } 
   ::= { hm2DHCPServerPoolEntry 12 }

hm2DHCPServerPoolVlanId  OBJECT-TYPE 
   SYNTAX      Integer32
   MAX-ACCESS  read-create
   STATUS      current 
   DESCRIPTION 
      "The Vlan ID of the entry that is used
      to lease the IP Address. A value of -1 
      corresponds to management vlan (the default),
      any other value (1-4042) represents a specific VLAN"
   ::= { hm2DHCPServerPoolEntry 13 }
   
-- Pool Options
hm2DHCPServerPoolOptionConfFileName  OBJECT-TYPE 
   SYNTAX      DisplayString (SIZE (0..70)) 
   MAX-ACCESS  read-create 
   STATUS      current 
   DESCRIPTION 
      "Full specified name of the configuration file
      e.g. tftp://192.9.200.1/cfg/config1.sav.
      An empty string zeros the SNAME and the FILE field 
      in the DHCP header."     
   ::= { hm2DHCPServerPoolEntry 30 } 

hm2DHCPServerPoolOptionGateway  OBJECT-TYPE 
   SYNTAX      IpAddress
   MAX-ACCESS  read-create 
   STATUS      current 
   DESCRIPTION 
      "The IPv4 address of the Gateway.
      A value of 0 disables the attachment of the
      option field in the DHCP message."
   ::= { hm2DHCPServerPoolEntry 31 }

hm2DHCPServerPoolOptionNetmask  OBJECT-TYPE 
   SYNTAX      IpAddress
   MAX-ACCESS  read-create 
   STATUS      current 
   DESCRIPTION 
      "The subnet mask.
      A value of 0 disables the attachment of the
      option field in the DHCP message."
   ::= { hm2DHCPServerPoolEntry 32 }
   
hm2DHCPServerPoolOptionWINS  OBJECT-TYPE 
   SYNTAX      IpAddress
   MAX-ACCESS  read-create 
   STATUS      current 
   DESCRIPTION 
      "The IPv4 address of the WINS Server.
      A value of 0 disables the attachment of the
      option field in the DHCP message."
   ::= { hm2DHCPServerPoolEntry 33 }

hm2DHCPServerPoolOptionDNS  OBJECT-TYPE 
   SYNTAX      IpAddress
   MAX-ACCESS  read-create 
   STATUS      current 
   DESCRIPTION 
      "The IPv4 address of the DNS Server.
      A value of 0 disables the attachment of the
      option field in the DHCP message."
   ::= { hm2DHCPServerPoolEntry 34 }

hm2DHCPServerPoolOptionHostname  OBJECT-TYPE 
   SYNTAX      DisplayString (SIZE (0..64))
   MAX-ACCESS  read-create 
   STATUS      current 
   DESCRIPTION 
      "The name of the client (Option 12).
      An empty string disables the attachment of the
      option field in the DHCP message."
   ::= { hm2DHCPServerPoolEntry 35 }

hm2DHCPServerPoolMethod  OBJECT-TYPE
   SYNTAX      INTEGER
   {
         none (1),
         config (2),
         ttdp (3)
   }
   MAX-ACCESS  read-write
   STATUS      current
   DESCRIPTION
          "The source of the DHCP Server Pool. User can set the object to none(1), config(2), ttdp(3)."
   DEFVAL  { none } 
   ::= { hm2DHCPServerPoolEntry 36 }

hm2DHCPServerPoolErrorStatus  OBJECT-TYPE 
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current 
   DESCRIPTION 
      "The error Code by create a new Pool." 
   ::= { hm2DHCPServerPoolEntry 99 }

hm2DHCPServerPoolRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This object indicates the status of this entry."
    ::= { hm2DHCPServerPoolEntry 100 }
    
--
-- DHCP Server Lease Group
--
hm2DHCPServerLeaseTable  OBJECT-TYPE 
   SYNTAX      SEQUENCE OF Hm2DHCPServerLeaseEntry 
   MAX-ACCESS  not-accessible 
   STATUS      current 
   DESCRIPTION 
      "A table containing the DHCP server leases."
   ::= { hm2DHCPServerLeaseGroup 1 } 
 
hm2DHCPServerLeaseEntry  OBJECT-TYPE 
   SYNTAX      Hm2DHCPServerLeaseEntry 
   MAX-ACCESS  not-accessible 
   STATUS      current 
   DESCRIPTION 
      "A logical row in the hm2DHCPServerLeaseTable." 
   INDEX { 
      hm2DHCPServerLeasePoolIndex,
      hm2DHCPServerLeaseIpAddress
   } 
   ::= { hm2DHCPServerLeaseTable 1}
 
Hm2DHCPServerLeaseEntry ::= SEQUENCE { 
   hm2DHCPServerLeasePoolIndex              Unsigned32,
   hm2DHCPServerLeaseIpAddress              IpAddress,
   hm2DHCPServerLeaseState                  INTEGER,
   hm2DHCPServerLeaseTimeRemaining          Unsigned32,
   hm2DHCPServerLeaseIfIndex                Integer32,
   hm2DHCPServerLeaseClientMacAddress       MacAddress,
   hm2DHCPServerLeaseGateway                IpAddress,
   hm2DHCPServerLeaseClientId               OCTET STRING,
   hm2DHCPServerLeaseRemoteId               OCTET STRING,
   hm2DHCPServerLeaseCircuitId              OCTET STRING,
   hm2DHCPServerLeaseStartTime              Unsigned32,  
   hm2DHCPServerLeaseAction                 INTEGER,
   hm2DHCPServerLeaseVlanId			  	   Integer32
}

hm2DHCPServerLeasePoolIndex  OBJECT-TYPE 
   SYNTAX      Unsigned32 (1..128)
   MAX-ACCESS  read-only
   STATUS      current 
   DESCRIPTION 
      "The index of the hm2DHCPServerPoolTable above." 
   ::= { hm2DHCPServerLeaseEntry 1 }
   
hm2DHCPServerLeaseIpAddress  OBJECT-TYPE 
   SYNTAX      IpAddress
   MAX-ACCESS  read-only
   STATUS      current 
   DESCRIPTION 
      "This is an IP address from the pool with
      index hm2DHCPServerLeasePoolIndex."
   ::= { hm2DHCPServerLeaseEntry 2 }   

hm2DHCPServerLeaseState  OBJECT-TYPE 
   SYNTAX      INTEGER  {
               bootp(1),
               offering(2),
               requesting(3),
               bound(4),
               renewing(5),
               rebinding(6),
               declined(7),
               released(8)  
               }
   MAX-ACCESS  read-only
   STATUS      current 
   DESCRIPTION 
      "The state of the lease."
   ::= { hm2DHCPServerLeaseEntry 3 }

hm2DHCPServerLeaseTimeRemaining  OBJECT-TYPE 
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current 
   DESCRIPTION 
      "The remaining time of the lease configured in
      hm2DHCPServerPoolLeaseTime."
   ::= { hm2DHCPServerLeaseEntry 4 }  

hm2DHCPServerLeaseIfIndex  OBJECT-TYPE 
   SYNTAX      Integer32
   MAX-ACCESS  read-only
   STATUS      current 
   DESCRIPTION 
      "The interface index where the lease
      is currently active."
   ::= { hm2DHCPServerLeaseEntry 5 }  

hm2DHCPServerLeaseClientMacAddress  OBJECT-TYPE 
   SYNTAX      MacAddress
   MAX-ACCESS  read-only
   STATUS      current 
   DESCRIPTION 
      "The MAC Address of the  entry
      that has leased the IP Address."
   ::= { hm2DHCPServerLeaseEntry 6 } 

hm2DHCPServerLeaseGateway  OBJECT-TYPE 
   SYNTAX      IpAddress
   MAX-ACCESS  read-only 
   STATUS      current 
   DESCRIPTION 
      "The IPv4 address of the Gatewayinterface
      that was used to lease the IP Address."
   ::= { hm2DHCPServerLeaseEntry 7 }

hm2DHCPServerLeaseClientId  OBJECT-TYPE 
   SYNTAX      OCTET STRING (SIZE (0..255))
   MAX-ACCESS  read-only
   STATUS      current 
   DESCRIPTION 
      "The Client Identifier of the entry
      that was used to lease the IP Address."
   ::= { hm2DHCPServerLeaseEntry 8 }
    
hm2DHCPServerLeaseRemoteId  OBJECT-TYPE 
   SYNTAX      OCTET STRING (SIZE (0..255))
   MAX-ACCESS  read-only
   STATUS      current 
   DESCRIPTION 
      "The Remote Identifier of the entry
      that was used to lease the IP Address."
   ::= { hm2DHCPServerLeaseEntry 9 }

hm2DHCPServerLeaseCircuitId  OBJECT-TYPE 
   SYNTAX      OCTET STRING (SIZE (0..255))
   MAX-ACCESS  read-only
   STATUS      current 
   DESCRIPTION 
      "The Cicuit Identifier of the entry
      that was used to lease the IP Address."
   ::= { hm2DHCPServerLeaseEntry 10 }

hm2DHCPServerLeaseStartTime  OBJECT-TYPE 
   SYNTAX      Unsigned32  
   MAX-ACCESS  read-only
   STATUS      current 
   DESCRIPTION 
      "Lease start Time."
   ::= { hm2DHCPServerLeaseEntry 11 }

hm2DHCPServerLeaseAction  OBJECT-TYPE 
   SYNTAX      INTEGER  {
   			   other(1),
               release(2)
               }
   MAX-ACCESS  read-write
   STATUS      current 
   DESCRIPTION 
      "Manually release this ip address for new assignment."
   ::= { hm2DHCPServerLeaseEntry 12 }

hm2DHCPServerLeaseVlanId  OBJECT-TYPE 
   SYNTAX      Integer32
   MAX-ACCESS  read-only
   STATUS      current 
   DESCRIPTION 
      "The Vlan ID of the entry that is used
      to lease the IP Address. A value of -1 
      corresponds to management vlan (the default),
      any other value (1-4042) represents a specific VLAN"
   ::= { hm2DHCPServerLeaseEntry 13 }

--
-- DHCP Server Interface Group
--
hm2DHCPServerIfConfigTable  OBJECT-TYPE 
   SYNTAX      SEQUENCE OF Hm2DHCPServerIfConfigEntry 
   MAX-ACCESS  not-accessible 
   STATUS      current 
   DESCRIPTION 
      "A table containing current configuration information
      for each interface." 
   ::= { hm2DHCPServerInterfaceGroup 1 } 
 
hm2DHCPServerIfConfigEntry  OBJECT-TYPE 
   SYNTAX      Hm2DHCPServerIfConfigEntry 
   MAX-ACCESS  not-accessible 
   STATUS      current 
   DESCRIPTION 
      "A logical row in the hm2DHCPServerIfConfigTable." 
   INDEX { 
      hm2DHCPServerIfConfigIndex 
   } 
   ::= { hm2DHCPServerIfConfigTable 1}
 
Hm2DHCPServerIfConfigEntry ::= SEQUENCE { 
   hm2DHCPServerIfConfigIndex                   InterfaceIndex,
   hm2DHCPServerIfConfigMode                    HmEnabledStatus
}

hm2DHCPServerIfConfigIndex  OBJECT-TYPE 
   SYNTAX      InterfaceIndex
   MAX-ACCESS  read-only
   STATUS      current 
   DESCRIPTION 
      "The index of the interface." 
   ::= { hm2DHCPServerIfConfigEntry 1 }

hm2DHCPServerIfConfigMode  OBJECT-TYPE 
   SYNTAX      HmEnabledStatus
   MAX-ACCESS  read-write 
   STATUS      current 
   DESCRIPTION 
      "Enable or disable DHCP server on this interface." 
   DEFVAL  { enable } 
   ::= { hm2DHCPServerIfConfigEntry 2 }



--
-- DHCP Server Counter Group
--
hm2DHCPServerCounterIfTable  OBJECT-TYPE 
   SYNTAX      SEQUENCE OF Hm2DHCPServerCounterIfEntry 
   MAX-ACCESS  not-accessible 
   STATUS      current 
   DESCRIPTION 
      "A table containing current configuration information
      for each interface." 
   ::= { hm2DHCPServerCounterGroup 2 } 
 
hm2DHCPServerCounterIfEntry  OBJECT-TYPE 
   SYNTAX      Hm2DHCPServerCounterIfEntry 
   MAX-ACCESS  not-accessible 
   STATUS      current 
   DESCRIPTION 
      "A logical row in the hm2DHCPServerCounterIfTable." 
   INDEX { 
      hm2DHCPServerCounterIfIndex 
   } 
   ::= { hm2DHCPServerCounterIfTable 1}
 
Hm2DHCPServerCounterIfEntry ::= SEQUENCE { 
   hm2DHCPServerCounterIfIndex                       InterfaceIndex,
   hm2DHCPServerCounterBootpRequests                 Counter32,
   hm2DHCPServerCounterBootpInvalids                 Counter32,
   hm2DHCPServerCounterBootpReplies                  Counter32,
   hm2DHCPServerCounterBootpDroppedUnknownClients    Counter32,
   hm2DHCPServerCounterBootpDroppedNotServingSubnet  Counter32,
   hm2DHCPServerCounterDhcpv4Discovers               Counter32,
   hm2DHCPServerCounterDhcpv4Offers                  Counter32,
   hm2DHCPServerCounterDhcpv4Requests                Counter32,
   hm2DHCPServerCounterDhcpv4Declines                Counter32,
   hm2DHCPServerCounterDhcpv4Acks                    Counter32,
   hm2DHCPServerCounterDhcpv4Naks                    Counter32,
   hm2DHCPServerCounterDhcpv4Releases                Counter32,
   hm2DHCPServerCounterDhcpv4Informs                 Counter32,
   hm2DHCPServerCounterDhcpv4ForcedRenews            Counter32,
   hm2DHCPServerCounterDhcpv4Invalids                Counter32,
   hm2DHCPServerCounterDhcpv4DroppedUnknownClient    Counter32,
   hm2DHCPServerCounterDhcpv4DroppedNotServingSubnet Counter32,
   hm2DHCPServerCounterMiscOtherDhcpServer           Counter32
   }

hm2DHCPServerCounterIfIndex  OBJECT-TYPE 
   SYNTAX      InterfaceIndex
   MAX-ACCESS  read-only
   STATUS      current 
   DESCRIPTION 
      "The index of the interface." 
   ::= { hm2DHCPServerCounterIfEntry 1 }
   
-- BOOTP Counter
hm2DHCPServerCounterBootpRequests  OBJECT-TYPE 
   SYNTAX      Counter32 
   MAX-ACCESS  read-only 
   STATUS      current 
   DESCRIPTION 
      "The number of packets received that contain a Message Type of 
      1 (BOOTREQUEST) in the first octet and do not contain option 
      number 53 (DHCP Message Type) in the options." 
   ::= { hm2DHCPServerCounterIfEntry 2 } 
 
hm2DHCPServerCounterBootpInvalids  OBJECT-TYPE 
   SYNTAX      Counter32 
   MAX-ACCESS  read-only 
   STATUS      current 
   DESCRIPTION 
      "The number of packets received that do not contain a Message 
      Type of 1 (BOOTREQUEST) in the first octet or are not valid 
      BOOTP packets (e.g., too short, invalid field in packet 
      header)." 
   ::= { hm2DHCPServerCounterIfEntry 3 } 
 
hm2DHCPServerCounterBootpReplies  OBJECT-TYPE 
   SYNTAX      Counter32 
   MAX-ACCESS  read-only 
   STATUS      current 
   DESCRIPTION 
      "The number of packets sent that contain a Message Type of 2 
      (BOOTREPLY) in the first octet and do not contain option 
      number 53 (DHCP Message Type) in the options." 
   ::= { hm2DHCPServerCounterIfEntry 4 } 
 
hm2DHCPServerCounterBootpDroppedUnknownClients  OBJECT-TYPE 
   SYNTAX      Counter32 
   MAX-ACCESS  read-only 
   STATUS      current 
   DESCRIPTION 
      "The number of BOOTP packets dropped due to the server not 
      recognizing or not providing service to the hardware address 
      received in the incoming packet." 
   ::= { hm2DHCPServerCounterIfEntry 5 } 
 
hm2DHCPServerCounterBootpDroppedNotServingSubnet  OBJECT-TYPE 
   SYNTAX      Counter32 
   MAX-ACCESS  read-only 
   STATUS      current 
   DESCRIPTION 
      "The number of BOOTP packets dropped due to the server not 
      being configured or not otherwise able to serve addresses on 
      the subnet from which this message was received." 
   ::= { hm2DHCPServerCounterIfEntry 6 }

-- DHCPv4 Counter
hm2DHCPServerCounterDhcpv4Discovers  OBJECT-TYPE 
   SYNTAX      Counter32 
   MAX-ACCESS  read-only 
   STATUS      current 
   DESCRIPTION 
      "The number of DHCPDISCOVER (option 53 with value 1) packets 
      received." 
   ::= { hm2DHCPServerCounterIfEntry 20 } 
 
hm2DHCPServerCounterDhcpv4Offers  OBJECT-TYPE 
   SYNTAX      Counter32 
   MAX-ACCESS  read-only 
   STATUS      current 
   DESCRIPTION 
      "The number of DHCPOFFER (option 53 with value 2) packets 
      sent." 
   ::= { hm2DHCPServerCounterIfEntry 21 } 
 
hm2DHCPServerCounterDhcpv4Requests  OBJECT-TYPE 
   SYNTAX      Counter32 
   MAX-ACCESS  read-only 
   STATUS      current 
   DESCRIPTION 
      "The number of DHCPREQUEST (option 53 with value 3) packets 
      received." 
   ::= { hm2DHCPServerCounterIfEntry 22 } 

hm2DHCPServerCounterDhcpv4Declines  OBJECT-TYPE 
   SYNTAX      Counter32 
   MAX-ACCESS  read-only 
   STATUS      current 
   DESCRIPTION 
      "The number of DHCPDECLINE (option 53 with value 4) packets 
      received." 
   ::= { hm2DHCPServerCounterIfEntry 23 } 
 
hm2DHCPServerCounterDhcpv4Acks  OBJECT-TYPE 
   SYNTAX      Counter32 
   MAX-ACCESS  read-only 
   STATUS      current 
   DESCRIPTION 
      "The number of DHCPACK (option 53 with value 5) packets sent." 
   ::= { hm2DHCPServerCounterIfEntry 24 } 
 
hm2DHCPServerCounterDhcpv4Naks  OBJECT-TYPE 
   SYNTAX      Counter32 
   MAX-ACCESS  read-only 
   STATUS      current 
   DESCRIPTION 
      "The number of DHCPNACK (option 53 with value 6) packets 
      sent." 
   ::= { hm2DHCPServerCounterIfEntry 25 } 
 
hm2DHCPServerCounterDhcpv4Releases  OBJECT-TYPE 
   SYNTAX      Counter32 
   MAX-ACCESS  read-only 
   STATUS      current 
   DESCRIPTION 
      "The number of DHCPRELEASE (option 53 with value 7) packets 
      received." 
   ::= { hm2DHCPServerCounterIfEntry 26 } 
 
hm2DHCPServerCounterDhcpv4Informs  OBJECT-TYPE 
   SYNTAX      Counter32 
   MAX-ACCESS  read-only 
   STATUS      current 
   DESCRIPTION 
      "The number of DHCPINFORM (option 53 with value 8) packets 
      received." 
   ::= { hm2DHCPServerCounterIfEntry 27 } 
 
hm2DHCPServerCounterDhcpv4ForcedRenews  OBJECT-TYPE 
   SYNTAX      Counter32 
   MAX-ACCESS  read-only 
   STATUS      current 
   DESCRIPTION 
      "The number of DHCPFORCERENEW (option 53 with value 9) packets 
      sent." 
   ::= { hm2DHCPServerCounterIfEntry 28 } 
 
hm2DHCPServerCounterDhcpv4Invalids  OBJECT-TYPE 
   SYNTAX      Counter32 
   MAX-ACCESS  read-only 
   STATUS      current 
   DESCRIPTION 
      "The number of DHCP packets received whose DHCP message type 
      (i.e., option number 53) is not understood or handled by the 
      server." 
   ::= { hm2DHCPServerCounterIfEntry 29 } 
 
hm2DHCPServerCounterDhcpv4DroppedUnknownClient  OBJECT-TYPE 
   SYNTAX      Counter32 
   MAX-ACCESS  read-only 
   STATUS      current 
   DESCRIPTION 
      "The number of DHCP packets dropped due to the server not 
      recognizing or not providing service to the client-id and/or 
      hardware address received in the incoming packet." 
   ::= { hm2DHCPServerCounterIfEntry 30 } 
 
hm2DHCPServerCounterDhcpv4DroppedNotServingSubnet  OBJECT-TYPE 
   SYNTAX      Counter32 
   MAX-ACCESS  read-only 
   STATUS      current 
   DESCRIPTION 
      "The number of DHCP packets dropped due to the server not 
      being configured or not otherwise able to serve addresses on 
      the subnet from which this message was received." 
   ::= { hm2DHCPServerCounterIfEntry 31 }

-- Misc Counter
hm2DHCPServerCounterMiscOtherDhcpServer  OBJECT-TYPE 
   SYNTAX      Counter32 
   MAX-ACCESS  read-only 
   STATUS      current 
   DESCRIPTION 
      "The number of BOOTP and DHCP packets from another
      DHCP server seen on this interface." 
   ::= { hm2DHCPServerCounterIfEntry 40 }

--
-- ***********************************************************
-- hm2DHCPServerSNMPExtensionGroup
-- ***********************************************************
--

hm2DHCPServerRowStatusInvalidConfigurationErrorReturn OBJECT-IDENTITY
   STATUS      current
   DESCRIPTION "DHCP Server pool with index {0} cannot be enabled, errors in data entry."
   ::= { hm2DHCPServerSNMPExtensionGroup 1 }

hm2DHCPServerConflictDHCPRrelayErrorReturn OBJECT-IDENTITY
   STATUS      current
   DESCRIPTION "{0} and {1} cannot be active at the same time."
   ::= { hm2DHCPServerSNMPExtensionGroup 2 }

END

