
            S O F T W A R E - R E L E A S E - D O C U M E N T

                 Hirschmann Automation and Control GmbH
              
            	      RSP Release 10.3.07
            		
                            2026/03/26
             		
                          C O N T E N T S
                          ===============


    1.   Limitations of the release RSP 10.3.07
    2.   Supported Hardware
    3.   History of Changes

   

This document is delivered with the software in the file 
"Readme_RSP.10.3.07.txt".

 

.-----------------------------------------------------------------------------.
| For superior functions like software update,                                |
| supported web browser and limitations of the platform release 10.3.07       | 
| please read the document Readme_10.3.07.txt.                                |
'-----------------------------------------------------------------------------'



1. Limitations of the release RSP 10.3.07
=============================================
Prerequisite for the update to a HiOS version 09.1.00 or higher is that the
device is running HiOS version 09.0.07 or higher. For an update of versions 
before 09.0.07, an update to HiOS 09.0.07 or higher is required first. 

Caution:
- If the update is done from an earlier version than HiOS 09.0.07, 
  the device might lose its device programming and cannot be used anymore. 

- Updating to HiOS 09.1.00 replaces the bootloader.
  Make sure that there is no power interruption during the update.
- The first boot after the update to HiOS 09.1.00 will take significantly longer.
- When downgrading from 09.1.00 to an earlier version, the device does not adopt 
  the configuration profile and the certificates automatically. Therefore, save 
  the configuration before the downgrade. Import this configuration profile after 
  the downgrade.

   
2. Supported Hardware
=====================
This platform software release 10.3.07 is released exclusively for the 
following hardware:

HiOS-RSP-10307.bin:
- RSP20
- RSP30
- RSP25
- RSP35

HiOS-RSP-MRP-10307.bin:
- RSP25
- RSP35

HiOS-RSP-PRP-10307.bin:
HiOS-RSP-HSR-10307.bin:
- RSP25 (hardware revision 2 unrestricted, for hardware revision 1 permissible up to +60° Celsius or +140° Fahrenheit ambient temperature)           
- RSP35 (hardware revision 2 unrestricted, for hardware revision 1 permissible up to +60° Celsius or +140° Fahrenheit ambient temperature) 

HiOS-RSP-DLR-10307.bin: (Since version 05.0.00)
- RSP25 (with Hardware configuration "D")
- RSP35 (with Hardware configuration "D")

HiOS-RSP-NAT-10307.bin:
- RSP25 with 3S software
- RSP35 with 3S software

Supported Software Level:
- 2S (since HW Revision 3)
- 2A
- 3S
 
For information on supported accessories, refer to the "User Manual Installation".
You will find the manuals under "https://www.doc.hirschmann.com". 
 
3. History of Changes
=====================

Software Release 03.0.00
------------------------
First version


Software Release 04.0.00
------------------------
Bugfixes (see Issue List)

New functions: 
- JumboFrames (12288 Byte Frames)
- Subring Manager
- Manual LED signalling

Software Level 3S:
- Loopback interface (2)
- Static routing (40 Entries)
- Port based routing
- VLAN based routing
- Routing templates
- VRRP
- HiVRRP
- VRRP tracking
- Net directed broadcasts
- ICMP Router Discovery (IRDP)
- Static route tracking
- Static reject routes
- Proxy ARP
- Static ARP entries
- Selective ARP Learning
- IGMPv1,IGMPv2,IGMPv3
- IGMP Proxy
- ICMP filter
- Configurable IP MTU
- BOOTP/DHCP layer 3 relay
- IP/UDP helper


Software Release 05.0.00
------------------------
Bugfixes (see Issue List)

New Functions: 
- Device Level Ring (DLR) (with Hardware configuration "D" and software with DLR support)
- HiDiscovery v2 server
- EtherNet/IP Protocol
- Modbus TCP
- PROFINET Protocol
- Port Monitor Overload detection
- Port Monitor Link Speed and Duplex Monitor
- Port Mirroring N:1
- System resource monitor
- CLI script download over HTTP(S)
- Management MAC Address Conflict Detection
- DHCP server pools for multicast requests
- RSPAN
- VLAN mirroring
- HIPER-Ring Client (Ring Switch)
- LDAP
- Extended ACL filter

Software Level 3S:
- OSPFv2
- RIPv1, RIPv2


Software Release 06.0.00
------------------------
Bugfixes (see Issue List)

New Functions:
- Syslog over TLS
- RSTP over HSR (with software with HSR support)
- Configurable fixed MRP redundant port
- Redundant Coupling Protocol (RCP)
- Ring/Net Coupling
- TLS 1.2
- FTP Client
- RSTP Ring Only Mode
- Link Loss Alert
- Web: Port Tooltip
- Upload certificate for mail server
- Subring with Link Aggregation
- GMRP
- GVRP

Software Level 3S:
- 1:1 NAT
- OSPF fast Hello mode


Software Release 06.1.00
------------------------
Bugfixes (see Issue List)

New Functions:
- Option to allow management on probe port
- Multiple Spanning Tree

Software Level 3S:
- Select source interface for copy commands and Radius


Software Release 07.0.00
------------------------
Bugfixes (see Issue List)

New Functions:
- HTML5-based Graphical User Interface
- Backup the Config on a Remote Server
- Clear Config Keep IP
- HSR over Gigabit (with hardware revision 2 and software with HSR support)
- MAC Authentication Bypass Format Options

Software Level 3S:
- ACD for Router Interfaces
- Source-Routing can be activated/deactivated

Software Release 07.0.04
------------------------
Bugfixes (see Issue List)

Changed Functions:
- Import / Export CLI scripts via grafical user interface.
- SSH: support for new ciphers.
- SSH: DSA auth. key support removed.
- PRP over Gigabit (with hardware revision 2 and software with PRP support)

Software Release 08.0.00
------------------------
Bugfixes (see Issue List)

New Functions:
- Automatic login by HiVision
- CLI script load on boot 
- Changed defaults: SNMPv1/v2 and telnet are disabled.

Software Release 07.1.00 and 08.1.00
------------------------------------
Bugfixes (see Issue List)

New Functions:
- Password change on first login
  Protocols that require a login (e.g. SNMPv3) remain deactivated until the password is changed. 

Software Release 08.4.01
------------------------
Bugfixes (see Issue List)

New Functions:
- BOOTP/DHCP options (DHCP client) can be switched off.
- Display delivered PoE current in mA (additional to the power in W).

Software Level 2A/3S:
- Display differences to default configuration in the graphical user interface.
- New parameter "index" in the CLI for adding and deleting ACL rules. 

Software Release 08.6.00
------------------------
Bugfixes (see Issue List)

New Functions:
- OPC UA Server
- Protocol packet statistics

Software Release 08.7.00
------------------------------------
Bugfixes (see Issue List)

New Functions: 
Software Level 2A/3S:
- Loop-Protection function

Software Release 09.0.00
------------------------
Bugfixes (see Issue List)

New Functions:
- Responsive GUI

Software Level 2A/3S:
- Double VLAN Tagging 

Software Release 09.1.00
------------------------
Bugfixes (see Issue List)

New Functions:
- Signed firmware images
- Update 802.1X to Version 2010
- Profinet Combined family GSDML
- Profinet new stack , spec 2.41 compliant
- VLAN configuration for EtherNet/IP
- IPv6-Management
- 802.1AS-2011
- LLDP IPv6 Support

Software Release 09.2.00
------------------------
Bugfixes (see Issue List)

New Functions:
- SNMPv3 Traps

Software Level 2A:
- SNMPv1/v2 Read-Only
- Interface Shutdown via Tracking

Software Release 09.4.00
------------------------
Bugfixes (see Issue List)

New Functions:
- SNMPv3 Traps (GUI)

Software Release 10.0.00
------------------------
Bugfixes (see Issue List)

New Functions:
- SSH Known Host verification

Software Level 2A/3S:
- Certificates/CRLs validation (LDAP, Email Logging, Syslog over TLS)
- Service Discovery (with ITxPT Module Inventory)
- RSPAN with dedicated destination port 
- 802.1AS-2020

Software Release 10.3.00
------------------------
Bugfixes (see Issue List)

New Functions:
- DHCP server PXE support

Software Release 10.3.07
------------------------
Bugfixes (see Issue List)
