
            S O F T W A R E - R E L E A S E - D O C U M E N T

                 Hirschmann Automation and Control GmbH
              
            	      MACH104 Release 09.1.14
            		
                             2024/10/09
             		
                           C O N T E N T S
                           ===============


    1.   Limitations of the release MACH104 09.1.14
    2.   Hardware Considerations
    3.   History of Changes

   

This document is delivered with the software in the file 
"Readme_MACH104.09.1.14.txt".

 

.-----------------------------------------------------------------------------.
| For superior functions like software update,                                |
| supported web browser and limitations of the platform release 09.1.14       | 
| please read the document Readme_09.1.14.txt.                                |
'-----------------------------------------------------------------------------'



1. Limitations of the release MACH104 09.1.14
=============================================
(01) In the mode "Discard unknown multicasts" following standard multicast
     addresses were defined as static filters and so have the state known:
     - FF:FF:FF:FF:FF:FF (Broadcast)
     - 01:80:C2:00:00:00 (Spanning Tree)
     - 01:80:C2:00:00:20 (GMRP)
     - 01:80:C2:00:00:21 (GVRP)
     - 01:00:5E:00:01:01 (SNTP-Multicast)
     - 01:00:5E:00:01:81 - 01:00:5E:00:01:84 (PTP-Multicasts)
     - 01:1B:19:00:00:00 (PTPv2 L2 Multicast)
     - 01:0E:CF:00:00:00 (DCP)
     - 01:15:4E:00:00:01 - 01:15:4E:00:00:02 (MRP)
     - 01:00:5E:7F:10:0C (HiDiscoveryv2)
(02) Link aggregation in Hiper Ring or in the redundant ringcoupling
     is not supported.


     
2. Hardware Considerations
==========================
This platform software release 09.1.14 is released exclusively for the 
following hardware:

- Software m100geL2P.bin supports L2P and L3P hardware variants
- Software m100geL3P.bin supports L3P hardware variants (Since SW 08.0.00)

- MACH104-20TX-F       		(Since SW 05.1.00)
- MACH104-20TX-FR      		(Since SW 05.1.00)
- MACH104-20TX-F-4PoE 		(Since SW 05.1.00)
- MACH104-16TX-PoEP			(Since SW 07.0.00)
- MACH104-16TX-PoEP-R		(Since SW 07.0.00)
- MACH104-16TX-PoEP-E		(Since SW 07.0.00)
- MACH104-16TX-PoEP+2X		(Since SW 07.0.00)
- MACH104-16TX-PoEP+2X-R	(Since SW 07.0.00)
- MACH104-16TX-PoEP+2X-E	(Since SW 07.0.00)
 + ACA 21-USB         		(Since SW 05.1.00)
 + ACA 22-USB         		(Since SW 05.1.00)
 + ACA 22A-USB         		(Since SW 05.1.00)
 + M-SFP-SX/LC              (Since SW 05.1.00)
 + M-SFP-MX/LC              (Since SW 05.1.00)
 + M-SFP-LX/LC              (Since SW 05.1.00)
 + M-SFP-LX+/LC             (Since SW 05.1.00)
 + M-SFP-LH/LC              (Since SW 05.1.00)
 + M-SFP-LH+/LC             (Since SW 05.1.00)
 + M-SFP-BIDI               (Since SW 05.1.00)
 + M-SFP-TX/RJ45            (Since SW 05.1.00)
 + M-FAST SFP-LH/LC         (Since SW 05.1.00)
 + M-FAST SFP-SM/LC         (Since SW 05.1.00)
 + M-FAST SFP-SM+/LC        (Since SW 05.1.00)
 + M-FAST SFP-MM/LC         (Since SW 05.1.00)

3. History of Changes
=====================

Software Release 05.1.00
------------------------
All functions of L2P:
- Autonegotiation or manual port configuration
- Store and Forward Switching, Flow Control
- VLANs (256 out of 4042), Prioritization (8 Queues), Tagging
- 8 Strict Priority Queues per port
- Independant VLAN learning
- Dynamic Unicast address entries (up to 8000)
- Static Unicast and Multicast address entries (up to 100)
- Dynamic Multicast address entries (up to 1000)
- IGMP-Snooping (v1, v2, Querier, Forward All)
- Rapid Spanning Tree
- HIPER-Ring
- Redundant Coupling of HIPER Rings and network segments
- Port Mirroring (1 source port to 1 monitoring port)
- 1(2) signal contact(s) for status monitoring and manual configuration
- Interface-Statistics, RMON (1,2,3,9)
- BOOTP/DHCP with auto configuration
- BOOTP/DHCP relay with option 82
- Fast aging on linkdown
- TFTP (software update, loading and saving the configuration)
- Auto Configuration Adapter ACA 21-USB (software update, loading and saving the 
  configuration)
- SNMP v1, Traps
- SNMP v2c, v3
- V.24 (System Monitor, Command Line Interface)
- Telnet (Command Line Interface)
- Web Based Management
- Diagnosis and self test function on cold start
- Error logging local
- SysLog support
- ACA21-USB password protection
- Address-based port-security
- HiDiscovery
- IEEE 1588 client without hardware support
- Egress broadcast limiter per port
- LLDP
- SFP management
- HTTP Update
- SNTP Client + Server
- Support for traceroute
- VLAN 0 Mode for switching of priority only tagged frames.
- Unknown Multicast Filtering
- Additional ingress and egress paket limiter
- Bridge-MIB: dot1dTpFdbTable supports addresses from all VLANs
- Security Data Sheet from IAONA integrated
- Management Address Conflict Detection
- Automatic configuration undo
- Access to Management from all VLANs
- HTTP config file transfer
- MRP (Media Redundancy Protocol - IEC Ring)
- Loginname and password up to 32 characters
- Transmission of oversize packets up to 1552 bytes
- Device status indication
- Disable Learning
- Telnet client in webinterface
- Batterybuffered Realtime Clock
- Telnet Client (Outbound Telnet)
- CLI Scripting
- 802.1x security
- GMRP (with Forward All)
- GVRP
- Cable test (copper only)
- Link Aggregation (up to 7 groups with 4 ports for each group), each dynamic(LACP) or static
- SNMPv3 Data Encryption
- SSHv1 (DES)
- Configuration as script load/save
- GMRP Forward all
- Dynamic VLAN configuration protocol GVRP
- Customer specific preconfiguration (script)
- Ethernet/IP Protocol
- Enhancement of portsecurity to 10 addresses per port
- IGMP Snooping Enhancements (Automatic query ports, query ports to portmask configurable)
- „Not in sync“ display if configuration in Flash/ACA and running config are different
- Configurable priority of the management agent answers
- QoS: TOS/DSCP prioritization
- Shared VLAN Learning
- Config rollback function: Show IP Address of the monitoring station
- Autocrossing configurable
- RAM Test on/off (with new Bootcode)
- IGMP Snooping Improvements
- RSTP actualization to 802.1D-2004
- MRP with 200ms ring recovery
- HIPER-Ring: Option to reduce maximum ring recovery time.
- DHCP server per port
- LLDP Enhancement to detect some configuration errors
- Profinet IO Protocol
- Profinet Version 2.2 (PDEV) for all devices
- Profinet: GSDML file generator enhancements
- Profinet: Standalone GSDML generator
- Profinet: Automatic device exchange with Engineering Station
- Profinet: PnP functionality of port modules
- Profinet: Completion of LLDP-Implementation for PNIO-MIB
- Profinet: Transmission of switch data in Profinet I/O data
- Optimization of Link detection (Hardware dependend)
- RSTP enhancement (Port Auto Edge)
- RSTP and MRP Ring in combination
- No reset configurable in case of error
- Ethernet/IP: Transmission of DIP switch status in I/O data
- MAC based port security: Ranges with a bitmask configurable
- Show CPU / Memory utilization in CLI
- Configure RMON alarms in CLI
- SNMPv3 Authentication over RADIUS

New functions of L2P:
- Hardware support for MAR1040 and MACH104
- New WEB-Interface wizzard for IP/MAC port security
- New event for device status / signal contacts: „ACA not in sync“
- Profinet: Enable/disable DCP Protocol per port
- Profinet: Enable/disable Fast-Start-Up support per port (Hardware dependend)

Software Release 06.0.00
------------------------
Bugfixes (see issuelist)

New functions of L2P:
- Port-Mirroring N:1
- Trap for Configuration Saving and Changing
- Address Relearn Detection
- Duplex Mismatch Detection
- SNTP Client and Server separately configurable
- Removed Security Data Sheet (IAONA)
- Configurable CLI banner
- Switch Dump: Download System Information in one ZIP File
- SNMP Logging
- Configure Syslog Settings over WEB
- Profinet: MRP Configurable over Simatic S7
- Profinet: LLDP Extensions
- Automatic Software Update over ACA21
- Multiple Spanning Tree (MSTP)
- RSTP Standard MIB
- Restricted Management Access

Software Release 07.0.00
------------------------
Bugfixes (see issuelist)

New functions of L2P:
- LLDP-MED
- Voice VLAN
- PoE+ Management
- 802.1x Multi Client Authentication
- Guest VLAN / Unauthenticated VLAN for 802.1x
- RADIUS VLAN Assignment
- New configuration check dialog
- Offline configuration
- Port Monitor (Link flap & CRC)
- Advanced Ring Configuration & Diagnostics for MRP
- Port Security with up to 50 MACs per port
- Reload/Reboot with configurable delay
- SFP power also shown in dBm
- Switch to backup SW via Web
- Automatic script load from ACA21 on boot
- IEEE 1588-2002 (PTPv1) and IEEE1588-2008 (PTPv2) two-step BC & TC
- Double-VLAN-Tagging / VLAN-Tunneling

Software Release 07.1.00
------------------------
Bugfixes (see issuelist)

New functions of L2P:
- HTTPs Web login

Software Release 07.1.04
------------------------
Bugfixes (see issuelist)
- Discard unknown multicast option for GMRP

Software Release 08.0.00
------------------------
Bugfixes (see issuelist)

New functions of L2P:
- Ethernet/IP: Configurable TTL and EDS AOP support
- Configuration Signature
- DHCP-Relay per port configuration
- Pre-Login-Banner
- DHCP Option 43 support
- DHCP Server configurable ping check.
- Overload detection (as part of Port Monitor)
- Auto Disable
- Port Mirroring Extensions
- MAC notification
- SSH Version 2
- Strong encryption for HTTPS
- Jumbo Frame support

New functions of L3P:
- ACLs supporting Layer 4 fragments

Software Release 08.0.05
------------------------
Bugfixes (see issuelist)

- Removed Rx Power State for SFPs.

Software Release 09.0.00
------------------------
Bugfixes (see issuelist)

New functions of L2P:
- HiDiscovery v2 support
- DHCP Relay per Interface
- Configurable number of addresses per interface for Port Security
- Admin State for System Monitor 1
- Link Speed and Duplex Monitor in port monitor 
- Auto-disable for Link / Duplex Monitor
- Auto-disable for Port Security
- Configurable CLI banner via CLI
- Configurable SNMP v1/v2 community synchronization
- Manual PoE power management
- Profinet GSDML File Version 2.3
- Configuration locking if Profinet AR is active. 

New functions of L3P:
- Increase Static unicast routes to 512

Software Release 09.0.06
------------------------
Bugfixes (see issuelist)

New functions
- MAC Address conflict detection

Software Release 09.0.12
------------------------
Bugfixes (see issuelist)

New functions of L3P:
- PIM-DM static entries support

Software Release 09.0.15
------------------------
Bugfixes (see issuelist)

New functions:
- Support for up to 4 Subrings

Software Release 09.0.17
------------------------
Bugfixes (see issuelist)

New functions of L2P and L3P:
- Added the possibility to configure the auto-negotiate capability bits

Software Release 09.1.00
------------------------
Bugfixes (see issuelist)

New functions:
- Changed defaults: SNMPv1 and SNMPv2 are disabled.
- Password change on first login
  Protocols that require a login (e.g. SNMPv3) remain deactivated until the password is changed. 

Software Release 09.1.01
------------------------
Bugfixes (see issuelist)

New functions:
- PTP Boundary Clock: New "master-only" option. If activated, no other masters will be allowed on that port.  

Software Release 09.1.02
------------------------
Bugfixes (see issuelist)

New functions:
- SSH Version 1 was removed.
- The insecure OpenSSH option "diffie-hellman-group1-sha1 Key Exchange" was removed.

Software Release 09.1.04
------------------------
Bugfixes (see issuelist)

New functions:
- Added 1000ms ring recovery for MRP.
- Added 1000ms ring recovery for Sub-Ring.

Software Release 09.1.06
------------------------
Bugfixes (see issuelist)

New functions of L2P and L3P:
- Option to encrypt the exported file containing the device configuration.

Software Release 09.1.14
------------------------
Bugfixes (see issuelist)
