
Important Software Update Information to version 07.1.00 (or higher)
--------------------------------------------------------------------


New designations for the software images of the Octopus family devices 
----------------------------------------------------------------------

    device                  new designation         previous designation
                            since 07.1.00           till 07.1.00
    --------------------    ----------------        ----------------
    Octopus 8M, 16M, 24M    omL2P.bin               octL2P.bin
    Octopus OS 20/30        orL2P.bin               osL2P.bin
    Octopus OS 32           omL2P.bin               -



Update instruction for the Octopus 8M, Octopus 16M and Octopus 24M devices
--------------------------------------------------------------------------

Requirements:
The device has the device software version 07.0.03 (or higher) and the boot
software version 05.0.00 (or higher) installed.

The currently installed version of the device software and boot software
you find in the CLI with the command "show sysinfo".
Example:

        show sysinfo
        ...
        Boot Software Release.......................... L2P-06.0.03
        ...
        Running Software Release....................... L2P-07.0.03
        ...


Step 1:
        - Update the device software to version 07.0.03.
          Use for this the image octL2P.bin.
        - Restart the device.

Step 2:
        - Update the boot software. Use the CLI only; type the command:
            copy tftp://<server IP>/<path>/octL2P_boot.img system:bootcode
        - Restart the device.

Step 3:
        - Update the device software to version 07.1.00 (or higher). 
          Use for this the image omL2P.bin.
          Consider the new designations of the software images.
