
HM2-POE-MIB DEFINITIONS ::= BEGIN

--
-- *************************************************************
-- Hirschmann Power over Ethernet Management MIB
-- *************************************************************
--

IMPORTS
    MODULE-IDENTITY, NOTIFICATION-TYPE,
    OBJECT-TYPE, 
    Integer32			        FROM SNMPv2-SMI -- RFC 2578
    SnmpAdminString				FROM SNMP-FRAMEWORK-MIB
    hm2IfacePhysIndex           FROM HM2-DEVMGMT-MIB
    HmEnabledStatus, HmTimeHHMM24,
    hm2ConfigurationMibs        FROM HM2-TC-MIB;

hm2PoeMgmtMib MODULE-IDENTITY
	LAST-UPDATED "201110310000Z" -- October 31, 2011
    ORGANIZATION "Hirschmann Automation and Control GmbH"
    CONTACT-INFO
        "Postal:     Stuttgarter Str. 45-51
                     72654 Neckartenzlingen
                     Germany
         Phone:      +49 7127 140
         E-mail:     hac.support@belden.com"
    DESCRIPTION
        "Hirschmann Power over Ethernet Management MIB. This MIB contains
         the private extensions to the RFC 3621.
         Copyright (C) 2011. All Rights Reserved."
    REVISION     "201110310000Z" -- October 31, 2011
    DESCRIPTION
         "Initial version."
    ::= { hm2ConfigurationMibs 12 }

--
-- *************************************************************
-- hm2PoeMgmtMib
-- *************************************************************
--

hm2PoeMgmtMibNotifications	OBJECT IDENTIFIER ::= { hm2PoeMgmtMib 0 }
hm2PoeMgmtMibObjects		OBJECT IDENTIFIER ::= { hm2PoeMgmtMib 1 }
-- hm2PoeMgmtMibConformance		OBJECT IDENTIFIER ::= { hm2PoeMgmtMib 2 }


--
-- *************************************************************
-- hm2PoeMgmtMib groups
-- *************************************************************
--

hm2PoeMgmtGroup 		OBJECT IDENTIFIER ::= { hm2PoeMgmtMibObjects 1 }


--
-- *************************************************************
-- hm2PoeMgmtGlobalGroup
-- *************************************************************
--

hm2PoeMgmtGlobalGroup	OBJECT IDENTIFIER ::= { hm2PoeMgmtGroup 1 }

hm2PoeMgmtAdminStatus	OBJECT-TYPE
						SYNTAX HmEnabledStatus
						MAX-ACCESS read-write
						STATUS current
						DESCRIPTION
							"Enables/disables Power over Ethernet management on this device."
						DEFVAL  { enable }
						::= { hm2PoeMgmtGlobalGroup 1 }

hm2PoeMgmtReservedPower	OBJECT-TYPE
						SYNTAX Integer32
						MAX-ACCESS read-only
						STATUS current
						DESCRIPTION
							"Reserved system power for active Power over Ethernet ports in Watts."
						::= { hm2PoeMgmtGlobalGroup 2 }

--
-- *************************************************************
-- hm2PoeMgmtPsuTable
-- *************************************************************
--

hm2PoeMgmtPsuTable		OBJECT-TYPE
						SYNTAX SEQUENCE OF Hm2PoeMgmtPsuEntry
						MAX-ACCESS not-accessible
						STATUS current
						DESCRIPTION
							"This table contains objects for each power supply type of
							 the device (internal or external power supply)."
						::= { hm2PoeMgmtGroup 2 }

hm2PoeMgmtPsuEntry		OBJECT-TYPE
						SYNTAX Hm2PoeMgmtPsuEntry
						MAX-ACCESS not-accessible
						STATUS current
						DESCRIPTION
							"The entries of the hm2PoeMgmtPsuTable."
						INDEX { hm2PoeMgmtModulePowerSource }
						::= { hm2PoeMgmtPsuTable 1 }

Hm2PoeMgmtPsuEntry		::= SEQUENCE {
							hm2PoeMgmtPsuPower							Integer32,
							hm2PoeMgmtPsuReservedPower					Integer32,
							hm2PoeMgmtPsuDeliveredPower					Integer32
						}

hm2PoeMgmtPsuPower		OBJECT-TYPE
						SYNTAX Integer32
						MAX-ACCESS read-only
						STATUS current
						DESCRIPTION
							"The power budget per psu type expressed in Watts. Psu types could
							 be internal or external."
						::= { hm2PoeMgmtPsuEntry 1 }

hm2PoeMgmtPsuReservedPower	OBJECT-TYPE
						SYNTAX Integer32
						MAX-ACCESS read-only
						STATUS current
						DESCRIPTION
							"The reserved power (depending on actual power classes) 
							per psu type expressed in Watts."
						::= { hm2PoeMgmtPsuEntry 2 }

hm2PoeMgmtPsuDeliveredPower 	OBJECT-TYPE
						SYNTAX Integer32
						MAX-ACCESS read-only
						STATUS current
						DESCRIPTION
							"The measured usage power per psu type expressed in Watts."
						::= { hm2PoeMgmtPsuEntry 3 }

--
-- *************************************************************
-- hm2PoeMgmtPortTable
-- *************************************************************
--

hm2PoeMgmtPortTable		OBJECT-TYPE
						SYNTAX SEQUENCE OF Hm2PoeMgmtPortEntry
						MAX-ACCESS not-accessible
						STATUS current
						DESCRIPTION
							"This table contains objects for each Power over Ethernet interface of
							the device."
						::= { hm2PoeMgmtGroup 3 }

hm2PoeMgmtPortEntry		OBJECT-TYPE
						SYNTAX Hm2PoeMgmtPortEntry
						MAX-ACCESS not-accessible
						STATUS current
						DESCRIPTION
							"The entry of the hm2PoeMgmtPortTable."
						INDEX { hm2IfacePhysIndex }
						::= { hm2PoeMgmtPortTable 1 }

Hm2PoeMgmtPortEntry 	::= SEQUENCE {
						hm2PoeMgmtPortAdminEnable			HmEnabledStatus,
						hm2PoeMgmtPortConsumptionPower		Integer32,
						hm2PoeMgmtPortDetectionStatus   	INTEGER,
						hm2PoeMgmtPortPowerPriority			INTEGER,
						hm2PoeMgmtPortPowerClassification  	INTEGER,
						hm2PoeMgmtPortName					SnmpAdminString,
						hm2PoeMgmtPortAllowedClassBits  	BITS,
						hm2PoeMgmtPortAutoShutdown			HmEnabledStatus,
						hm2PoeMgmtPortAutoShutdownTimeStart HmTimeHHMM24,
						hm2PoeMgmtPortAutoShutdownTimeEnd	HmTimeHHMM24,
						hm2PoeMgmtPortClassValid            INTEGER,
						hm2PoeMgmtPortFastStartup			HmEnabledStatus,
						hm2PoeMgmtPortMaxConsumptionPower   Integer32,
						hm2PoeMgmtPortPowerLimit            Integer32
						}

hm2PoeMgmtPortAdminEnable OBJECT-TYPE
    					SYNTAX HmEnabledStatus
    					MAX-ACCESS read-write
    					STATUS current
					    DESCRIPTION
					        "enable (1) An interface which can provide the PSE functions.
					         disable(2) The interface will act - as it would - if it had no PSE
					         function."
					    DEFVAL { enable }
					    ::= { hm2PoeMgmtPortEntry 1 }

hm2PoeMgmtPortConsumptionPower OBJECT-TYPE
						SYNTAX Integer32
						MAX-ACCESS read-only
						STATUS current
						DESCRIPTION
							"Measured usage power per interface expressed in Milliwatts."
						::= { hm2PoeMgmtPortEntry 2 }

hm2PoeMgmtPortDetectionStatus OBJECT-TYPE
					    SYNTAX INTEGER   {
					             disabled(1),
					             searching(2),
					             deliveringPower(3),
					             fault(4),
					             test(5),
					             otherFault(6)
					    }
					    MAX-ACCESS read-only
					    STATUS current
					    DESCRIPTION
					        "Describes the operational status of the port PD detection.
					         A value of disabled(1)- indicates that the PSE State diagram
					         is in the state DISABLED.
					         A value of deliveringPower(3) - indicates that the PSE State
					         diagram is in the state POWER_ON.
					         A value of fault(4) - indicates that the PSE State diagram is
					         in the state TEST_ERROR.
					         A value of test(5) - indicates that the PSE State diagram is
					         in the state TEST_MODE.
					         A value of otherFault(6) - indicates that the PSE State
					         diagram is in the state IDLE due to the variable
					         error_conditions.
					         A value of searching(2)- indicates the PSE State diagram is
					         in a state other than those listed above."
					         
					    ::= { hm2PoeMgmtPortEntry 3 }
					    
hm2PoeMgmtPortPowerPriority OBJECT-TYPE
					    SYNTAX INTEGER   {
					               critical(1),
					               high(2),
					               low(3)
					     }
					    MAX-ACCESS read-write
					    STATUS current
					    DESCRIPTION
					        "This object controls the priority of the port from the point
					         of view of a power management algorithm.  The priority that
					         is set by this variable could be used by a control mechanism
					         that prevents over current situations by disconnecting first
					         ports with lower power priority.  Ports that connect devices
					         critical to the operation of the network - like the E911
					         telephones ports - should be set to higher priority."
					         
					    DEFVAL { low }     
					    ::= { hm2PoeMgmtPortEntry 4 }
					    
hm2PoeMgmtPortPowerClassification OBJECT-TYPE
					    SYNTAX INTEGER    {
					               class0(1),
					               class1(2),
					               class2(3),
					               class3(4),
					               class4(5)
					    }
					    MAX-ACCESS read-only
					    STATUS current
					    DESCRIPTION
					        "Classification is a way to tag different terminals on the
					        Power over LAN network according to their power consumption.
					        Devices such as IP telephones, WLAN access points and others,
					        will be classified according to their power requirements.
					
					        The meaning of the classification labels is defined in the
					        IEEE specification.
					
					       This variable is valid only while a PD is being powered,
					        that is, while the attribute hm2PoeMgmtPortDetectionStatus
					        is reporting the enumeration deliveringPower."
					    DEFVAL { class0 }
					    ::= { hm2PoeMgmtPortEntry 5 }
   
hm2PoeMgmtPortName		OBJECT-TYPE
					    SYNTAX SnmpAdminString (SIZE(1..32))
					    MAX-ACCESS read-write
					    STATUS current
					    DESCRIPTION
					        "A manager will set the value of this variable to indicate
					         the type of powered device that is connected to the port.
					         The default value supplied by the agent if no value has
					         ever been set should be a zero-length octet string."
					    DEFVAL { " " }     
					    ::= { hm2PoeMgmtPortEntry 6 }

hm2PoeMgmtPortAllowedClassBits	OBJECT-TYPE
						SYNTAX      BITS {
							class0(0),
							class1(1),
							class2(2),
							class3(3),
							class4(4)
						}
						MAX-ACCESS read-write
						STATUS current
						DESCRIPTION
							"Bit mask which defines allowed classes per interface."
						DEFVAL { { class0, class1, class2, class3, class4 } }
						::= { hm2PoeMgmtPortEntry 7 }

hm2PoeMgmtPortAutoShutdown	OBJECT-TYPE
						SYNTAX HmEnabledStatus
						MAX-ACCESS read-write
						STATUS current
						DESCRIPTION
							"Enables/disables automatic shutdown functionality per interface."
						DEFVAL { disable }
						::= { hm2PoeMgmtPortEntry 8 }
						
hm2PoeMgmtPortAutoShutdownTimeStart	OBJECT-TYPE
						SYNTAX HmTimeHHMM24
						MAX-ACCESS read-write
						STATUS current
						DESCRIPTION
							"Start time for the automatic shutdown functionality per interface."
						DEFVAL { "00:00" }
						::= { hm2PoeMgmtPortEntry 9 }

hm2PoeMgmtPortAutoShutdownTimeEnd	OBJECT-TYPE
						SYNTAX HmTimeHHMM24
						MAX-ACCESS read-write
						STATUS current
						DESCRIPTION
							"End time for the automatic shutdown functionality per interface."
						DEFVAL { "00:00" }
						::= { hm2PoeMgmtPortEntry 10 }
						
hm2PoeMgmtPortClassValid	OBJECT-TYPE
						SYNTAX INTEGER   {
									        invalid(0),
									          valid(1)
									     }
						MAX-ACCESS read-only
						STATUS current
						DESCRIPTION
							"Evaluates if class represented through pethPsePortPowerClassifications
							 is valid or not. Class is valid if PD is delivered with power or in case
							 of power exceeding through a connected device."
						::= { hm2PoeMgmtPortEntry 11 }

hm2PoeMgmtPortFastStartup	OBJECT-TYPE
						SYNTAX HmEnabledStatus
						MAX-ACCESS read-write
						STATUS current
						DESCRIPTION
							"Enables/disables Power over Ethernet fast startup mode on given port.
							 The default value is 'disable'."
						DEFVAL { disable }
						::= { hm2PoeMgmtPortEntry 12 }

hm2PoeMgmtPortMaxConsumptionPower  OBJECT-TYPE
						SYNTAX Integer32
						MAX-ACCESS read-only
						STATUS current
						DESCRIPTION
							"The  maximum observed power consumption (hm2PoeMgmtPortMaxConsumptionPower)
							value expressed in milliwatts used by the PD.
							The value is reset to 0 if the PoE admin state is set to disable
							or if a disconnect of the PD is detected."
						::= { hm2PoeMgmtPortEntry 13 }

hm2PoeMgmtPortPowerLimit OBJECT-TYPE
						SYNTAX Integer32 (0..30000)
						MAX-ACCESS read-write
						STATUS current
						DESCRIPTION
							"The power limit per port expressed in milliwatts. If set to
							zero the power consumption limitation is disabled."
						DEFVAL { 0 }
						::= { hm2PoeMgmtPortEntry 14 }

--
-- *************************************************************
-- hm2PoeMgmtModuleTable
-- *************************************************************
--

hm2PoeMgmtModuleTable	OBJECT-TYPE
						SYNTAX SEQUENCE OF Hm2PoeMgmtModuleEntry
						MAX-ACCESS not-accessible
						STATUS current
						DESCRIPTION
							"This table contains objects for each plugged PoE module of
							the device. If the device is non-modular and supports PoE it
							contains only one entry."
						::= { hm2PoeMgmtGroup 4 }

hm2PoeMgmtModuleEntry	OBJECT-TYPE
						SYNTAX Hm2PoeMgmtModuleEntry
						MAX-ACCESS not-accessible
						STATUS current
						DESCRIPTION
							"The entries of the hm2PoeMgmtModuleTable."
						INDEX { hm2PoeMgmtModuleUnitIndex, hm2PoeMgmtModuleSlotIndex }
						::= { hm2PoeMgmtModuleTable 1 }

Hm2PoeMgmtModuleEntry	::= SEQUENCE {
							hm2PoeMgmtModuleUnitIndex					Integer32,
							hm2PoeMgmtModuleSlotIndex					Integer32,
							hm2PoeMgmtModulePower						Integer32,
							hm2PoeMgmtModuleMaximumPower				Integer32,
							hm2PoeMgmtModuleReservedPower				Integer32,
							hm2PoeMgmtModuleDeliveredPower				Integer32,
							hm2PoeMgmtModulePowerSource					INTEGER,
							hm2PoeMgmtModuleUsageThreshold				Integer32,
							hm2PoeMgmtModuleNotificationControlEnable	HmEnabledStatus
						}

hm2PoeMgmtModuleUnitIndex	OBJECT-TYPE
						SYNTAX Integer32
						MAX-ACCESS not-accessible
						STATUS current
						DESCRIPTION
							"Unit number - for stacking devices."
						::= { hm2PoeMgmtModuleEntry 1 }

hm2PoeMgmtModuleSlotIndex	OBJECT-TYPE
						SYNTAX Integer32
						MAX-ACCESS not-accessible
						STATUS current
						DESCRIPTION
							"Slot number of the plugged PoE module."
						::= { hm2PoeMgmtModuleEntry 2 }

hm2PoeMgmtModulePower	OBJECT-TYPE
						SYNTAX Integer32 (0..1000)
						MAX-ACCESS read-write
						STATUS current
						DESCRIPTION
							"Configurable power budget per module expressed in Watts. The default
							value is hm2PoeMgmtModuleMaximumPower and depends on the hardware."
						DEFVAL { 1000 }
						::= { hm2PoeMgmtModuleEntry 3 }

hm2PoeMgmtModuleMaximumPower	OBJECT-TYPE
						SYNTAX Integer32 (0..1000)
						MAX-ACCESS read-only
						STATUS current
						DESCRIPTION
							"Maximum available power budget per module expressed in Watts. This
							value depends on the device or module."
						::= { hm2PoeMgmtModuleEntry 4 }

hm2PoeMgmtModuleReservedPower	OBJECT-TYPE
						SYNTAX Integer32
						MAX-ACCESS read-only
						STATUS current
						DESCRIPTION
							"The reserved power (depending on actual power classes) 
							per module expressed in Watts."
						::= { hm2PoeMgmtModuleEntry 5 }

hm2PoeMgmtModuleDeliveredPower	OBJECT-TYPE
						SYNTAX Integer32
						MAX-ACCESS read-only
						STATUS current
						DESCRIPTION
							"The measured usage power per module expressed in Watts."
						::= { hm2PoeMgmtModuleEntry 6 }
						
hm2PoeMgmtModulePowerSource 	OBJECT-TYPE
						SYNTAX INTEGER   {
									        internal(0),
									        external(1)
									     }
						MAX-ACCESS read-only
						STATUS current
						DESCRIPTION
							"This object displays the type of the PoE power source.
							 internal (0) means that the PoE power is used from the internal PSU and
							 external (1) means that a external PoE PSU must be installed and connected to this module."
						::= { hm2PoeMgmtModuleEntry 7 }
	
hm2PoeMgmtModuleUsageThreshold OBJECT-TYPE
						SYNTAX Integer32 (1..99)
						MAX-ACCESS read-write
						STATUS current
						DESCRIPTION
							"The usage power threshold per module expressed in percent. 
							If this threshold is exceeded a alarm is initiated."
						DEFVAL { 90 }
						::= { hm2PoeMgmtModuleEntry 8 }
	
hm2PoeMgmtModuleNotificationControlEnable OBJECT-TYPE
						SYNTAX 	HmEnabledStatus
						MAX-ACCESS 	read-write
						STATUS current
						DESCRIPTION
							"This object controls, on a per-module basis, whether
							or not notifications from the agent are enabled. "
						DEFVAL { enable }
						::= { hm2PoeMgmtModuleEntry 9 }


--
-- *************************************************************
-- hm2PoeMgmtMibNotifications
-- *************************************************************
--

hm2PoeMgmtModulePowerUsageOnNotification NOTIFICATION-TYPE
						OBJECTS { hm2PoeMgmtModuleDeliveredPower }
						STATUS current
						DESCRIPTION 
							"This Notification indicate PSE Threshold usage indication 
							is on, the usage power is above the threshold. 
							At least 500 msec must elapse between notifications being 
							emitted by the same object instance."
						::= { hm2PoeMgmtMibNotifications 1 }

hm2PoeMgmtModulePowerUsageOffNotification NOTIFICATION-TYPE
						OBJECTS { hm2PoeMgmtModuleDeliveredPower }
						STATUS current
						DESCRIPTION 
							"This Notification indicate PSE Threshold usage indication 
							is on, the usage power is below the threshold. 
							At least 500 msec must elapse between notifications being 
							emitted by the same object instance."
						::= { hm2PoeMgmtMibNotifications 2 }


hm2PoeMgmtPortMaxConfiguredPowerLimitExceeded NOTIFICATION-TYPE
						OBJECTS	{ hm2IfacePhysIndex, hm2PoeMgmtPortMaxConsumptionPower, hm2PoeMgmtPortPowerLimit }
						STATUS  current
						DESCRIPTION
							"This trap reports an exceeding of the configured power limit.
							This notification indicates that a PD consumes more power
							that the maximum configured on the port and the system reserved
							the maximum power required for the negotiated class."
						::= { hm2PoeMgmtMibNotifications 3 }

END

