
HM2-LOGGING-MIB DEFINITIONS ::= BEGIN

--
-- *************************************************************
-- Hirschmann Logging MIB
-- *************************************************************
--

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, 
    NOTIFICATION-TYPE, 
    Integer32, Counter32, Unsigned32
    								FROM SNMPv2-SMI -- RFC 2578
    TEXTUAL-CONVENTION,
    DisplayString,
    RowStatus						FROM SNMPv2-TC
    SnmpAdminString     			FROM SNMP-FRAMEWORK-MIB
	InetPortNumber, InetAddress,
	InetAddressType					FROM INET-ADDRESS-MIB
    hm2ConfigurationMibs, 
    HmEnabledStatus,
    HmTimeSeconds1970				FROM HM2-TC-MIB
    Hm2TlsVersions,
    Hm2TlsCipherSuites				FROM HM2-MGMTACCESS-MIB;

hm2LoggingMib MODULE-IDENTITY
	LAST-UPDATED "201208080000Z" -- August 8, 2012
    ORGANIZATION "Hirschmann Automation and Control GmbH"
    CONTACT-INFO
        "Postal:     Stuttgarter Str. 45-51
                     72654 Neckartenzlingen
                     Germany
         Phone:      +49 7127 140
         E-mail:     hac.support@belden.com"
    DESCRIPTION
        "Hirschmann Logging MIB.
         Copyright (C) 2012. All Rights Reserved."
    REVISION     "201208080000Z" -- August 8, 2012
    DESCRIPTION
         "Modify hm2LogSyslogServerIPAddrType description because DNS was added."
    REVISION     "201103160000Z" -- March 16, 2011
    DESCRIPTION
         "Initial version."
    ::= { hm2ConfigurationMibs 23 }

--
-- *************************************************************
-- Textual Conventions
-- *************************************************************
--         
HmAgentLogSeverity ::= TEXTUAL-CONVENTION
		STATUS       current
		DESCRIPTION
		"Severity code used in determining the SysLog priority value."
		REFERENCE
		"RFC3164 - 4.1.1: Table 2"
		SYNTAX  INTEGER {
        	 	 	 	 emergency(0),     -- System is unusable. System failure has occurred.
        	 	 	 	 alert(1),         -- Action must be taken immediately. Unrecoverable
        	 	 	 	 	 	 	 	   --  failure of a component. System failure likely.
        	 	 	 	 critical(2),      -- Critical conditions. Recoverable failure of a
        	 	 	 	 	 	 	 	   --  component that may lead to system failure.
        	 	 	     error(3),         -- Error conditions. Recoverable failure of a component.
        	 	 	     warning(4),       -- Warning conditions. Minor failure, e.g.
        	 	 	     	 	 	 	   --  misconfiguration of a component.
        	 	 	     notice(5),        -- Normal but significant conditions.
        	 	 	     informational(6), -- Informational messages.
        	 	 	     debug(7)          -- Debug-level messages.
         	 	 	 	 }         
         
--
-- *************************************************************
-- hm2LoggingMib
-- *************************************************************
--
hm2LoggingMibNotifications		OBJECT IDENTIFIER ::= { hm2LoggingMib 0 }
hm2LoggingMibObjects			OBJECT IDENTIFIER ::= { hm2LoggingMib 1 }
-- hm2LoggingMibConformance			OBJECT IDENTIFIER ::= { hm2LoggingMib 2 }

--
-- *************************************************************
-- hm2LoggingMib groups
-- *************************************************************
--
hm2LogSnmpLoggingGroup			OBJECT IDENTIFIER ::= { hm2LoggingMibObjects 1 }
hm2LogCliCommandsLoggingGroup	OBJECT IDENTIFIER ::= { hm2LoggingMibObjects 2 }
hm2LogConsoleLoggingGroup		OBJECT IDENTIFIER ::= { hm2LoggingMibObjects 3 }
hm2LogBufferedLoggingGroup		OBJECT IDENTIFIER ::= { hm2LoggingMibObjects 4 }
hm2LogSyslogGroup				OBJECT IDENTIFIER ::= { hm2LoggingMibObjects 5 }
hm2LogPersistentGroup			OBJECT IDENTIFIER ::= { hm2LoggingMibObjects 6 }
hm2LogCounterGroup				OBJECT IDENTIFIER ::= { hm2LoggingMibObjects 7 }
hm2LogTemperatureGroup			OBJECT IDENTIFIER ::= { hm2LoggingMibObjects 8 }
hm2LogAuditGroup				OBJECT IDENTIFIER ::= { hm2LoggingMibObjects 9 }
hm2LogEmailAlertGroup			OBJECT IDENTIFIER ::= { hm2LoggingMibObjects 10 }


--
-- *************************************************************
-- hm2LogSnmpLoggingGroup
-- *************************************************************
--

hm2LogSnmpLogGetRequest	OBJECT-TYPE
			SYNTAX		HmEnabledStatus
			MAX-ACCESS	read-write
			STATUS		current
			DESCRIPTION
					"Enable logging of SNMP GET requests."
			DEFVAL { disable }
			::= { hm2LogSnmpLoggingGroup 1 }


hm2LogSnmpLogSetRequest	OBJECT-TYPE
			SYNTAX		HmEnabledStatus
			MAX-ACCESS	read-write
			STATUS		current
			DESCRIPTION
					"Enable logging of SNMP SET requests."
			DEFVAL { disable }
			::= { hm2LogSnmpLoggingGroup 2 }


hm2LogSnmpLogGetSeverity	OBJECT-TYPE
			SYNTAX		HmAgentLogSeverity
			MAX-ACCESS	read-write
			STATUS		current
			DESCRIPTION
					"Define the log severity for SNMP GET requests."
			DEFVAL { notice }
			::= { hm2LogSnmpLoggingGroup 3 }


hm2LogSnmpLogSetSeverity	OBJECT-TYPE
			SYNTAX		HmAgentLogSeverity
			MAX-ACCESS	read-write
			STATUS		current
			DESCRIPTION
					"Define the log severity for SNMP SET requests."
			DEFVAL { notice }
			::= { hm2LogSnmpLoggingGroup 4 }


--
-- *************************************************************
-- hm2LogCliCommandsLoggingGroup
-- *************************************************************
--

hm2LogCliCommandsAdminStatus	OBJECT-TYPE
			SYNTAX		HmEnabledStatus
			MAX-ACCESS	read-write
			STATUS		current
			DESCRIPTION
					"Administratively enable/disable the logging of the CLI commands."
			DEFVAL { disable }
			::= { hm2LogCliCommandsLoggingGroup 1 }


--
-- *************************************************************
-- hm2LogConsoleLoggingGroup
-- *************************************************************
--

hm2LogConsoleAdminStatus	OBJECT-TYPE
			SYNTAX		HmEnabledStatus
			MAX-ACCESS	read-write
			STATUS		current
			DESCRIPTION
					"Admin mode for console logs"
			DEFVAL { disable }
			::= { hm2LogConsoleLoggingGroup 1 }


hm2LogConsoleSeverityFilter	OBJECT-TYPE
			SYNTAX		HmAgentLogSeverity
			MAX-ACCESS	read-write
			STATUS		current
			DESCRIPTION
					"Severity filter for console logs"
			DEFVAL { warning }
			::= { hm2LogConsoleLoggingGroup 2 }


--
-- *************************************************************
-- hm2LogBufferedLoggingGroup
-- *************************************************************
--

hm2LogBufferdLogLevelThreshold	OBJECT-TYPE
			SYNTAX		HmAgentLogSeverity
			MAX-ACCESS	read-write
			STATUS		current
			DESCRIPTION
					"Severities at or below this threshold are logged in the buffered log 
					and will not be overwritten by lower priority log messages."
			DEFVAL { warning }
			::= { hm2LogBufferedLoggingGroup 1 }


--
-- *************************************************************
-- hm2LogSyslogGroup
-- *************************************************************
--

hm2LogSyslogAdminStatus	OBJECT-TYPE
			SYNTAX		HmEnabledStatus
			MAX-ACCESS	read-write
			STATUS		current
			DESCRIPTION
					"Enable or disable syslog logging globally."
			DEFVAL { disable }
			::= { hm2LogSyslogGroup 1 }

hm2LogSyslogClientTlsVersions OBJECT-TYPE
			SYNTAX			Hm2TlsVersions
			MAX-ACCESS		read-write
			STATUS			current
			DESCRIPTION		"The TLS versions supported by the syslog client."
			DEFVAL {{ tlsv1-2 }}
			::= { hm2LogSyslogGroup  2 }

hm2LogSyslogClientTlsCipherSuites OBJECT-TYPE
			SYNTAX			Hm2TlsCipherSuites
			MAX-ACCESS		read-write
			STATUS			current
			DESCRIPTION		"The cipher suite supported by the syslog client."
			DEFVAL {{
					tls-rsa-with-aes-128-cbc-sha,
					tls-dhe-rsa-with-aes-128-cbc-sha,
					tls-ecdhe-rsa-with-aes-128-cbc-sha,
					tls-ecdhe-rsa-with-aes-128-gcm-sha256
					}}
			::= { hm2LogSyslogGroup  3 }

hm2LogSyslogServerTable	OBJECT-TYPE
			SYNTAX SEQUENCE OF Hm2LogSyslogServerEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
					"A list of syslog servers"
			::= { hm2LogSyslogGroup 10 }


hm2LogSyslogServerEntry	OBJECT-TYPE
			SYNTAX		Hm2LogSyslogServerEntry
			MAX-ACCESS	not-accessible
			STATUS current
			DESCRIPTION "An entry of syslog servers"
			INDEX { hm2LogSyslogServerIndex }
			::= { hm2LogSyslogServerTable 1 }


Hm2LogSyslogServerEntry ::= SEQUENCE {
		hm2LogSyslogServerIndex			Integer32,			-- index in the table
		hm2LogSyslogServerIPAddrType	InetAddressType,	-- address type of InetAddress
		hm2LogSyslogServerIPAddr		InetAddress,		-- IP address or domain name of syslog server
		hm2LogSyslogServerUdpPort		InetPortNumber,		-- port number of syslog server
		hm2LogSyslogServerLevelUpto		HmAgentLogSeverity,	-- minimal severity to be logged
		hm2LogSyslogServerLogType		INTEGER,			-- syslog or audit trail
		hm2LogSyslogServerRowStatus		RowStatus,			-- table row status
		hm2LogSyslogServerTransportType  INTEGER  -- type of transport used to deliver log messages
}

hm2LogSyslogServerIndex	OBJECT-TYPE
			SYNTAX		Integer32 (1..8)
			MAX-ACCESS	read-only
			STATUS		current
			DESCRIPTION
					"An index that uniquely identifies the entry
					in the table and so the syslog server."
			::= { hm2LogSyslogServerEntry 1 }


hm2LogSyslogServerIPAddrType	OBJECT-TYPE
			SYNTAX		InetAddressType
			MAX-ACCESS	read-create
			STATUS		current
			DESCRIPTION
					"Address type for server IP address.
					Currently, only ipv4(1) and dns(16) are supported."
			DEFVAL { ipv4 }
		::= { hm2LogSyslogServerEntry 2 }


hm2LogSyslogServerIPAddr	OBJECT-TYPE
			SYNTAX		InetAddress
			MAX-ACCESS	read-create
			STATUS		current
			DESCRIPTION
					"IP address of syslog server for logging."
			DEFVAL  { '00000000'H } -- 0.0.0.0
			::= { hm2LogSyslogServerEntry 3 }


hm2LogSyslogServerUdpPort	OBJECT-TYPE
			SYNTAX		InetPortNumber
			MAX-ACCESS	read-create
			STATUS		current
			DESCRIPTION
					"TCP or UDP port used for syslog server transmission. If this value is
					zero then the default port 514 is used."
			DEFVAL  { 514 }
			::= { hm2LogSyslogServerEntry 4 }


hm2LogSyslogServerLevelUpto	OBJECT-TYPE
			SYNTAX		HmAgentLogSeverity
			MAX-ACCESS	read-create
			STATUS		current
			DESCRIPTION
					"Up to log level to be sent to this syslog server."
			DEFVAL  { warning }
			::= { hm2LogSyslogServerEntry 5 }


hm2LogSyslogServerLogType   OBJECT-TYPE
			SYNTAX		INTEGER	{
						systemlog(1),
						audittrail(2)
						}
			MAX-ACCESS	read-create
			STATUS		current
			DESCRIPTION
					"Defines the type of log messages to be sent to the syslog server.
					systemlog  (1): Define the system event log entries as stored also in
					the system event log.
					audittrail (2): Define the audit trail log entries."
			DEFVAL  { systemlog }
			::= { hm2LogSyslogServerEntry 6 }


hm2LogSyslogServerRowStatus	OBJECT-TYPE
			SYNTAX		RowStatus
			MAX-ACCESS	read-create
			STATUS		current
			DESCRIPTION
					"Syslog server entry status.
					active(1)		- This syslog server is active.
					notInService(2)	- Row has been suspended.
					notReady(3)		- Row has incomplete values.
					createAndGo(4)	- Accept row values and activate.
					createAndWait(5)- Accept row values and wait.
					destroy(6) 		- Set to this value to remove this syslog server entry."
			::= { hm2LogSyslogServerEntry 7 }

hm2LogSyslogServerTransportType	OBJECT-TYPE
			SYNTAX		INTEGER	{
								udp(1),
								tls(2)
						}
			MAX-ACCESS	read-create
			STATUS		current
			DESCRIPTION  
			        "The transport type used to deliver the log messages to the syslog server. 
			        When set to udp(1) the syslog messages are sent over UDP on the configured port.
                    When set to tls(2) the syslog messages are sent over TLS 
                    on configured TCP port (hm2LogSyslogServerUdpPort)."
			DEFVAL  { udp }
			::= { hm2LogSyslogServerEntry 8 }

--
-- *************************************************************
-- hm2LogPersistentGroup
-- *************************************************************
--

hm2LogPersistAdminStatus	OBJECT-TYPE
			SYNTAX		HmEnabledStatus
			MAX-ACCESS	read-write
			STATUS		current
			DESCRIPTION
					"Enable or disable persistent logging globally."
			DEFVAL { enable }
			::= { hm2LogPersistentGroup 1 }


hm2LogPersistMaxFileSize	OBJECT-TYPE
			SYNTAX			Integer32 (0..4096)
			MAX-ACCESS		read-write
			STATUS 		current
			DESCRIPTION
					"Maximum persistent logfile size on non-volatile medium in Kbytes
					(0..4096). If this value is zero logging is disabled."
			DEFVAL { 1024 }
			::= { hm2LogPersistentGroup 2 }


hm2LogPersistFilesMax	OBJECT-TYPE
			SYNTAX			Integer32 (0..25)
			MAX-ACCESS		read-write
			STATUS 		current
			DESCRIPTION
					"Maximum number of persistent logfiles on non-volatile medium (0..25).
					If this value is zero logging and archiving is disabled."
			DEFVAL { 4 }
			::= { hm2LogPersistentGroup 3 }


hm2LogPersistLevelUpto	OBJECT-TYPE
			SYNTAX		HmAgentLogSeverity
			MAX-ACCESS	read-write
			STATUS		current
			DESCRIPTION
					"Up to log level to be sent to the persistent log"
			DEFVAL { warning }
			::= { hm2LogPersistentGroup 4 }

hm2LogPersistentFileTable	OBJECT-TYPE
			SYNTAX SEQUENCE OF Hm2LogPersistentFileEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
					"A list of persistent log files"
			::= { hm2LogPersistentGroup 5 }


hm2LogPersistentFileEntry	OBJECT-TYPE
			SYNTAX		Hm2LogPersistentFileEntry
			MAX-ACCESS	not-accessible
			STATUS	current
			DESCRIPTION "An entry of persistent log files"
			INDEX { hm2LogPersistentFileIndex }
			::= { hm2LogPersistentFileTable 1 }


Hm2LogPersistentFileEntry ::= SEQUENCE {
		hm2LogPersistentFileIndex		Integer32,		-- index in the table
		hm2LogPersistentFileName		DisplayString,	-- The name of the file
		hm2LogPersistentFileSize		Integer32			-- The size of the file in bytes
}


hm2LogPersistentFileIndex	OBJECT-TYPE
			SYNTAX		Integer32
			MAX-ACCESS		not-accessible
			STATUS 		current
			DESCRIPTION
					"The index of the table."
			::= { hm2LogPersistentFileEntry 1 }


hm2LogPersistentFileName	OBJECT-TYPE
			SYNTAX		DisplayString
			MAX-ACCESS	read-only
			STATUS		current
			DESCRIPTION
					"The name of the log file."
			::= { hm2LogPersistentFileEntry 2 }


hm2LogPersistentFileSize	OBJECT-TYPE
			SYNTAX		Integer32
			MAX-ACCESS	read-only
			STATUS		current
			DESCRIPTION
					"The size of the file in bytes."
			::= { hm2LogPersistentFileEntry 3 }



--
-- *************************************************************
-- hm2LogCounterGroup
-- *************************************************************
--

hm2LogCounterOperatingHours	OBJECT-TYPE
			SYNTAX		Integer32
			MAX-ACCESS	read-only
			STATUS		current
			DESCRIPTION
					"Cumulated uptime of the device in seconds."
			::= { hm2LogCounterGroup 1 }


hm2LogCounterFlashTable	OBJECT-TYPE
			SYNTAX SEQUENCE OF Hm2LogCounterFlashEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
					"A list of log counter entries"
			::= { hm2LogCounterGroup 10 }


hm2LogCounterFlashEntry	OBJECT-TYPE
			SYNTAX		Hm2LogCounterFlashEntry
			MAX-ACCESS	not-accessible
			STATUS	current
			DESCRIPTION "An entry of log counter entries"
			INDEX { hm2LogCounterFlashBlock }
			::= { hm2LogCounterFlashTable 1 }


Hm2LogCounterFlashEntry ::= SEQUENCE {
		hm2LogCounterFlashBlock			INTEGER,		-- Which blocks are counted
		hm2LogCounterFlashDescription	DisplayString,	-- Textual description of block
		hm2LogCounterFlashCount			Integer32,		-- How many blocks are counted
		hm2LogCounterFlashValue			Integer32		-- How often the blocks were erased
}


hm2LogCounterFlashBlock	OBJECT-TYPE
			SYNTAX		INTEGER {
							bootBlock(1),
							fileSystem(2),
							imageStorage(3),
							parameters(4),
							formatFs(5),
							userFormatFs(6),
							dhcpBindings(7),
							persistentLog(8)
						}
			MAX-ACCESS	not-accessible
			STATUS		current
			DESCRIPTION
					"The name of the flash region."
			::= { hm2LogCounterFlashEntry 1 }


hm2LogCounterFlashDescription	OBJECT-TYPE
			SYNTAX		DisplayString
			MAX-ACCESS	read-only
			STATUS		current
			DESCRIPTION
					"The textual description of the group."
			::= { hm2LogCounterFlashEntry 2 }


hm2LogCounterFlashCount	OBJECT-TYPE
			SYNTAX		Integer32
			MAX-ACCESS	read-only
			STATUS		current
			DESCRIPTION
					"The number of flash sectors in this group."
			::= { hm2LogCounterFlashEntry 3 }


hm2LogCounterFlashValue	OBJECT-TYPE
			SYNTAX		Integer32
			MAX-ACCESS	read-only
			STATUS		current
			DESCRIPTION
					"The number of sector erase operations performed for this group."
			::= { hm2LogCounterFlashEntry 4 }


--
-- *************************************************************
-- hm2LogTemperatureGroup
-- *************************************************************
--

hm2LogTempMinimum	OBJECT-TYPE
			SYNTAX		Integer32
			MAX-ACCESS	read-only
			STATUS		current
			DESCRIPTION
					"Minimal temperature on the device in 10th of centigrade (Celsius)."
			::= { hm2LogTemperatureGroup 1 }
			
hm2LogTempMaximum	OBJECT-TYPE
			SYNTAX		Integer32
			MAX-ACCESS	read-only
			STATUS		current
			DESCRIPTION
					"Maximal temperature on the device in 10th of centigrade (Celsius)."
			::= { hm2LogTemperatureGroup 2 }
			
hm2LogTempVariationCount	OBJECT-TYPE
			  SYNTAX		Integer32
			  MAX-ACCESS	read-only
			  STATUS		current
			  DESCRIPTION
					"Number of variations (up or down) by minimum 20 centigrade (Celsius) in maximum one hour period."
			::= { hm2LogTemperatureGroup 3 }			


hm2LogTempHistTable	OBJECT-TYPE
			SYNTAX SEQUENCE OF Hm2LogTempHistEntry
			MAX-ACCESS not-accessible
			STATUS current
			DESCRIPTION
					"A list of temperature ranges and how many hours the
					device has been in these ranges (histogram)."
			::= { hm2LogTemperatureGroup 10 }


hm2LogTempHistEntry	OBJECT-TYPE
			SYNTAX		Hm2LogTempHistEntry
			MAX-ACCESS	not-accessible
			STATUS	current
			DESCRIPTION "An entry of temperature ranges and how many hours the
					     device has been in these ranges (histogram)."
			INDEX { hm2LogTempHistIndex }
			::= { hm2LogTempHistTable 1 }


Hm2LogTempHistEntry ::= SEQUENCE {
		hm2LogTempHistIndex				Integer32,		-- Index
		hm2LogTempHistRangeMin			Integer32,		-- Lower bound of the range
		hm2LogTempHistRangeMax			Integer32,		-- Upper bound of the range
		hm2LogTempHistTime				Integer32		-- How many minutes were spent in this range
}

hm2LogTempHistIndex	OBJECT-TYPE
			SYNTAX		Integer32
			MAX-ACCESS	not-accessible
			STATUS		current
			DESCRIPTION
					"Index"
			::= { hm2LogTempHistEntry 1 }

hm2LogTempHistRangeMin	OBJECT-TYPE
			SYNTAX		Integer32
			MAX-ACCESS	read-only
			STATUS		current
			DESCRIPTION
					"The lower bound of the range in 10th of centigrade (Celsius)."
			::= { hm2LogTempHistEntry 2 }

hm2LogTempHistRangeMax	OBJECT-TYPE
			SYNTAX		Integer32
			MAX-ACCESS	read-only
			STATUS		current
			DESCRIPTION
					"The upper bound of the range in 10th of centigrade (Celsius)."
			::= { hm2LogTempHistEntry 3 }

hm2LogTempHistTime	OBJECT-TYPE
			SYNTAX		Integer32
			MAX-ACCESS	read-only
			STATUS		current
			DESCRIPTION
					"The time spent in this range in minutes."
			::= { hm2LogTempHistEntry 4 }

--
-- *************************************************************
-- hm2LogAuditGroup
-- *************************************************************
--

hm2LogAuditTrailComment	OBJECT-TYPE
			SYNTAX		DisplayString (SIZE (0|1..80))
			MAX-ACCESS	read-write
			STATUS		current
			DESCRIPTION
					"Enter a Comment to begin or end a group of entries in the
					 audit trail. Returns an empty string when read."
			DEFVAL			{ "" }
			::= { hm2LogAuditGroup 1 }
			
--
-- *************************************************************
-- hm2LogEmailAlertGroup
-- *************************************************************
--

hm2LogEmailAdminStatus		OBJECT-TYPE
			SYNTAX			HmEnabledStatus
			MAX-ACCESS		read-write
			STATUS			current
			DESCRIPTION		"Admin mode for logging email-alert."
			DEFVAL			{ disable }
			::= { hm2LogEmailAlertGroup 1 }

hm2LogEmailFromAddress		OBJECT-TYPE
			SYNTAX			SnmpAdminString (SIZE (0..255))
			MAX-ACCESS		read-write
			STATUS			current
			DESCRIPTION		"Mail address from which the mail has be sent."
			DEFVAL			{ "" }
			::= { hm2LogEmailAlertGroup 2 }
			
hm2LogEmailLogDuration		OBJECT-TYPE
			SYNTAX			Integer32(30..1440)
			MAX-ACCESS		read-write
			STATUS			current
			DESCRIPTION		"Periodic timer (in minutes) to send an email-alert."
			DEFVAL			{ 30 }
			::= { hm2LogEmailAlertGroup 3 }

hm2LogEmailUrgentSeverity	OBJECT-TYPE
			SYNTAX			HmAgentLogSeverity
			MAX-ACCESS		read-write
			STATUS 			current
			DESCRIPTION 	"Log Severity at/below which the email-alert to be sent immediately."
			DEFVAL			{ alert }
			::= { hm2LogEmailAlertGroup 4 }

hm2LogEmailNonUrgentSeverity	OBJECT-TYPE
			SYNTAX				HmAgentLogSeverity
			MAX-ACCESS			read-write
			STATUS 				current
			DESCRIPTION 		"Log Severity at/below which the log should	be saved
								in a buffer and sent as an email-alert later(In case
								of log duration timeout / log buffer overflow )."
			DEFVAL				{ warning }
			::= { hm2LogEmailAlertGroup 5 }

hm2LogEmailNumEmailsSent	OBJECT-TYPE
			SYNTAX			Counter32 
			MAX-ACCESS		read-only
			STATUS 			current
			DESCRIPTION 	"Number of email alerts that have been sent successfully."
			::= { hm2LogEmailAlertGroup 6 }

hm2LogEmailNumEmailFailures	OBJECT-TYPE
			SYNTAX			Counter32 
			MAX-ACCESS		read-only
			STATUS 			current
			DESCRIPTION 	"Number of email alerts that could not be sent."
			::= { hm2LogEmailAlertGroup 7 }

hm2LogEmailTimeOfLastMailSent  	OBJECT-TYPE
			SYNTAX			HmTimeSeconds1970  
			MAX-ACCESS		read-only
			STATUS 			current
			DESCRIPTION 	"Local system time (hm2SystemLocalTime) when the last mail was sent."
			::= { hm2LogEmailAlertGroup 8 }  

hm2LogEmailAction		   	OBJECT-TYPE
			SYNTAX			INTEGER { 
									  other(1),
									  test(2), 
									  non-urgent(3)
									}
			MAX-ACCESS		read-write
			STATUS 			current
			DESCRIPTION 	"After configuring all email alert settings, set this object 
							to 'test' to sendt a test message to the configured address(es). 
							Setting the object to 'non-urgent' will force the device to 
							immediately sent all buffered logs to the configured email 
							server(s)/address(es). 
							When read the object is read it always returns 'other'. 
							The object can't be set as 'other'."
			::= { hm2LogEmailAlertGroup 9 }
			
hm2LogEmailTestMessageType  OBJECT-TYPE
			SYNTAX			INTEGER { 
									  urgent(1), 
									  non-urgent(2)
									}
			MAX-ACCESS		read-write
			STATUS 			current
			DESCRIPTION 	"Message type for testing email alert functionality."
			DEFVAL			{ urgent }
			::= { hm2LogEmailAlertGroup 10 }
			
hm2LogEmailTestMessageBody  OBJECT-TYPE
			SYNTAX			SnmpAdminString (SIZE (0..255))
			MAX-ACCESS		read-write
			STATUS 			current
			DESCRIPTION 	"Message body for testing email alert functionality."
			DEFVAL			{ "" }
			::= { hm2LogEmailAlertGroup 11 }
			
--
-- *************************************************************			
-- hm2LogEmailToAddressTable
-- *************************************************************
--
hm2LogEmailToAddressTable 		OBJECT-TYPE
			SYNTAX SEQUENCE OF	Hm2LogEmailToAddressEntry
			MAX-ACCESS 			not-accessible
			STATUS 				current
			DESCRIPTION			"The table listing the destination email address and the message type."
			::= { hm2LogEmailAlertGroup 15 }

hm2LogEmailToAddressEntry		OBJECT-TYPE
			SYNTAX			Hm2LogEmailToAddressEntry
			MAX-ACCESS		not-accessible
			STATUS 			current
			DESCRIPTION 	"The table entry listing the destination email address and the message type."
			INDEX { hm2LogEmailToAddrMessageIndex }
			::= { hm2LogEmailToAddressTable 1 }

Hm2LogEmailToAddressEntry::= SEQUENCE {
	hm2LogEmailToAddrMessageIndex		Integer32,			-- index			
	hm2LogEmailToAddrMessageType		INTEGER,			-- log message type
	hm2LogEmailToAddrAddress			SnmpAdminString,	-- email sender address
	hm2LogEmailToAddrEntryStatus		RowStatus			-- to create, change or delete the entry
}

hm2LogEmailToAddrMessageIndex		OBJECT-TYPE
			SYNTAX			Integer32 (1..10)
			MAX-ACCESS		not-accessible
			STATUS 			current
			DESCRIPTION 	"An integer used only for indexing purposes.
	           	   	   	     Generally monotonically increasing from 1 as new
	           	   	   	     addresses are configured. Re-use of values for this 
	           	   	   	     index should be avoided."
			::= { hm2LogEmailToAddressEntry 1 }
			
hm2LogEmailToAddrMessageType		OBJECT-TYPE
			SYNTAX			INTEGER {
									urgent(1), 
									non-urgent(2) }
			MAX-ACCESS		read-create
			STATUS 			current
			DESCRIPTION 	"Log message type."
			DEFVAL		{ urgent }			
			::= { hm2LogEmailToAddressEntry 2 }

hm2LogEmailToAddrAddress			OBJECT-TYPE
			SYNTAX			SnmpAdminString (SIZE (0..255))
			MAX-ACCESS		read-create
			STATUS 			current
			DESCRIPTION 	"Email address to which the email-alert to be sent."
			DEFVAL		{ "" }			
			::= { hm2LogEmailToAddressEntry 3 }

hm2LogEmailToAddrEntryStatus			OBJECT-TYPE
			SYNTAX			RowStatus
			MAX-ACCESS		read-create
			STATUS 			current
			DESCRIPTION 	"Create, change or delete the entry."
			::= { hm2LogEmailToAddressEntry 4 }
		
--
-- *************************************************************			
-- hm2LogEmailSubjectTable
-- *************************************************************
--
hm2LogEmailSubjectTable OBJECT-TYPE
			SYNTAX 	SEQUENCE OF Hm2LogEmailSubjectEntry
			MAX-ACCESS 		not-accessible
			STATUS 			current
			DESCRIPTION		"List of subject of the email for particular message type."
			::= { hm2LogEmailAlertGroup 16 }
				
hm2LogEmailSubjectEntry OBJECT-TYPE
			SYNTAX 			Hm2LogEmailSubjectEntry
			MAX-ACCESS 		not-accessible
			STATUS 			current
			DESCRIPTION		"This entry shows what kind of subject to be used for the given message 	

					type."
			INDEX 			{ hm2LogEmailSubjectMessageType}
			::= { hm2LogEmailSubjectTable 1 }

Hm2LogEmailSubjectEntry ::= SEQUENCE {
			hm2LogEmailSubjectMessageType 	INTEGER,
			hm2LogEmailSubject 				SnmpAdminString,
			hm2LogEmailSubjectEntryStatus 	RowStatus
			}

hm2LogEmailSubjectMessageType OBJECT-TYPE
			SYNTAX 			INTEGER { 
							urgent(1), 
							non-urgent(2)
							}
			MAX-ACCESS 		not-accessible
			STATUS 			current
			DESCRIPTION		"Log message Type"
			::= { hm2LogEmailSubjectEntry 1 }

hm2LogEmailSubject OBJECT-TYPE
			SYNTAX 			SnmpAdminString (SIZE (0..255))
			MAX-ACCESS 		read-create
			STATUS 			current
			DESCRIPTION		"Email subject for given message type."
			DEFVAL 			{ "" }			
			::= { hm2LogEmailSubjectEntry 2}

hm2LogEmailSubjectEntryStatus OBJECT-TYPE
			SYNTAX 			RowStatus
			MAX-ACCESS 		read-create
			STATUS 			current
			DESCRIPTION		"Create, change or delete the entry."
			::= { hm2LogEmailSubjectEntry 3 }			

--
-- *************************************************************			
-- hm2LogEmailMailServerTable
-- *************************************************************
--		
hm2LogEmailMailServerTable OBJECT-TYPE
			SYNTAX SEQUENCE OF 	Hm2LogEmailMailServerEntry
			MAX-ACCESS 		not-accessible
			STATUS 			current
			DESCRIPTION		"The (conceptual) table listing the mail servers."
			::= { hm2LogEmailAlertGroup 17 }

hm2LogEmailMailServerEntry OBJECT-TYPE
			SYNTAX 			Hm2LogEmailMailServerEntry
			MAX-ACCESS 		not-accessible
			STATUS 			current
			DESCRIPTION		"This entry shows the conmfiguration for the mail server(s)."
			INDEX 			{ hm2LogEmailSmtpAddrIndex }
			::= { hm2LogEmailMailServerTable 1 }

Hm2LogEmailMailServerEntry ::= SEQUENCE {
			hm2LogEmailSmtpAddrIndex	Integer32,
			hm2LogEmailSmtpAddrDescr	SnmpAdminString,
			hm2LogEmailSmtpAddrType 	InetAddressType,
			hm2LogEmailSmtpAddr 		InetAddress,
			hm2LogEmailSmtpPort 		InetPortNumber,
			hm2LogEmailSmtpSecurity 	INTEGER,
			hm2LogEmailSmtpLoginID 		SnmpAdminString,
			hm2LogEmailSmtpPassword 	SnmpAdminString,
			hm2LogEmailSmtpEntryStatus 	RowStatus,
			hm2LogEmailSmtpTimeout 		Unsigned32
			}

hm2LogEmailSmtpAddrIndex OBJECT-TYPE
			SYNTAX 			Integer32 (1..5)
			MAX-ACCESS 		not-accessible
			STATUS 			current
			DESCRIPTION		"An integer used only for indexing purposes.
							 Re-use of values for this index is allowed."
			::= { hm2LogEmailMailServerEntry 1 }

hm2LogEmailSmtpAddrDescr OBJECT-TYPE
			SYNTAX 			SnmpAdminString (SIZE (0..255))
			MAX-ACCESS 		read-create
			STATUS 			current
			DESCRIPTION		"The description of the server configured."
			DEFVAL  		{ "" }
			::= { hm2LogEmailMailServerEntry 2 }
			
hm2LogEmailSmtpAddrType OBJECT-TYPE
			SYNTAX 			InetAddressType
			MAX-ACCESS 		read-create
			STATUS 			current
			DESCRIPTION		"Email SMTP address type."
			DEFVAL  		{ ipv4 }
			::= { hm2LogEmailMailServerEntry 3 }

hm2LogEmailSmtpAddr OBJECT-TYPE
			SYNTAX 			InetAddress
			MAX-ACCESS 		read-create
			STATUS 			current
			DESCRIPTION		"SMTP server address."
			DEFVAL  		{ '00000000'H } -- 0.0.0.0
			::= { hm2LogEmailMailServerEntry 4 }

hm2LogEmailSmtpPort OBJECT-TYPE
			SYNTAX 			InetPortNumber
			MAX-ACCESS 		read-create
			STATUS 			current
			DESCRIPTION		"SMTP port number. When this object is set to 0, it resets to factory default port number 25."
			DEFVAL  		{ 25 }
			::= { hm2LogEmailMailServerEntry 5 }

hm2LogEmailSmtpSecurity OBJECT-TYPE
			SYNTAX 			INTEGER {
							none(1), 
							tlsv1(2) 
							}
			MAX-ACCESS 		read-create
			STATUS 			current
			DESCRIPTION		"This is the authentication mechanism that should be used."
			DEFVAL  		{ none }
			::= { hm2LogEmailMailServerEntry 6 }

hm2LogEmailSmtpLoginID OBJECT-TYPE
			SYNTAX 			SnmpAdminString (SIZE (0..255)) 
			MAX-ACCESS 		read-create
			STATUS 			current
			DESCRIPTION		"This user id is used while the switch/router is being authenticated by the SMTP server,
					         if the hm2LogEmailSmtpSecurity is configured to 'tlsv1'."
			DEFVAL  		{ "" }
			::= { hm2LogEmailMailServerEntry 7 }

hm2LogEmailSmtpPassword OBJECT-TYPE
			SYNTAX 			SnmpAdminString (SIZE (0..255))
			MAX-ACCESS 		read-create
			STATUS 			current
			DESCRIPTION		"This password is used while the switch/router is being authenticated by the SMTP server,
							 if the hm2LogEmailSmtpSecurity is configured to 'tlsv1'."
			DEFVAL  		{ "" }
			::= { hm2LogEmailMailServerEntry 8 }

hm2LogEmailSmtpEntryStatus OBJECT-TYPE
			SYNTAX 			RowStatus
			MAX-ACCESS 		read-create
			STATUS 			current
			DESCRIPTION		"Create, change or delete the entry."
			::= { hm2LogEmailMailServerEntry 9 }

hm2LogEmailSmtpTimeout OBJECT-TYPE
			SYNTAX 			Unsigned32 (1..15)
			MAX-ACCESS 		read-create
			STATUS 			current
			DESCRIPTION 	"Time out duration (in seconds) before packets are retransmitted."
			DEFVAL   		{ 3 }
			::= { hm2LogEmailMailServerEntry 10 }

hm2LogEmailClientTlsVersions OBJECT-TYPE
			SYNTAX			Hm2TlsVersions
			MAX-ACCESS		read-write
			STATUS			current
			DESCRIPTION		"The TLS version supported by the email-alert logging client."
			DEFVAL			{{ tlsv1-0, tlsv1-2 }}
			::= { hm2LogEmailAlertGroup  18 }

hm2LogEmailClientTlsCipherSuites OBJECT-TYPE
			SYNTAX			Hm2TlsCipherSuites
			MAX-ACCESS		read-write
			STATUS			current
			DESCRIPTION		"The cipher suite supported by the email-alert logging client."
			DEFVAL			{{
								tls-dhe-rsa-with-aes-128-cbc-sha,
								tls-ecdhe-rsa-with-aes-128-cbc-sha,
								tls-ecdhe-rsa-with-aes-128-gcm-sha256
							}}
			::= { hm2LogEmailAlertGroup  19 }

-- 
-- ***********************************************************
-- hm2LoggingMibNotifications
-- ***********************************************************
--

hm2LogAuditStartNextSector NOTIFICATION-TYPE
    STATUS       current
    DESCRIPTION
                 "A notification shall be sent when the audit trail has filled one
                 sector and starts a new one."
   ::= { hm2LoggingMibNotifications 1 }

hm2LogEmailSendFailed NOTIFICATION-TYPE
	OBJECTS { hm2LogEmailNumEmailFailures }
	STATUS current
	DESCRIPTION
	"Whenever a mail sending to the SMTP server is failed, this trap is sent with a count of how many times the
	 connection to the SMTP server is failed so far."
	::= { hm2LoggingMibNotifications 2 }
			
END

