HM2-PLATFORM-RADIUS-MIB DEFINITIONS ::= BEGIN

-- 
-- ***********************************************************
-- Hirschmann Platform Radius MIB
-- ***********************************************************
--

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, 
    IpAddress, 
    Unsigned32,
    Integer32                           FROM SNMPv2-SMI
    RowStatus, DisplayString            FROM SNMPv2-TC
    InetAddress, InetAddressType        FROM INET-ADDRESS-MIB
    InterfaceIndexOrZero           	    FROM IF-MIB
    hm2PlatformMibs, HmEnabledStatus	FROM HM2-TC-MIB;

hm2PlatformRadius MODULE-IDENTITY
	LAST-UPDATED "201306050000Z" -- June 05, 2013
   	ORGANIZATION "Hirschmann Automation and Control GmbH"
    CONTACT-INFO
        "Postal:     Stuttgarter Str. 45-51
                     72654 Neckartenzlingen
                     Germany
         Phone:      +49 7127 140
         E-mail:     hac.support@belden.com"
    DESCRIPTION
          "The Hirschmann Private Platform2 MIB for Client Radius Authentication and Accounting.
           Copyright (C) 2011-2013. All Rights Reserved."
    -- Revision history.
    REVISION
          "201306050000Z" -- June 05, 2013
    DESCRIPTION
          "Range of hm2AgentRadiusServerRetransmit adjusted.
           Behavior of hm2AgentRadiusServerTimeout, hm2AgentRadiusServerRetransmit,
           hm2AgentRadiusServerDeadtime and hm2AgentRadiusServerSourceIPAddr clarified."
    REVISION
          "201303010000Z" -- March 01, 2013
    DESCRIPTION
          "Shared secret key length updated. Radius source interface related object added."
    REVISION
          "201106210000Z"
    DESCRIPTION
          "Initial version."
    ::= { hm2PlatformMibs 8 }

    --**************************************************************************************
    -- hm2AgentRadiusConfigGroup
    --
    --**************************************************************************************

    hm2AgentRadiusConfigGroup 				 OBJECT IDENTIFIER ::= { hm2PlatformRadius 1 }
    hm2SNMPExtensionRadiusGroup				 OBJECT IDENTIFIER ::= { hm2PlatformRadius 2 }

    hm2AgentRadiusMaxTransmit OBJECT-TYPE
         SYNTAX      Unsigned32 (1..15)
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "Maximum number of retransmissions of a RADIUS request packet"
         DEFVAL { 4 }
         ::= { hm2AgentRadiusConfigGroup 1 }

    hm2AgentRadiusTimeout OBJECT-TYPE
         SYNTAX      Unsigned32 (1..30)
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "Time out duration (in seconds) before packets are retransmitted."
         DEFVAL { 5 }
         ::= { hm2AgentRadiusConfigGroup 2 } 
         
    hm2AgentRadiusAccountingMode OBJECT-TYPE
         SYNTAX      HmEnabledStatus
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "Identifies if RADIUS accounting has been enabled or not."
         DEFVAL { disable }
         ::= { hm2AgentRadiusConfigGroup 3 }
         
    hm2AgentRadiusStatsClear OBJECT-TYPE
         SYNTAX      HmEnabledStatus
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "When set to enable(1), all RADIUS statistics will be reset."
         DEFVAL { disable }
         ::= { hm2AgentRadiusConfigGroup 4 }
         
    hm2AgentRadiusAccountingIndexNextValid OBJECT-TYPE
         SYNTAX      Integer32 (0|1..2147483647)
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Indicates the next valid index into the hm2AgentRadiusAccountingConfigTable 
                     for creation.  If no additional entries are allowed, this will be 0."
         ::= { hm2AgentRadiusConfigGroup 5 }

    --**************************************************************************************
    -- hm2AgentRadiusAccountingConfigTable
    --
    --**************************************************************************************

    hm2AgentRadiusAccountingConfigTable OBJECT-TYPE
         SYNTAX      SEQUENCE OF Hm2AgentRadiusAccountingConfigEntry
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION
                     "Table with information about RADIUS accounting server IP
                     addresses, port numbers and shared secrets. Only one entry is
                     supported at this time."
         ::= { hm2AgentRadiusConfigGroup 6 }

    hm2AgentRadiusAccountingConfigEntry OBJECT-TYPE
         SYNTAX      Hm2AgentRadiusAccountingConfigEntry
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION
                     "Entry consisting of configuration data for a RADIUS accounting server."
         INDEX       { hm2AgentRadiusAccountingServerIndex }
         ::= { hm2AgentRadiusAccountingConfigTable 1 }
         
    Hm2AgentRadiusAccountingConfigEntry ::=
         SEQUENCE {
         hm2AgentRadiusAccountingServerIndex
                 Integer32,
         hm2AgentRadiusAccountingServerAddress
                 InetAddress,
         hm2AgentRadiusAccountingServerAddressType
                 InetAddressType,
         hm2AgentRadiusAccountingPort
                 Unsigned32,
         hm2AgentRadiusAccountingSecret
                 DisplayString,
         hm2AgentRadiusAccountingStatus
                 RowStatus,
         hm2AgentRadiusAccountingServerName
                 DisplayString,
         hm2AgentRadiusAccountingServerAddrType
                 InetAddressType,
         hm2AgentRadiusAccountingServerAddr
                 InetAddress
         }

    hm2AgentRadiusAccountingServerIndex OBJECT-TYPE
         SYNTAX      Integer32 (1..2147483647)
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION
                     "Unique index of the configured RADIUS accounting server.  The next valid
                     value of this object for creation is specified by 
                     hm2AgentRadiusAccountingIndexNextValid."
         ::= { hm2AgentRadiusAccountingConfigEntry 1 }

    hm2AgentRadiusAccountingServerAddress OBJECT-TYPE
         SYNTAX      InetAddress
         MAX-ACCESS  read-create
         STATUS      deprecated
         DESCRIPTION
                     "This object is deprecated in favour of hm2AgentRadiusAccountingServerAddr.
                     IP Address of the configured RADIUS accounting server.
                     This object cannot be changed after creation."
         ::= { hm2AgentRadiusAccountingConfigEntry 2 }
     
   hm2AgentRadiusAccountingServerAddressType OBJECT-TYPE
         SYNTAX      InetAddressType
         MAX-ACCESS  read-create
         STATUS      deprecated
         DESCRIPTION
                     "This object is deprecated in favour of hm2AgentRadiusAccountingServerAddrType.
                     IP Address Type of the configured RADIUS accounting server.
                     This object cannot be changed after creation."
         ::= { hm2AgentRadiusAccountingConfigEntry 3 }

    hm2AgentRadiusAccountingPort OBJECT-TYPE
         SYNTAX      Unsigned32 (0..65535)
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "Port number for the RADIUS accounting server."
         DEFVAL { 1813 }
         ::= { hm2AgentRadiusAccountingConfigEntry 4 }

    hm2AgentRadiusAccountingSecret OBJECT-TYPE
         SYNTAX      DisplayString (SIZE(0|1..64))
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "Configured shared sercret for the RADIUS accounting server."
         ::= { hm2AgentRadiusAccountingConfigEntry 5 }

    hm2AgentRadiusAccountingStatus OBJECT-TYPE
         SYNTAX      RowStatus
         MAX-ACCESS  read-create
         STATUS      current
         DESCRIPTION
                     "Creates or destroys a RADIUS accounting server entry.
                     During creation, the next available index is specified by the
                     hm2AgentRadiusAccountingIndexNextValid object.  Rows creation using
                     a different value for hm2AgentRadiusAccountingServerIndex will fail.
                     
                     active(1)       - This entry is active.
                     notInService(2) - This entry is administratively disabled.
                     notReady(3)     - DNS resolution of host name has failed.
                     createAndGo(4)  - Creates a new entry.
                     createAndWait(5)- Creates a new entry.
                     destroy(6)      - Deletes an entry."
         ::= { hm2AgentRadiusAccountingConfigEntry 6 }

    hm2AgentRadiusAccountingServerName OBJECT-TYPE
         SYNTAX      DisplayString (SIZE(1..32))
         MAX-ACCESS  read-create
         STATUS      current
         DESCRIPTION
                     "Configured identification name for the RADIUS accounting
                      server."
         ::= { hm2AgentRadiusAccountingConfigEntry 7 }

    hm2AgentRadiusAccountingServerAddrType OBJECT-TYPE
         SYNTAX      InetAddressType
         MAX-ACCESS  read-create
         STATUS      current
         DESCRIPTION
                     "Inet address type of the configured RADIUS accounting server.
                     This object cannot be changed after creation."
         ::= { hm2AgentRadiusAccountingConfigEntry 248 }

    hm2AgentRadiusAccountingServerAddr OBJECT-TYPE
         SYNTAX      InetAddress
         MAX-ACCESS  read-create
         STATUS      current
         DESCRIPTION
                     "Inet address of the configured RADIUS accounting server.
                     This object cannot be changed after creation."
         ::= { hm2AgentRadiusAccountingConfigEntry 249 }

    --**************************************************************************************
    
    hm2AgentRadiusServerIndexNextValid OBJECT-TYPE
         SYNTAX      Integer32 (0|1..2147483647)
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Indicates the next valid index into the hm2AgentRadiusServerConfigTable 
                     for creation.  If no additional entries are allowed, this will be 0."
         ::= { hm2AgentRadiusConfigGroup 7 }
    
    --**************************************************************************************
    -- hm2AgentRadiusServerConfigTable
    --
    --**************************************************************************************

    hm2AgentRadiusServerConfigTable OBJECT-TYPE
         SYNTAX      SEQUENCE OF Hm2AgentRadiusServerConfigEntry
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION
                     "Table with information about RADIUS authentication server IP
                     addresses, port numbers and shared secrets."
         ::= { hm2AgentRadiusConfigGroup 8 }

    hm2AgentRadiusServerConfigEntry OBJECT-TYPE
         SYNTAX      Hm2AgentRadiusServerConfigEntry
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION
                     "Entry consisting of configuration data for a RADIUS 
                     authentication server."
         INDEX       { hm2AgentRadiusServerIndex }
         ::= { hm2AgentRadiusServerConfigTable 1 }
         
    Hm2AgentRadiusServerConfigEntry ::=
         SEQUENCE {
         hm2AgentRadiusServerIndex
                 Integer32,
         hm2AgentRadiusServerAddressType
                 InetAddressType,
         hm2AgentRadiusServerPort
                 Unsigned32,
         hm2AgentRadiusServerSecret
                 DisplayString,
         hm2AgentRadiusServerPrimaryMode
                 HmEnabledStatus,
         hm2AgentRadiusServerCurrentMode
                 INTEGER,
         hm2AgentRadiusServerMsgAuth
                 HmEnabledStatus,
         hm2AgentRadiusServerRowStatus
                 RowStatus,
         hm2AgentRadiusServerName
                 DisplayString,
         hm2AgentRadiusServerInetAddress
                 InetAddress,
         hm2AgentRadiusServerTimeout               
                 Unsigned32,
         hm2AgentRadiusServerRetransmit            
                 Unsigned32,
         hm2AgentRadiusServerDeadtime              
                 Unsigned32,
         hm2AgentRadiusServerSourceIPAddr          
                 IpAddress,
         hm2AgentRadiusServerPriority              
                 Unsigned32,
         hm2AgentRadiusServerUsageType             
                 INTEGER,
         hm2AgentRadiusServerInetAddrType
                 InetAddressType,
         hm2AgentRadiusServerInetAddr
         		 InetAddress
         }

    hm2AgentRadiusServerIndex OBJECT-TYPE
         SYNTAX      Integer32 (1..2147483647)
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION
                     "Unique index of the configured RADIUS server"
         ::= { hm2AgentRadiusServerConfigEntry 1 }
  
    hm2AgentRadiusServerAddressType OBJECT-TYPE
         SYNTAX      InetAddressType
         MAX-ACCESS  read-create
         STATUS      deprecated
         DESCRIPTION
                     "This object is deprecated in favour of hm2AgentRadiusServerInetAddrType.
                     IP Address Type of the configured RADIUS server.
                     This object cannot be changed after creation."
         ::= { hm2AgentRadiusServerConfigEntry 3 }

    hm2AgentRadiusServerPort OBJECT-TYPE
         SYNTAX      Unsigned32 (0..65535)
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "Port number for the RADIUS server."
         DEFVAL { 1812 }
         ::= { hm2AgentRadiusServerConfigEntry 4 }

    hm2AgentRadiusServerSecret OBJECT-TYPE
         SYNTAX      DisplayString (SIZE(0|1..64))
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "Configured shared sercret for the RADIUS server."
         ::= { hm2AgentRadiusServerConfigEntry 5 }

    hm2AgentRadiusServerPrimaryMode OBJECT-TYPE
         SYNTAX      HmEnabledStatus
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "Configure the RADIUS server to be the primary server. If there is any 
                     other server that is configured to be primary, that server is set to be 
                     a seconday server and this entry is set primary."
         ::= { hm2AgentRadiusServerConfigEntry 6 }

    hm2AgentRadiusServerCurrentMode OBJECT-TYPE
         SYNTAX      INTEGER {
                     yes(1),
                     no(2)
                     }
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Indicate if the RADIUS server is the current server in use for
                     authentication."
         ::= { hm2AgentRadiusServerConfigEntry 7 }

    hm2AgentRadiusServerMsgAuth OBJECT-TYPE
         SYNTAX      HmEnabledStatus
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "Enable or disable the message authenticator attribute for this 
                     RADIUS server."
         ::= { hm2AgentRadiusServerConfigEntry 8 }

    hm2AgentRadiusServerRowStatus OBJECT-TYPE
         SYNTAX      RowStatus
         MAX-ACCESS  read-create
         STATUS      current
         DESCRIPTION
                     "Creates or destroys a RADIUS authentication server entry.
                     During creation, the next available index is specified by the
                     hm2AgentRadiusServerIndexNextValid object.  Rows creation using
                     a different value for hm2AgentRadiusServerIndex will fail.
                     
                     active(1)       - This entry is active.
                     notInService(2) - This entry is administratively disabled.
                     notReady(3)     - DNS resolution of host name has failed.
                     createAndGo(4)  - Creates a new entry.
                     createAndWait(5)- Creates a new entry.
                     destroy(6)      - Deletes an entry."
         ::= { hm2AgentRadiusServerConfigEntry 9 }

    hm2AgentRadiusServerName OBJECT-TYPE
         SYNTAX      DisplayString (SIZE(1..32))
         MAX-ACCESS  read-create
         STATUS      current
         DESCRIPTION
                     "Configured identification name for the RADIUS server."
         ::= { hm2AgentRadiusServerConfigEntry 10 }

    hm2AgentRadiusServerInetAddress OBJECT-TYPE
         SYNTAX      InetAddress
         MAX-ACCESS  read-create
         STATUS      deprecated
         DESCRIPTION
                     "This object is deprecated in favour of hm2AgentRadiusServerInetAddr.
                     IP Address of the configured RADIUS server.
                     This object cannot be changed after creation."
         ::= { hm2AgentRadiusServerConfigEntry 11 }
  
    hm2AgentRadiusServerTimeout            OBJECT-TYPE
         SYNTAX      Unsigned32 (1..30)
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "Time out duration (in seconds) before packets are retransmitted.
                      Note that hm2AgentRadiusTimeout will override this MIB object:
                      - During row creation, hm2AgentRadiusTimeout specifies the default value.
                      - Writing to hm2AgentRadiusTimeout will also update the value of this MIB
                        object for all existing rows."
         ::= { hm2AgentRadiusServerConfigEntry 12 }

    hm2AgentRadiusServerRetransmit         OBJECT-TYPE
         SYNTAX      Unsigned32 (1..15)
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "Maximum number of retransmissions of a RADIUS request packet																																													
                      Note that hm2AgentRadiusMaxTransmit will override this MIB object:
                      - During row creation, hm2AgentRadiusMaxTransmit specifies the default value.
                      - Writing to hm2AgentRadiusMaxTransmit will also update the value of this MIB
                        object for all existing rows."
         ::= { hm2AgentRadiusServerConfigEntry 13 }

    hm2AgentRadiusServerDeadtime         OBJECT-TYPE
         SYNTAX      Unsigned32 (0..2000)
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "Length of time (in minutes) for which a RADIUS server is skipped over by transaction requests.
                      Note that hm2AgentRadiusDeadTime will override this MIB object:
                      - During row creation, hm2AgentRadiusDeadTime specifies the default value.
                      - Writing to hm2AgentRadiusDeadTime will also update the value of this MIB
                        object for all existing rows."
         ::= { hm2AgentRadiusServerConfigEntry 14 }

    hm2AgentRadiusServerSourceIPAddr       OBJECT-TYPE
         SYNTAX      IpAddress
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "Source IP address that will be used for the communication with RADIUS servers.
                      Note that hm2AgentRadiusSourceIPAddr will override this MIB object:
                      - During row creation, hm2AgentRadiusSourceIPAddr specifies the default value.
                      - Writing to hm2AgentRadiusSourceIPAddr will also update the value of this MIB
                        object for all existing rows."
         ::= { hm2AgentRadiusServerConfigEntry 15 }

    hm2AgentRadiusServerPriority   OBJECT-TYPE
         SYNTAX      Unsigned32 (0..65535)
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "Priority specifies the order in which the servers will be used, where 0 is the highest
                     priority in radius server config mode."
         DEFVAL { 0 }
         ::= { hm2AgentRadiusServerConfigEntry 16 }

    hm2AgentRadiusServerUsageType OBJECT-TYPE
         SYNTAX      INTEGER {
                     all(1),
                     login(2),
                     dot1x(3)
                     }
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "Specify the usage type of the server."
         DEFVAL  { all }
         ::= { hm2AgentRadiusServerConfigEntry 17 }

    hm2AgentRadiusServerInetAddrType OBJECT-TYPE
         SYNTAX      InetAddressType
         MAX-ACCESS  read-create
         STATUS      current
         DESCRIPTION
                     "Inet address type of the configured RADIUS server.
                     This object cannot be changed after creation."
         ::= { hm2AgentRadiusServerConfigEntry 248 }
         
    hm2AgentRadiusServerInetAddr OBJECT-TYPE
         SYNTAX      InetAddress
         MAX-ACCESS  read-create
         STATUS      current
         DESCRIPTION
                     "Inet address of the configured RADIUS server.
                     This object cannot be changed after creation."
         ::= { hm2AgentRadiusServerConfigEntry 249 }

    --**************************************************************************************

    hm2AgentRadiusAuthenticationServers OBJECT-TYPE
         SYNTAX      Unsigned32 
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Number of RADIUS authentication servers that have been configured."         
         ::= { hm2AgentRadiusConfigGroup 9 }
    
    hm2AgentRadiusAccountingServers OBJECT-TYPE
         SYNTAX      Unsigned32 
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Number of RADIUS accounting servers that have been configured."         
         ::= { hm2AgentRadiusConfigGroup 10 }
    
    hm2AgentRadiusNamedAuthenticationServerGroups OBJECT-TYPE
         SYNTAX      Unsigned32 
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Number of configured RADIUS named authentication server groups."         
         ::= { hm2AgentRadiusConfigGroup 11 }
    
    hm2AgentRadiusNamedAccountingServerGroups OBJECT-TYPE
         SYNTAX      Unsigned32 
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                     "Number of configured RADIUS named accounting server groups."         
         ::= { hm2AgentRadiusConfigGroup 12 }
    
    hm2AgentRadiusDeadTime OBJECT-TYPE
         SYNTAX      Unsigned32 (0..2000)
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "Length of time (in minutes) for which a RADIUS server is skipped over by transaction requests."
         DEFVAL { 0 }
         ::= { hm2AgentRadiusConfigGroup 13 }

    hm2AgentRadiusSourceIPAddr OBJECT-TYPE
         SYNTAX      IpAddress
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "Source IP address that will be used for the communication with RADIUS servers."
         DEFVAL 	{ '00000000'H }
         ::= { hm2AgentRadiusConfigGroup 15 }

    hm2AgentRadiusNasIpAddress OBJECT-TYPE
         SYNTAX      IpAddress
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "Used to set the NAS-IP address for the radius server."
         DEFVAL 	{ '00000000'H }
         ::= { hm2AgentRadiusConfigGroup  16 }

    hm2AgentAuthorizationNetworkRadiusMode OBJECT-TYPE
         SYNTAX      HmEnabledStatus
         MAX-ACCESS  read-write
         STATUS      current
         DESCRIPTION
                     "Used to enable/disable VLAN assignment mode."
         DEFVAL  { disable }
         ::= { hm2AgentRadiusConfigGroup 17}

   hm2AgentRadiusSourceInterface OBJECT-TYPE
       SYNTAX      InterfaceIndexOrZero
       MAX-ACCESS  read-write
       STATUS      current
       DESCRIPTION
               "A source-interface selection on an Interface Index (like vlan based
               routing interface, port based routing interface, loopback interface).
               A non-zero value indicates ifIndex for the corresponding interface 
               entry in the ifTable is selected. A zero value indicates the 
               source-interface un-selection.
               The frames will not necessarily be sent on this interface, only the
               IP address of the interface will be used as source."
       DEFVAL { 0 }
       ::= { hm2AgentRadiusConfigGroup 18 }

    --**************************************************************************************
    -- hm2SNMPExtensionRadiusGroup
    --**************************************************************************************

   hm2SNMPExtensionRadiusVLANAssignModeInvalid OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "Indicates that the VLAN assignment mode contains an invalid value. It can
                       only be enabled or disabled."
           ::= { hm2SNMPExtensionRadiusGroup 1 }

   hm2SNMPExtensionRadiusServerDeadTimeInvalid OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "Indicates that the radius authentication server entry contains
                        an invalid value for dead time that cannot be processed."
           ::= { hm2SNMPExtensionRadiusGroup 2 }

   hm2SNMPExtensionRadiusServerSecretInvalid OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "Indicates that the radius authentication server entry contains
                        an invalid value for secret that cannot be processed."
           ::= { hm2SNMPExtensionRadiusGroup 3 }

   hm2SNMPExtensionRadiusServerPrimaryModeInvalid OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "Indicates that the radius authentication server entry contains
                        an invalid value for primary server that cannot be processed."
           ::= { hm2SNMPExtensionRadiusGroup 4 }

   hm2SNMPExtensionRadiusServerNameInvalid OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "Indicates that the radius authentication server entry contains
                        an invalid value for server name that cannot be processed."
           ::= { hm2SNMPExtensionRadiusGroup 5 }

   hm2SNMPExtensionRadiusRetransmitInvalid OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "Indicates that the radius global entry contains an invalid value
                        for retransmits (max.) that cannot be processed."
           ::= { hm2SNMPExtensionRadiusGroup 6 }

   hm2SNMPExtensionRadiusTimeoutInvalid OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "Indicates that the radius global entry contains an invalid value
                        for timeout(s) that cannot be processed."
           ::= { hm2SNMPExtensionRadiusGroup 7 }

   hm2SNMPExtensionRadiusNASIPAddrInvalid OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "Indicates that the radius global entry contains an invalid value
                        for NAS IP address(attribute 4) that cannot be processed."
           ::= { hm2SNMPExtensionRadiusGroup 8 }

   hm2SNMPExtensionRadiusServerMSGAuthInvalid OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "Indicates that the message authenticator contains an invalid value. It can
                       only be enabled or disabled."
           ::= { hm2SNMPExtensionRadiusGroup 9 }

   hm2SNMPExtensionRadiusServerUsageTypeInvalid OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "Indicates that the entry for server usage type is invalid. It can
                       only have values 'all' or 'login'."
           ::= { hm2SNMPExtensionRadiusGroup 10 }

END
