
            S O F T W A R E - R E L E A S E - D O C U M E N T

                 Hirschmann Automation and Control GmbH
              
            	      GRS106 Release 09.4.04
            		
                            2024/06/20
             		
                          C O N T E N T S
                          ===============


    1.   Limitations of the release GRS106 09.4.04
    2.   Supported Hardware
    3.   History of Changes



This document is delivered with the software in the file 
"Readme_GRS106.09.4.04.txt".



.-----------------------------------------------------------------------------.
| For superior functions like software update,                                |
| supported web browser and limitations of the platform release 09.4.04       |
| please read the document Readme_09.4.04.txt.                                |
'-----------------------------------------------------------------------------'



1. Limitations of the release GRS106 09.4.04
==============================================

USB-C: The Out-of-Band management interface exclusively supports CLI access via
     terminal emulation.

Port capabilities: Based on hardware configuration, ports 1/1 - 1/4 on GRS115/116
     will exclusively support 10G and/or 1G speeds.

Port capabilities: Based on hardware configuration, ports 1/1 - 1/4 on GRS115/116
     will support frame sizes of up to 10240 bytes.

MACsec: GRS115/116 are MACsec hardware ready with software functionality enabled
     in a future release.


2. Supported Hardware
=====================
This platform software release 09.4.04 is released exclusively for the 
following hardware:

HiOS-GRS-09404.bin:
- GRS105-6F8F16T       (Since SW 08.9.00)
- GRS105-6F8T16T       (Since SW 08.9.00)
- GRS106-6F8F16T       (Since SW 08.9.00)
- GRS106-6F8T16T       (Since SW 08.9.00)
- GRS115-6F8F16T       (Since SW 09.1.00)
- GRS115-6F8T16T       (Since SW 09.1.00)
- GRS116-6F8F16T       (Since SW 09.1.00)
- GRS116-6F8T16T       (Since SW 09.1.00)


Supported Software Level:
- 2S                   (GRS...2S, GRS...2A)
- 2A                   (GRS...2A)
- 3A                   (Unicast Routing)

For information on supported accessories, refer to the "User Manual Installation".
You will find the manuals under "https://www.doc.hirschmann.com".

3. History of Changes
=====================

Software Release 08.9.00
------------------------
First Version

New Functions:
- Humidity Sensor
- Responsive GUI

Software Release 09.0.00
------------------------
Bugfixes (see Issue List)

Software Level 2A:
- Double VLAN Tagging 

Software Release 09.1.00
------------------------
Bugfixes (see Issue List)

New Functions:
- EtherNet/IP
- VLAN configuration for EtherNet/IP
- Modbus TCP
- PROFINET, spec 2.41 compliant
- Signed firmware images
- Update 802.1X to Version 2010
- LLDP IPv6 Support

Software Release 09.2.00
------------------------
Bugfixes (see Issue List)

New Functions:
- SNMPv3 Traps

Software Level 2A:
- SNMPv1/v2 Read-Only
- Interface Shutdown via Tracking

Software Release 09.4.00
------------------------
Bugfixes (see Issue List)

New Functions:
- SNMPv3 Traps (GUI)

Software Level 3A:
- L3A UR

Software Release 09.4.04
------------------------
Bugfixes (see Issue List)
